$VDEV | Back to Index page

| Prolog Control Block Contents $VDEV DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

$VDEV Prolog | Top of page

     NAME       : LGRVDEV
     DESCRIPTION: Relocation mapping for HCPVDEV
     DSECT      : $VDEV
     FUNCTION   : LGRVDEV describes those fields of the VDEV that
                  will be migrated to the destination system during
                  guest relocation.
     LOCATED BY : This is a mapping of the RDODATA area within the
                  RDOBK during guest relocation.
     CREATED BY : HCPRLFVF - VDEV Formatter for LGR
     DELETED BY : HCPRLDRL - Release storage associated with an RDP
     RELOCATION CONSIDERATIONS : This control block is used during live guest
                  relocation.  It is used to relocate a control block
                  defined in a corresponding HCP COPY file.  Any
                  fields or bits defined in HCPVDEV which are
                  required on the destination system must be defined
                  here, and code must be added to migrate the field
                  or bit during a relocation.

$VDEV Control Block Content | Top of page

     $VDEV DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      $VDEV          Relocation mapping for HCPVDEV
              00000003       $VDEV_VER      3 $VDEV mapping version.
                                            $VDEV_VER is independent of the
                                            CP level and need only be changed
                                            when this DSECT is changed. The
                                            convention is to increment by 1.
    0000    0 Signed       2 $VDEV_HDRL     Header length (in bytes)
    0002    2 Signed       2 $VDEV_BITL     Length of mapped bits (in bytes)
    0004    4 Signed       4 *              Reserved for future use
              00000008       $VDEV_HDLN     *-$VDEV Length of header (bytes)
          Bit map: Contains the VDEV flags that are subject to
                   relocation. These bits are defined sequentially,
                   regardless of how they are defined in HCPVDEV.
                   This yields a consistent mapping that ensures
                   compatibility when a guest is relocated between
                   systems at differing service levels.
                   Names in the comments column indicate the control
                   block byte which contains the flag. This name is
                   subject to change if the flag definition changes.
             ====> NEVER change bits which already exist here.
             ====> NEVER change the order of bits in this section.
             ====> ALWAYS add new bits at the end of this section,
                   together with new flag bytes as required.
    0008    8 Signed       2 $VDEV_BITS (0) Bit map area
    0008    8 Bitstring    1 $VDEV0
              1... ....      $VDEVBUSY      X'80' $VDEVBUSY ALL VDEVSTAT
              .1.. ....      $VDEVPRCE      X'40' $VDEVPRCE ALL VDEVSTAT
              ..1. ....      $VDEVCLRF      X'20' $VDEVCLRF ALL VDEVSTAT
              ...1 ....      $VDEVHLTF      X'10' $VDEVHLTF ALL VDEVSTAT
              .... 1...      $VDEVSUSP      X'08' $VDEVSUSP ALL VDEVSTAT
              .... .1..      $VDEVRPND      X'04' $VDEVRPND ALL VDEVSTAT
              .... ..1.      $VDEVQUED      X'02' $VDEVQUED ALL VDEVSTAT
              .... ...1      $VDEVCATT      X'01' $VDEVCATT ALL VDEVSTAT
    0009    9 Bitstring    1 $VDEV1
              1... ....      $VDEVIMRS      X'80' $VDEVIMRS ALL VDEVWAIT
              .1.. ....      $VDEVWINT      X'40' $VDEVWINT ALL VDEVWAIT
              ..1. ....      $VDEVIOPQ      X'20' $VDEVIOPQ QDIO VDEVIOP1
              ...1 ....      $VDEVNSIM      X'10' $VDEVNSIM VNET VDEVVNET
              .... 1...      $VDEVINTV      X'08' $VDEVINTV ALL VDEVAFLG
              .... .1..      $VDEVDED       X'04' $VDEVDED ALL VDEVAFLG
              .... ..1.      $VDEVFULL      X'02' $VDEVFULL DASD VDEVAFLG
              .... ...1      $VDEVDVFP      X'01' $VDEVDVFP DASD VDEVFFLG
    000A   10 Bitstring    1 $VDEV2
              1... ....      $VDEVBPCI      X'80' $VDEVBPCI ALL VDEVBFLG
              .1.. ....      $VDEVBSUI      X'40' $VDEVBSUI ALL VDEVBFLG
              ..1. ....      $VDEVQACT      X'20' $VDEVQACT QDIO VDEVBFLG
              ...1 ....      $VDEVVMIO      X'10' $VDEVVMIO ALL VDEVBFLG
              .... 1...      $VDEVBCC0      X'08' $VDEVBCC0 ALL VDEVBFLG
              .... .1..      $VDEVRO        X'04' $VDEVRO ALL VDEVDFLG
              .... ..1.      $VDEVRSRL      X'02' $VDEVRSRL ALL VDEVDFLG
              .... ...1      $VDEVNSEG      X'01' $VDEVNSEG DASD VDEVDFLG
    000B   11 Bitstring    1 $VDEV3
              1... ....      $VDEVINT3      X'80' $VDEVINT3 CONS VDEVCFLG
              .1.. ....      $VDEVPPA1      X'40' $VDEVPPA1 CONS VDEVCFLG
              ..1. ....      $VDEVGSUS      X'20' $VDEVGSUS CONS VDEVCFLG
              ...1 ....      $VDEVDING      X'10' $VDEVDING CONS VDEVCFLG
              .... 1...      $VDEVATTN      X'08' $VDEVATTN CONS VDEVCFLG
              .... .1..      $VDEVBRGS      X'04' $VDEVBRGS CONS VDEVCFLG
              .... ..1.      $VDEVLNKS      X'02' $VDEVLNKS DASD VDEVFFLG
              .... ...1      $VDEVLNKE      X'01' $VDEVLNKE DASD VDEVFFLG
    000C   12 Bitstring    1 $VDEV4
              1... ....      $VDEVQDSK      X'80' $VDEVQDSK DASD VDEVFFLG
              .1.. ....      $VDEVFBA       X'40' $VDEVFBA DASD VDEVFFLG
              ..1. ....      $VDEVNRSM      X'20' $VDEVNRSM DASD VDEVPFLG
              ...1 ....      $VDEVDPRE      X'10' $VDEVDPRE ALL VDEVPFLG
              .... .1..      $VDEVTENB      X'04' $VDEVTENB TAPE VDEVPFLG
              .... ..1.      $VDEVSHRD      X'02' $VDEVSHRD TAPE VDEVPFLG
              .... ...1      $VDEVMBSF      X'01' $VDEVMBSF QDIO VDEVBFLG
    000D   13 Bitstring    1 $VDEV5
              1... ....      $VDEVPVBA      X'80' $VDEVPVBA DASD VDEVPVFG
              .1.. ....      $VDEVPVAL      X'40' $VDEVPVAL DASD VDEVPVFG
              ..1. ....      $VDEVHPAL      X'20' $VDEVHPAL DASD VDEVPVFG
              ...1 ....      $VDEVHPBA      X'10' $VDEVHPBA DASD VDEVPVFG
              .... 1...      $VDEVRFID      X'08' $VDEVRFID DASD VDEVSFLG
              .... .1..      $VDEVSCPI      X'04' $VDEVSCPI DASD VDEVSFLG
              .... ...1      $VDEVNODT      X'01' $VDEVNODT ALL VDEVLGRI
    000E   14 Bitstring    1 $VDEV6
              1... ....      $VDEVCNA       X'80' $VDEVCNA DASD VDEVMNGT
              .1.. ....      $VDEVSCTL      X'40' $VDEVSCTL DASD VDEVMNGT
              ..1. ....      $VDEVDCTL      X'20' $VDEVDCTL DASD VDEVMNGT
              ...1 ....      $VDEVNCTL      X'10' $VDEVNCTL DASD VDEVMNGT
              .... 1...      $VDEVSWDD      X'08' $VDEVSWDD VNET VDEVSWFL
              .... .1..      $VDEVD2A8      X'04' $VDEVD2A8 VNET VDEVSWFL
              .... ..1.      $VDEVIFCC      X'02' $VDEVIFCC QDIO VDEVLGRI
              .... ...1      $VDEVSSNT      X'01' $VDEVSSNT DASD VDEVSSNT
          NOTES      : $VDEV7 bits do NOT map to VDEV bits
    000F   15 Bitstring    1 $VDEV7
              1... ....      $VDEVCONS      X'80' $VDEVCONS CONS This is the
                                            VIRTUAL CONSOLE
              .1.. ....      $VDEVNICB      X'40' $VDEVNICB VNET This is a
                                            BASE NIC
              ..1. ....      $VDEVISMD      X'20' $VDEVISMD MDISK This is an
                                            MDISK
              .... 1...      $VDEVOSAB      X'08' $VDEVOSAB OSA This is a
                                            base OSA
              .... .1..      $VDEVOSAN      X'04' $VDEVOSAN OSA This is a
                                            non-base OSA
              .... ..1.      $VDEVQESB      X'02' $VDEVQESB OSA/FCP QEBSM
                                            enabled on source
          NOTES      : $VDEV8 bits do NOT map to VDEV bits
    0010   16 Bitstring    1 $VDEV8         Flags unique to LGRVDEV
              1... ....      $VDEVNOAS      X'80' $VDEVNOAS TAPE
                                            RDEVTPFG,RDEVNOAS
              .1.. ....      $VDEVNOMS      X'40' $VDEVNOMS TAPE
                                            RDEVTPFG,RDEVNOMS
              ..1. ....      $VDEVENCR      X'20' $VDEVENCR TAPE
                                            RDEVTPF2,RDEVENCR
              ...1 ....      $VDEVURAC      X'10' $VDEVURAC FCP
                                            RDEVFCLN,RDEVURAC
              .... 1...      $VDEVRECC      X'08' $VDEVRECC MDISK
                                            MDIMDCFL,MDIRECAC
              .... .1..      $VDEVWKAL      X'04' $VDEVWKAL MDISK
                                            MDISTAT,MDIWRKAL
              .... ..1.      $VDEVMDCA      X'02' $VDEVMDCA MDISK
                                            MDIMDCFL,MDIMDCA
              .... ...1      $VDEVMDCD      X'01' $VDEVMDCD MDISK
                                            MDIMDCFL,MDIMDCD
    0011   17 Bitstring    1 $VDEV9
              1... ....      $VDEV1END      X'80' $VDEV1END DASD
                                            VDEVSFLG,VDEV1END
    0012   18 Bitstring    7 *              RESERVED FOR FUTURE USE
              00000011       $VDEV_BLEN     *-$VDEV_BITS Length of bit map
                                            area
          Data:    Contains all HCPVDEV data that is subject to
                   relocation, except for flag bits, which are
                   handled separately.
                   All fields are defined as XLnn to avoid alignment
                   warnings and to pack the data efficiently.
             ====> NEVER change fields which already exist here.
             ====> NEVER change the order of fields in this section.
             ====> ALWAYS add new fields at the end of this section.
                   together with new flag bytes as required.
    0019   25 Bitstring    1 $VDEV_DATA (0) Start of data map
    0019   25 Bitstring    4 $VDEVFPNT      ALL Forward interruption pointer
    001D   29 Bitstring    4 $VDEVBPNT      ALL Backward interruption pointer
    0021   33 Bitstring    2 $VDEVSUB       ALL Virtual subchannel number
    0023   35 Bitstring    1 $VDEVCLAS      ALL Device class
    0024   36 Bitstring    1 $VDEVTYPE      ALL Device Type
    0025   37 Bitstring   28 $VDEVPMCW (0)  ALL Path Managment Control Word
    0025   37 Bitstring    4 $VDEVINTP      ALL Interrupt parameter
    0029   41 Bitstring    2 *              ALL IRCF and CTL
    002B   43 Bitstring    2 $VDEVDEV       ALL Virtual Device Number
    002D   45 Bitstring   20 *              ALL Rest of PMCW
    0041   65 Bitstring    4 $VDEVNIOR      ALL HLA of SSCH pending IORBK
    0045   69 Bitstring    4 $VDEVSIOR      ALL HLA of IORBK holding sense
                                            data
    0049   73 Bitstring    4 $VDEVPIOR      ALL HLA of Pending interrupt
                                            IORBK
    004D   77 Bitstring    4 $VDEVAEVT      DASD Pointer to list of asych
                                            events
    0051   81 Bitstring    4 $VDEVIOCT      ALL Count of virtual I/O requests
                                            issued
    0055   85 Bitstring    4 $VDEVTMCT      ALL Count of virtual Transport
                                            Mode I/O requests issued
    0059   89 Bitstring    8 $VDEVTIME      ALL TOD Clock at device creation
    0061   97 Bitstring    4 $VDEVUIOR      ALL Pending unsol IORBK,came in
                                            after UC
    0065  101 Bitstring    4 $VDEVIOCA      ALL Count of actual I/Os
                                            initiated by CP
    0069  105 Bitstring    1 $VDEVMODL      ALL Virtual device model number
    006A  106 Bitstring    1 $VDEVCPIE      ALL Channel path in error mask
    006B  107 Bitstring    1 $VDEVCRDR      ALL Count of I/O redrives to
                                            simulation
    006C  108 Bitstring    1 $VDEVLCNT      ALL Current line count
    006D  109 Bitstring    3 $VDEVLTOD      ALL Bytes 2-4 of TOD clock when
                                            LCNT reset
    0070  112 Bitstring    4 $VDEVBKIA      DASD BKIBK address
    0074  116 Bitstring    1 $VDEVPMSK      ALL Quiesce/Resume message path
                                            mask
    0075  117 Bitstring    8 $VDEVMBLK      ALL 64-bit measurement block
                                            address
    007D  125 Bitstring    4 $VDEVGCHR      ALL Guest Characteristics
                  FIELDS FROM DASD SPECIFIC AREA OF VDEV
    0081  129 Bitstring    4 $VDEVPOSN      DASD Virtual DASD Arm position
    0085  133 Bitstring    4 $VDEVSEXT      DASD Minidisk Start of EXTent
                                            (cyls or blks)
    0089  137 Bitstring    4 $VDEVEEXT      DASD Minidisk End of EXTent (cyls
                                            or blks)
                  FIELDS FROM TAPE SPECIFIC AREA OF VDEV
    008D  141 Bitstring    4 $VDEVDYPT      TAPE Pointer to Tape Pathing
                                            control block
                  FIELDS FROM CTCA SPECIFIC AREA OF VDEV
    0091  145 Bitstring    8 $VDEVCUSR      CTCA Restricted USERID for
                                            coupling
    0099  153 Bitstring    4 $VDEVCTCD      CTCA CTCA designation
                  FIELDS FROM SPOOL Console / Unit Record
                         SPECIFIC AREA OF VDEV
    009D  157 Bitstring    4 $VDEVVSP       CONS Virtual Spool Block address
    00A1  161 Bitstring    4 $VDEVVPX       CONS PRT Extension Block address
    00A5  165 Bitstring    4 $VDEVVDS       CONS Device Simulation pointer
                  FIELDS COPIED FROM NON-VDEV CONTROL BLOCKS
    00A9  169 Bitstring    1 $VDEVIDSZ      ALL Byte length of DUID/EQID
    00B0  176 Dbl-Word     8 $VDEVID (5)    ALL EQID/DUID
    00D8  216 Bitstring    1 $VDEVKYA1      TAPE First KEY attribute
    00D9  217 Bitstring   64 $VDEVKYL1      TAPE First KEY
    0119  281 Bitstring    1 $VDEVKYA2      TAPE Second KEY attribute
    011A  282 Bitstring   64 $VDEVKYL2      TAPE Second KEY
    015A  346 Bitstring    8 $VDEVURFI      FCP = RDEVURAC
    0162  354 Bitstring    2 $VDEVPBAS      DASD Base VDEV devno
                                            (PAV/HYPERPAV)
    0164  356 Bitstring    1 *              Reserved for IBM use
    0165  357 Bitstring    1 $VDEVSRCV      Version on source system. If 0,
                                            then source is pre-6.3 level.
              00000001       $VDEV_S63      1 Source at release 6.3 or later
    0166  358 Bitstring    4 $VDEV_PTRSH    VDisk ASCPTRSH Copy
    016A  362 Bitstring    4 $VDEV_CSPST    VDisk ASCCSPST Copy
    016E  366 Bitstring    4 $VDEV_CSPGR    VDisk ASCCSPGR Copy
    0172  370 Bitstring    4 $VDEV_CSPGW    VDisk ASCCSPGW Copy
    0176  374 Bitstring    4 $VDEV_CSXRD    VDisk ASCCSXRD Copy
    017A  378 Bitstring    4 $VDEV_CSXWT    VDisk ASCCSXWT Copy
    017E  382 Bitstring    4 $VDEV_CSMIG    VDisk ASCCSMIG Copy
          MDISK fields needed to create an MDISK on the destination.
    0182  386 Bitstring    8 $VDEVOUSER     MDISK MDIOUSER copy
    018A  394 Bitstring    2 $VDEVOVDEV     MDISK MDIOVDEV copy
          This array is used to hold the subchannel IDs for a base
          NIC and all associated non-base NICs.
    018C  396 Bitstring    2 $VDEVSIDC      VNET # entries in $VDEVSIDL
    018E  398 Bitstring    2 $VDEVSIDN      VNET Next available entry in
                                            $VDEVSIDLS
    0190  400 Bitstring   64 $VDEVSIDL (0)  VNET Array of subchannel IDs
    0190  400 Bitstring    4 * (16)         VNET 16 4-byte (word) entries
              00000010       $VDEVSIDM      (*-$VDEVSIDL)/4 Max number of 4
                                            byte entries
    01D0  464 Bitstring    1 $VDEVNTYP      VNET Network Device Type
                                            (NICTYPE)
    01D1  465 Bitstring    8 $VDEVLNAM      VNET LANNAME (LANBK)
          Real device number count/offset.
          If $VDEVOSAB=1, then this is the COUNT of OSAs requiring
          consecutive real device numbers.
          If $VDEVOSAN=1, then this is the OFFSET from the base OSA
          real device number.
    01D9  473 Bitstring    2 $VDEVOSAO      OSA
          $VDEV_VER 2 support
    01DB  475 Bitstring    4 $VDEVDVLH      VNET NICVLANS (DVLHEAD)
    01DF  479 Bitstring    2 $VDEVVCTR      VNET NICVLCTR
    01E1  481 Bitstring    2 $VDEVPVID      VNET NICVPVID
    01E3  483 Bitstring    1 $VDEVPORT      VNET NICVPORT
    01E4  484 Bitstring    1 $VDEVVLPT      VNET LANVLFLT and NICVPORT values
          $VDEV_VER 3 support
    01E5  485 Bitstring    4 $VDEVNETO      VNET Link to LGRNETWK extension
    01E9  489 Bitstring    4 $VDEV_CSINT    VDisk ASCCSINT Copy
    01ED  493 Bitstring    4 $VDEV_CSREL    VDisk ASCCSREL Copy
    01F1  497 Bitstring    4 $VDEV_CSINV    VDisk ASCCSINV Copy
    01F5  501 Bitstring    4 $VDEV_CSPFI    VDisk ASCCSPFI Copy
    01F9  505 Bitstring    4 $VDEV_CSPFA    VDisk ASCCSPFA Copy
    01FD  509 Bitstring    4 $VDEV_CSFRY    VDisk ASCCSFRY Copy
    0201  513 Bitstring    4 $VDEV_CSFNR    VDisk ASCCSFNR Copy
    0205  517 Bitstring    4 $VDEV_CSXRL    VDisk ASCCSXRL Copy
              00000209       $VDEVBYSZ      *-$VDEV Byte length of $VDEV
              00000042       $VDEVSIZE      ((*-$VDEV)+7)/8 DWord length of
                                            $VDEV

$VDEV Storage Layout | Top of page

    *** $VDEV - Relocation mapping for HCPVDEV
    *
    *     +-------------+-------------+---------------------------+
    *   0 | $VDEV_HDRL  | $VDEV_BITL  |///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    *   8 |$VDEV0|$VDEV1|$VDEV2|$VDEV3|$VDEV4|$VDEV5|$VDEV6|$VDEV7|
    *     +------+------+------+------+------+------+------+------+
    *  10 |$VDEV8|$VDEV9|/////////////////////////////////////////|
    *     +------+------+--------------------+--------------------+
    *  18 |//////|        $VDEVFPNT          |    $VDEVBPNT-      |
    *     +------+-------------+------+------+--------------------+
    *  20 |-(01D)|  $VDEVSUB   |(023) |(024) |    $VDEVINTP-      |
    *     +------+-------------+------+------+--------------------+
    *  28 |-(025)|/////////////|  $VDEVDEV   |////////////////////|
    *     +------+-------------+-------------+////////////////////|
    *  30 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |//////+---------------------------+--------------------+
    *  40 |//////|        $VDEVNIOR          |    $VDEVSIOR-      |
    *     +------+---------------------------+--------------------+
    *  48 |-(045)|        $VDEVPIOR          |    $VDEVAEVT-      |
    *     +------+---------------------------+--------------------+
    *  50 |-(04D)|        $VDEVIOCT          |    $VDEVTMCT-      |
    *     +------+---------------------------+--------------------+
    *  58 |-(055)|                  $VDEVTIME-                    |
    *     +------+---------------------------+--------------------+
    *  60 |-(059)|        $VDEVUIOR          |    $VDEVIOCA-      |
    *     +------+------+------+------+------+--------------------+
    *  68 |-(065)|(069) |(06A) |(06B) |(06C) |     $VDEVLTOD      |
    *     +------+------+------+------+------+--------------------+
    *  70 |        $VDEVBKIA          |(074) |      (075)-        |
    *     +---------------------------+------+--------------------+
    *  78 |           -$VDEVMBLK             |    $VDEVGCHR-      |
    *     +------+---------------------------+--------------------+
    *  80 |-(07D)|        $VDEVPOSN          |    $VDEVSEXT-      |
    *     +------+---------------------------+--------------------+
    *  88 |-(085)|        $VDEVEEXT          |    $VDEVDYPT-      |
    *     +------+---------------------------+--------------------+
    *  90 |-(08D)|                  $VDEVCUSR-                    |
    *     +------+---------------------------+--------------------+
    *  98 |-(091)|        $VDEVCTCD          |     $VDEVVSP-      |
    *     +------+---------------------------+--------------------+
    *  A0 |-(09D)|         $VDEVVPX          |     $VDEVVDS-      |
    *     +------+------+--------------------+--------------------+
    *  A8 |-(0A5)|(0A9) |/////////////////////////////////////////|
    *     +------+------+-----------------------------------------+
    *  B0 |                                                       |
    *     =                       $VDEVID                         =
    *     |                                                       |
    *     +------+------------------------------------------------+
    *  D8 |(0D8) |                                                |
    *     +------+                                                |
    *  E0 |                                                       |
    *     =                      $VDEVKYL1                        =
    *     |      +------+-----------------------------------------+
    * 118 |      |(119) |                                         |
    *     +------+------+                                         |
    * 120 |                                                       |
    *     =                      $VDEVKYL2                        =
    *     |             +-----------------------------------------+
    *     |             |               $VDEVURFI-                |
    *     +-------------+-------------+------+------+-------------+
    * 160 |   -(15A)    | $VDEVPBAS   |//////|(165) |$VDEV_PTRSH- |
    *     +-------------+-------------+------+------+-------------+
    * 168 |   -(166)    |       $VDEV_CSPST         |$VDEV_CSPGR- |
    *     +-------------+---------------------------+-------------+
    * 170 |   -(16E)    |       $VDEV_CSPGW         |$VDEV_CSXRD- |
    *     +-------------+---------------------------+-------------+
    * 178 |   -(176)    |       $VDEV_CSXWT         |$VDEV_CSMIG- |
    *     +-------------+---------------------------+-------------+
    * 180 |   -(17E)    |              $VDEVOUSER-                |
    *     +-------------+-------------+-------------+-------------+
    * 188 |   -(182)    | $VDEVOVDEV  | $VDEVSIDC   | $VDEVSIDN   |
    *     +-------------+-------------+-------------+-------------+
    * 190 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +------+------------------------------------------------+
    * 1D0 |(1D0) |                  $VDEVLNAM-                    |
    *     +------+-------------+---------------------------+------+
    * 1D8 |-(1D1)| $VDEVOSAO   |        $VDEVDVLH          |(1DF)-|
    *     +------+-------------+------+------+-------------+------+
    * 1E0 |-(1DF)| $VDEVPVID   |(1E3) |(1E4) |    $VDEVNETO-      |
    *     +------+-------------+------+------+--------------------+
    * 1E8 |-(1E5)|       $VDEV_CSINT         |   $VDEV_CSREL-     |
    *     +------+---------------------------+--------------------+
    * 1F0 |-(1ED)|       $VDEV_CSINV         |   $VDEV_CSPFI-     |
    *     +------+---------------------------+--------------------+
    * 1F8 |-(1F5)|       $VDEV_CSPFA         |   $VDEV_CSFRY-     |
    *     +------+---------------------------+--------------------+
    * 200 |-(1FD)|       $VDEV_CSFNR         |   $VDEV_CSXRL-     |
    *     +------+---------------------------+--------------------+
    * 208 |-(205)| 209
    *     +------+
    *
    *** $VDEV - Relocation mapping for HCPVDEV

$VDEV Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    $VDEV_BITL     0002
    $VDEV_BITS     0008
    $VDEV_BLEN     0012 00000011
    $VDEV_CSFNR    0201
    $VDEV_CSFRY    01FD
    $VDEV_CSINT    01E9
    $VDEV_CSINV    01F1
    $VDEV_CSMIG    017E
    $VDEV_CSPFA    01F9
    $VDEV_CSPFI    01F5
    $VDEV_CSPGR    016E
    $VDEV_CSPGW    0172
    $VDEV_CSPST    016A
    $VDEV_CSREL    01ED
    $VDEV_CSXRD    0176
    $VDEV_CSXRL    0205
    $VDEV_CSXWT    017A
    $VDEV_DATA     0019
    $VDEV_HDLN     0004 00000008
    $VDEV_HDRL     0000
    $VDEV_PTRSH    0166
    $VDEV_S63      0165 00000001
    $VDEV_VER      0000 00000003
    $VDEVAEVT      004D
    $VDEVATTN      000B 08
    $VDEVBCC0      000A 08
    $VDEVBKIA      0070
    $VDEVBPCI      000A 80
    $VDEVBPNT      001D
    $VDEVBRGS      000B 04
    $VDEVBSUI      000A 40
    $VDEVBUSY      0008 80
    $VDEVBYSZ      0205 00000209
    $VDEVCATT      0008 01
    $VDEVCLAS      0023
    $VDEVCLRF      0008 20
    $VDEVCNA       000E 80
    $VDEVCONS      000F 80
    $VDEVCPIE      006A
    $VDEVCRDR      006B
    $VDEVCTCD      0099
    $VDEVCUSR      0091
    $VDEVDCTL      000E 20
    $VDEVDED       0009 04
    $VDEVDEV       002B
    $VDEVDING      000B 10
    $VDEVDPRE      000C 10
    $VDEVDVFP      0009 01
    $VDEVDVLH      01DB
    $VDEVDYPT      008D
    $VDEVD2A8      000E 04
    $VDEVEEXT      0089
    $VDEVENCR      0010 20
    $VDEVFBA       000C 40
    $VDEVFPNT      0019
    $VDEVFULL      0009 02
    $VDEVGCHR      007D
    $VDEVGSUS      000B 20
    $VDEVHLTF      0008 10
    $VDEVHPAL      000D 20
    $VDEVHPBA      000D 10
    $VDEVID        00B0
    $VDEVIDSZ      00A9
    $VDEVIFCC      000E 02
    $VDEVIMRS      0009 80
    $VDEVINTP      0025
    $VDEVINTV      0009 08
    $VDEVINT3      000B 80
    $VDEVIOCA      0065
    $VDEVIOCT      0051
    $VDEVIOPQ      0009 20
    $VDEVISMD      000F 20
    $VDEVKYA1      00D8
    $VDEVKYA2      0119
    $VDEVKYL1      00D9
    $VDEVKYL2      011A
    $VDEVLCNT      006C
    $VDEVLNAM      01D1
    $VDEVLNKE      000B 01
    $VDEVLNKS      000B 02
    $VDEVLTOD      006D
    $VDEVMBLK      0075
    $VDEVMBSF      000C 01
    $VDEVMDCA      0010 02
    $VDEVMDCD      0010 01
    $VDEVMODL      0069
    $VDEVNCTL      000E 10
    $VDEVNETO      01E5
    $VDEVNICB      000F 40
    $VDEVNIOR      0041
    $VDEVNOAS      0010 80
    $VDEVNODT      000D 01
    $VDEVNOMS      0010 40
    $VDEVNRSM      000C 20
    $VDEVNSEG      000A 01
    $VDEVNSIM      0009 10
    $VDEVNTYP      01D0
    $VDEVOSAB      000F 08
    $VDEVOSAN      000F 04
    $VDEVOSAO      01D9
    $VDEVOUSER     0182
    $VDEVOVDEV     018A
    $VDEVPBAS      0162
    $VDEVPIOR      0049
    $VDEVPMCW      0025
    $VDEVPMSK      0074
    $VDEVPORT      01E3
    $VDEVPOSN      0081
    $VDEVPPA1      000B 40
    $VDEVPRCE      0008 40
    $VDEVPVAL      000D 40
    $VDEVPVBA      000D 80
    $VDEVPVID      01E1
    $VDEVQACT      000A 20
    $VDEVQDSK      000C 80
    $VDEVQESB      000F 02
    $VDEVQUED      0008 02
    $VDEVRECC      0010 08
    $VDEVRFID      000D 08
    $VDEVRO        000A 04
    $VDEVRPND      0008 04
    $VDEVRSRL      000A 02
    $VDEVSCPI      000D 04
    $VDEVSCTL      000E 40
    $VDEVSEXT      0085
    $VDEVSHRD      000C 02
    $VDEVSIDC      018C
    $VDEVSIDL      0190
    $VDEVSIDM      0190 00000010
    $VDEVSIDN      018E
    $VDEVSIOR      0045
    $VDEVSIZE      0205 00000042
    $VDEVSRCV      0165
    $VDEVSSNT      000E 01
    $VDEVSUB       0021
    $VDEVSUSP      0008 08
    $VDEVSWDD      000E 08
    $VDEVTENB      000C 04
    $VDEVTIME      0059
    $VDEVTMCT      0055
    $VDEVTYPE      0024
    $VDEVUIOR      0061
    $VDEVURAC      0010 10
    $VDEVURFI      015A
    $VDEVVCTR      01DF
    $VDEVVDS       00A5
    $VDEVVLPT      01E4
    $VDEVVMIO      000A 10
    $VDEVVPX       00A1
    $VDEVVSP       009D
    $VDEVWINT      0009 40
    $VDEVWKAL      0010 04
    $VDEV0         0008
    $VDEV1         0009
    $VDEV1END      0011 80
    $VDEV2         000A
    $VDEV3         000B
    $VDEV4         000C
    $VDEV5         000D
    $VDEV6         000E
    $VDEV7         000F
    $VDEV8         0010
    $VDEV9         0011

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:32:19 EDT.
Copyright IBM Corporation, 1990, 2020