INFBK | Back to Index page

| Prolog Control Block Contents INFBK DSECT INF0HDR DSECT INF0HDYG DSECT INF0MAC DSECT INF0PAR DSECT INF0HYP DSECT INF0GST DSECT INFCHDR DSECT INF1BK DSECT INF1YGHD DSECT INF1MAC DSECT INF1PAR DSECT INF1HYP DSECT INF1GST DSECT INF2BK DSECT INF2GST DSECT INF3BK DSECT INF3GST DSECT INF4BK DSECT INF4POOL DSECT INF5BK DSECT INF6BK DSECT INF6MEM DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

INFBK Prolog | Top of page

     NAME       : HCPINFBK
     DESCRIPTION: Mappings for STHYI
                  Store Hypervisor Information
     DSECT      : INFBK
     FUNCTION   :
                  The INFBK structure describes the response buffer for
                  the STHYI instruction for each of the supported function
                  codes.
                  Programs written and compiled using a version of HCPINFBK
                  COPY from one release of z/VM can be executed on a newer
                  release of z/VM without change.
     LOCATED BY : Function code X'0000': Obtain CPU Capacity Information.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0001': Hypervisor Environment Information.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0002': Guest List.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0003': Designated Guest Information.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0004': Resource Pool List.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0005': Designated Resource Pool Information
                  STHYI R2 contains the guest logical
                  address of the response buffer.
                  Function code X'0006': Resource Pool Member List.
                  STHYI R2 contains the guest logical
                  address of the response buffer.
     CREATED BY : HCPSHIMN
     DELETED BY : HCPSHIMN
     REFERENCES :
     SERIALIZED : Guest instruction-stream serialization.
     RELOCATION CONSIDERATIONS : None
     COMPATIBILITY AND MIGRATION CONCERNS : None
     GENERAL NOTES      :
                  Changes made to HCPINFBK COPY are made in a compatible
                  way, so that programs written and compiled using one release
                  of HCPINFBK COPY can be executed on a new release of z/VM
                  without change, provided:
                  - offset fields are used to locate the contents of
                  sections of the response buffer,
                  - length fields are used to determine whether fields are
                  included in the response buffer,
                  - count fields are used to determine how many of a
                  repeated section are included in the response buffer,
                  - validity bits are used to determine whether values
                  of certain fields are meaningful.
                  - the length of the common header section (INFCHDR) will
                  never change to prevent shifting offsets of fields
                  in the function-code-specific block following the
                  common header.
                  See each individual function code for details on usage
                  and contents.
                  INFBKs for function codes 1 through 6 include a version
                  number for the INFBK format.

INFBK Control Block Content | Top of page

     INFBK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INFBK          Mappings for STHYI
    0000    0 Signed       8 INFRESP        Minimum response buffer size for
                                            all function codes.
            Return Codes
              00000000       INFRCOK        0 Success
              00000004       INFRFC         4 Unsupported function code
              00000008       INFRCAUT       8 Unauthorized function code
              0000000C       INFRCMIS       12 Missing or invalid name
              00000010       INFRCNAM       16 Specified name is unknown
              00000014       INFRCBUF       20 Response buffer is too small
              00000018       INFRCNXT       24 Next, unused return code
            Function code Values
              00000000       INFCAPAC       0 FC=0 - Obtain CPU Capacity Info
              00000001       INFHYPER       1 FC=1 - Hypervisor Environment
                                            Info
              00000002       INFGSTL        2 FC=2 - Guest List
              00000003       INFGSTI        3 FC=3 - Designated Guest Info
              00000004       INFPOOLL       4 FC=4 - Resource Pool List
              00000005       INFPOOLI       5 FC=5 - Designated Resource Pool
                                            Information
              00000006       INFPOOLM       6 FC=6 - Resource Pool Member
                                            List
            Function code x'0000': Return CPU Capacity Information
            The response buffer for function code x'0000' consists
            of five or more sections of data:
             Header Section
             Machine Section
             Partition Section
             Hypervisor Section 1
             Guest Section 1
             Hypervisor Section 2 (may not be present)
             Guest Section 2      (may not be present)
             Hypervisor Section 3 (may not be present)
             Guest Section 3      (may not be present)
           One to three levels of Hypervisors and Guests may be
           reported.
            Function code X'0000' Response Buffer
            Header Section

     INF0HDR DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0HDR        Mappings for STHYI
    0000    0 Bitstring    1 INFHFLG1       Header Flag Byte 1 These flag
                                            settings indicate the environment
                                            that the instruction was executed
                                            in and may influence the value of
                                            validity bits. The validity bits,
                                            not these flags, should be used
                                            to determine if a field is valid.
              1... ....      INFGPDU        X'80' INFGPDU Global Performance
                                            Data unavailable
              .1.. ....      INFSTHYI       X'40' INFSTHYI One or more
                                            hypervisor levels below this
                                            level does not support the STHYI
                                            instruction. When this flag is
                                            set the value of INFGPDU is not
                                            meaningful because the state of
                                            the Global Performance Data
                                            setting cannot be determined.
              ..1. ....      INFVSI         X'20' INFVSI Virtualization stack
                                            is incomplete. This bit indicates
                                            one of 2 cases: 1. One or more
                                            hypervisor levels do not support
                                            STHYI. For this case INFSTHYI
                                            will also be set. 2. There were
                                            more than 3 levels of
                                            guest/hypervisor information to
                                            report.
              ...1 ....      INFBASIC       X'10' INFBASIC Execution
                                            environment is not within a
                                            logical partition.
    0001    1 Bitstring    1 INFHFLG2       Header Flag Byte 2 reserved for
                                            IBM use
    0002    2 Bitstring    1 INFHVAL1       Header Validity Byte 1 Reserved
                                            for IBM use
    0003    3 Bitstring    1 INFHVAL2       Header Validity Byte 2 Reserved
                                            for IBM use
    0004    4 Bitstring    3 *              Reserved for IBM use
    0007    7 Signed       1 INFHYGCT       Count of reported hypervisors/
                                            guests. This indicates how many
                                            hypervisor/guest sections are in
                                            the response buffer up to a
                                            maximum of 3.
              00000003       INF0YGMX       3 Maximum Hypervisor/Guest
                                            sections
    0008    8 Signed       2 INFHTOTL       Total length of the response
                                            buffer in bytes, including the
                                            Header, Machine, Partition, and
                                            Hypervisor and Guest sections.
    000A   10 Signed       2 INFHDLN        Length of Header Section in bytes
    000C   12 Signed       2 INFMOFF        Offset to Machine Section mapped
                                            by INF0MAC
    000E   14 Signed       2 INFMLEN        Length of Machine Section in
                                            bytes
    0010   16 Signed       2 INFPOFF        Offset to Partition Section
                                            mapped by INF0PAR
    0012   18 Signed       2 INFPLEN        Length of Partition Section in
                                            bytes
    0014   20 Signed       8 INFHYGS1       Hypervisor/Guest Header 1
    0014   20 Signed       2 INFHOFF1       Offset to Hypervisor Section 1,
                                            mapped by INF0HYP
    0016   22 Signed       2 INFHLEN1       Length of Hypervisor Section 1 in
                                            bytes
    0018   24 Signed       2 INFGOFF1       Offset to Guest Section 1 mapped
                                            by INF0GST
    001A   26 Signed       2 INFGLEN1       Length of Guest Section 1 in
                                            bytes
    001C   28 Signed       8 INFHYGS2       Hypervisor/Guest Header 2
    001C   28 Signed       2 INFHOFF2       Offset to Hypervisor Section 2
                                            mapped by INF0HYP
    001E   30 Signed       2 INFHLEN2       Length of Hypervisor Section 2 in
                                            bytes
    0020   32 Signed       2 INFGOFF2       Offset to Guest Section 2 mapped
                                            by INF0GST
    0022   34 Signed       2 INFGLEN2       Length of Guest Section 2 in
                                            bytes
    0024   36 Signed       8 INFHYGS3       Hypervisor/Guest Header 3
    0024   36 Signed       2 INFHOFF3       Offset to Hypervisor Section 3
                                            mapped by INF0HYP
    0026   38 Signed       2 INFHLEN3       Length of Hypervisor Section 3 in
                                            bytes
    0028   40 Signed       2 INFGOFF3       Offset to Guest Section 3 mapped
                                            by INF0GST
    002A   42 Signed       2 INFGLEN3       Length of Guest Section 3 in
                                            bytes
    002C   44 Bitstring    4 *              Reserved for IBM use
              00000030       INF0HDSZ       *-INF0HDR Size of header in bytes
              00000006       INF0HDSD       (*-INF0HDR+7)/8 Size of Header in
                                            doublewords
            Function code X'0000' Response Buffer
            Hypervisor/Guest section description

     INF0HDYG DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0HDYG       Mappings for STHYI
    0000    0 Signed       2 INFYOFF        Offset to Hypervisor Section
                                            mapped by INF0HYP
    0002    2 Signed       2 INFYLEN        Length of Hypervisor Section in
                                            bytes
    0004    4 Signed       2 INFGOFF        Offset to Guest Section mapped by
                                            INF0GST
    0006    6 Signed       2 INFGLEN        Length of Guest Section in bytes
              00000008       INF0HYSZ       *-INF0HDYG Size of section
                                            description in bytes
              00000001       INF0HYSD       (*-INF0HDYG+7)/8 Size of section
                                            description in doublewords.
            Function code X'0000' Response Buffer
            Machine Section

     INF0MAC DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0MAC        Mappings for STHYI
    0000    0 Bitstring    1 INFMFLG1       Machine Flag Byte 1
              1... ....      INFMPOOL       X'80' INFMPOOL Reserved for IBM
                                            use.
    0001    1 Bitstring    1 INFMFLG2       Machine Flag Byte 2 reserved for
                                            IBM use
    0002    2 Bitstring    1 INFMVAL1       Machine Validity Byte 1
              1... ....      INFMPROC       X'80' INFMPROC Processor Count
                                            Validity When this bit is on, it
                                            indicates that INFMSCPS,
                                            INFMDCPS, INFMSIFL, and INFMDIFL
                                            contain valid counts. The
                                            validity bit may be off when: -
                                            STHYI support is not available on
                                            a lower level hypervisor, or -
                                            Global Performance Data is not
                                            enabled.
              .1.. ....      INFMMID        X'40' INFMMID Machine ID Validity
                                            This bit being on indicates that
                                            a SYSIB 1.1.1 was obtained from
                                            STSI and information reported in
                                            the following fields is valid:
                                            INFMTYPE, INFMMANU, INFMSEQ, and
                                            INFMPMAN.
              ..1. ....      INFMMNAM       X'20' INFMMNAM Machine Name
                                            Validity This bit being on
                                            indicates that the INFMNAME field
                                            is valid.
              ...1 ....      INFMPLNV       X'10' INFMPLNV Reserved for IBM
                                            use.
              .... 1...      INFMZIIPV      X'08' INFMZIIPV Machine zIIP
                                            reporting validity. When on, the
                                            INFMSZIIP and INFMDZIIP fields
                                            are valid.
    0003    3 Bitstring    1 INFMVAL2       Machine Validity Byte 2 Reserved
                                            for IBM use
    0004    4 Signed       2 INFMSCPS       Count of shared CPs configured in
                                            the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            (INFMPROC)
    0006    6 Signed       2 INFMDCPS       Count of dedicated CPs configured
                                            in the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            (INFMPROC)
    0008    8 Signed       2 INFMSIFL       Count of shared IFLs configured
                                            in the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            (INFMPROC)
    000A   10 Signed       2 INFMDIFL       Count of dedicated IFLs
                                            configured in the machine or in
                                            the physical partition if the
                                            system is physically partitioned.
                                            (Valid if (INFMPROC)
    000C   12 Character    8 INFMNAME       Machine Name, in EBCDIC format.
                                            This is the CPC name associated
                                            with the processor. (Valid if
                                            (INFMMNAM)
    0014   20 Character    4 INFMTYPE       Machine Type, in EBCDIC format.
                                            This is the machine type reported
                                            by STSI 1.1.1 (Basic Machine
                                            Configuration). (Valid if
                                            (INFMMID)
    0018   24 Character   16 INFMMANU       Machine Manufacturer, in EBCDIC
                                            format. This is the name of the
                                            manufacturer of the configuration
                                            reported by STSI 1.1.1. (Valid if
                                            (INFMMID)
    0028   40 Character   16 INFMSEQ        Sequence Code, in EBCDIC format.
                                            This is the sequence code of the
                                            configuration reported by STSI
                                            1.1.1. (Valid if (INFMMID)
    0038   56 Character    4 INFMPMAN       Plant of Manufacture, in EBCDIC
                                            format. This is the 4-byte code
                                            reported by STSI 1.1.1. (Valid if
                                            (INFMMID)
    003C   60 Bitstring    4 *              Reserved for IBM use
    0040   64 Character    8 INFMPLNM       Reserved for IBM use.
    0048   72 Signed       2 INFMSZIIP      Count of shared zIIPs configured
                                            in the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            INFMZIIPV)
    004A   74 Signed       2 INFMDZIIP      Count of dedicated zIIPs
                                            configured in the machine or in
                                            the physical partition if the
                                            system is physically partitioned.
                                            (Valid if INFMZIIPV)
    004C   76 Bitstring    4 *              Reserved for IBM use
              00000050       INF0MSIZ       *-INF0MAC Size of Machine Section
                                            in bytes
              0000000A       INF0MSZD       (*-INF0MAC+7)/8 Size of Machine
                                            Section in doublewords
            Function code X'0000' Response Buffer
            Partition Section

     INF0PAR DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0PAR        Mappings for STHYI
    0000    0 Bitstring    1 INFPFLG1       Partition Flag Byte 1
              1... ....      INFPMTEN       X'80' INFPMTEN Multithreading
                                            (MT) is enabled.
              .1.. ....      INFPPOOL       X'40' INFPPOOL Reserved for IBM
                                            use.
    0001    1 Bitstring    1 INFPFLG2       Partition Flag Byte 2 reserved
                                            for IBM use.
    0002    2 Bitstring    1 INFPVAL1       Partition Validity Byte 1
              1... ....      INFPPROC       X'80' INFPPROC Processor Count
                                            Validity This bit being on
                                            indicates that INFPSCPS,
                                            INFPDCPS, INFPSIFL, and INFPDIFL
                                            contain valid counts. When
                                            INFPZIIPV is on, INFPSZIIP and
                                            INFPDZIPP contain valid cnts.
              .1.. ....      INFPWBCC       X'40' INFPWBCC Partition
                                            weight-based capped capacity
                                            validity. This bit being on
                                            indicates that INFPWBCP and
                                            INFPWBIF are valid. When
                                            INFPZIIPV is also on, INFPWBZIIP
                                            is valid.
              ..1. ....      INFPACC        X'20' INFPACC Partition absolute
                                            capped capacity validity. This
                                            bit being on indicates that
                                            INFPABCP and INFPABIF are valid.
                                            When INFPZIIPV is also on,
                                            INFPABZIIP is valid.
              ...1 ....      INFPPID        X'10' INFPPID Partition ID
                                            Validity. This bit being on
                                            indicates that a SYSIB 2.2.2 was
                                            obtained from STSI and
                                            information reported in the
                                            following fields is valid:
                                            INFPPNUM, INFPPNAM
              .... 1...      INFPLGVL       X'08' INFPLGVL LPAR Group
                                            Absolute Capacity Capping
                                            information validity This bit
                                            being on indicates that INFPLGNM,
                                            INFPLGCP and INFPLGIF are valid.
                                            When INFPZIIPV is also on,
                                            INFPLGZIIP is valid.
              .... .1..      INFPPLNV       X'04' INFPPLNV Reserved for IBM
                                            use.
              .... ..1.      INFPZIIPV      X'02' INFPZIIPV Partition zIIP
                                            reporting validity. When on,
                                            INFPSZIIP and INFPDZIIP are
                                            valid, and INFPWBZIIP, INFPABZIIP
                                            and INFPLGZIIP may be valid
                                            depending on additional validity
                                            bits.
    0003    3 Bitstring    1 INFPVAL2       Partition Validity Byte 2
                                            reserved for IBM use.
    0004    4 Signed       2 INFPPNUM       Logical Partition Number. This is
                                            the Logical-Partition Number
                                            reported by STSI 2.2.2. (Valid if
                                            INFPPID)
    0006    6 Signed       2 INFPSCPS       Count of shared logical CP cores
                                            configured for this partition.
                                            (Valid if INFPPROC)
    0008    8 Signed       2 INFPDCPS       Count of dedicated logical CP
                                            cores configured for this
                                            partition. (Valid if INFPPROC)
    000A   10 Signed       2 INFPSIFL       Count of shared logical IFL cores
                                            configured for this partition.
                                            (Valid if INFPPROC)
    000C   12 Signed       2 INFPDIFL       Count of dedicated logical IFL
                                            cores configured for this
                                            partition. (Valid if INFPPROC)
    000E   14 Bitstring    2 *              Reserved for IBM use
    0010   16 Character    8 INFPPNAM       Logical Partition Name, in EBCDIC
                                            format. This is the Logical-
                                            Partition Name reported by STSI
                                            2.2.2. (Valid if INFPPID)
    0018   24 Signed       4 INFPWBCP       Partition weight-based capped
                                            capacity for CPs, a scaled number
                                            where X'00010000' represents one
                                            core. Cap is applicable only to
                                            shared processors. Zero if not
                                            capped. (Valid if INFPWBCC)
    001C   28 Signed       4 INFPABCP       Partition absolute capped
                                            capacity for CPs, a scaled number
                                            where X'00010000' represents one
                                            core. Cap is applicable only to
                                            shared processors. Zero if not
                                            capped. (Valid if INFPACC)
    0020   32 Signed       4 INFPWBIF       Partition weight-based capped
                                            capacity for IFLs, a scaled
                                            number where X'00010000'
                                            represents one core. Cap is
                                            applicable only to shared
                                            processors. Zero if not capped.
                                            (Valid if INFPWBCC)
    0024   36 Signed       4 INFPABIF       Partition absolute capped
                                            capacity for IFLs, a scaled
                                            number where X'00010000'
                                            represents one core. Cap is
                                            applicable only to shared
                                            processors. Zero if not capped.
                                            (Valid if INFPACC)
    0028   40 Character    8 INFPLGNM       LPAR Group Name (Valid if
                                            INFPLGVL) EBCDIC, padded on right
                                            with blanks when in an LPAR group
                                            and valid. Binary zeros
                                            otherwise. Only reported when
                                            there is a group cap on CP, IFL
                                            or zIIP CPU types and the
                                            partition has the capped CPU
                                            type.
    0030   48 Signed       4 INFPLGCP       LPAR Group Absolute Capacity
                                            Value for the CP CPU type when
                                            nonzero. Nonzero only when
                                            INFPLGNM is nonzero and a cap is
                                            defined for this LPAR Group for
                                            the CP CPU type. When nonzero,
                                            contains a scaled number where
                                            X'00010000' represents one core.
                                            (Valid if INFPLGVL)
    0034   52 Signed       4 INFPLGIF       LPAR Group Absolute Capacity
                                            Value for the IFL CPU type when
                                            nonzero. Nonzero only when
                                            INFPLGNM is nonzero and a cap is
                                            defined for this LPAR Group for
                                            the IFL CPU type. When nonzero,
                                            contains a scaled number where
                                            X'00010000' represents one core.
                                            (Valid if INFPLGVL)
    0038   56 Character    8 INFPPLNM       Reserved for IBM use.
    0040   64 Signed       2 INFPSZIIP      Count of shared logical zIIP
                                            cores configured for this
                                            partition. (Valid if INFPZIIPV)
    0042   66 Signed       2 INFPDZIIP      Count of dedicated logical zIIP
                                            cores configured for this
                                            partition. (Valid if INFPZIIPV)
    0044   68 Signed       4 INFPWBZIIP     Partition weight-based capped
                                            capacity for zIIPs, a scaled
                                            number where X'00010000'
                                            represents one core. Cap is
                                            applicable only to shared
                                            processors. Zero if not capped.
                                            (Valid if INFPWBCC & INFPZIIPV)
    0048   72 Signed       4 INFPABZIIP     Partition absolute capped
                                            capacity for zIIPs, a scaled
                                            number where X'00010000'
                                            represents one core. Cap is
                                            applicable only to shared
                                            processors. Zero if not capped.
                                            (Valid if INFPACC & INFPZIIPV)
    004C   76 Signed       4 INFPLGZIIP     LPAR Group Absolute Capacity
                                            Value for the zIIP CPU type when
                                            nonzero. Nonzero only when
                                            INFPLGNM is nonzero and a cap is
                                            defined for this LPAR Group for
                                            the zIIP CPU type. When nonzero,
                                            contains a scaled number where
                                            X'00010000' represents one core.
                                            (Valid if INFPLGVL & INFPZIIPV)
              00000050       INF0PSIZ       *-INF0PAR Size of Partition
                                            Section in bytes
              0000000A       INF0PSZD       (*-INF0PAR+7)/8 Size of Partition
                                            Section in doublewords
            Function code X'0000' Response Buffer
            Hypervisor Section

     INF0HYP DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0HYP        Mappings for STHYI
    0000    0 Bitstring    1 INFYFLG1       Hypervisor Flag Byte 1
              1... ....      INFYLMCN       X'80' INFYLMCN Consumption method
                                            is used to enforce Limithard
                                            caps.
              .1.. ....      INFYLMPR       X'40' INFYLMPR If on, Limithard
                                            caps use prorated core time for
                                            capping. If off, raw CPU time is
                                            used.
              ..1. ....      INFYMTEN       X'20' INFYMTEN Hypervisor is
                                            MT-enabled.
    0001    1 Bitstring    1 INFYFLG2       Hypervisor Flag Byte 2 Reserved
                                            for IBM use
    0002    2 Bitstring    1 INFYVAL1       Hypervisor Validity Byte 1
              1... ....      INFYZIIPV      X'80' INFYZIIPV Hypervisor zIIP
                                            reporting validity. When on,
                                            INFYSZIIP, INFYZIIPT fields are
                                            valid.
    0003    3 Bitstring    1 INFYVAL2       Hypervisor Validity Byte 2
                                            Reserved for IBM use
    0004    4 Signed       1 INFYTYPE       Hypervisor type
              00000001       INFYTVM        X'01' INFYTVM z/VM is the
                                            hypervisor
              00000002       INFYTKVM       X'02' INFYTKVM KVM is the
                                            hypervisor
              00000003       INFYTZCX       X'03' INFYTZCX zCX is the
                                            hypervisor
    0005    5 Bitstring    1 *              Reserved for IBM use
    0006    6 Bitstring    1 INFYCPT        Threads in use per CP core. This
                                            value is reported for the current
                                            configuration settings even when
                                            the guest CPUs are not dispatched
                                            on CPs. The value is set only
                                            when SMT enabled as indicated by
                                            INFYFLG1.INFYMTEN.
    0007    7 Bitstring    1 INFYIFLT       Threads in use per IFL core. This
                                            value is reported for the current
                                            configuration settings even when
                                            the guest CPUs are not dispatched
                                            on IFLs. The value is set only
                                            when SMT enabled as indicated by
                                            INFYFLG1.INFYMTEN.
    0008    8 Character    8 INFYSYID       System Identifier, in EBCDIC
                                            format, left justified and padded
                                            with blanks. This is the value
                                            generally specified on the
                                            SYSTEM_IDentifier statement in
                                            the system configuration file.
                                            Blank if non-existent.
    0010   16 Character    8 INFYCLNM       Cluster Name, in EBCDIC format,
                                            left justified and padded with
                                            blanks. This is the name on the
                                            SSI statement in the system
                                            configuration file. Blank if
                                            non-existent.
    0018   24 Signed       2 INFYSCPS       Number of CP cores shared by
                                            non-dedicated CP-dispatched
                                            virtual CPUs of this hypervisor.
    001A   26 Signed       2 INFYDCPS       Number of CP cores dedicated to
                                            CP-dispatched virtual CPUs of
                                            this hypervisor.
    001C   28 Signed       2 INFYSIFL       Number of IFL cores shared by
                                            non-dedicated IFL-dispatched
                                            virtual CPUs of this hypervisor.
    001E   30 Signed       2 INFYDIFL       Number of IFL cores dedicated to
                                            IFL-dispatched virtual CPUs of
                                            this hypervisor.
    0020   32 Bitstring    8 INFYINSF (0)   Mask of installed function codes.
                                            Bit position corresponding to the
                                            function code number is on if the
                                            function code is supported by
                                            this hypervisor. Bits may be on
                                            even if the guest is not
                                            authorized.
    0020   32 Bitstring    1 INFYINS0       Function codes 0-7.
              1... ....      INFYFCCP       X'80' INFYFCCP FC=0 - Obtain CPU
                                            Capacity Info.
              .1.. ....      INFYFHYP       X'40' INFYFHYP FC=1 - Hypervisor
                                            Environment Info
              ..1. ....      INFYFGLS       X'20' INFYFGLS FC=2 - Guest List
              ...1 ....      INFYFGST       X'10' INFYFGST FC=3 - Designated
                                            Guest Info
              .... 1...      INFYFPLS       X'08' INFYFPLS FC=4 - Resource
                                            Pool List
              .... .1..      INFYFPDS       X'04' INFYFPDS FC=5 - Designated
                                            Resource Pool Information
              .... ..1.      INFYFPML       X'02' INFYFPML FC=6 - Resource
                                            Pool Member List
    0021   33 Bitstring    1 INFYINS1       Function codes 8-15.
    0022   34 Bitstring    1 INFYINS2       Function codes 16-23.
    0023   35 Bitstring    1 INFYINS3       Function codes 24-31.
    0024   36 Bitstring    1 INFYINS4       Function codes 32-39.
    0025   37 Bitstring    1 INFYINS5       Function codes 40-47.
    0026   38 Bitstring    1 INFYINS6       Function codes 48-55.
    0027   39 Bitstring    1 INFYINS7       Function codes 56-63.
    0028   40 Bitstring    8 INFYAUTF (0)   Mask of authorized function
                                            codes. Bit position corresponding
                                            to the function code number is on
                                            if the function code is supported
                                            by this hypervisor and the guest
                                            has been authorized in the
                                            directory.
    0028   40 Bitstring    1 INFYAUT0       Function codes 0-7.
              1... ....      INFYFCCP       X'80' INFYFCCP FC=0 - Obtain CPU
                                            Capacity Info.
              .1.. ....      INFYFHYP       X'40' INFYFHYP FC=1 - Hypervisor
                                            Environment Info
              ..1. ....      INFYFGLS       X'20' INFYFGLS FC=2 - Guest List
              ...1 ....      INFYFGST       X'10' INFYFGST FC=3 - Designated
                                            Guest Info
              .... 1...      INFYFPLS       X'08' INFYFPLS FC=4 - Resource
                                            Pool List
              .... .1..      INFYFPDS       X'04' INFYFPDS FC=5 - Designated
                                            Resource Pool Information
              .... ..1.      INFYFPML       X'02' INFYFPML FC=6 - Resource
                                            Pool Member List
    0029   41 Bitstring    1 INFYAUT1       Function codes 8-15.
    002A   42 Bitstring    1 INFYAUT2       Function codes 16-23.
    002B   43 Bitstring    1 INFYAUT3       Function codes 24-31.
    002C   44 Bitstring    1 INFYAUT4       Function codes 32-39.
    002D   45 Bitstring    1 INFYAUT5       Function codes 40-47.
    002E   46 Bitstring    1 INFYAUT6       Function codes 48-55.
    002F   47 Bitstring    1 INFYAUT7       Function codes 56-63.
    0030   48 Bitstring    1 INFYZIIPT      Threads in use per zIIP core.
                                            This value is reported for the
                                            current configuration settings
                                            even when the guest CPUs are not
                                            dispatched on zIIPs. The value is
                                            set only when SMT enabled as
                                            indicated by INFYFLG1.INFYMTEN.
                                            (Valid if INFYZIIPV)
    0031   49 Bitstring    1 *              Reserved for IBM use.
    0032   50 Signed       2 INFYSZIIP      Number of zIIP cores shared by
                                            non-dedicated zIIP-dispatched
                                            virtual CPUs of this hypervisor.
                                            (Valid if INFYZIIPV). Note: zIIP
                                            virtual CPUs are never dedicated.
    0034   52 Signed       4 *              Reserved for IBM use.
              00000038       INF0YSIZ       *-INF0HYP Size of Hypervisor
                                            Section in bytes
              00000007       INF0YSZD       (*-INF0HYP+7)/8 Size of
                                            Hypervisor Section in doublewords
            Function code X'0000' Response Buffer
            Guest Section
            All counts of CPs, IFLs, and zIIPs and capacity values
            are based on quantities of cores when multithreading is
            enabled. While virtual CPUs are thread dispatched
            they have the potential of consuming an entire core.
            Therefore virtual CP, IFL and zIIP counts are counts of
            virtual CPUs but treated as counts of cores.

     INF0GST DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF0GST        Mappings for STHYI
    0000    0 Bitstring    1 INFGFLG1       Guest Flag Byte 1
              1... ....      INFGMOB        X'80' INFGMOB Guest mobility is
                                            enabled.
              .1.. ....      INFGMCPT       X'40' INFGMCPT Guest has multiple
                                            CPU types
              ..1. ....      INFGCPLH       X'20' INFGCPLH Guest CP dispatch
                                            type has LIMITHARD cap.
              ...1 ....      INFGIFLH       X'10' INFGIFLH Guest IFL dispatch
                                            type has LIMITHARD cap.
              .... 1...      INFGVCPT       X'08' INFGVCPT Virtual CPs are
                                            thread dispatched.
              .... .1..      INFGVIFT       X'04' INFGVIFT Virtual IFLs are
                                            thread dispatched
              .... ..1.      INFGZIIPH      X'02' INFGZIIPH Guest zIIP
                                            dispatch type has LIMITHARD cap
                                            (Valid if INFGZIIPV).
              .... ...1      INFGVZIIPT     X'01' INFGVZIIPT Virtual zIIPs
                                            are thread dispatched (Valid if
                                            INFGZIIPV).
    0001    1 Bitstring    1 INFGFLG2       Guest Flag Byte 2 Reserved for
                                            IBM use
    0002    2 Bitstring    1 INFGVAL1       Guest Validity Byte 1
              1... ....      INFGZIIPV      X'80' INFGZIIPV Guest zIIP
                                            reporting validity. When on,
                                            INFGSZIIP, INFGZIIPDT,
                                            INFGZIIPCC, INFGPZCC fields, and
                                            INFGZIIPH, INFGVZIIPT, INFGPZLH,
                                            and INFGPZPC flags are valid.
    0003    3 Bitstring    1 INFGVAL2       Guest Validity Byte 2 Reserved
                                            for IBM use
    0004    4 Character    8 INFGUSID       Guest's userid, in EBCDIC format
    000C   12 Signed       2 INFGSCPS       Number of guest shared CPs
    000E   14 Signed       2 INFGDCPS       Number of guest dedicated CPs
    0010   16 Signed       1 INFGCPDT       Dispatch type for guest CPs This
                                            field is valid if INFGSCPS or
                                            INFGDCPS is greater than zero.
                                            Always INGGPUCCP.
              00000000       INFGPUCCP      X'00' INFGPUCCP General Purpose
                                            (CP)
              00000003       INFGPUCIFL     X'03' INFGPUCIFL Integrated Fac
                                            for Linux (IFL).
              00000005       INFGPUCZIP     X'05' INFGPUCZIP zSeries
                                            Integrated Information Processor
                                            (zIIP).
              000000FF       INFGPUCZCP     X'FF' INFGPUCZCP May be
                                            dispatched on zIIP and CP
                                            Processors due to spillover.
    0011   17 Bitstring    3 *              Reserved for IBM use
    0014   20 Signed       4 INFGCPCC       Guest current capped capacity for
                                            CP-dispatched, shared vCPUs, a
                                            scaled number where X'00010000'
                                            represents one core. Zero if not
                                            capped.
    0018   24 Signed       2 INFGSIFL       Number of guest shared IFLs
    001A   26 Signed       2 INFGDIFL       Number of guest dedicated IFLs
    001C   28 Signed       1 INFGIFDT       Dispatch type for guest IFLs.
                                            This field is valid if INFGSIFL
                                            or INFGDIFL is greater than zero.
                                            May be INFGPUCIFL or INFGPUCCP.
              00000000       INFGPUCCP      X'00' INFGPUCCP General Purpose
                                            (CP)
              00000003       INFGPUCIFL     X'03' INFGPUCIFL Integrated Fac
                                            for Linux (IFL).
              00000005       INFGPUCZIP     X'05' INFGPUCZIP zSeries
                                            Integrated Information Processor
                                            (zIIP).
              000000FF       INFGPUCZCP     X'FF' INFGPUCZCP May be
                                            dispatched on zIIP and CP
                                            Processors due to spillover.
    001D   29 Bitstring    3 *              Reserved for IBM use
    0020   32 Signed       4 INFGIFCC       Guest current capped capacity for
                                            IFL-dispatched, shared vCPUs, a
                                            scaled number where X'00010000'
                                            represents one core. Zero if not
                                            capped.
    0024   36 Bitstring    1 INFGPFLG       Resource Pool Capping Flags
              1... ....      INFGPCLH       X'80' INFGPCLH Resource Pool's CP
                                            virtual type has LIMITHARD cap.
              .1.. ....      INFGPCPC       X'40' INFGPCPC Resource Pool's CP
                                            virtual type has CAPACITY cap.
              ..1. ....      INFGPILH       X'20' INFGPILH Resource Pool's
                                            IFL virtual type has LIMITHARD
                                            cap.
              ...1 ....      INFGPIFC       X'10' INFGPIFC Resource Pool's
                                            IFL virtual type has CAPACITY
                                            cap.
              .... 1...      INFPRCTM       X'08' INFPRCTM Resource Pool uses
                                            prorated core time.
              .... .1..      INFGPZLH       X'04' INFGPZLH Resource Pool's
                                            zIIP virtual type has LIMITHARD
                                            cap. (Valid if INFGZIIPV)
              .... ..1.      INFGPZPC       X'02' INFGPZPC Resource Pool's
                                            zIIP virtual type has CAPACITY
                                            cap. (Valid if INFGZIIPV)
    0025   37 Bitstring    3 *              Reserved for IBM use
    0028   40 Character    8 INFGPNAM       Resource pool name. Blanks if not
                                            Resource Pool.
    0030   48 Signed       4 INFGPCCC       Resource pool capped capacity for
                                            shared virtual CPs, a scaled
                                            number where X'00010000'
                                            represents one core if capped.
                                            Zero if not capped.
    0034   52 Signed       4 INFGPICC       Resource pool capped capacity for
                                            shared virtual IFLs, a scaled
                                            number where X'00010000'
                                            represents one core if capped.
                                            Zero if not capped.
    0038   56 Signed       2 INFGSZIIP      Number of guest shared zIIPs.
                                            (Valid if INFYZIIPV). Note: zIIP
                                            virtual CPUs are never dedicated.
    003A   58 Signed       1 INFGZIIPDT     Dispatch type for guest zIIPs.
                                            This field is set when INFGSZIPP
                                            > 0. May be INFGPUCZIIP,
                                            INFGPUCCP or INFGPUCZCP. (Valid
                                            if INFGZIIPV)
              00000000       INFGPUCCP      X'00' INFGPUCCP General Purpose
                                            (CP)
              00000003       INFGPUCIFL     X'03' INFGPUCIFL Integrated Fac
                                            for Linux (IFL).
              00000005       INFGPUCZIP     X'05' INFGPUCZIP zSeries
                                            Integrated Information Processor
                                            (zIIP).
              000000FF       INFGPUCZCP     X'FF' INFGPUCZCP May be
                                            dispatched on zIIP and CP
                                            Processors due to spillover.
    003B   59 Bitstring    1 *              Reserved for IBM use.
    003C   60 Signed       4 INFGZIIPCC     Guest current capped capacity for
                                            zIIP-dispatched, shared vCPUs, a
                                            scaled number where X'00010000'
                                            represents one core. Zero if not
                                            capped. (Valid if INFGZIIPV)
    0040   64 Signed       4 INFGPZCC       Resource pool capped capacity for
                                            shared virtual zIIPs, a scaled
                                            number where X'00010000'
                                            represents one core if capped.
                                            Zero if not capped. (Valid if
                                            INFGZIIPV)
    0044   68 Signed       4 *              Reserved for IBM use.
              00000048       INF0GSIZ       *-INF0GST Size of Guest Section
                                            in bytes
              00000009       INF0GSZD       (*-INF0GST+7)/8 Size of Guest
                                            Section in doublewords

     INFCHDR DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INFCHDR        Mappings for STHYI
          INFCHDR - INFBK Common Header of Response Buffer
            - This common header section defines the beginning
              of the response buffer for function codes that
              insert it at the start of the function-code-specific
              response buffer definition.
            - The INFxBK of each function-code-specific response
              buffer imbedding this common header describes the
              changes introduced for all version codes as a set
              of equates defined for the redefinition of INFCVRSN.
              The service level that introduced the change is also
              noted in the comment on the equates.
            - Function codes that don't return a list will have
              zero values in INFCLSOF, INFCENLN and INFCCTEN.
            - Function codes that return a list but have no list
              data to return will return zero values in INFCLSOF
              and INFCCTEN, but returns the entry length in INFCENLN.
            - If the definition of this common header changes then
              the version number for all function codes that use
              it will be increased to indicate the change in the
              response buffer format for that function code.
            - The length of the common header section (INFCHDR) will
              never change to prevent shifting offsets of fields
              in the function-code-specific block following the
              common header.
    0000    0 Signed       2 INFCVRSN       Version number indicating the
                                            format of the response buffer for
                                            the requested function code. See
                                            response buffer for each function
                                            code for associated versions.
    0002    2 Signed       2 INFCHDLN       Length of the full header that
                                            imbedded this common section.
    0004    4 Signed       4 INFCTOTL       Total length of the actual data
                                            returned in all sections of the
                                            response buffer.
    0008    8 Signed       2 INFCRQSZ       Required buffer size as a number
                                            of 4K pages needed to hold the
                                            complete response.
    000A   10 Signed       2 INFCLSOF       Offset to start of list from the
                                            beginning of the INFxBK imbedding
                                            this common header DSECT. Entries
                                            are mapped by function-
                                            code-specific entry definitions.
    000C   12 Signed       2 INFCENLN       Length of list entry.
    000E   14 Signed       2 *              Reserved for IBM use
    0010   16 Signed       4 INFCCTEN       Count of list entries.
    0014   20 Signed       4 *              Reserved for IBM use
    0018   24 Dbl-Word     8 * (3)          Reserved for IBM use
    0030   48 Dbl-Word     8 INFCFCUS (2)   Function code-specific section.
                                            Used only if redefined within an
                                            INFxBK imbedding INFCHDR DSECT.
                                            It can be redefined to add
                                            section offsets and lengths.
              00000040       INFCSB1        *-INFCHDR Version 1 length in
                                            bytes of the Common Header.
              00000008       INFCSD1        (*-INFCHDR+7)/8 Version 1 length
                                            in doublewords of the Common
                                            Header.
              00000040       INFCSZB        *-INFCHDR Maximum supported
                                            version length in bytes of the
                                            Common Header.
              00000008       INFCSZD        (*-INFCHDR+7)/8 Maximum supported
                                            version length in doublewords of
                                            the Common Header.

     INF1BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1BK         Mappings for STHYI
            Function code x'0001': Hypervisor Environment Information
            This function code reports on the environment of the
            invoker of STHYI.
            The response buffer for function code x'0001' consists
            of five or more sections of data:
             Header Section       (INF1BK DSECT, imbeds INF1CHDR)
             Machine Section      (INF1MAC DSECT)
             Partition Section    (INF1PAR DSECT)
             Hypervisor Section 1 (INF1HYP DSECT)
             Guest Section 1      (INF1GST DSECT)
             Hypervisor Section 2 (may not be present)
             Guest Section 2      (may not be present)
             Hypervisor Section 3 (may not be present)
             Guest Section 3      (may not be present)
            One to three levels of hypervisors and guests may be
            reported. When the guest is running second level or
            higher, hypervisor/guest section 1 is filled in by the
            hypervisor running closest to the hardware, with its
            guest filling in the next section, etc. for a maximum
            of 3 levels.
            The format of this response buffer is determined by the
            hypervisor closest to the LPAR. When running directly
            in a partition, there is only one level of hypervisor
            involved in constructing the response so the version is
            the same for all sections. However when running second
            level the version of this block is generally determined
            by the first level hypervisor.
            The formats of the pairs of hypervisor and guest
            sections may differ. The specified version number
            describes the format of that section.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-UTIL.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
            Update Log - see equates under INF1VRSN.
    0000    0 Bitstring   64 INF1CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF1VRSN       Response buffer version.
              00000001       INF1V00001     X'0001' INF1V00001 Initial
                                            version. APAR VM66105.
    0040   64 Bitstring    1 INF1HFL1       Header Flag Byte 1 These flag
                                            settings indicate the environment
                                            that the instruction was executed
                                            in and may influence the value of
                                            validity bits. The validity bits,
                                            not these flags, should be used
                                            to determine if a field contains
                                            valid data.
              1... ....      INF1GPDU       X'80' INF1GPDU Global Performance
                                            Data unavailable.
              .1.. ....      INF1STHY       X'40' INF1STHY One or more
                                            hypervisor levels below this
                                            level does not support the STHYI
                                            instruction. When this flag is
                                            set the value of INF1GPDU is not
                                            meaningful because the state of
                                            the Global Performance Data
                                            setting cannot be determined.
              ..1. ....      INF1VSI        X'20' INF1VSI Virtualization
                                            stack is incomplete. This bit
                                            indicates one of 2 cases: 1. One
                                            or more hypervisor levels do not
                                            support STHYI or the FC as
                                            indicated by INF1STHY, INF1FCFC
                                            or INF1FCAU. 2. There were more
                                            than 3 levels of guest/hypervisor
                                            information to report.
              ...1 ....      INF1BASC       X'10' INF1BASC Execution
                                            environment is not within a
                                            logical partition.
              .... 1...      INF1FCFC       X'08' INF1FCFC A lower level
                                            hypervisor supports STHYI but not
                                            this function code. When this
                                            flag is set the value of INF1GPDU
                                            is not meaningful because the
                                            state of the Global Performance
                                            Data setting cannot be
                                            determined.
              .... .1..      INF1FCAU       X'04' INF1FCAU A lower level
                                            hypervisor supports STHYI FC=1
                                            but the guest is not authorized.
                                            When this flag is set the value
                                            of INF1GPDU is not meaningful
                                            because the state of the Global
                                            Performance Data setting cannot
                                            be determined.
    0041   65 Bitstring    1 INF1HFL2       Reserved for IBM use
    0042   66 Bitstring    1 INF1HVL1       Reserved for IBM use
    0043   67 Bitstring    1 INF1HVL2       Reserved for IBM use
    0044   68 Signed       3 *              Reserved for IBM use
    0047   71 Signed       1 INF1HYGC       Count of reported hypervisors/
                                            guests. This indicates how many
                                            hypervisor/guest sections are in
                                            the response buffer up to a
                                            maximum of 3.
              00000003       INF1YGMX       3,1,C'X' Maximum Hypervisor/Guest
                                            sections
    0048   72 Signed       2 INF1MOFF       Offset from start of INF1BK to
                                            Machine Section mapped by INF1MAC
    004A   74 Signed       2 INF1MLEN       Length of Machine Section in
                                            bytes
    004C   76 Signed       2 INF1POFF       Offset from start of INF1BK to
                                            Partition Section mapped by
                                            INF1PAR
    004E   78 Signed       2 INF1PLEN       Len of Partition Section in bytes
    0050   80 Bitstring   16 INF1HYG1 (0)   Hypervisor/Guest Header 1
    0050   80 Signed       2 INF1YOF1       Offset from start of INF1BK to
                                            Hypervisor Section 1, mapped by
                                            INF1HYP.
    0052   82 Signed       2 INF1YLN1       Length of Hypervisor Section 1 in
                                            bytes.
    0054   84 Signed       2 INF1YVR1       Version number of this hypervisor
                                            section. Corresponds to the FC=1
                                            version for this hypervisor.
    0056   86 Signed       2 *              Reserved for IBM use.
    0058   88 Signed       2 INF1GOF1       Offset from start of INF1BK to
                                            Guest Section 1 mapped by
                                            INF3GST.
    005A   90 Signed       2 INF1GLN1       Length of Guest Section 1 in
                                            bytes
    005C   92 Signed       2 INF1GVR1       Version number of this guest
                                            section. Corresponds to the FC=3
                                            version for this hypervisor.
    005E   94 Signed       2 *              Reserved for IBM use.
    0060   96 Bitstring   16 INF1HYG2 (0)   Hypervisor/Guest Header 2
    0060   96 Signed       2 INF1YOF2       Offset from start of INF1BK to
                                            Hypervisor Section 2 mapped by
                                            INF1HYP.
    0062   98 Signed       2 INF1YLN2       Length of Hypervisor Section 2 in
                                            bytes.
    0064  100 Signed       2 INF1YVR2       Version number of this hypervisor
                                            section. Corresponds to the FC=1
                                            version for this hypervisor.
    0066  102 Signed       2 *              Reserved for IBM use.
    0068  104 Signed       2 INF1GOF2       Offset from start of INF1BK to
                                            Guest Section 2 mapped by
                                            INF3GST.
    006A  106 Signed       2 INF1GLN2       Length of Guest Section 2 in
                                            bytes
    006C  108 Signed       2 INF1GVR2       Version number of this guest
                                            section. Corresponds to the FC=3
                                            version for this hypervisor.
    006E  110 Signed       2 *              Reserved for IBM use.
    0070  112 Bitstring   16 INF1HYG3 (0)   Hypervisor/Guest Header 3
    0070  112 Signed       2 INF1YOF3       Offset from start of INF1BK to
                                            Hypervisor Section 3 mapped by
                                            INF1HYP.
    0072  114 Signed       2 INF1YLN3       Length of Hypervisor Section 3 in
                                            bytes.
    0074  116 Signed       2 INF1YVR3       Version number of this hypervisor
                                            section. Corresponds to the FC=1
                                            version for this hypervisor.
    0076  118 Signed       2 *              Reserved for IBM use.
    0078  120 Signed       2 INF1GOF3       Offset from start of INF1BK to
                                            Guest Section 3 mapped by
                                            INF3GST.
    007A  122 Signed       2 INF1GLN3       Length of Guest Section 3 in
                                            bytes
    007C  124 Signed       2 INF1GVR3       Version number of this guest
                                            section. Corresponds to the FC=3
                                            version for this hypervisor.
    007E  126 Signed       2 *              Reserved for IBM use.
              00000080       INF1BSB1       *-INF1BK Version 1 length in
                                            bytes of the Hypervisor
                                            Environment Information header.
              00000010       INF1BSD1       (*-INF1BK+7)/8 Version 1 length
                                            in doublewords of the Hypervisor
                                            Environment Information header.
              00000080       INF1BSZB       *-INF1BK Length in bytes for
                                            newest version of the Hypervisor
                                            Environment Information header.
              00000010       INF1BSZD       (*-INF1BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Hypervisor Environment
                                            Information header.

     INF1YGHD DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1YGHD       Mappings for STHYI
            Function code X'0001' Response Buffer
            Hypervisor/Guest section description
    0000    0 Signed       2 INF1YOFF       Offset from start of INF1BK to
                                            Hypervisor Section mapped by
                                            INF1HYP
    0002    2 Signed       2 INF1YLEN       Length of Hypervisor Section in
                                            bytes
    0004    4 Signed       2 INF1YVRS       Version number of this hypervisor
                                            section. Corresponds to the FC=1
                                            version for this hypervisor.
    0006    6 Signed       2 *              Reserved for IBM use.
    0008    8 Signed       2 INF1GOFF       Offset from start of INF1BK to
                                            Guest Section mapped by INF3GST.
    000A   10 Signed       2 INF1GLEN       Length of Guest Section in bytes
    000C   12 Signed       2 INF1GVRS       Version number of this guest
                                            section. Corresponds to the FC=3
                                            version for this hypervisor.
    000E   14 Signed       2 *              Reserved for IBM use.
              00000010       INF1YGB1       *-INF1YGHD Version 1 length in
                                            bytes of the Hypervisor/Guest
                                            entry.
              00000002       INF1YGD1       (*-INF1YGHD+7)/8 Version 1 length
                                            in doublewords of the
                                            Hypervisor/Guest entry.
              00000010       INF1YGSB       *-INF1YGHD Length in bytes for
                                            newest version of the
                                            Hypervisor/Guest entry.
              00000002       INF1YGSD       (*-INF1YGHD+7)/8 Length in
                                            doublewords for newest version of
                                            the Hypervisor/Guest entry.

     INF1MAC DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1MAC        Mappings for STHYI
            Function code X'0001' Response Buffer
            Machine Section
    0000    0 Bitstring    1 INF1MFL1       Machine Flag Byte 1
              1... ....      INF1MPOOL      X'80' INF1MPOOL Reserved for IBM
                                            use.
    0001    1 Bitstring    1 INF1MFL2       Machine Flag Byte 2 Reserved for
                                            IBM use.
    0002    2 Bitstring    1 INF1MVL1       Machine Field Validity Byte 1
              1... ....      INF1MPROC      X'80' INF1MPROC Processor Count
                                            Validity When on, INF1MSCP,
                                            INF1MDCP, INF1MSIF, and INF1MDIF
                                            contain valid counts. Off when
                                            virtualization stack is
                                            incomplete (INF1HFL1.INF1VSI on).
              .1.. ....      INF1MIDV       X'40' INF1MIDV Machine ID
                                            Validity This bit being on
                                            indicates that a SYSIB 1.1.1 was
                                            obtained from STSI and
                                            information reported in the
                                            following fields is valid:
                                            INF1MTYP, INF1MMAN, INF1MSEQ, and
                                            INF1MPMA.
              ..1. ....      INF1MNMV       X'20' INF1MNMV Machine Name
                                            Validity This bit being on
                                            indicates that the INF1MNAM field
                                            is valid.
              ...1 ....      INF1MPLNV      X'10' INF1MPLNV Reserved for IBM
                                            use.
    0003    3 Bitstring    1 INF1MVL2       Reserved for IBM use
    0004    4 Signed       2 INF1MSCP       Count of shared CPs configured in
                                            the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            INF1MPROC)
    0006    6 Signed       2 INF1MDCP       Count of dedicated CPs configured
                                            in the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            INF1MPROC)
    0008    8 Signed       2 INF1MSIF       Count of shared IFLs configured
                                            in the machine or in the physical
                                            partition if the system is
                                            physically partitioned. (Valid if
                                            INF1MPROC)
    000A   10 Signed       2 INF1MDIF       Count of dedicated IFLs
                                            configured in the machine or in
                                            the physical partition if the
                                            system is physically partitioned.
                                            (Valid if INF1MPROC)
    000C   12 Character    4 INF1MTYP       Machine Type, in EBCDIC format.
                                            This is the machine type reported
                                            by STSI 1.1.1 (Basic Machine
                                            Configuration). (Valid if
                                            INF1MIDV)
    0010   16 Character    8 INF1MNAM       Machine Name, in EBCDIC format.
                                            This is the CPC name associated
                                            with the processor. (Valid if
                                            INF1MNMV)
    0018   24 Character   16 INF1MMAN       Machine Manufacturer, in EBCDIC
                                            format. This is the name of the
                                            manufacturer of the configuration
                                            reported by STSI 1.1.1. (Valid if
                                            INF1MIDV)
    0028   40 Character   16 INF1MSEQ       Sequence Code, in EBCDIC format.
                                            This is the sequence code of the
                                            configuration reported by STSI
                                            1.1.1. (Valid if INF1MIDV)
    0038   56 Character    4 INF1MPMA       Plant of Manufacture, in EBCDIC
                                            format. This is the 4-byte code
                                            reported by STSI 1.1.1. (Valid if
                                            INF1MIDV)
    003C   60 Signed       4 *              Reserved for IBM use
    0040   64 Character    8 INF1MPLNM      Reserved for IBM use.
              00000048       INF1MSB1       *-INF1MAC Version 1 length in
                                            bytes of the Machine Section.
              00000009       INF1MSD1       (*-INF1MAC+7)/8 Version 1 length
                                            in doublewords of the Machine
                                            Section.
              00000048       INF1MSZB       *-INF1MAC Length in bytes for
                                            newest version of the Machine
                                            Section.
              00000009       INF1MSZD       (*-INF1MAC+7)/8 Length in
                                            doublewords for newest version of
                                            the Machine Section.

     INF1PAR DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1PAR        Mappings for STHYI
            Function code X'0001' Response Buffer
            Partition Section
    0000    0 Bitstring    1 INF1PFL1       Partition Flag Byte 1
              1... ....      INF1PMTE       X'80' INF1PMTE Multithreading
                                            (MT) is enabled
              .1.. ....      INF1PPOOL      X'40' INF1PPOOL Reserved for IBM
                                            use.
              ..1. ....      INF1PWTFL      X'20' INF1PWTFL Wait Completion
                                            flag is set. This flag is not
                                            reliable when INF1PVL1.INF1PUTV
                                            is not set.
    0001    1 Bitstring    1 INF1PFL2       Partition Flag Byte 2 reserved
                                            for IBM use.
    0002    2 Bitstring    1 INF1PVL1       Partition Field Validity Byte 1
              1... ....      INF1PPRC       X'80' INF1PPRC Processor
                                            Configuration Validity. This bit
                                            being on indicates that INF1PSCP,
                                            INF1PDCP, INF1PSIF, and INF1PDIF
                                            contain valid counts and
                                            INF1PRCPU and INF1PCMOD are
                                            known.
              .1.. ....      INF1PWCV       X'40' INF1PWCV Partition
                                            weight-based capped capacity
                                            validity. This bit being on
                                            indicates that INF1PWBC and
                                            INF1PWBI are valid.
              ..1. ....      INF1PACC       X'20' INF1PACC Partition absolute
                                            capped capacity validity. This
                                            bit being on indicates that
                                            INF1PABC and INF1PABI are valid.
              ...1 ....      INF1PIDV       X'10' INF1PIDV Partition ID
                                            Validity. This bit being on
                                            indicates that a SYSIB 2.2.2 was
                                            obtained from STSI and
                                            information reported in the
                                            following fields is valid:
                                            INF1PPNU, INF1PPNA.
              .... 1...      INF1PLGV       X'08' INF1PLGV LPAR Group
                                            Absolute Capacity Capping
                                            information validity This bit
                                            being on indicates that INF1PLGN,
                                            INF1PLGC, INF1PLGI, INF1PGUCA,
                                            INF1PGUIA, INF1PGUCC, and
                                            INF1PGUIC are valid.
              .... .1..      INF1PPLNV      X'04' INF1PPLNV Reserved for IBM
                                            use.
              .... ..1.      INF1PENV       X'02' INF1PENV Partition
                                            Entitlement and related
                                            information validity. This bit
                                            being on indicates that INF1PENC,
                                            INF1PENI, INF1PSXCA, INF1PSXIA,
                                            INF1PSXCC, INF1PSXIC, INF1PUCPA,
                                            INF1PUIFA, INF1PUCPC, INF1PUIFC
                                            are valid.
              .... ...1      INF1PUTV       X'01' INF1PUTV Partition Core
                                            Utilization and related
                                            information validity. This bit
                                            being on indicates that
                                            INF1PFL1.INF1PWTFL, INF1PUTOD,
                                            INF1PACTC, INF1PLPTC, INF1POLTC,
                                            INF1PWTTC, INF1PMTIC, INF1PACTI,
                                            INF1PLPTI, INF1POLTI, INF1PWTTI,
                                            and INF1PMTII are valid.
    0003    3 Bitstring    1 INF1PVL2       Reserved for IBM use
    0004    4 Signed       2 INF1PSCP       Count of shared logical CP cores
                                            configured for this partition.
                                            (Valid if INF1PPRC)
    0006    6 Signed       2 INF1PDCP       Count of dedicated logical CP
                                            cores configured for this
                                            partition. (Valid if INF1PPRC)
    0008    8 Signed       2 INF1PSIF       Count of shared logical IFL cores
                                            configured for this partition.
                                            (Valid if INF1PPRC)
    000A   10 Signed       2 INF1PDIF       Count of dedicated logical IFL
                                            cores configured for this
                                            partition. (Valid if INF1PPRC)
    000C   12 Signed       2 INF1PPNU       Logical Partition Number. This is
                                            the Logical-Partition Number
                                            reported by STSI 2.2.2. (Valid if
                                            INF1PIDV)
    000E   14 Signed       1 INF1PCMOD      Logical Partition Config Mode.
              00000080       INF1PCMGN      X'80' INF1PCMGN General (ESA390)
                                            logical configuration mode
              00000040       INF1PCMLI      X'40' INF1PCMLI Linux logical
                                            configuration mode
              00000020       INF1PCMVM      X'20' INF1PCMVM VM logical
                                            configuration mode
              00000010       INF1PCMCF      X'10' INF1PCMCF CF logical
                                            configuration mode
    000F   15 Signed       1 INF1PRCPU      Partition primary CPU type. Valid
                                            if INF1PVL1.INF1PPRC is on.
              00000000       INF1PUCCP      X'00' INF1PUCCP General Purpose
                                            (CP)
              00000003       INF1PUCIFL     X'03' INF1PUCIFL Integrated Fac
                                            for Linux (IFL).
    0010   16 Character    8 INF1PPNA       Logical Partition Name, in EBCDIC
                                            format. This is the Logical-
                                            Partition Name reported by STSI
                                            2.2.2. (Valid if INF1PIDV)
          Partition Capacity Caps
    0018   24 Signed       4 INF1PWBC       Partition weight-based capped
                                            capacity for CPs, a scaled number
                                            where X'00010000' represents one
                                            CPU. Zero if not capped. Cap is
                                            applicable only to shared
                                            processors. (Valid if INF1PWCV)
    001C   28 Signed       4 INF1PABC       Partition absolute capped
                                            capacity for CPs, a scaled number
                                            where X'00010000' represents one
                                            core. Zero if not capped. Cap is
                                            applicable only to shared
                                            processors. (Valid if INF1PACC)
    0020   32 Signed       4 INF1PWBI       Partition weight-based capped
                                            capacity for IFLs, a scaled
                                            number where X'00010000'
                                            represents one core. Zero if not
                                            capped. Cap is applicable only to
                                            shared processors. (Valid if
                                            INF1PWCV)
    0024   36 Signed       4 INF1PABI       Partition absolute capped
                                            capacity for IFLs, a scaled
                                            number where X'00010000'
                                            represents one core. Zero if not
                                            capped. Cap is applicable only to
                                            shared processors. (Valid if
                                            INF1PACC)
    0028   40 Character    8 INF1PLGN       LPAR Group Name (Valid if
                                            INF1PLGV) EBCDIC, padded on right
                                            with blanks when in an LPAR group
                                            and valid. Binary zeros
                                            otherwise. Only reported when
                                            there is a group cap on CP or IFL
                                            CPU types and the par- tition has
                                            the capped CPU type.
    0030   48 Signed       4 INF1PLGC       LPAR Group Absolute Capacity
                                            Value for the CP CPU type when
                                            nonzero. Nonzero only when
                                            INF1PLGN is nonzero and a cap is
                                            defined for this LPAR Group for
                                            the CP CPU type. When nonzero,
                                            contains a scaled number where
                                            X'00010000' represents one core.
                                            (Valid if INF1PLGV)
    0034   52 Signed       4 INF1PLGI       LPAR Group Absolute Capacity
                                            Value for the IFL CPU type when
                                            nonzero. Nonzero only when
                                            INF1PLGN is nonzero and a cap is
                                            defined for this LPAR Group for
                                            the IFL CPU type. When nonzero,
                                            contains a scaled number where
                                            X'00010000' represents one core.
                                            (Valid if INF1PLGV)
    0038   56 Character    8 INF1PPLNM      Reserved for IBM use. Processor
                                            Entitlement and Available
                                            Capacity Entitlement values are
                                            current values for the partition.
                                            Share of extra capacity varies
                                            over time. The sum of the
                                            calculated values at each
                                            hiperdispatch interval and the
                                            count of those intervals are
                                            provided so an average between
                                            two STHYI invocations can be
                                            calculated. INF1PENC, INF1PENI,
                                            INF1PSXCA, INF1PSXCA, INF1PSXIA,
                                            INF1PSXCC and INF1PSXIC are
                                            monotonically increasing for the
                                            life of the system.
    0040   64 Signed       4 INF1PENC       Partition Entitled Capacity Value
                                            for the CP CPU type when nonzero.
                                            It is a scaled number where
                                            X'00010000' represents one core.
                                            The value will have been reduced
                                            to the count of CP processors if
                                            the entitlement was larger.
                                            (Valid if INF1PENV)
    0044   68 Signed       4 INF1PENI       Partition Entitled Capacity Value
                                            for the IFL CPU type when
                                            nonzero. It is a scaled number
                                            where X'00010000' represents one
                                            core. The value will have been
                                            reduced to the count of IFL
                                            processors if the entitlement was
                                            larger. (Valid if INF1PENV)
    0048   72 Signed       8 INF1PSXCA      Partition calculated Share of
                                            Extra capacity in the interval:
                                            number of physical CP CPUs/cores
                                            which this partition could have
                                            used. A scaled number where
                                            X'00010000' represents one
                                            CPU/core. Aggregated for
                                            INF1PSXCC intervals. (Valid if
                                            INF1PENV)
    0050   80 Signed       8 INF1PSXIA      Partition calculated Share of
                                            Extra capacity in the interval:
                                            number of physical IFL CPUs/cores
                                            which this partition could have
                                            used. A scaled number where
                                            X'00010000' represents one
                                            CPU/core. Aggregated for
                                            INF1PSXIC intervals. (Valid if
                                            INF1PENV)
    0058   88 Signed       4 INF1PSXCC      Count of intervals aggregated in
                                            INF1PSXCA. (Valid if INF1PENV)
    005C   92 Signed       4 INF1PSXIC      Count of intervals aggregated in
                                            INF1PSXIA. (Valid if INF1PENV)
          Partition Utilization
            Partition utilization varies over time. The sum of the
            calculated values at each hiperdispatch interval and the
            count of those intervals are provided so an average
            between two STHYI invocations can be calculated.
            INF1PUCPA, INF1PUIFA, INF1PUCPC and INF1PUIFC are
            monotonically increasing for the life of the system.
    0060   96 Signed       8 INF1PUCPA      Partition Calculated Utilization
                                            in the interval; number of
                                            physical CP CPUs/cores of this
                                            type which were consumed, a
                                            scaled number where X'00010000'
                                            represents one CPU/core.
                                            Aggregated for INF1PUCPC
                                            intervals. (Valid if INF1PENV)
    0068  104 Signed       8 INF1PUIFA      Partition Calculated Utilization
                                            in the interval; number of
                                            physical IFL CPUs/cores of this
                                            type which were consumed, a
                                            scaled number where X'00010000'
                                            represents one CPU/core.
                                            Aggregated for INF1PUIFC
                                            intervals. (Valid if INF1PENV)
    0070  112 Signed       4 INF1PUCPC      Count of intervals aggregated in
                                            INF1PUCPA. (Valid if INF1PENV)
    0074  116 Signed       4 INF1PUIFC      Count of intervals aggregated in
                                            INF1PUIFA. (Valid if INF1PENV)
          LPAR Groups Utilization
            LPAR group utilization varies over time. The sum of the
            calculated values at each hiperdispatch interval and the
            count of those intervals are provided so an average
            between two STHYI invocations can be calculated.
            LPAR Groups can be defined for a single CPU type and a
            partition can belong to only 1 group.
            INF1PGUCA, INF1PGUIA, INF1PGUCC and INF1PGUIC are
            monotonically increasing for the life of the system.
    0078  120 Signed       8 INF1PGUCA      LPAR Group Utilization Value for
                                            the CP CPU type when nonzero.
                                            Nonzero only when INF1PLGN is
                                            nonzero and a cap is defined for
                                            this LPAR Group for the CP CPU
                                            type. When nonzero, contains a
                                            scaled number where X'00010000'
                                            represents one core. Aggregated
                                            over INF1PGUCC intervals. (Valid
                                            if INF1PLGV)
    0080  128 Signed       8 INF1PGUIA      LPAR Group Utilization Value for
                                            the IFL CPU type when nonzero.
                                            Nonzero only when INF1PLGN is
                                            nonzero and a cap is defined for
                                            this LPAR Group for the IFL CPU
                                            type. When nonzero, contains a
                                            scaled number where X'00010000'
                                            represents one core. Aggregated
                                            over INF1PGUIC intervals. (Valid
                                            if INF1PLGV)
    0088  136 Signed       4 INF1PGUCC      Count of intervals aggregated in
                                            INF1PGUCA. (Valid if INF1PLGV)
    008C  140 Signed       4 INF1PGUIC      Count of intervals aggregated in
                                            INF1PGUIA. (Valid if INF1PLGV)
          Core utilization
            The utilization counts are monotonically increasing values.
            The delta between values from 2 STHYI invocations can be
            used to determine the change in the values during the
            interval.  The length of the interval is determined from
            the INF1PUTOD value delta. These fields are valid when
            INF1PVL1.INF1PUTV is set. The values of the fields in this
            section are based on data available at the time specified
            in the INF1PUTOD field.
    0090  144 Signed       8 INF1PUTOD      Host TOD value at the time when
                                            the partition's core utilization
                                            information was last determined.
                                            (Valid if INF1PUTV)
    0098  152 Signed       8 INF1PACTC      Aggregate number of microseconds
                                            physical CP cores were assigned
                                            to this partition's logical
                                            cores. (Valid if INF1PUTV)
    00A0  160 Signed       8 INF1PLPTC      Aggregate number of microseconds
                                            excluding LPAR management time
                                            while physical CP cores were
                                            assigned to this partition's
                                            logical cores. (Valid if
                                            INF1PUTV)
    00A8  168 Signed       8 INF1POLTC      Aggregate number of microseconds
                                            while logical CP cores of this
                                            partition were online. (Valid if
                                            INF1PUTV)
    00B0  176 Signed       8 INF1PWTTC      Aggregate number of microseconds
                                            while logical CP cores of this
                                            partition were in wait state. If
                                            MT enabled, accumulates when no
                                            processors of core are running.
                                            Not updated if INF1PWTFL=1.
                                            (Valid if INF1PUTV)
    00B8  184 Signed       8 INF1PMTIC      Aggregate number of microseconds
                                            while logical CP cores of this
                                            partition were active but some of
                                            the logical processors of the
                                            core are in any of these states:
                                            enabled wait, disabled wait,
                                            stopped state, check-stop state,
                                            or program interrupt loop. Zero
                                            when MT disabled. (Valid if
                                            INF1PUTV)
    00C0  192 Signed       8 INF1PACTI      Aggregate number of microseconds
                                            physical IFL cores were assigned
                                            to this partition's logical
                                            cores. (Valid if INF1PUTV)
    00C8  200 Signed       8 INF1PLPTI      Aggregate number of microseconds
                                            excluding LPAR management time
                                            while physical IFL cores were
                                            assigned to this partition's
                                            logical cores. (Valid if
                                            INF1PUTV)
    00D0  208 Signed       8 INF1POLTI      Aggregate number of microseconds
                                            while logical IFL cores of this
                                            partition were online. (Valid if
                                            INF1PUTV)
    00D8  216 Signed       8 INF1PWTTI      Aggregate number of microseconds
                                            while logical IFL cores of this
                                            partition were in wait state. If
                                            MT enabled, accumulates when no
                                            processors of core are running.
                                            Not updated if INF1PWTFL=1.
                                            (Valid if INF1PUTV)
    00E0  224 Signed       8 INF1PMTII      Aggregate number of microseconds
                                            while logical IFL cores of this
                                            partition were active but some of
                                            the logical processors of the
                                            core are in any of these states:
                                            enabled wait, disabled wait,
                                            stopped state, check-stop state,
                                            or program interrupt loop. Zero
                                            when MT disabled. (Valid if
                                            INF1PUTV)
              000000E8       INF1PSB1       *-INF1PAR Version 1 length in
                                            bytes of the Partition Section.
              0000001D       INF1PSD1       (*-INF1PAR+7)/8 Version 1 length
                                            in doublewords of the Partition
                                            Section.
              000000E8       INF1PSZB       *-INF1PAR Length in bytes for
                                            newest version of the Partition
                                            Section.
              0000001D       INF1PSZD       (*-INF1PAR+7)/8 Length in
                                            doublewords for newest version of
                                            the Partition Section.

     INF1HYP DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1HYP        Mappings for STHYI
            Function code X'0001' Response Buffer
            Hypervisor Section
    0000    0 Bitstring    1 INF1YFL1       Hypervisor Flag Byte 1
              1... ....      INF1YLMC       X'80' INF1YLMC Consumption method
                                            is used to enforce Limithard
                                            caps.
              .1.. ....      INF1YLMP       X'40' INF1YLMP If on, Limithard
                                            caps use prorated core time for
                                            capping. If off, raw CPU time is
                                            used.
              ..1. ....      INF1YMTE       X'20' INF1YMTE Hypervisor is
                                            MT-enabled.
              ...1 ....      INF1YVRT       X'10' INF1YVRT Vertical
                                            polarization is in use. If off,
                                            horizontal topology is in use,
                                            and INF1YPKF, INF1YXUSC,
                                            INF1YXUSI, INF1YPADC, and
                                            INF1YPADI are not meaningful.
    0001    1 Bitstring    1 INF1YFL2       Hypervisor Flag Byte 2 Reserved
                                            for IBM use
    0002    2 Bitstring    1 INF1YVL1       Reserved for IBM use
    0003    3 Bitstring    1 INF1YVL2       Reserved for IBM use
    0004    4 Signed       1 INF1YTYP       Hypervisor type
              00000001       INF1YTVM       X'01' INF1YTVM z/VM is the
                                            hypervisor
    0005    5 Bitstring    1 *              Reserved for IBM use
    0006    6 Bitstring    1 INF1YCPT       Threads in use per CP core. This
                                            value is reported for the current
                                            configuration settings even when
                                            the guest CPUs are not dispatched
                                            on CPs. The value is set only
                                            when SMT enabled as indicated by
                                            INF1YFL1.INF1YMTE.
    0007    7 Bitstring    1 INF1YIFT       Threads in use per IFL core. This
                                            value is reported for the current
                                            configuration settings even when
                                            the guest CPUs are not dispatched
                                            on IFLs. The value is set only
                                            when SMT enabled as indicated by
                                            INF1YFL1.INF1YMTE.
    0008    8 Character    8 INF1YSID       System Identifier, in EBCDIC
                                            format, left justified and padded
                                            with blanks. This is the value
                                            generally specified on the
                                            SYSTEM_IDentifier statement in
                                            the system configuration file.
                                            Blank if non-existent.
    0010   16 Character    8 INF1YCLN       Cluster Name, in EBCDIC format,
                                            left justified and padded with
                                            blanks. This is the name on the
                                            SSI statement in the system
                                            configuration file. Blank if the
                                            member isn't in an SSI cluster.
          Core counts
    0018   24 Signed       2 INF1YSCP       Number of CP cores shared by
                                            non-dedicated CPUs of the guests
                                            of this hypervisor.
    001A   26 Signed       2 INF1YDCP       Number of CP cores dedicated to
                                            guest CPUs of this hypervisor.
    001C   28 Signed       2 INF1YSIF       Number of IFL cores shared by
                                            non-dedicated CPUs of the guests
                                            of this hypervisor.
    001E   30 Signed       2 INF1YDIF       Number of IFL cores dedicated to
                                            guest CPUs of this hypervisor.
          Total shares
    0020   32 Signed       4 INF1YASC       Sum of absolute shares for all
                                            logged on CP-dispatched VMDBKs
                                            (excluding dedicated VMDBKs). A
                                            scaled number where X'00010000'
                                            represents one CPU.
    0024   36 Signed       4 INF1YASI       Sum of absolute shares for all
                                            logged on IFL-dispatched VMDBKs
                                            (excluding dedicated VMDBKs). A
                                            scaled number where X'00010000'
                                            represents one CPU.
    0028   40 Signed       4 INF1YRSC       Sum of relative shares for all
                                            logged on CP-dispatched VMDBKs
                                            (excluding dedicated VMDBKs).
    002C   44 Signed       4 INF1YRSI       Sum of relative shares for all
                                            logged on IFL-dispatched VMDBKs
                                            (excluding dedicated VMDBKs).
          Total adds to the limit list
    0030   48 Signed       4 INF1YLCC       Approximate count of adds to the
                                            limit-list of CP dispatched
                                            VMDBKs. Monotonically increasing.
    0034   52 Signed       4 INF1YLCI       Approximate count of adds to the
                                            limit-list of IFL dispatched
                                            VMDBKs. Monotonically increasing.
          High-frequency sampling period.
    0038   56 Signed       4 INF1YMONH      Current Monitor high-frequency
                                            (HF) sampling interval in
                                            hundredths of seconds. Value is 0
                                            when high frequency sampling is
                                            not active.
          Hiperdispatch Settings
    003C   60 Signed       1 INF1YPKF       HiperDispatch Unparking setting.
                                            Not used if INF1YFL1.INF1YVRT=0.
              00000000       INF1YPLG       X'00' INF1YPLG SRM UNPARKING
                                            LARGE (default)
              00000001       INF1YPMD       X'01' INF1YPMD SRM UNPARKING
                                            MEDIUM
              00000002       INF1YPSM       X'02' INF1YPSM SRM UNPARKING
                                            SMALL
    003D   61 Signed       1 INF1YXUSC      SRM EXCESSUSE for General (CP)
                                            processor type. Not used if
                                            INF1YFL1.INF1YVRT=0.
              00000010       INF1YXHI       16 INF1YXHI -Indicates the system
                                            should be aggressive in using
                                            unentitled CPU/core capacity.
              00000008       INF1YXMD       8 INF1YXMD -Indicates the system
                                            should be moderately aggressive
                                            in using unentitled CPU/core
                                            capacity.
              00000001       INF1YXLO       1 INF1YXLO -Indicates the system
                                            should not be aggressive in using
                                            unentitled CPU/core capacity.
              00000002       INF1YXNO       2 INF1YXNO -Indicates the system
                                            should not use unentitled
                                            CPU/core capacity.
    003E   62 Signed       1 INF1YXUSI      SRM EXCESSUSE for IFL processor
                                            type. Not used if
                                            INF1YFL1.INF1YVRT=0.
              00000010       INF1YXHI       16 INF1YXHI -Indicates the system
                                            should be aggressive in using
                                            unentitled CPU/core capacity.
              00000008       INF1YXMD       8 INF1YXMD -Indicates the system
                                            should be moderately aggressive
                                            in using unentitled CPU/core
                                            capacity.
              00000001       INF1YXLO       1 INF1YXLO -Indicates the system
                                            should not be aggressive in using
                                            unentitled CPU/core capacity.
              00000002       INF1YXNO       2 INF1YXNO -Indicates the system
                                            should not use unentitled
                                            CPU/core capacity.
    003F   63 Bitstring    1 *              Reserved for IBM use
    0040   64 Signed       4 INF1YPADC      SRM CPUPAD value, a scaled number
                                            where X'00010000' represents one
                                            General (CP) CPU/core. Not used
                                            if INF1YFL1.INF1YVRT=0.
    0044   68 Signed       4 INF1YPADI      SRM CPUPAD value, a scaled number
                                            where X'00010000' represents one
                                            IFL CPU/core. Not used if
                                            INF1YFL1.INF1YVRT=0.
          Logical Processor (not core) Utilization
          The values in these fields are the aggregate of individual
          online processors. When a processor is varied online, the
          value is reset. The length of the interval is determined
          from the INF1YUTOD value delta. INF1YUTOD is set from the
          TOD clock at the start of the calculation of these values.
    0048   72 Signed       8 INF1YUTOD      TOD value at the start of the
                                            hypervisor logical processor
                                            utilization calculations.
    0050   80 Signed       8 INF1YUTC       Total CPU time in microseconds
                                            spent on online CP processors
                                            charged to guests. Monotonically
                                            increasing.
    0058   88 Signed       8 INF1YUTI       Total CPU time in microseconds
                                            spent on online IFL processors
                                            charged to guests. Monotonically
                                            increasing.
    0060   96 Signed       8 INF1YSTC       Total CPU time in microseconds
                                            spent on online CP processors
                                            charged to SYSTEM. Monotonically
                                            increasing.
    0068  104 Signed       8 INF1YSTI       Total CPU time in microseconds
                                            spent on online IFL processors
                                            charged to SYSTEM. Monotonically
                                            increasing.
    0070  112 Signed       8 INF1YWTC       Total elapsed time in
                                            microseconds spent on online CP
                                            processors while in system wait
                                            state. Does not include parked
                                            wait time. Monotonically
                                            increasing.
    0078  120 Signed       8 INF1YWTI       Total elapsed time in
                                            microseconds spent on online IFL
                                            processors while in system wait
                                            state. Does not include parked
                                            wait time. Monotonically
                                            increasing.
    0080  128 Signed       8 INF1YPTC       Total elapsed time in
                                            microseconds spent on online CP
                                            processors while in the parked
                                            state. Monotonically increasing.
    0088  136 Signed       8 INF1YPTI       Total elapsed time in
                                            microseconds spent on online IFL
                                            processors while in the parked
                                            state. Monotonically increasing.
              00000090       INF1YSB1       *-INF1HYP Version 1 length in
                                            bytes of the Hypervisor Section.
              00000012       INF1YSD1       (*-INF1HYP+7)/8 Version 1 length
                                            in doublewords of the Hypervisor
                                            Section.
              00000090       INF1YSZB       *-INF1HYP Length in bytes for
                                            newest version of the Hypervisor
                                            Section.
              00000012       INF1YSZD       (*-INF1HYP+7)/8 Length in
                                            doublewords for newest version of
                                            the Hypervisor Section.

     INF1GST DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF1GST        Mappings for STHYI
            Function code X'0001' Response Buffer
            Guest Section - description of STHYI issuer.
            This matches the guest section of function code 3 as
            defined by the INF3GST DSECT.
    0000    0 Bitstring  320 INF1GSTI       Mapped by INF3GST which lacks the
                                            FC=3 header.
              00000140       INF1GSB1       INF3GSB1 Version 1 length in
                                            bytes of the Guest Description.
              00000028       INF1GSD1       INF3GSD1 Version 1 length in
                                            doublewords of the Guest
                                            Description.
              00000140       INF1GSZB       INF3GSZB Length in bytes for
                                            newest version of the Guest
                                            Description.
              00000028       INF1GSZD       INF3GSZD Length in doublewords
                                            for newest version of the Guest
                                            Description.

     INF2BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF2BK         Mappings for STHYI
            Function code x'0002': Guest List
            This function code returns a list of all guests logged
            on to the system. Guests in the process of logging on,
            logging off, being forced, or relocating to this system
            are excluded.
            This function code requires the length of the buffer as
            a number of 4K pages to be specified. See the STHYI
            documentation for details of how this is specified.
            The response buffer for function code x'0002' consists
            of 2 sections of data:
            - Header Section (INF2BK DSECT, imbeds INFCHDR DSECT)
              - use offset to Guest list, length of entry, and
                count of entries to process the list.
              - The offset in INFCLSOF is from the beginning
                of the INF2BK.
            - Guest list. The list is returned as an array with
              the count of entries, offset to the first entry and
              the entry length defined by the common header.
              - The array entries are defined by INF2GST DSECT.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-GUEST.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
             - CC=3 RC=20 - Response buffer is too small.
                          - INFCRQSZ specifies required buffer size.
                          - Values are also provided in INFCVRSN,
                            INFCHDLN and INFCTOTL. Other response
                            buffer contents are unpredictable.
            Update Log - see equates under INF2VRSN.
            Function code X'0002' Response Buffer
            Header Section
    0000    0 Bitstring   64 INF2CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF2VRSN       Response buffer version.
              00000001       INF2V00001     X'0001' INF2V00001 Initial
                                            version. APAR VM66105.
              00000040       INF2BSB1       *-INF2BK Version 1 length in
                                            bytes of the Guest List header.
              00000008       INF2BSD1       (*-INF2BK+7)/8 Version 1 length
                                            in doublewords of the Guest List
                                            header.
              00000040       INF2BSZB       *-INF2BK Length in bytes for
                                            newest version of the Guest List
                                            header.
              00000008       INF2BSZD       (*-INF2BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Guest List header.

     INF2GST DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF2GST        Mappings for STHYI
            Function code X'0002' Response Buffer
            Guest List Entry Description
    0000    0 Character    8 INF2GUID       Guest's userid, in EBCDIC format.
    0008    8 Character    8 INF2GACN       User accounting number in EBCDIC
                                            format.
    0010   16 Signed       4 INF2GTOD       Bits 0-31 of host TOD at guest
                                            logon.
    0014   20 Bitstring    1 INF2GFLG       Guest list entry flag byte 1.
              .... 1...      INF2GLINI      X'08' INF2GLINI Guest identified
                                            itself as running Linux using a
                                            control program identification
                                            interface.
              .... .1..      INF2GLINH      X'04' INF2GLINH Guest may be
                                            running Linux based on
                                            heuristics. Set only if INF2GLINI
                                            is not set.
    0015   21 Signed       1 INF2GCMOD      Virtual Configuration Mode
              00000080       INF2GCMGN      X'80' INF2GCMGN General (ESA390)
                                            virtual configuration mode
              00000040       INF2GCMLI      X'40' INF2GCMLI Linux virtual
                                            configuration mode
              00000020       INF2GCMVM      X'20' INF2GCMVM VM virtual
                                            configuration mode
              00000010       INF2GCMCF      X'10' INF2GCMCF CF virtual
                                            configuration mode
    0016   22 Bitstring    1 INF2GAFFN      Guest CPUAFFINITY settings.
              1... ....      INF2GAFON      X'80' INF2GAFON CPUAFFINITY is
                                            ON, but may be suppressed. If
                                            off, then INF2GAFSUP will not be
                                            on.
              .1.. ....      INF2GAFSUP     X'40' INF2GAFSUP CPUAFFINTY is
                                            suppressed.
    0017   23 Bitstring    1 INF2GPRTP      Guest primary virtual CPU type.
              00000000       INF2PUCCP      X'00' INF2PUCCP General Purpose
                                            (CP)
              00000003       INF2PUCIFL     X'03' INF2PUCIFL Integrated Fac
                                            for Linux (IFL).
    0018   24 Bitstring    1 INF2GPRDT      Guest primary vCPU dispatch type.
              00000000       INF2PUCCP      X'00' INF2PUCCP General Purpose
                                            (CP)
              00000003       INF2PUCIFL     X'03' INF2PUCIFL Integrated Fac
                                            for Linux (IFL).
    0019   25 Bitstring    7 *              Reserved for IBM use.
              00000020       INF2GSB1       *-INF2GST Version 1 length in
                                            bytes of the Guest List entry.
              00000004       INF2GSD1       (*-INF2GST+7)/8 Version 1 length
                                            in doublewords of the Guest List
                                            entry.
              00000020       INF2GSZB       *-INF2GST Length in bytes for
                                            newest version of the Guest List
                                            entry.
              00000004       INF2GSZD       (*-INF2GST+7)/8 Length in
                                            doublewords for newest version of
                                            the Guest List entry.

     INF3BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF3BK         Mappings for STHYI
            Function code x'0003': Designated Guest Information
            This function code returns the description of the
            specified guest.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-GUEST.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
             - CC=3 RC=12 - Missing or invalid guest name.
                          - The response buffer is not modified.
             - CC=3 RC=16 - Named guest is not logged on.
                          - The response buffer is not modified.
            Update Log - see equates under INF3VRSN.
            Function code X'0003' Response Buffer
    0000    0 Bitstring   64 INF3CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF3VRSN       Response buffer version.
              00000001       INF3V00001     X'0001' INF3V00001 Initial
                                            version. APAR VM66105.
    0040   64 Bitstring  320 INF3GSTI       Guest Information section mapped
                                            by INF3GST DSECT.
              00000180       INF3BSB1       *-INF3BK Version 1 length in
                                            bytes of the Guest Information
                                            response.
              00000030       INF3BSD1       (*-INF3BK+7)/8 Version 1 length
                                            in doublewords of the Guest
                                            Information response.
              00000180       INF3BSZB       *-INF3BK Length in bytes for
                                            newest version of the Guest
                                            Information response.
              00000030       INF3BSZD       (*-INF3BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Guest Information response.

     INF3GST DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF3GST        Mappings for STHYI
            Function code X'0003' Response Buffer
            Guest Description section
            This DSECT is also used for the guest section of the
            function code 1 response buffer.
    0000    0 Character    8 INF3GUID       Guest's userid, in EBCDIC format.
    0008    8 Character    8 INF3GACN       User accounting number in EBCDIC
                                            format.
    0010   16 Bitstring    1 INF3GFLG       Guest Flag Byte
              1... ....      INF3GMOB       X'80' INF3GMOB Guest mobility is
                                            enabled.
              .... 1...      INF3GLINI      X'08' INF3GLINI Guest identified
                                            itself as running Linux using a
                                            control program identification
                                            interface.
              .... .1..      INF3GLINH      X'04' INF3GLINH Guest may be
                                            running Linux based on
                                            heuristics. Set only if INF3GLINI
                                            is not set.
    0011   17 Bitstring    1 INF3GVAL       Reserved for IBM use
    0012   18 Signed       1 INF3GCMOD      Virtual Configuration Mode
              00000080       INF3GCMGN      X'80' INF3GCMGN General (ESA390)
                                            virtual configuration mode
              00000040       INF3GCMLI      X'40' INF3GCMLI Linux virtual
                                            configuration mode
              00000020       INF3GCMVM      X'20' INF3GCMVM VM virtual
                                            configuration mode
              00000010       INF3GCMCF      X'10' INF3GCMCF CF virtual
                                            configuration mode
    0013   19 Bitstring    1 INF3GPRTP      Guest primary virtual CPU type.
              00000000       INF3PUCCP      X'00' INF3PUCCP General Purpose
                                            (CP)
              00000003       INF3PUCIFL     X'03' INF3PUCIFL Integrated Fac
                                            for Linux (IFL).
    0014   20 Signed       4 INF3GTOD       Bits 0-31 of host TOD at guest
                                            logon.
    0018   24 Character    8 INF3GPNA       Resource pool name. Blanks if not
                                            in a Resource Pool. High
                                            frequency sampler counts These
                                            counts are the number of times
                                            that CP and IFL CPUs of the guest
                                            are observed in each state. These
                                            counts are reset to zero when
                                            Monitor commands are issued that
                                            disable high-frequency sampling.
                                            Otherwise they are monotonically
                                            increasing values. INF1YMONH
                                            provides the high-frequency
                                            sampling interval for the state
                                            testing. For each virtual CPU
                                            type, the order of the count
                                            fields is the order that the
                                            states are tested so that if a
                                            vCPU is in multiple states, it is
                                            counted with the first state that
                                            matches so that it is counted in
                                            one and only one state. The one
                                            exception is that when a guest is
                                            on the dormant list and SVM wait
                                            they are counted in both
                                            INF3GDLSC and INF3GDSSC for
                                            virtual CPs and for IFLs, both
                                            INF3GDLSI and INF3GDSSI. The
                                            values are aggregate values for
                                            all guest virtual CPUs of that
                                            type. See Monitor record MRUSEINT
                                            D4 R4 for additional information.
    0020   32 Signed       4 INF3GIWSC      I/O Wait Samples for CPs. Times
                                            vCPU found in I/O wait for
                                            asynchronous I/O.
    0024   36 Signed       4 INF3GCFSC      Console Function Wait samples for
                                            CPs. Times vCPU found in console
                                            function wait.
    0028   40 Signed       4 INF3GSMSC      Simulation Wait samples for CPs.
                                            Times vCPU found using CPU.
    002C   44 Signed       4 INF3GPWSC      Page Wait Samples for CPs. Times
                                            vCPU found in page wait.
    0030   48 Signed       4 INF3GLSC       Limit list Samples for CPs. Times
                                            vCPU found on limit list.
    0034   52 Signed       4 INF3GDSC       CPU Delay Samples for CPs. Times
                                            vCPU found waiting for CPU.
    0038   56 Signed       4 INF3GCSC       CPU Using Samples for CPs. Times
                                            vCPU found using CPU.
    003C   60 Signed       4 INF3GESSC      E-list SVM Wait Samples for CPs.
                                            Times vCPU found on the eligible
                                            list and in SVM wait.
    0040   64 Signed       4 INF3GLDSC      Loading User Samples for CPs.
                                            Times vCPU considered to be a
                                            loading user and not on the
                                            dormant list.
    0044   68 Signed       4 INF3GDLSC      Dormant User Samples for CPs.
                                            Times vCPU was found to be on the
                                            dormant list.
    0048   72 Signed       4 INF3GDSSC      SVM Wait Samples for CPs. Times
                                            vCPU found in the dormant list
                                            and in SVM wait. Also counted in
                                            INF3GDLSC.
    004C   76 Signed       4 INF3GIASC      I/O Active Samples for CPs. Times
                                            vCPU found with asynchronous I/O
                                            outstanding, causing it to be
                                            left in the Dispatch List.
    0050   80 Signed       4 INF3GTISC      Test Idle Samples for CPs. Times
                                            vCPU found in test idle and not
                                            in SVM wait.
    0054   84 Signed       4 INF3GTSSC      Test Idle & SVM Wait Samples for
                                            CPs. Times vCPU found in test
                                            idle and SVM wait.
    0058   88 Signed       4 INF3GPASC      Page Fault Active Samples for
                                            CPs. Times vCPU had active page
                                            fault requests active but was not
                                            in page wait.
    005C   92 Signed       4 INF3GOSC       Other Samples for CPs. Times vCPU
                                            found in other state.
    0060   96 Signed       4 INF3GTSC       Total Samples for CPs. Times vCPU
                                            state sampled.
    0064  100 Signed       4 INF3GIWSI      I/O Wait Samples for IFLs. Times
                                            vCPU found in I/O wait for
                                            asynchronous I/O.
    0068  104 Signed       4 INF3GCFSI      Console Function Wait samples for
                                            IFLs. Times vCPU found in console
                                            function wait.
    006C  108 Signed       4 INF3GSMSI      Simulation Wait samples for IFLs.
                                            Times vCPU found using CPU.
    0070  112 Signed       4 INF3GPWSI      Page Wait Samples for IFLs. Times
                                            vCPU found in page wait.
    0074  116 Signed       4 INF3GLSI       Limit list Samples for IFLs.
                                            Times vCPU found on limit list.
    0078  120 Signed       4 INF3GDSI       CPU Delay Samples for IFLs. Times
                                            vCPU found waiting for CPU.
    007C  124 Signed       4 INF3GCSI       CPU Using Samples for IFLs. Times
                                            vCPU found using CPU.
    0080  128 Signed       4 INF3GESSI      E-list SVM Wait Samples for IFLs.
                                            Times vCPU found on the eligible
                                            list and in SVM wait.
    0084  132 Signed       4 INF3GLDSI      Loading User Samples for IFLs.
                                            Times vCPU considered to be a
                                            loading user and not on the
                                            dormant list.
    0088  136 Signed       4 INF3GDLSI      Dormant User Samples for IFLs.
                                            Times vCPU was found to be on the
                                            dormant list.
    008C  140 Signed       4 INF3GDSSI      SVM Wait Samples for IFLs. Times
                                            vCPU found in the dormant list
                                            and in SVM wait. Also counted in
                                            INF3GDLSC.
    0090  144 Signed       4 INF3GIASI      I/O Active Samples for IFLs.
                                            Times vCPU found with
                                            asynchronous I/O outstanding,
                                            causing it to be left in the
                                            Dispatch List.
    0094  148 Signed       4 INF3GTISI      Test Idle Samples for IFLs. Times
                                            vCPU found in test idle and not
                                            in SVM wait.
    0098  152 Signed       4 INF3GTSSI      Test Idle & SVM Wait Samples for
                                            IFLs. Times vCPU found in test
                                            idle and SVM wait.
    009C  156 Signed       4 INF3GPASI      Page Fault Active Samples for
                                            IFLs. Times vCPU had active page
                                            fault requests active but was not
                                            in page wait.
    00A0  160 Signed       4 INF3GOSI       Other Samples for IFLs. Times
                                            vCPU found in other state.
    00A4  164 Signed       4 INF3GTSI       Total Samples for IFLs. Times
                                            vCPU state sampled. CPU resources
                                            information
    00A8  168 Bitstring    1 INF3CFLG       Guest CPU Flag Byte
              .1.. ....      INF3CMCT       X'40' INF3CMCT Guest has multiple
                                            CPU types
              ..1. ....      INF3CVCT       X'20' INF3CVCT Virtual CPs are
                                            thread dispatched
              ...1 ....      INF3CVIT       X'10' INF3CVIT Virtual IFLs are
                                            thread dispatched
    00A9  169 Bitstring    1 INF3CAFFN      Guest CPUAFFINITY settings.
              1... ....      INF3CAFON      X'80' INF3CAFON CPUAFFINITY is
                                            ON, but may be suppressed. If
                                            off, then INF3CAFSUP will not be
                                            on.
              .1.. ....      INF3CAFSUP     X'40' INF3CAFSUP CPUAFFINTY is
                                            suppressed.
    00AA  170 Signed       2 INF3CMCPU      Maximum number of guest CPUs
                                            based on user directory setting.
    00AC  172 Signed       4 *              Reserved for IBM use.
    00B0  176 Signed       8 INF3CTCPP      Total virtual and simulation time
                                            while running a virtual CP on a
                                            primary CPU, in prorated core
                                            time microseconds. Only provided
                                            when SMT is enabled
                                            (INF1YFL1.INF1YMTE).
                                            Monotonically increasing.
    00B8  184 Signed       8 INF3CTCPS      Total virtual and simulation time
                                            while running a virtual CP on a
                                            2ndary CPU, in prorated core time
                                            microseconds. Only provided when
                                            SMT is enabled
                                            (INF1YFL1.INF1YMTE).
                                            Monotonically increasing.
    00C0  192 Signed       8 INF3CTCRP      Total virtual and simulation time
                                            while running a virtual CP on a
                                            primary CPU, in raw core time
                                            microseconds. Monotonically
                                            increasing.
    00C8  200 Signed       8 INF3CTCRS      Total virtual and simulation time
                                            while running a virtual CP on a
                                            secondary CPU, in raw core time
                                            microseconds. Monotonically
                                            increasing.
    00D0  208 Signed       2 INF3CSCP       Number of guest shared CPs.
    00D2  210 Signed       2 INF3CDCP       Number of guest dedicated CPs.
    00D4  212 Signed       2 INF3CRCP       Number of non-stopped guest CPs.
    00D6  214 Signed       2 *              Reserved for IBM use.
    00D8  216 Signed       1 INF3CCDT       Dispatch type for guest CPs This
                                            field is valid if INF3CSCP,
                                            INF3CDCP or INF3CRCP is greater
                                            than zero. Always INF3PUCCP.
    00D9  217 Bitstring    1 INF3CCSCF      Current share flags for CPs.
              .1.. ....      INF3CCLHC      X'40' INF3CCLHC Current max share
                                            for CP-dispatched vCPUs is
                                            LIMITHARD if on. Max share for
                                            type CP is LIMITSOFT if off.
              ..1. ....      INF3CCNAC      X'20' INF3CCNAC Current normal
                                            share for CP-dispatched vCPUs is
                                            ABSOLUTE if on. Normal share for
                                            type CP is RELATIVE if off.
              ...1 ....      INF3CCMAC      X'10' INF3CCMAC Current max share
                                            for CP-dispatched vCPUs is
                                            ABSOLUTE if on. Max share for
                                            type CP is RELATIVE if off.
    00DA  218 Bitstring    1 INF3CISCF      Initial share flags for CPs.
              .1.. ....      INF3CILHC      X'40' INF3CILHC Initial max share
                                            for CP-dispatched vCPUs is
                                            LIMITHARD if on. Max share for
                                            type CP is LIMITSOFT if off. This
                                            is the setting at logon.
              ..1. ....      INF3CINAC      X'20' INF3CINAC Initial normal
                                            share for CP-dispatched vCPUs is
                                            ABSOLUTE if on. Normal share for
                                            type CP is RELATIVE if off. This
                                            is the setting at logon.
              ...1 ....      INF3CIMAC      X'10' INF3CIMAC Initial max share
                                            for CP-dispatched vCPUs is
                                            ABSOLUTE if on. Max share for
                                            type CP is RELATIVE if off. This
                                            is the setting at logon.
    00DB  219 Bitstring    1 *              Reserved for IBM use
    00DC  220 Signed       4 INF3CCNSC      Current normal relative share for
                                            CP-dispatched vCPUs. The value is
                                            zero when the user has an
                                            ABSOLUTE share value for CPs, or
                                            has a dedicated virtual CPU or is
                                            in the process of being logged
                                            off.
    00E0  224 Signed       4 INF3CCASC      Current ABSOLUTE share for
                                            CP-dispatched vCPUs. Unit of
                                            value is a hexadecimal factor
                                            scaled 16 bits. For example,
                                            X'00010000' = 1.00(100%),
                                            X'0000C000' = 0.75(75%),
                                            X'00008000' = 0.50(50%), etc. Set
                                            to zero when the user has a
                                            RELATIVE share value for CPs.
    00E4  228 Signed       4 INF3CCMSC      Current Max share for
                                            CP-dispatched vCPUs. This value
                                            is set to zero if no Max share
                                            exists for CPs. If the Max share
                                            is Absolute, then the units of
                                            the value are the same as for
                                            INF3CCASC. Otherwise as for
                                            INF3CCNSC.
    00E8  232 Signed       4 INF3CINSC      Initial (logon) normal relative
                                            share for CP-dispatched vCPUs.
                                            This value will be zero when the
                                            initial (logon) share is ABSOLUTE
                                            for CPs, or the user has a
                                            dedicated virtual CPU or is in
                                            the process of being logged off.
    00EC  236 Signed       4 INF3CIASC      Initial (logon) ABSOLUTE share
                                            for CP-dispatched vCPUs. Unit of
                                            value is a hexadecimal factor
                                            scaled 16 bits. For example,
                                            X'00010000' = 1.00(100%),
                                            X'0000C000' = 0.75(75%),
                                            X'00008000' = 0.50(50%), etc.
                                            This value will be zero when the
                                            initial (logon) share for CPs is
                                            relative.
    00F0  240 Signed       4 INF3CIMSC      Initial (logon) Max share for
                                            CP-dispatched vCPUs. This value
                                            will be zero if no initial
                                            (logon) Max share exists for CPs.
                                            If the Max share is Absolute,
                                            then the units of the value are
                                            the same as for INF3CIASC.
                                            Otherwise as for INF3CINSC.
    00F4  244 Signed       4 *              Reserved for IBM use.
    00F8  248 Signed       8 INF3CTIPP      Total virtual and simulation time
                                            while running a virtual IFL on a
                                            primary CPU, in prorated core
                                            time microseconds. Only provided
                                            when SMT is enabled
                                            (INF1YFL1.INF1YMTE).
                                            Monotonically increasing.
    0100  256 Signed       8 INF3CTIPS      Total virtual and simulation time
                                            while running a virtual IFL on a
                                            2ndary CPU, in prorated core time
                                            microseconds. Only provided when
                                            SMT is enabled
                                            (INF1YFL1.INF1YMTE).
                                            Monotonically increasing.
    0108  264 Signed       8 INF3CTIRP      Total virtual and simulation time
                                            while running a virtual IFL on a
                                            primary CPU, in raw core time
                                            microseconds. Monotonically
                                            increasing.
    0110  272 Signed       8 INF3CTIRS      Total virtual and simulation time
                                            while running a virtual IFL on a
                                            secondary CPU, in raw core time
                                            microseconds. Monotonically
                                            increasing.
    0118  280 Signed       2 INF3CSIF       Number of guest shared IFLs.
    011A  282 Signed       2 INF3CDIF       Number of guest dedicated IFLs.
    011C  284 Signed       2 INF3CRIF       Number of non-stopped guest IFLs.
    011E  286 Signed       2 *              Reserved for IBM use.
    0120  288 Signed       1 INF3CIDT       Dispatch type for guest IFLs.
                                            This field is valid if INF3SCPS,
                                            INF3CDCP or INF3CRCP is greater
                                            than zero.
              00000000       INF3PUCCP      X'00' INF3PUCCP General Purpose
                                            (CP)
              00000003       INF3PUCIFL     X'03' INF3PUCIFL Integrated Fac
                                            for Linux (IFL).
    0121  289 Bitstring    1 INF3CCSIF      Current share flags for IFLs.
              .1.. ....      INF3CCLHI      X'40' INF3CCLHI Current max share
                                            for IFL-dispatched vCPUs is
                                            LIMITHARD if on. Max share for
                                            type IFL is LIMITSOFT if off.
              ..1. ....      INF3CCNAI      X'20' INF3CCNAI Current normal
                                            share for IFL-dispatched vCPUs is
                                            ABSOLUTE if on. Normal share for
                                            type IFL is RELATIVE if off.
              ...1 ....      INF3CCMAI      X'10' INF3CCMAI Current max share
                                            for IFL-dispatched vCPUs is
                                            ABSOLUTE if on. Max share for
                                            type IFL is RELATIVE if off.
    0122  290 Bitstring    1 INF3CISIF      Initial share flags for IFLs.
              .1.. ....      INF3CILHI      X'40' INF3CILHI Initial max share
                                            for IFL-dispatched vCPUs is
                                            LIMITHARD if on. Max share for
                                            type IFL is LIMITSOFT if off.
                                            This is the setting at logon.
              ..1. ....      INF3CINAI      X'20' INF3CINAI Initial normal
                                            share for IFL-dispatched vCPUs is
                                            ABSOLUTE if on. Normal share for
                                            type IFL is RELATIVE if off. This
                                            is the setting at logon.
              ...1 ....      INF3CIMAI      X'10' INF3CIMAI Initial max share
                                            for IFL-dispatched vCPUs is
                                            ABSOLUTE if on. Max share for
                                            type IFL is RELATIVE if off. This
                                            is the setting at logon.
    0123  291 Bitstring    1 *              Reserved for IBM use
    0124  292 Signed       4 INF3CCNSI      Current normal relative share for
                                            IFL-dispatched vCPUs. The value
                                            is zero when the user has an
                                            ABSOLUTE share value for IFLs, or
                                            has a dedicated virtual CPU or is
                                            in the process of being logged
                                            off.
    0128  296 Signed       4 INF3CCASI      Current ABSOLUTE share for
                                            IFL-dispatched vCPUs. Unit of
                                            value is a hexadecimal factor
                                            scaled 16 bits. For example,
                                            X'00010000' = 1.00(100%),
                                            X'0000C000' = 0.75(75%),
                                            X'00008000' = 0.50(50%), etc. The
                                            value is zero when the user has a
                                            RELATIVE share value for IFLs.
    012C  300 Signed       4 INF3CCMSI      Current Max share for
                                            IFL-dispatched vCPUs. This value
                                            will be zero if no Max share
                                            exists for IFLs. If the Max share
                                            is Absolute, then the units of
                                            the value are the same as for
                                            INF3CCASI. Otherwise as for
                                            INF3CCNSI.
    0130  304 Signed       4 INF3CINSI      Initial (logon) normal relative
                                            share for IFL-dispatched vCPUs.
                                            This value will be zero when the
                                            initial (logon) share is ABSOLUTE
                                            for IFLs, or the user has a
                                            dedicated virtual CPU or is in
                                            the process of being logged off.
    0134  308 Signed       4 INF3CIASI      Initial (logon) ABSOLUTE share
                                            for IFL-dispatched vCPUs. Unit of
                                            value is a hexadecimal factor
                                            scaled 16 bits. For example,
                                            X'00010000' = 1.00(100%),
                                            X'0000C000' = 0.75(75%),
                                            X'00008000' = 0.50(50%), etc.
                                            This value will be zero when the
                                            initial (logon) share is relative
                                            for IFLs.
    0138  312 Signed       4 INF3CIMSI      Initial (logon) Max share for
                                            IFL-dispatched vCPUs. This value
                                            will be zero if no initial
                                            (logon) Max share exists for
                                            IFLs. If the Max share is
                                            Absolute, then the units of the
                                            value are the same as for
                                            INF3CIASI. Otherwise as for
                                            INF3CINSI.
    013C  316 Signed       4 *              Reserved for IBM use.
              00000140       INF3GSB1       *-INF3GST Version 1 length in
                                            bytes of the Guest Description.
              00000028       INF3GSD1       (*-INF3GST+7)/8 Version 1 length
                                            in doublewords of the Guest
                                            Description.
              00000140       INF3GSZB       *-INF3GST Length in bytes for
                                            newest version of the Guest
                                            Description.
              00000028       INF3GSZD       (*-INF3GST+7)/8 Length in
                                            doublewords for newest version of
                                            the Guest Description.

     INF4BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF4BK         Mappings for STHYI
            Function code x'0004': Resource Pool List
            This function code returns a list of all Resource
            Pools defined on the system.
            This function code requires the length of the buffer as
            a number of 4K pages to be specified. See the STHYI
            documentation for details of how this is specified.
            The response buffer for function code x'0004' consists
            of 2 sections of data:
            - Header Section (INF2BK DSECT, imbeds INFCHDR DSECT)
              - use offset to Resource Pool list, length of entry,
                and count of entries to process the list.
              - The offset in INFCLSOF is from the beginning
                of the INF4BK.
              - if the count is zero there is no list so the offset
                and length will be zero.
            - Resource Pool list. The list is returned as an array
              with the count of entries, offset to the first entry
              and the entry length defined by the common header.
            - The array entry structure is defined by INF4POOL DSECT.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-RESPOOL.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
             - CC=3 RC=20 - Response buffer is too small.
                          - INFCRQSZ specifies required buffer size.
                          - Values are also provided in INFCVRSN,
                            INFCHDLN and INFCTOTL. Other response
                            buffer contents are unpredictable.
            Update Log - see equates under INF4VRSN.
            Function code X'0004' Response Buffer
            Header Section
    0000    0 Bitstring   64 INF4CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF4VRSN       Response buffer version.
              00000001       INF4V00001     X'0001' INF4V00001 Initial
                                            version. APAR VM66105.
              00000040       INF4BSB1       *-INF4BK Version 1 length in
                                            bytes of the Resource Pool List
                                            header.
              00000008       INF4BSD1       (*-INF4BK+7)/8 Version 1 length
                                            in doublewords of the Resource
                                            Pool List header.
              00000040       INF4BSZB       *-INF4BK Length in bytes for
                                            newest version of the Resource
                                            Pool List header.
              00000008       INF4BSZD       (*-INF4BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Resource Pool List header.

     INF4POOL DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF4POOL       Mappings for STHYI
            Function code X'0004' Response Buffer
            Resource Pool List Entry Description
    0000    0 Character    8 INF4PNAM       Resource Pool name.
    0008    8 Character    8 INF4PCRE       Resource Pool creator userid.
              00000010       INF4PSB1       *-INF4POOL Version 1 length in
                                            bytes of the Resource Pool List
                                            entry.
              00000002       INF4PSD1       (*-INF4POOL+7)/8 Version 1 length
                                            in doublewords of the Resource
                                            Pool List entry.
              00000010       INF4PSZB       *-INF4POOL Length in bytes for
                                            newest version of the Resource
                                            Pool List entry.
              00000002       INF4PSZD       (*-INF4POOL+7)/8 Length in
                                            doublewords for newest version of
                                            the Resource Pool List entry.

     INF5BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF5BK         Mappings for STHYI
            Function code x'0005': Designated Resource Pool Info
            This function code returns the description of the
            specified Resource Pool.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-RESPOOL.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
             - CC=3 RC=12 - Missing or invalid Resource Pool Name.
                          - The response buffer is not modified.
             - CC=3 RC=16 - Named Resource Pool does not exist.
                          - The response buffer is not modified.
            Update Log - see equates under INF5VRSN.
            Function code X'0005' Response Buffer
    0000    0 Bitstring   64 INF5CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF5VRSN       Response buffer version.
              00000001       INF5V00001     X'0001' INF5V00001 Initial
                                            version. APAR VM66105.
    0040   64 Character    8 INF5PLNA       Resource pool name.
    0048   72 Character    8 INF5PCRE       Resource Pool creator's user ID.
    0050   80 Signed       8 INF5STMP       Host TOD value at the time of the
                                            last change to the Resource Pool
                                            definition.
          Resource Pool CPU Limits and usage information.
          A CPU can have a capacity limit for either CP or IFL
          virtual CPU type. That limit can be specified as either
          a CAPACITY or LIMITHARD limit. Therefore never more than
          one of INF5CCCL,INF5CCCC,INF5CICL or INF5CICC will be on.
    0058   88 Bitstring    1 INF5CFLG       Resource Pool CPU Capping Flags
              1... ....      INF5CCLC       X'80' INF5CCLC Resource Pool's CP
                                            virtual type has LIMITHARD cap.
              .1.. ....      INF5CCCC       X'40' INF5CCCC Resource Pool's CP
                                            virtual type has CAPACITY cap.
              ..1. ....      INF5CILC       X'20' INF5CILC Resource Pool's
                                            IFL virtual type has LIMITHARD
                                            cap.
              ...1 ....      INF5CICC       X'10' INF5CICC Resource Pool's
                                            IFL virtual type has CAPACITY
                                            cap.
              .... 1...      INF5CPCT       X'08' INF5CPCT Resource Pool uses
                                            prorated core time.
              .... .1..      INF5CSUP       X'04' INF5CSUP IFL CPUAFFINITY is
                                            suppressed. Not set for CP
                                            resource pools.
    0059   89 Bitstring    3 *              Reserved for IBM use.
    005C   92 Signed       4 INF5CLIM       Resource pool maximum share for
                                            shared virtual CPUs. Scaled
                                            number where X'00010000'
                                            represents 1 core if the cap is a
                                            CAPACITY cap, or 100% of the real
                                            processors if the cap is a
                                            LIMITHARD cap. Zero if not
                                            capped. INF5CFLG specifies the
                                            capped CPU type.
    0060   96 Signed       8 INF5CTIM       Total Time consumed by guests
                                            vCPUs in the Resource Pool since
                                            it was created. Monotonically
                                            increasing in microseconds. If MT
                                            is enabled, this field contains
                                            prorated core time; Otherwise,
                                            this field contains raw CPU time.
    0068  104 Signed       4 INF5CLMN       Total number of times the
                                            Resource Pool was limited since
                                            it was created. Monotonically
                                            increasing. Incremented at end of
                                            group limit.
    006C  108 Signed       4 INF5CCTL       Total number of times vCPUs of
                                            members of the Resource Pool were
                                            limited since it was created.
                                            Monotonically increasing. Updated
                                            at the start of the vCPU limit.
    0070  112 Signed       8 INF5CTML       Total time limited for vCPUs of
                                            all members of the Resource Pool
                                            since it was created.
                                            Monotonically increasing in
                                            microseconds. Updated at the
                                            start of the vCPU limit.
    0078  120 Signed       4 INF5CIFLA      IFL CPUAFFINITY toggle sequence
                                            number. It is incremented when
                                            IFL CPUAFFINITY suppression is
                                            turned on or off for pools with
                                            members.
    007C  124 Signed       4 *              Reserved for IBM use.
              00000080       INF5BSB1       *-INF5BK Version 1 length in
                                            bytes of the Resource Pool
                                            Information response.
              00000010       INF5BSD1       (*-INF5BK+7)/8 Version 1 length
                                            in doublewords of the Resource
                                            Pool Information response.
              00000080       INF5BSZB       *-INF5BK Length in bytes for
                                            newest version of the Resource
                                            Pool Information response.
              00000010       INF5BSZD       (*-INF5BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Resource Pool Information
                                            response.

     INF6BK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF6BK         Mappings for STHYI
            Function code x'0006': Resource Pool Member List
            This function code returns the list of members of the
            specified Resource Pool.
            This function code requires the length of the buffer as
            a number of 4K pages to be specified. See the STHYI
            documentation for details of how this is specified.
            The response buffer for function code x'0006' consists
            of 2 sections of data:
            - Header Section (INF2BK DSECT, imbeds INFCHDR DSECT)
              - use offset to Resource Pool member list, length of
                entry, and count of entries to process the list.
              - The offset in INFCLSOF is from the beginning
                of the INF6BK.
              - if the count is zero there is no list so the offset
                and length will be zero.
            - Resource Pool Member list is returned as an array
              with the count of entries, offset to the first entry
              and the entry length defined by the common header.
            - The array entry structure is defined by INF6MEM DSECT.
            Use of this function code is authorized in the User
            Directory by OPTION STHYI-RESPOOL.
            Error responses:
             - CC=3 RC=4  - Unsupported function code
                          - The response buffer is not modified.
             - CC=3 RC=8  - Not authorized for function code
                          - The response buffer is not modified.
             - CC=3 RC=12 - Missing or invalid Resource Pool Name.
                          - The response buffer is not modified.
             - CC=3 RC=16 - Named Resource Pool does not exist.
                          - The response buffer is not modified.
             - CC=3 RC=20 - Response buffer is too small.
                          - INFCRQSZ specifies required buffer size.
                          - Values are also provided in INFCVRSN,
                            INFCHDLN and INFCTOTL. Other response
                            buffer contents are unpredictable.
            Update Log - see equates under INF6VRSN.
            Function code X'0006' Response Buffer
            Header Section
    0000    0 Bitstring   64 INF6CHDR       Common section of header mapped
                                            by INFCHDR DSECT.
    0000    0 Signed       2 INF6VRSN       Response buffer version.
              00000001       INF6V00001     X'0001' INF6V00001 Initial
                                            version. APAR VM66105.
    0040   64 Character    8 INF6PLNA       Resource pool name.
              00000048       INF6BSB1       *-INF6BK Version 1 length in
                                            bytes of the Resource Pool Member
                                            List header.
              00000009       INF6BSD1       (*-INF6BK+7)/8 Version 1 length
                                            in doublewords of the Resource
                                            Pool Member List header.
              00000048       INF6BSZB       *-INF6BK Length in bytes for
                                            newest version of the Resource
                                            Pool Member List header.
              00000009       INF6BSZD       (*-INF6BK+7)/8 Length in
                                            doublewords for newest version of
                                            the Resource Pool Member List
                                            header.

     INF6MEM DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      INF6MEM        Mappings for STHYI
            Function code X'0006' Response Buffer
            Resource Pool Member List Entry Description
    0000    0 Character    8 INF6MNAM       Resource Pool member name.
              00000008       INF6MSB1       *-INF6MEM Version 1 length in
                                            bytes of the Resource Pool Member
                                            List entry.
              00000001       INF6MSD1       (*-INF6MEM+7)/8 Version 1 length
                                            in doublewords of the Resource
                                            Pool Member List entry.
              00000008       INF6MSZB       *-INF6MEM Length in bytes for
                                            newest version of the Resource
                                            Pool Member List entry.
              00000001       INF6MSZD       (*-INF6MEM+7)/8 Length in
                                            doublewords for newest version of
                                            the Resource Pool Member List
                                            entry.

INFBK Storage Layout | Top of page

    *** INFBK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                       INFRESP                         |
    *     +-------------------------------------------------------+
    *   8
    *
    *** INFBK - Mappings for STHYI

    *** INF0HDR - Mappings for STHYI
    *
    *     +------+------+------+------+--------------------+------+
    *   0 |:HFLG1|:HFLG2|:HVAL1|:HVAL2|////////////////////|:HYGCT|
    *     +------+------+------+------+-------------+------+------+
    *   8 |  INFHTOTL   |  INFHDLN    |  INFMOFF    |  INFMLEN    |
    *     +-------------+-------------+-------------+-------------+
    *  10 |  INFPOFF    |  INFPLEN    |        INFHYGS1-          |
    *     +-------------+-------------+---------------------------+
    *  18 |          -(014)           | 1C
    *     +---------------------------+
    *
    *** INF0HDR - Mappings for STHYI

    *** Overlay for INFHYGS1 in INF0HDR
    *
    *                                 +-------------+-------------+
    *  10 ...                      14 |  INFHOFF1   |  INFHLEN1   |
    *     +-------------+-------------+-------------+-------------+
    *  18 |  INFGOFF1   |  INFGLEN1   |        INFHYGS2-          |
    *     +-------------+-------------+---------------------------+
    *  20 |          -(01C)           | 24
    *     +---------------------------+
    *
    *** Overlay for INFHYGS1 in INF0HDR

    *** Overlay for INFHYGS2 in INF0HDR
    *
    *                                 +-------------+-------------+
    *  18 ...                      1C |  INFHOFF2   |  INFHLEN2   |
    *     +-------------+-------------+-------------+-------------+
    *  20 |  INFGOFF2   |  INFGLEN2   |        INFHYGS3-          |
    *     +-------------+-------------+---------------------------+
    *  28 |          -(024)           | 2C
    *     +---------------------------+
    *
    *** Overlay for INFHYGS2 in INF0HDR

    *** Overlay for INFHYGS3 in INF0HDR
    *
    *                                 +-------------+-------------+
    *  20 ...                      24 |  INFHOFF3   |  INFHLEN3   |
    *     +-------------+-------------+-------------+-------------+
    *  28 |  INFGOFF3   |  INFGLEN3   |///////////////////////////|
    *     +-------------+-------------+---------------------------+
    *  30
    *
    *** Overlay for INFHYGS3 in INF0HDR

    *** INF0HDYG - Mappings for STHYI
    *
    *     +-------------+-------------+-------------+-------------+
    *   0 |  INFYOFF    |  INFYLEN    |  INFGOFF    |  INFGLEN    |
    *     +-------------+-------------+-------------+-------------+
    *   8
    *
    *** INF0HDYG - Mappings for STHYI

    *** INF0MAC - Mappings for STHYI
    *
    *     +------+------+------+------+-------------+-------------+
    *   0 |:MFLG1|:MFLG2|:MVAL1|:MVAL2|  INFMSCPS   |  INFMDCPS   |
    *     +------+------+------+------+-------------+-------------+
    *   8 |  INFMSIFL   |  INFMDIFL   |        INFMNAME-          |
    *     +-------------+-------------+---------------------------+
    *  10 |          -(00C)           |         INFMTYPE          |
    *     +---------------------------+---------------------------+
    *  18 |                       INFMMANU                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  28 |                       INFMSEQ                         |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  38 |         INFMPMAN          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  40 |                       INFMPLNM                        |
    *     +-------------+-------------+---------------------------+
    *  48 | INFMSZIIP   | INFMDZIIP   |///////////////////////////|
    *     +-------------+-------------+---------------------------+
    *  50
    *
    *** INF0MAC - Mappings for STHYI

    *** INF0PAR - Mappings for STHYI
    *
    *     +------+------+------+------+-------------+-------------+
    *   0 |:PFLG1|:PFLG2|:PVAL1|:PVAL2|  INFPPNUM   |  INFPSCPS   |
    *     +------+------+------+------+-------------+-------------+
    *   8 |  INFPDCPS   |  INFPSIFL   |  INFPDIFL   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  10 |                       INFPPNAM                        |
    *     +---------------------------+---------------------------+
    *  18 |         INFPWBCP          |         INFPABCP          |
    *     +---------------------------+---------------------------+
    *  20 |         INFPWBIF          |         INFPABIF          |
    *     +---------------------------+---------------------------+
    *  28 |                       INFPLGNM                        |
    *     +---------------------------+---------------------------+
    *  30 |         INFPLGCP          |         INFPLGIF          |
    *     +---------------------------+---------------------------+
    *  38 |                       INFPPLNM                        |
    *     +-------------+-------------+---------------------------+
    *  40 | INFPSZIIP   | INFPDZIIP   |        INFPWBZIIP         |
    *     +-------------+-------------+---------------------------+
    *  48 |        INFPABZIIP         |        INFPLGZIIP         |
    *     +---------------------------+---------------------------+
    *  50
    *
    *** INF0PAR - Mappings for STHYI

    *** INF0HYP - Mappings for STHYI
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:YFLG1|:YFLG2|:YVAL1|:YVAL2|:YTYPE|//////|:YCPT |:YIFLT|
    *     +------+------+------+------+------+------+------+------+
    *   8 |                       INFYSYID                        |
    *     +-------------------------------------------------------+
    *  10 |                       INFYCLNM                        |
    *     +-------------+-------------+-------------+-------------+
    *  18 |  INFYSCPS   |  INFYDCPS   |  INFYSIFL   |  INFYDIFL   |
    *     +------+------+------+------+------+------+------+------+
    *  20 |:YINS0|:YINS1|:YINS2|:YINS3|:YINS4|:YINS5|:YINS6|:YINS7|
    *     +------+------+------+------+------+------+------+------+
    *  28 |:YAUT0|:YAUT1|:YAUT2|:YAUT3|:YAUT4|:YAUT5|:YAUT6|:YAUT7|
    *     +------+------+------+------+------+------+------+------+
    *  30 |(030) |//////| INFYSZIIP   |///////////////////////////|
    *     +------+------+-------------+---------------------------+
    *  38
    *
    *** INF0HYP - Mappings for STHYI

    *** INF0GST - Mappings for STHYI
    *
    *     +------+------+------+------+---------------------------+
    *   0 |:GFLG1|:GFLG2|:GVAL1|:GVAL2|        INFGUSID-          |
    *     +------+------+------+------+-------------+-------------+
    *   8 |          -(004)           |  INFGSCPS   |  INFGDCPS   |
    *     +------+--------------------+-------------+-------------+
    *  10 |:GCPDT|////////////////////|         INFGCPCC          |
    *     +------+------+-------------+------+--------------------+
    *  18 |  INFGSIFL   |  INFGDIFL   |:GIFDT|////////////////////|
    *     +-------------+-------------+------+--------------------+
    *  20 |         INFGIFCC          |:GPFLG|////////////////////|
    *     +---------------------------+------+--------------------+
    *  28 |                       INFGPNAM                        |
    *     +---------------------------+---------------------------+
    *  30 |         INFGPCCC          |         INFGPICC          |
    *     +-------------+------+------+---------------------------+
    *  38 | INFGSZIIP   |(03A) |//////|        INFGZIIPCC         |
    *     +-------------+------+------+---------------------------+
    *  40 |         INFGPZCC          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  48
    *
    *** INF0GST - Mappings for STHYI

    *** INFCHDR - Mappings for STHYI
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  INFCVRSN   |  INFCHDLN   |         INFCTOTL          |
    *     +-------------+-------------+-------------+-------------+
    *   8 |  INFCRQSZ   |  INFCLSOF   |  INFCENLN   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  10 |         INFCCTEN          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  18 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  30 |                       INFCFCUS                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40
    *
    *** INFCHDR - Mappings for STHYI

    *** INF1BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF1CHDR                        =
    *     |                                                       |
    *     +------+------+------+------+--------------------+------+
    *  40 |:1HFL1|:1HFL2|:1HVL1|:1HVL2|////////////////////|:1HYGC|
    *     +------+------+------+------+-------------+------+------+
    *  48 |  INF1MOFF   |  INF1MLEN   |  INF1POFF   |  INF1PLEN   |
    *     +-------------+-------------+-------------+-------------+
    *  50 |  INF1YOF1   |  INF1YLN1   |  INF1YVR1   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  58 |  INF1GOF1   |  INF1GLN1   |  INF1GVR1   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  60 |  INF1YOF2   |  INF1YLN2   |  INF1YVR2   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  68 |  INF1GOF2   |  INF1GLN2   |  INF1GVR2   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  70 |  INF1YOF3   |  INF1YLN3   |  INF1YVR3   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  78 |  INF1GOF3   |  INF1GLN3   |  INF1GVR3   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  80
    *
    *** INF1BK - Mappings for STHYI

    *** Overlay for INF1BK+(INFCVRSN-INFCHDR) in INF1BK
    *
    *     +-------------+
    *   0 |  INF1VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF1BK+(INFCVRSN-INFCHDR) in INF1BK

    *** INF1YGHD - Mappings for STHYI
    *
    *     +-------------+-------------+-------------+-------------+
    *   0 |  INF1YOFF   |  INF1YLEN   |  INF1YVRS   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *   8 |  INF1GOFF   |  INF1GLEN   |  INF1GVRS   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    *  10
    *
    *** INF1YGHD - Mappings for STHYI

    *** INF1MAC - Mappings for STHYI
    *
    *     +------+------+------+------+-------------+-------------+
    *   0 |:1MFL1|:1MFL2|:1MVL1|:1MVL2|  INF1MSCP   |  INF1MDCP   |
    *     +------+------+------+------+-------------+-------------+
    *   8 |  INF1MSIF   |  INF1MDIF   |         INF1MTYP          |
    *     +-------------+-------------+---------------------------+
    *  10 |                       INF1MNAM                        |
    *     +-------------------------------------------------------+
    *  18 |                       INF1MMAN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  28 |                       INF1MSEQ                        |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  38 |         INF1MPMA          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  40 |                      INF1MPLNM                        |
    *     +-------------------------------------------------------+
    *  48
    *
    *** INF1MAC - Mappings for STHYI

    *** INF1PAR - Mappings for STHYI
    *
    *     +------+------+------+------+-------------+-------------+
    *   0 |:1PFL1|:1PFL2|:1PVL1|:1PVL2|  INF1PSCP   |  INF1PDCP   |
    *     +------+------+------+------+-------------+------+------+
    *   8 |  INF1PSIF   |  INF1PDIF   |  INF1PPNU   |(00E) |(00F) |
    *     +-------------+-------------+-------------+------+------+
    *  10 |                       INF1PPNA                        |
    *     +---------------------------+---------------------------+
    *  18 |         INF1PWBC          |         INF1PABC          |
    *     +---------------------------+---------------------------+
    *  20 |         INF1PWBI          |         INF1PABI          |
    *     +---------------------------+---------------------------+
    *  28 |                       INF1PLGN                        |
    *     +---------------------------+---------------------------+
    *  30 |         INF1PLGC          |         INF1PLGI          |
    *     +---------------------------+---------------------------+
    *  38 |                      INF1PPLNM                        |
    *     +---------------------------+---------------------------+
    *  40 |         INF1PENC          |         INF1PENI          |
    *     +---------------------------+---------------------------+
    *  48 |                      INF1PSXCA                        |
    *     +-------------------------------------------------------+
    *  50 |                      INF1PSXIA                        |
    *     +---------------------------+---------------------------+
    *  58 |        INF1PSXCC          |        INF1PSXIC          |
    *     +---------------------------+---------------------------+
    *  60 |                      INF1PUCPA                        |
    *     +-------------------------------------------------------+
    *  68 |                      INF1PUIFA                        |
    *     +---------------------------+---------------------------+
    *  70 |        INF1PUCPC          |        INF1PUIFC          |
    *     +---------------------------+---------------------------+
    *  78 |                      INF1PGUCA                        |
    *     +-------------------------------------------------------+
    *  80 |                      INF1PGUIA                        |
    *     +---------------------------+---------------------------+
    *  88 |        INF1PGUCC          |        INF1PGUIC          |
    *     +---------------------------+---------------------------+
    *  90 |                      INF1PUTOD                        |
    *     +-------------------------------------------------------+
    *  98 |                      INF1PACTC                        |
    *     +-------------------------------------------------------+
    *  A0 |                      INF1PLPTC                        |
    *     +-------------------------------------------------------+
    *  A8 |                      INF1POLTC                        |
    *     +-------------------------------------------------------+
    *  B0 |                      INF1PWTTC                        |
    *     +-------------------------------------------------------+
    *  B8 |                      INF1PMTIC                        |
    *     +-------------------------------------------------------+
    *  C0 |                      INF1PACTI                        |
    *     +-------------------------------------------------------+
    *  C8 |                      INF1PLPTI                        |
    *     +-------------------------------------------------------+
    *  D0 |                      INF1POLTI                        |
    *     +-------------------------------------------------------+
    *  D8 |                      INF1PWTTI                        |
    *     +-------------------------------------------------------+
    *  E0 |                      INF1PMTII                        |
    *     +-------------------------------------------------------+
    *  E8
    *
    *** INF1PAR - Mappings for STHYI

    *** INF1HYP - Mappings for STHYI
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:1YFL1|:1YFL2|:1YVL1|:1YVL2|:1YTYP|//////|:1YCPT|:1YIFT|
    *     +------+------+------+------+------+------+------+------+
    *   8 |                       INF1YSID                        |
    *     +-------------------------------------------------------+
    *  10 |                       INF1YCLN                        |
    *     +-------------+-------------+-------------+-------------+
    *  18 |  INF1YSCP   |  INF1YDCP   |  INF1YSIF   |  INF1YDIF   |
    *     +-------------+-------------+-------------+-------------+
    *  20 |         INF1YASC          |         INF1YASI          |
    *     +---------------------------+---------------------------+
    *  28 |         INF1YRSC          |         INF1YRSI          |
    *     +---------------------------+---------------------------+
    *  30 |         INF1YLCC          |         INF1YLCI          |
    *     +---------------------------+------+------+------+------+
    *  38 |        INF1YMONH          |:1YPKF|(03D) |(03E) |//////|
    *     +---------------------------+------+------+------+------+
    *  40 |        INF1YPADC          |        INF1YPADI          |
    *     +---------------------------+---------------------------+
    *  48 |                      INF1YUTOD                        |
    *     +-------------------------------------------------------+
    *  50 |                       INF1YUTC                        |
    *     +-------------------------------------------------------+
    *  58 |                       INF1YUTI                        |
    *     +-------------------------------------------------------+
    *  60 |                       INF1YSTC                        |
    *     +-------------------------------------------------------+
    *  68 |                       INF1YSTI                        |
    *     +-------------------------------------------------------+
    *  70 |                       INF1YWTC                        |
    *     +-------------------------------------------------------+
    *  78 |                       INF1YWTI                        |
    *     +-------------------------------------------------------+
    *  80 |                       INF1YPTC                        |
    *     +-------------------------------------------------------+
    *  88 |                       INF1YPTI                        |
    *     +-------------------------------------------------------+
    *  90
    *
    *** INF1HYP - Mappings for STHYI

    *** INF1GST - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF1GSTI                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 140
    *
    *** INF1GST - Mappings for STHYI

    *** INF2BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF2CHDR                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40
    *
    *** INF2BK - Mappings for STHYI

    *** Overlay for INF2BK+(INFCVRSN-INFCHDR) in INF2BK
    *
    *     +-------------+
    *   0 |  INF2VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF2BK+(INFCVRSN-INFCHDR) in INF2BK

    *** INF2GST - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                       INF2GUID                        |
    *     +-------------------------------------------------------+
    *   8 |                       INF2GACN                        |
    *     +---------------------------+------+------+------+------+
    *  10 |         INF2GTOD          |:2GFLG|(015) |(016) |(017) |
    *     +------+--------------------+------+------+------+------+
    *  18 |(018) |////////////////////////////////////////////////|
    *     +------+------------------------------------------------+
    *  20
    *
    *** INF2GST - Mappings for STHYI

    *** INF3BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF3CHDR                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                                                       |
    *     =                       INF3GSTI                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 180
    *
    *** INF3BK - Mappings for STHYI

    *** Overlay for INF3BK+(INFCVRSN-INFCHDR) in INF3BK
    *
    *     +-------------+
    *   0 |  INF3VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF3BK+(INFCVRSN-INFCHDR) in INF3BK

    *** INF3GST - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                       INF3GUID                        |
    *     +-------------------------------------------------------+
    *   8 |                       INF3GACN                        |
    *     +------+------+------+------+---------------------------+
    *  10 |:3GFLG|:3GVAL|(012) |(013) |         INF3GTOD          |
    *     +------+------+------+------+---------------------------+
    *  18 |                       INF3GPNA                        |
    *     +---------------------------+---------------------------+
    *  20 |        INF3GIWSC          |        INF3GCFSC          |
    *     +---------------------------+---------------------------+
    *  28 |        INF3GSMSC          |        INF3GPWSC          |
    *     +---------------------------+---------------------------+
    *  30 |         INF3GLSC          |         INF3GDSC          |
    *     +---------------------------+---------------------------+
    *  38 |         INF3GCSC          |        INF3GESSC          |
    *     +---------------------------+---------------------------+
    *  40 |        INF3GLDSC          |        INF3GDLSC          |
    *     +---------------------------+---------------------------+
    *  48 |        INF3GDSSC          |        INF3GIASC          |
    *     +---------------------------+---------------------------+
    *  50 |        INF3GTISC          |        INF3GTSSC          |
    *     +---------------------------+---------------------------+
    *  58 |        INF3GPASC          |         INF3GOSC          |
    *     +---------------------------+---------------------------+
    *  60 |         INF3GTSC          |        INF3GIWSI          |
    *     +---------------------------+---------------------------+
    *  68 |        INF3GCFSI          |        INF3GSMSI          |
    *     +---------------------------+---------------------------+
    *  70 |        INF3GPWSI          |         INF3GLSI          |
    *     +---------------------------+---------------------------+
    *  78 |         INF3GDSI          |         INF3GCSI          |
    *     +---------------------------+---------------------------+
    *  80 |        INF3GESSI          |        INF3GLDSI          |
    *     +---------------------------+---------------------------+
    *  88 |        INF3GDLSI          |        INF3GDSSI          |
    *     +---------------------------+---------------------------+
    *  90 |        INF3GIASI          |        INF3GTISI          |
    *     +---------------------------+---------------------------+
    *  98 |        INF3GTSSI          |        INF3GPASI          |
    *     +---------------------------+---------------------------+
    *  A0 |         INF3GOSI          |         INF3GTSI          |
    *     +------+------+-------------+---------------------------+
    *  A8 |:3CFLG|(0A9) | INF3CMCPU   |///////////////////////////|
    *     +------+------+-------------+---------------------------+
    *  B0 |                      INF3CTCPP                        |
    *     +-------------------------------------------------------+
    *  B8 |                      INF3CTCPS                        |
    *     +-------------------------------------------------------+
    *  C0 |                      INF3CTCRP                        |
    *     +-------------------------------------------------------+
    *  C8 |                      INF3CTCRS                        |
    *     +-------------+-------------+-------------+-------------+
    *  D0 |  INF3CSCP   |  INF3CDCP   |  INF3CRCP   |/////////////|
    *     +------+------+------+------+-------------+-------------+
    *  D8 |:3CCDT|(0D9) |(0DA) |//////|        INF3CCNSC          |
    *     +------+------+------+------+---------------------------+
    *  E0 |        INF3CCASC          |        INF3CCMSC          |
    *     +---------------------------+---------------------------+
    *  E8 |        INF3CINSC          |        INF3CIASC          |
    *     +---------------------------+---------------------------+
    *  F0 |        INF3CIMSC          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  F8 |                      INF3CTIPP                        |
    *     +-------------------------------------------------------+
    * 100 |                      INF3CTIPS                        |
    *     +-------------------------------------------------------+
    * 108 |                      INF3CTIRP                        |
    *     +-------------------------------------------------------+
    * 110 |                      INF3CTIRS                        |
    *     +-------------+-------------+-------------+-------------+
    * 118 |  INF3CSIF   |  INF3CDIF   |  INF3CRIF   |/////////////|
    *     +------+------+------+------+-------------+-------------+
    * 120 |:3CIDT|(121) |(122) |//////|        INF3CCNSI          |
    *     +------+------+------+------+---------------------------+
    * 128 |        INF3CCASI          |        INF3CCMSI          |
    *     +---------------------------+---------------------------+
    * 130 |        INF3CINSI          |        INF3CIASI          |
    *     +---------------------------+---------------------------+
    * 138 |        INF3CIMSI          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 140
    *
    *** INF3GST - Mappings for STHYI

    *** INF4BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF4CHDR                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40
    *
    *** INF4BK - Mappings for STHYI

    *** Overlay for INF4BK+(INFCVRSN-INFCHDR) in INF4BK
    *
    *     +-------------+
    *   0 |  INF4VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF4BK+(INFCVRSN-INFCHDR) in INF4BK

    *** INF4POOL - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                       INF4PNAM                        |
    *     +-------------------------------------------------------+
    *   8 |                       INF4PCRE                        |
    *     +-------------------------------------------------------+
    *  10
    *
    *** INF4POOL - Mappings for STHYI

    *** INF5BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF5CHDR                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                       INF5PLNA                        |
    *     +-------------------------------------------------------+
    *  48 |                       INF5PCRE                        |
    *     +-------------------------------------------------------+
    *  50 |                       INF5STMP                        |
    *     +------+--------------------+---------------------------+
    *  58 |:5CFLG|////////////////////|         INF5CLIM          |
    *     +------+--------------------+---------------------------+
    *  60 |                       INF5CTIM                        |
    *     +---------------------------+---------------------------+
    *  68 |         INF5CLMN          |         INF5CCTL          |
    *     +---------------------------+---------------------------+
    *  70 |                       INF5CTML                        |
    *     +---------------------------+---------------------------+
    *  78 |        INF5CIFLA          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  80
    *
    *** INF5BK - Mappings for STHYI

    *** Overlay for INF5BK+(INFCVRSN-INFCHDR) in INF5BK
    *
    *     +-------------+
    *   0 |  INF5VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF5BK+(INFCVRSN-INFCHDR) in INF5BK

    *** INF6BK - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       INF6CHDR                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                       INF6PLNA                        |
    *     +-------------------------------------------------------+
    *  48
    *
    *** INF6BK - Mappings for STHYI

    *** Overlay for INF6BK+(INFCVRSN-INFCHDR) in INF6BK
    *
    *     +-------------+
    *   0 |  INF6VRSN   | 2
    *     +-------------+
    *
    *** Overlay for INF6BK+(INFCVRSN-INFCHDR) in INF6BK

    *** INF6MEM - Mappings for STHYI
    *
    *     +-------------------------------------------------------+
    *   0 |                       INF6MNAM                        |
    *     +-------------------------------------------------------+
    *   8
    *
    *** INF6MEM - Mappings for STHYI

INFBK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    INFBASIC       0000 10
    INFCAPAC       0000 00000000
    INFCCTEN       0010
    INFCENLN       000C
    INFCFCUS       0030
    INFCHDLN       0002
    INFCLSOF       000A
    INFCRQSZ       0008
    INFCSB1        0030 00000040
    INFCSD1        0030 00000008
    INFCSZB        0030 00000040
    INFCSZD        0030 00000008
    INFCTOTL       0004
    INFCVRSN       0000
    INFGCPCC       0014
    INFGCPDT       0010
    INFGCPLH       0000 20
    INFGDCPS       000E
    INFGDIFL       001A
    INFGFLG1       0000
    INFGFLG2       0001
    INFGIFCC       0020
    INFGIFDT       001C
    INFGIFLH       0000 10
    INFGLEN        0006
    INFGLEN1       001A
    INFGLEN2       0022
    INFGLEN3       002A
    INFGMCPT       0000 40
    INFGMOB        0000 80
    INFGOFF        0004
    INFGOFF1       0018
    INFGOFF2       0020
    INFGOFF3       0028
    INFGPCCC       0030
    INFGPCLH       0024 80
    INFGPCPC       0024 40
    INFGPDU        0000 80
    INFGPFLG       0024
    INFGPICC       0034
    INFGPIFC       0024 10
    INFGPILH       0024 20
    INFGPNAM       0028
    INFGPUCCP      0010 00000000
    INFGPUCCP      001C 00000000
    INFGPUCCP      003A 00000000
    INFGPUCIFL     0010 00000003
    INFGPUCIFL     001C 00000003
    INFGPUCIFL     003A 00000003
    INFGPUCZCP     0010 000000FF
    INFGPUCZCP     001C 000000FF
    INFGPUCZCP     003A 000000FF
    INFGPUCZIP     0010 00000005
    INFGPUCZIP     001C 00000005
    INFGPUCZIP     003A 00000005
    INFGPZCC       0040
    INFGPZLH       0024 04
    INFGPZPC       0024 02
    INFGSCPS       000C
    INFGSIFL       0018
    INFGSTI        0000 00000003
    INFGSTL        0000 00000002
    INFGSZIIP      0038
    INFGUSID       0004
    INFGVAL1       0002
    INFGVAL2       0003
    INFGVCPT       0000 08
    INFGVIFT       0000 04
    INFGVZIIPT     0000 01
    INFGZIIPCC     003C
    INFGZIIPDT     003A
    INFGZIIPH      0000 02
    INFGZIIPV      0002 80
    INFHDLN        000A
    INFHFLG1       0000
    INFHFLG2       0001
    INFHLEN1       0016
    INFHLEN2       001E
    INFHLEN3       0026
    INFHOFF1       0014
    INFHOFF2       001C
    INFHOFF3       0024
    INFHTOTL       0008
    INFHVAL1       0002
    INFHVAL2       0003
    INFHYGCT       0007
    INFHYGS1       0014
    INFHYGS2       001C
    INFHYGS3       0024
    INFHYPER       0000 00000001
    INFMDCPS       0006
    INFMDIFL       000A
    INFMDZIIP      004A
    INFMFLG1       0000
    INFMFLG2       0001
    INFMLEN        000E
    INFMMANU       0018
    INFMMID        0002 40
    INFMMNAM       0002 20
    INFMNAME       000C
    INFMOFF        000C
    INFMPLNM       0040
    INFMPLNV       0002 10
    INFMPMAN       0038
    INFMPOOL       0000 80
    INFMPROC       0002 80
    INFMSCPS       0004
    INFMSEQ        0028
    INFMSIFL       0008
    INFMSZIIP      0048
    INFMTYPE       0014
    INFMVAL1       0002
    INFMVAL2       0003
    INFMZIIPV      0002 08
    INFPABCP       001C
    INFPABIF       0024
    INFPABZIIP     0048
    INFPACC        0002 20
    INFPDCPS       0008
    INFPDIFL       000C
    INFPDZIIP      0042
    INFPFLG1       0000
    INFPFLG2       0001
    INFPLEN        0012
    INFPLGCP       0030
    INFPLGIF       0034
    INFPLGNM       0028
    INFPLGVL       0002 08
    INFPLGZIIP     004C
    INFPMTEN       0000 80
    INFPOFF        0010
    INFPOOLI       0000 00000005
    INFPOOLL       0000 00000004
    INFPOOLM       0000 00000006
    INFPPID        0002 10
    INFPPLNM       0038
    INFPPLNV       0002 04
    INFPPNAM       0010
    INFPPNUM       0004
    INFPPOOL       0000 40
    INFPPROC       0002 80
    INFPRCTM       0024 08
    INFPSCPS       0006
    INFPSIFL       000A
    INFPSZIIP      0040
    INFPVAL1       0002
    INFPVAL2       0003
    INFPWBCC       0002 40
    INFPWBCP       0018
    INFPWBIF       0020
    INFPWBZIIP     0044
    INFPZIIPV      0002 02
    INFRCAUT       0000 00000008
    INFRCBUF       0000 00000014
    INFRCMIS       0000 0000000C
    INFRCNAM       0000 00000010
    INFRCNXT       0000 00000018
    INFRCOK        0000 00000000
    INFRESP        0000
    INFRFC         0000 00000004
    INFSTHYI       0000 40
    INFVSI         0000 20
    INFYAUTF       0028
    INFYAUT0       0028
    INFYAUT1       0029
    INFYAUT2       002A
    INFYAUT3       002B
    INFYAUT4       002C
    INFYAUT5       002D
    INFYAUT6       002E
    INFYAUT7       002F
    INFYCLNM       0010
    INFYCPT        0006
    INFYDCPS       001A
    INFYDIFL       001E
    INFYFCCP       0020 80
    INFYFCCP       0028 80
    INFYFGLS       0020 20
    INFYFGLS       0028 20
    INFYFGST       0020 10
    INFYFGST       0028 10
    INFYFHYP       0020 40
    INFYFHYP       0028 40
    INFYFLG1       0000
    INFYFLG2       0001
    INFYFPDS       0020 04
    INFYFPDS       0028 04
    INFYFPLS       0020 08
    INFYFPLS       0028 08
    INFYFPML       0020 02
    INFYFPML       0028 02
    INFYIFLT       0007
    INFYINSF       0020
    INFYINS0       0020
    INFYINS1       0021
    INFYINS2       0022
    INFYINS3       0023
    INFYINS4       0024
    INFYINS5       0025
    INFYINS6       0026
    INFYINS7       0027
    INFYLEN        0002
    INFYLMCN       0000 80
    INFYLMPR       0000 40
    INFYMTEN       0000 20
    INFYOFF        0000
    INFYSCPS       0018
    INFYSIFL       001C
    INFYSYID       0008
    INFYSZIIP      0032
    INFYTKVM       0004 00000002
    INFYTVM        0004 00000001
    INFYTYPE       0004
    INFYTZCX       0004 00000003
    INFYVAL1       0002
    INFYVAL2       0003
    INFYZIIPT      0030
    INFYZIIPV      0002 80
    INF0GSIZ       0044 00000048
    INF0GSZD       0044 00000009
    INF0HDSD       002C 00000006
    INF0HDSZ       002C 00000030
    INF0HYSD       0006 00000001
    INF0HYSZ       0006 00000008
    INF0MSIZ       004C 00000050
    INF0MSZD       004C 0000000A
    INF0PSIZ       004C 00000050
    INF0PSZD       004C 0000000A
    INF0YGMX       0007 00000003
    INF0YSIZ       0034 00000038
    INF0YSZD       0034 00000007
    INF1BASC       0040 10
    INF1BSB1       007E 00000080
    INF1BSD1       007E 00000010
    INF1BSZB       007E 00000080
    INF1BSZD       007E 00000010
    INF1CHDR       0000
    INF1FCAU       0040 04
    INF1FCFC       0040 08
    INF1GLEN       000A
    INF1GLN1       005A
    INF1GLN2       006A
    INF1GLN3       007A
    INF1GOFF       0008
    INF1GOF1       0058
    INF1GOF2       0068
    INF1GOF3       0078
    INF1GPDU       0040 80
    INF1GSB1       0000 00000140
    INF1GSD1       0000 00000028
    INF1GSTI       0000
    INF1GSZB       0000 00000140
    INF1GSZD       0000 00000028
    INF1GVRS       000C
    INF1GVR1       005C
    INF1GVR2       006C
    INF1GVR3       007C
    INF1HFL1       0040
    INF1HFL2       0041
    INF1HVL1       0042
    INF1HVL2       0043
    INF1HYGC       0047
    INF1HYG1       0050
    INF1HYG2       0060
    INF1HYG3       0070
    INF1MDCP       0006
    INF1MDIF       000A
    INF1MFL1       0000
    INF1MFL2       0001
    INF1MIDV       0002 40
    INF1MLEN       004A
    INF1MMAN       0018
    INF1MNAM       0010
    INF1MNMV       0002 20
    INF1MOFF       0048
    INF1MPLNM      0040
    INF1MPLNV      0002 10
    INF1MPMA       0038
    INF1MPOOL      0000 80
    INF1MPROC      0002 80
    INF1MSB1       0040 00000048
    INF1MSCP       0004
    INF1MSD1       0040 00000009
    INF1MSEQ       0028
    INF1MSIF       0008
    INF1MSZB       0040 00000048
    INF1MSZD       0040 00000009
    INF1MTYP       000C
    INF1MVL1       0002
    INF1MVL2       0003
    INF1PABC       001C
    INF1PABI       0024
    INF1PACC       0002 20
    INF1PACTC      0098
    INF1PACTI      00C0
    INF1PCMCF      000E 00000010
    INF1PCMGN      000E 00000080
    INF1PCMLI      000E 00000040
    INF1PCMOD      000E
    INF1PCMVM      000E 00000020
    INF1PDCP       0006
    INF1PDIF       000A
    INF1PENC       0040
    INF1PENI       0044
    INF1PENV       0002 02
    INF1PFL1       0000
    INF1PFL2       0001
    INF1PGUCA      0078
    INF1PGUCC      0088
    INF1PGUIA      0080
    INF1PGUIC      008C
    INF1PIDV       0002 10
    INF1PLEN       004E
    INF1PLGC       0030
    INF1PLGI       0034
    INF1PLGN       0028
    INF1PLGV       0002 08
    INF1PLPTC      00A0
    INF1PLPTI      00C8
    INF1PMTE       0000 80
    INF1PMTIC      00B8
    INF1PMTII      00E0
    INF1POFF       004C
    INF1POLTC      00A8
    INF1POLTI      00D0
    INF1PPLNM      0038
    INF1PPLNV      0002 04
    INF1PPNA       0010
    INF1PPNU       000C
    INF1PPOOL      0000 40
    INF1PPRC       0002 80
    INF1PRCPU      000F
    INF1PSB1       00E0 000000E8
    INF1PSCP       0004
    INF1PSD1       00E0 0000001D
    INF1PSIF       0008
    INF1PSXCA      0048
    INF1PSXCC      0058
    INF1PSXIA      0050
    INF1PSXIC      005C
    INF1PSZB       00E0 000000E8
    INF1PSZD       00E0 0000001D
    INF1PUCCP      000F 00000000
    INF1PUCIFL     000F 00000003
    INF1PUCPA      0060
    INF1PUCPC      0070
    INF1PUIFA      0068
    INF1PUIFC      0074
    INF1PUTOD      0090
    INF1PUTV       0002 01
    INF1PVL1       0002
    INF1PVL2       0003
    INF1PWBC       0018
    INF1PWBI       0020
    INF1PWCV       0002 40
    INF1PWTFL      0000 20
    INF1PWTTC      00B0
    INF1PWTTI      00D8
    INF1STHY       0040 40
    INF1VRSN       0000
    INF1VSI        0040 20
    INF1V00001     0000 00000001
    INF1YASC       0020
    INF1YASI       0024
    INF1YCLN       0010
    INF1YCPT       0006
    INF1YDCP       001A
    INF1YDIF       001E
    INF1YFL1       0000
    INF1YFL2       0001
    INF1YGB1       000E 00000010
    INF1YGD1       000E 00000002
    INF1YGMX       0047 00000003
    INF1YGSB       000E 00000010
    INF1YGSD       000E 00000002
    INF1YIFT       0007
    INF1YLCC       0030
    INF1YLCI       0034
    INF1YLEN       0002
    INF1YLMC       0000 80
    INF1YLMP       0000 40
    INF1YLN1       0052
    INF1YLN2       0062
    INF1YLN3       0072
    INF1YMONH      0038
    INF1YMTE       0000 20
    INF1YOFF       0000
    INF1YOF1       0050
    INF1YOF2       0060
    INF1YOF3       0070
    INF1YPADC      0040
    INF1YPADI      0044
    INF1YPKF       003C
    INF1YPLG       003C 00000000
    INF1YPMD       003C 00000001
    INF1YPSM       003C 00000002
    INF1YPTC       0080
    INF1YPTI       0088
    INF1YRSC       0028
    INF1YRSI       002C
    INF1YSB1       0088 00000090
    INF1YSCP       0018
    INF1YSD1       0088 00000012
    INF1YSID       0008
    INF1YSIF       001C
    INF1YSTC       0060
    INF1YSTI       0068
    INF1YSZB       0088 00000090
    INF1YSZD       0088 00000012
    INF1YTVM       0004 00000001
    INF1YTYP       0004
    INF1YUTC       0050
    INF1YUTI       0058
    INF1YUTOD      0048
    INF1YVL1       0002
    INF1YVL2       0003
    INF1YVRS       0004
    INF1YVRT       0000 10
    INF1YVR1       0054
    INF1YVR2       0064
    INF1YVR3       0074
    INF1YWTC       0070
    INF1YWTI       0078
    INF1YXHI       003D 00000010
    INF1YXHI       003E 00000010
    INF1YXLO       003D 00000001
    INF1YXLO       003E 00000001
    INF1YXMD       003D 00000008
    INF1YXMD       003E 00000008
    INF1YXNO       003D 00000002
    INF1YXNO       003E 00000002
    INF1YXUSC      003D
    INF1YXUSI      003E
    INF2BSB1       0000 00000040
    INF2BSD1       0000 00000008
    INF2BSZB       0000 00000040
    INF2BSZD       0000 00000008
    INF2CHDR       0000
    INF2GACN       0008
    INF2GAFFN      0016
    INF2GAFON      0016 80
    INF2GAFSUP     0016 40
    INF2GCMCF      0015 00000010
    INF2GCMGN      0015 00000080
    INF2GCMLI      0015 00000040
    INF2GCMOD      0015
    INF2GCMVM      0015 00000020
    INF2GFLG       0014
    INF2GLINH      0014 04
    INF2GLINI      0014 08
    INF2GPRDT      0018
    INF2GPRTP      0017
    INF2GSB1       0019 00000020
    INF2GSD1       0019 00000004
    INF2GSZB       0019 00000020
    INF2GSZD       0019 00000004
    INF2GTOD       0010
    INF2GUID       0000
    INF2PUCCP      0017 00000000
    INF2PUCCP      0018 00000000
    INF2PUCIFL     0017 00000003
    INF2PUCIFL     0018 00000003
    INF2VRSN       0000
    INF2V00001     0000 00000001
    INF3BSB1       0040 00000180
    INF3BSD1       0040 00000030
    INF3BSZB       0040 00000180
    INF3BSZD       0040 00000030
    INF3CAFFN      00A9
    INF3CAFON      00A9 80
    INF3CAFSUP     00A9 40
    INF3CCASC      00E0
    INF3CCASI      0128
    INF3CCDT       00D8
    INF3CCLHC      00D9 40
    INF3CCLHI      0121 40
    INF3CCMAC      00D9 10
    INF3CCMAI      0121 10
    INF3CCMSC      00E4
    INF3CCMSI      012C
    INF3CCNAC      00D9 20
    INF3CCNAI      0121 20
    INF3CCNSC      00DC
    INF3CCNSI      0124
    INF3CCSCF      00D9
    INF3CCSIF      0121
    INF3CDCP       00D2
    INF3CDIF       011A
    INF3CFLG       00A8
    INF3CHDR       0000
    INF3CIASC      00EC
    INF3CIASI      0134
    INF3CIDT       0120
    INF3CILHC      00DA 40
    INF3CILHI      0122 40
    INF3CIMAC      00DA 10
    INF3CIMAI      0122 10
    INF3CIMSC      00F0
    INF3CIMSI      0138
    INF3CINAC      00DA 20
    INF3CINAI      0122 20
    INF3CINSC      00E8
    INF3CINSI      0130
    INF3CISCF      00DA
    INF3CISIF      0122
    INF3CMCPU      00AA
    INF3CMCT       00A8 40
    INF3CRCP       00D4
    INF3CRIF       011C
    INF3CSCP       00D0
    INF3CSIF       0118
    INF3CTCPP      00B0
    INF3CTCPS      00B8
    INF3CTCRP      00C0
    INF3CTCRS      00C8
    INF3CTIPP      00F8
    INF3CTIPS      0100
    INF3CTIRP      0108
    INF3CTIRS      0110
    INF3CVCT       00A8 20
    INF3CVIT       00A8 10
    INF3GACN       0008
    INF3GCFSC      0024
    INF3GCFSI      0068
    INF3GCMCF      0012 00000010
    INF3GCMGN      0012 00000080
    INF3GCMLI      0012 00000040
    INF3GCMOD      0012
    INF3GCMVM      0012 00000020
    INF3GCSC       0038
    INF3GCSI       007C
    INF3GDLSC      0044
    INF3GDLSI      0088
    INF3GDSC       0034
    INF3GDSI       0078
    INF3GDSSC      0048
    INF3GDSSI      008C
    INF3GESSC      003C
    INF3GESSI      0080
    INF3GFLG       0010
    INF3GIASC      004C
    INF3GIASI      0090
    INF3GIWSC      0020
    INF3GIWSI      0064
    INF3GLDSC      0040
    INF3GLDSI      0084
    INF3GLINH      0010 04
    INF3GLINI      0010 08
    INF3GLSC       0030
    INF3GLSI       0074
    INF3GMOB       0010 80
    INF3GOSC       005C
    INF3GOSI       00A0
    INF3GPASC      0058
    INF3GPASI      009C
    INF3GPNA       0018
    INF3GPRTP      0013
    INF3GPWSC      002C
    INF3GPWSI      0070
    INF3GSB1       013C 00000140
    INF3GSD1       013C 00000028
    INF3GSMSC      0028
    INF3GSMSI      006C
    INF3GSTI       0040
    INF3GSZB       013C 00000140
    INF3GSZD       013C 00000028
    INF3GTISC      0050
    INF3GTISI      0094
    INF3GTOD       0014
    INF3GTSC       0060
    INF3GTSI       00A4
    INF3GTSSC      0054
    INF3GTSSI      0098
    INF3GUID       0000
    INF3GVAL       0011
    INF3PUCCP      0013 00000000
    INF3PUCCP      0120 00000000
    INF3PUCIFL     0013 00000003
    INF3PUCIFL     0120 00000003
    INF3VRSN       0000
    INF3V00001     0000 00000001
    INF4BSB1       0000 00000040
    INF4BSD1       0000 00000008
    INF4BSZB       0000 00000040
    INF4BSZD       0000 00000008
    INF4CHDR       0000
    INF4PCRE       0008
    INF4PNAM       0000
    INF4PSB1       0008 00000010
    INF4PSD1       0008 00000002
    INF4PSZB       0008 00000010
    INF4PSZD       0008 00000002
    INF4VRSN       0000
    INF4V00001     0000 00000001
    INF5BSB1       007C 00000080
    INF5BSD1       007C 00000010
    INF5BSZB       007C 00000080
    INF5BSZD       007C 00000010
    INF5CCCC       0058 40
    INF5CCLC       0058 80
    INF5CCTL       006C
    INF5CFLG       0058
    INF5CHDR       0000
    INF5CICC       0058 10
    INF5CIFLA      0078
    INF5CILC       0058 20
    INF5CLIM       005C
    INF5CLMN       0068
    INF5CPCT       0058 08
    INF5CSUP       0058 04
    INF5CTIM       0060
    INF5CTML       0070
    INF5PCRE       0048
    INF5PLNA       0040
    INF5STMP       0050
    INF5VRSN       0000
    INF5V00001     0000 00000001
    INF6BSB1       0040 00000048
    INF6BSD1       0040 00000009
    INF6BSZB       0040 00000048
    INF6BSZD       0040 00000009
    INF6CHDR       0000
    INF6MNAM       0000
    INF6MSB1       0000 00000008
    INF6MSD1       0000 00000001
    INF6MSZB       0000 00000008
    INF6MSZD       0000 00000001
    INF6PLNA       0040
    INF6VRSN       0000
    INF6V00001     0000 00000001

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:28:38 EDT.
Copyright IBM Corporation, 1990, 2020