MCRBK | Back to Index page

| Prolog Control Block Contents MCRBK DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

MCRBK Prolog | Top of page

     NAME       : HCPMCRBK
     DESCRIPTION: Machine Check Record Block
     DSECT      : MCRBK
     FUNCTION   : HCPMCRBK contains information relative to a
                  machine check incident which (incident) is to be
                  reflected to a guest.
     LOCATED BY : Is a mapping of the parameters passed for
                  manufacturing a machine check or building the
                  message information when communicating a machine
                  check incident.
     CREATED BY : Any caller who wants to pass a machine check record
                  information.
     DELETED BY : The caller who creates it or the callee. This is
                  communicated via MCRFLAG1 in this control block.
     RELOCATION CONSIDERATIONS : None

MCRBK Control Block Content | Top of page

     MCRBK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      MCRBK          Machine Check Record Block
    0000    0 Dbl-Word     8 MCRMCIC (0)    Machine Check Interruption Code
    0000    0 Signed       4 MCRMCWD0 (0)   MCRMCIC word 0
    0000    0 Bitstring    2 MCRMCB01 (0)   MCRMCIC byte 0 and 1
    0000    0 Bitstring    1 MCRMCIC0       MCRMCIC byte 0
              1111 1111      MCIPRIM0       X'FF' MCIPRIM0 PRIMARY MACHINE
                                            CHECK BITS - BYTE 0
              1... ....      MCICSD         X'80' MCICSD SYSTEM DAMAGE BIT.
              .1.. ....      MCICPD         X'40' MCICPD PROCESSING DAMAGE
                                            BIT.
              ..1. ....      MCICSR         X'20' MCICSR SYSTEM RECOVERY BIT.
              ...1 ....      MCICITD        X'10' MCICITD INTERVAL TIMER
                                            DAMAGE. (370 GUESTS)
              .... 1...      MCICCD         X'08' MCICCD TIMING (CLOCK)
                                            FACILITY DAMAGE.
              .... .1..      MCICED         X'04' MCICED EXTERNAL DAMAGE.
              .... ...1      MCICDG         X'01' MCICDG DEGRADATION BIT.
    0001    1 Bitstring    1 MCRMCIC1       MCRMCIC byte 1
              1111 ....      MCIPRIM1       X'F0' MCIPRIM1 PRIMARY MACHINE
                                            CHECK BITS - BYTE 1
              1... ....      MCICW          X'80' MCICW WARNING BIT.
              .1.. ....      MCICCRW        X'40' MCICCRW PENDING-CRW REPORT.
              ..1. ....      MCICSP         X'20' MCICSP SERVICE PROCESSOR
                                            DAMAGE.
              ...1 ....      MCICCSD        X'10' MCICCSD CHANNEL-SUBSYSTEM
                                            DAMAGE.
              .... ..1.      MCICBU         X'02' MCICBU 'BACKED UP' BIT.
              .... ...1      MCICDL         X'01' MCICDL 'DELAYED' BIT. (370
                                            GUESTS)
    0002    2 Bitstring    1 MCRMCIC2       MCRMCIC byte 2
              1... ....      MCICSE         X'80' MCICSE STORAGE ERROR
                                            UNCORRECTED.
              .1.. ....      MCICSC         X'40' MCICSC STORAGE ERROR
                                            CORRECTED.
              ..1. ....      MCICKE         X'20' MCICKE STORAGE-KEY ERROR
                                            UNCORRECTED.
              ...1 ....      MCICSDG        X'10' MCICSDG STORAGE
                                            DEGRADATION. MODIFIES STORAGE
                                            ERROR CORRECTED.
              .... 1...      MCICVWP        X'08' MCICVWP BITS 12-15 OF MC
                                            OLD PSW VALID.
              .... .1..      MCICVMS        X'04' MCICVMS SYSTEM MASK & KEY
                                            OF MC OLD PSW VALID.
              .... ..1.      MCICVPM        X'02' MCICVPM PROGRAM MASK & CC
                                            OF MC OLD PSW VALID.
              .... ...1      MCICVIA        X'01' MCICVIA INSTR ADDR OF MC
                                            OLD PSW IS VALID.
    0003    3 Bitstring    1 MCRMCIC3       MCRMCIC byte 3
              1... ....      MCICVFA        X'80' MCICVFA FAILING STORAGE
                                            ADDRESS IS VALID.
              .1.. ....      MCICVVR        X'40' MCICVVR Vector Registers
                                            stored are valid
              ..1. ....      MCICVED        X'20' MCICVED EXTERNAL-DAMAGE
                                            CODE IS VALID.
              ...1 ....      MCICVFP        X'10' MCICVFP FP REGISTERS STORED
                                            ARE VALID.
              .... 1...      MCICVGR        X'08' MCICVGR GP REGISTERS STORED
                                            ARE VALID.
              .... .1..      MCICVCR        X'04' MCICVCR CONTROL REGISTERS
                                            STORED VALID.
              .... ..1.      MCIC30         X'02' MCIC30 MCIC.30
              .... ...1      MCICVST        X'01' MCICVST INST. MODIFIED
                                            STORAGE IS VALID.
    0004    4 Signed       4 MCRMCWD1 (0)   MCRMCIC word 1
    0004    4 Bitstring    1 MCRMCIC4       MCRMCIC byte 4
              1... ....      MCICIE         X'80' MCICIE INDIRECT STORAGE
                                            ERROR
              .1.. ....      MCICVAR        X'40' MCICVAR ACCESS REGISTERS
                                            STORED ARE VALID
              ..1. ....      MCICDA         X'20' MCICDA DELAYED ACCESS
                                            EXCEPTION BIT
              .... 1...      MCICVGS        X'08' MCICVGS Guarded Storage
                                            regs stored are valid
    0005    5 Bitstring    1 MCRMCIC5       MCRMCIC byte 5
              ..1. ....      MCICVTPR       X'20' MCICVTPR TOD programmable
                                            register validity
              ...1 ....      MCICVXFP       X'10' MCICVXFP Additional FP
                                            Registers Validity (ESA390) FP
                                            Control Register Validity (zArch)
              .... 1...      MCICAR         X'08' MCICAR Ancillary Report Bit
              .... ..1.      MCICVCT        X'02' MCICVCT CPU TIMER STORED IS
                                            VALID.
              .... ...1      MCICVCC        X'01' MCICVCC CLOCK COMPARATOR
                                            STORED IS VALID.
    0006    6 Bitstring    1 MCRMCIC6       MCRMCIC byte 6
    0007    7 Bitstring    1 MCRMCIC7       MCRMCIC byte 7
    0008    8 Signed       4 *
    000C   12 Signed       4 MCREDC (0)     Machine check external-damage
                                            code
    000C   12 Bitstring    1 MCREDCB0       MCREDC byte 0
              .... ....      MCEXTD0        X'00' MCEXTD0 No bits defined
    000D   13 Bitstring    1 MCREDCB1       MCREDC byte 1
              .... ....      MCEXTD1        X'00' MCEXTD1 No bits defined
    000E   14 Bitstring    1 MCREDCB2       MCREDC byte 2
              ...1 ....      MCEXTDSC       X'10' MCEXTDSC Bit 19 - ETR Sync
                                            check
    000F   15 Bitstring    1 MCREDCB3       MCREDC byte 3
              1... ....      MCEXTDSS       X'80' MCEXTDSS Bit 24 - STP Sync
                                            Check
              .1.. ....      MCEXTDIC       X'40' MCEXTDIC Bit 25 - Island
                                            Condition
              ..1. ....      MCEXTDCC       X'20' MCEXTDCC Bit 26 - CTN
                                            Configuration Change
              ...1 ....      MCEXTDCS       X'10' MCEXTDCS Bit 27 - STP Clock
                                            Source Error
    0010   16 Signed       4 MCRMCICX       Machine check interruption code
                                            extension
    0014   20 Bitstring    1 MCRFLAG1       Flag byte 1
              1... ....      MCRREAL        X'80' MCRREAL Failing storage
                                            address is real. If this bit is
                                            zero the failing storage address
                                            (if specified) is absolute. This
                                            bit is meaningful only when the
                                            MCRNULLA bit is 0.
              .1.. ....      MCRRELST       X'40' MCRRELST MCRBK storage is
                                            to be released by the guest
                                            machine service routines when
                                            this machine check is presented.
              ..1. ....      MCRNULLA       X'20' MCRNULLA Indicates that
                                            MCRFSAD/MCRGFAD contains a null
                                            address
    0015   21 Bitstring    1 *              Reserved for IBM use.
    0016   22 Bitstring    1 *              Reserved for IBM use.
    0017   23 Bitstring    1 *              Reserved for IBM use
    0018   24 Dbl-Word     8 MCRFLOG (2)    Fixed logout area
    0028   40 Dbl-Word     8 MCRGFAD (0)    64 bit failing storage addr
    0028   40 Signed       4 MCR64HI        High order 32 bits of 64 bit addr
    002C   44 Signed       4 MCRFSAD        Guest failing storage address
              0000002C       MCR64LO        MCRFSAD Low order 32 bits of 64
                                            bit addr
              00000030       MCRLEN         *-MCRBK MCRBK block size in bytes
              00000006       MCRSIZE        (MCRLEN+7)/8 MCRBK block size in
                                            doublewords
    0018   24 Dbl-Word     8 MCRFASIT       Failing-storage internal ASIT
    0000    0 Bitstring    2 *
    0002    2 Bitstring    4 MCRMCB25       MCRMCIC bytes 2-5
    0006    6 Bitstring    2 *

MCRBK Storage Layout | Top of page

    *** MCRBK - Machine Check Record Block
    *
    *     +------+------+------+------+------+------+------+------+
    *   0 |:MCIC0|:MCIC1|:MCIC2|:MCIC3|:MCIC4|:MCIC5|:MCIC6|:MCIC7|
    *     +------+------+------+------+------+------+------+------+
    *   8 |///////////////////////////|:EDCB0|:EDCB1|:EDCB2|:EDCB3|
    *     +---------------------------+------+------+------+------+
    *  10 |         MCRMCICX          |:FLAG1|//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    *  18 |                       MCRFLOG                         |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  28 |         MCR64HI           |         MCRFSAD           |
    *     +---------------------------+---------------------------+
    *  30
    *
    *** MCRBK - Machine Check Record Block

    *** Overlay for MCRFLOG in MCRBK
    *
    *     +-------------------------------------------------------+
    *  18 |                       MCRFASIT                        |
    *     +-------------------------------------------------------+
    *  20
    *
    *** Overlay for MCRFLOG in MCRBK

    *** Overlay for MCRMCIC in MCRBK
    *
    *     +-------------+---------------------------+-------------+
    *   0 |/////////////|         MCRMCB25          |/////////////|
    *     +-------------+---------------------------+-------------+
    *   8
    *
    *** Overlay for MCRMCIC in MCRBK

MCRBK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    MCEXTDCC       000F 20
    MCEXTDCS       000F 10
    MCEXTDIC       000F 40
    MCEXTDSC       000E 10
    MCEXTDSS       000F 80
    MCEXTD0        000C 00
    MCEXTD1        000D 00
    MCICAR         0005 08
    MCICBU         0001 02
    MCICCD         0000 08
    MCICCRW        0001 40
    MCICCSD        0001 10
    MCICDA         0004 20
    MCICDG         0000 01
    MCICDL         0001 01
    MCICED         0000 04
    MCICIE         0004 80
    MCICITD        0000 10
    MCICKE         0002 20
    MCICPD         0000 40
    MCICSC         0002 40
    MCICSD         0000 80
    MCICSDG        0002 10
    MCICSE         0002 80
    MCICSP         0001 20
    MCICSR         0000 20
    MCICVAR        0004 40
    MCICVCC        0005 01
    MCICVCR        0003 04
    MCICVCT        0005 02
    MCICVED        0003 20
    MCICVFA        0003 80
    MCICVFP        0003 10
    MCICVGR        0003 08
    MCICVGS        0004 08
    MCICVIA        0002 01
    MCICVMS        0002 04
    MCICVPM        0002 02
    MCICVST        0003 01
    MCICVTPR       0005 20
    MCICVVR        0003 40
    MCICVWP        0002 08
    MCICVXFP       0005 10
    MCICW          0001 80
    MCIC30         0003 02
    MCIPRIM0       0000 FF
    MCIPRIM1       0001 F0
    MCREDC         000C
    MCREDCB0       000C
    MCREDCB1       000D
    MCREDCB2       000E
    MCREDCB3       000F
    MCRFASIT       0018
    MCRFLAG1       0014
    MCRFLOG        0018
    MCRFSAD        002C
    MCRGFAD        0028
    MCRLEN         002C 00000030
    MCRMCB01       0000
    MCRMCB25       0002
    MCRMCIC        0000
    MCRMCICX       0010
    MCRMCIC0       0000
    MCRMCIC1       0001
    MCRMCIC2       0002
    MCRMCIC3       0003
    MCRMCIC4       0004
    MCRMCIC5       0005
    MCRMCIC6       0006
    MCRMCIC7       0007
    MCRMCWD0       0000
    MCRMCWD1       0004
    MCRNULLA       0014 20
    MCRREAL        0014 80
    MCRRELST       0014 40
    MCRSIZE        002C 00000006
    MCR64HI        0028
    MCR64LO        002C 0000002C

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:29:06 EDT.
Copyright IBM Corporation, 1990, 2020