Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRMTRILC

Prolog
Control Block Contents
Cross Reference

#### MRMTRILC Prolog

     DSECT NAME - MTRILC
     FUNCTION - Map a Monitor record.
     LOCATED By -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRMTRILC
     DESCRIPTIVE NAME - Monitor Sample Configuration Record
                        Domain 1 - Monitor Domain
                        Record 24 - ISFC Logical Link Configuration
     DESCRIPTION - Indicates the set of real devices comprising the
                   logical link to the specified node.
     NOTES:

#### MRMTRILC Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure    96  MTRILC                 Start of monitor record
       0   0  Character     0  MTRILC_MRHDR           Record header - see
                                                      MRRECHDR for details
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN               record length in bytes
       2   2  Unsigned      2  MRHDRZER               field of zeros
       4   4  Unsigned      1  MRHDRDM                domain identifier
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC                record identifier
       8   8  Character     8  MRHDRTOD               Time at which this record
                                                      was built. In time-of-day
                                                      (TOD) clock format. See IBM
                                                      System 370 XA Principle of
                                                      Operation for explanation of
                                                      format.
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END              End of header
      20  14  Character     8  MTRILC_NODEID          Partner node name
      28  1C  Unsigned      2  MTRILC_LNKDEVCT        Device count
      30  1E  Unsigned      2  *                      Reserved
      32  20  Character    64  MTRILC_LDVDEVID        Array of 1-16 device
                                                      numbers each represented by 4
                                                      characters.
      96  60  Character     0  MTRILC_END

#### MRMTRILC Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    MTRILC                     0     96
    MTRILC_END                60      0
    MTRILC_LDVDEVID           20     64
    MTRILC_LNKDEVCT           1C      2
    MTRILC_MRHDR               0      0
    MTRILC_NODEID             14      8

    This information is
    based on z/VM V7R2.0.

    Last updated on 09 August 2020 at 15:18:57.

    Copyright IBM Corporation, 1990, 2020