SIEBK | Back to Index page

| Prolog Control Block Contents SIEBK DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

SIEBK Prolog | Top of page

     NAME       : HCPSI2GB
     DESCRIPTION: SIE STATE DESCRIPTION (Format 2)
     DSECT      : SIEBK
     FUNCTION   :
                  This control block describes a guest (virtual
                  machine) to the interpretive-execution facility
                  of the machine (embodied in the SIE instruction).
                  It defines a SIE format-2 state description, which
                  is the operand of a host SIE instruction when CP is
                  running as a z/Arch mode host. The SIE state
                  description used by the host control program to run
                  a guest is imbedded in the VMDBK, which is
                  described by HCPVMDBK COPY.
                  The SIE state description is also used by a guest
                  control program operating in zArch mode to run a
                  virtual guest. In that context, it is the operand
                  of a guest SIE instruction.
                  This control block is defined by processor
                  architecture.
     LOCATED BY : VMDSDSC in the VMDBK
                  VMDSDSC in the V/SIE VMDBK (which is
                  identified by VMDTYPE = VMDTYPSI)
     CREATED BY : HCPBVM, HCPWVS
     DELETED BY : HCPUSO, HCPWSIFR
     COMMENTS   :
                  As noted above, VM uses the state description in two
                  contexts:
                  1) It is imbedded within the VMDBK which we use to
                  represent first-level guests (RGuests) when we issue
                  the SIE instruction to run those guests.  In this
                  case, we refer to it as a SIEBK.
                  Some of the comments on fields below apply only to the
                  SIEBKs which are imbedded in RGuest VMDBKs.  Those
                  comments are surrounded by the annotation:
                  [VMDBK only:   ].
                  2) It is an argument of an RGuest's SIE instruction.
                  In this context, it is not associated with a VMDBK --
                  at least, our usage can not depend on such an
                  association, as we are limited to the interface
                  specified by the interpretive-execution architecture.
                  When referring to such a state description, we call it
                  an SI1BK (if the RGuest is in ESA/370 or ESA/390 mode)
                  or an SI2BK (if the RGuest is in zArch mode).
                  Note that in processing such a state description, we
                  will translate it into a "shadow" state description
                  imbedded in a vSIE VMDBK; we may thereafter refer to
                  it as a SIEBK.  In general, "[VMDBK only:]" comments
                  do not apply to the SIEBKs in vSIE VMDBKs.

SIEBK Control Block Content | Top of page

     SIEBK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SIEBK          SIE STATE DESCRIPTOR BLOCK
    0000    0 Bitstring  512 SIESDSC (0)    Guest machine state description
                                            (format 2)
    0000    0 Signed       4 SIEINTWD (0)   Symbol on word boundary for
                                            Compare-and-Swap operations
    0000    0 Bitstring    1 SIENTVCT       Emulation intervention control
              ...1 ....      SIEIPWAI       X'10' SIEIPWAI Wait/Run bit. When
                                            this bit is set, the state
                                            description is "waiting", and
                                            host intervention is needed to
                                            make it runnable.
              .... 1...      SIEIPXTC       X'08' SIEIPXTC EXTERNAL CALL
                                            INTERRUPTION PENDING
              .... .1..      SIEIPSTP       X'04' SIEIPSTP SIE stopping
                                            control
              .... ..1.      SIEIPVIO       X'02' SIEIPVIO I/O INTERRUPTION
                                            PENDING
              .... ...1      SIEIPEXT       X'01' SIEIPEXT EXTERNAL
                                            INTERRUPTION PENDING
          SIESTATC is serialized in the following way:
           - Testing or modifying SIERUNNING requires Dispatch Lock.
           - Modifying any other bit requires Dispatch Lock AND
             either Guest Instruction-stream or Console Function
             Mode.  Testing any of these other bits only requires
             that 1 of the 3 previously mentioned serializations
             is held.
    0001    1 Bitstring    1 SIESTATC       SIE state control fields
              1... ....      SIERUNNING     X'80' SIERUNNING Indicates guest
                                            CPU is running
              .1.. ....      SIERSCB        X'40' SIERSCB SIE-state-retention
                                            retained- status control bit.
                                            When 1, an internal version of
                                            the contents of certain fields of
                                            the state description retained
                                            from a previous SIE instruction
                                            invocation may be used
              .... ..1.      SIEEXTMR       X'02' SIEEXTMR Expedite-Timer
                                            processing enabled
              .... ...1      SIEEXRUN       X'01' SIEEXRUN Expedite-Run
                                            processing enabled
             SIxMODE and SIxMODEX contain bits
          that can be used to determine the machine mode type.
          [VMDBK only:  In the state descriptions which VM imbeds in
          (RGuest) VMDBKs, these bits should NOT be used for this
          purpose anymore; instead, the HCPVMODE macro should be
          used to test for machine modes: System-370, ESA/370,
          ESA/XC.  370-XA machines are considered to be ESA/370.]
    0002    2 Bitstring    1 SIEMODEX       Machine mode control byte MX
              1... ....      SIERRF         X'80' SIERRF Region Relocate
                                            installed
              .1.. ....      SIE2NDVV       X'40' SIE2NDVV Indicates Rguest
                                            runs V=V guests via uVSIE
                                            (microcode VSIE). [VMDBK only:
                                            This bit is set at the first SIE
                                            instruction intercept if TRACE is
                                            not being used and SIERRF is set.
                                            Valid in all VMDBKs.]
              ..1. ....      SIE2NDVR       X'20' SIE2NDVR Indicates Rguest
                                            runs V=R guests via uVSIE
                                            (microcode VSIE). [VMDBK only:
                                            See SIE2NDVV comments for when
                                            set.]
              .... 1...      SIEESAME       X'08' SIEESAME Guest is in zArch
                                            mode
              .... ...1      SIEMCDS        X'01' SIEMCDS If MCDS facility is
                                            installed and ESA/370 mode is
                                            enabled, then the guest is in
                                            MCDS mode.
    0003    3 Bitstring    1 SIEMODE        Guest machine mode controls
              .... 1...      SIEVR          X'08' SIEVR V=R GUEST (PREFERRED
                                            STORAGE) STORAGE FOR THE V=R
                                            GUEST IS MAPPED SO THAT GUEST
                                            ABSOLUTE ADDRESSES ARE EQUAL TO
                                            HOST ABSOLUTE ADDRESSES.
              .... ...1      SIEGPE         X'01' SIEGPE This bit signifies
                                            that the guest per enhancement
                                            feature should be used. When set,
                                            guest per enhancement makes it so
                                            that guest PER is always enabled.
                                            This bit overrides bit 1 in the
                                            guest PSW.
    0004    4 Signed       4 SIEPREFX       Guest prefix register value in
                                            bits 1-18 or 1-19. The other bits
                                            are not part of the prefix value
                                            and must be masked off if
                                            SIEPREFX is used as a full word
                                            value. Either VMDPRFMK or MSKPFX
                                            in HCPEQUAT may be used to
                                            isolate the prefix value. MSKPFX
                                            can be used to mask off the
                                            non-prefix values. VMDPFXMK
                                            should be used to also ensure the
                                            correct value of bit 19 depending
                                            on whether the guest is ESA/390
                                            or z/Architecture mode.
    0008    8 Signed       4 *              Reserved for IBM hardware
    000C   12 Signed       4 *              Reserved for programmingg
    0010   16 Dbl-Word     8 *              Reserved for IBM hardware
    0018   24 Dbl-Word     8 *              Reserved for IBM hardware
    0020   32 Dbl-Word     8 *              Reserved for IBM hardware (former
                                            HIRES/LORES for 370 interval
                                            timer)
    0028   40 Bitstring    1 SIECPUT0 (0)   HIGH-ORDER BYTE OF CPU TIMER
              1... ....      SIECPUTN       X'80' SIECPUTN TIMER VALUE IS
                                            NEGATIVE
    0028   40 Signed       8 SIECPUTM       Guest CPU timer value [VMDBK
                                            only: This is usually managed by
                                            the interpretive-execution
                                            facility. See also the
                                            description of VMDVTZPT in the
                                            VMDBK.]
    0030   48 Signed       8 SIECKC         Guest clock comparator value
    0038   56 Signed       8 SIEEPOCH       Guest time-of-day clock epoch To
                                            define delta between host TOD
                                            clock and guest TOD clock - epoch
                                            is added to host TOD clock value
                                            to obtain guest TOD clock value
    0040   64 Bitstring    1 SIESVCTL       SVC interception controls
              1... ....      SIESVCNN       X'80' SIESVCNN INTERCEPT ALL SVC
                                            INSTRUCTIONS
              .1.. ....      SIESVC1C       X'40' SIESVC1C INTERCEPT ON SVC
                                            NUMBER IN SVC1N
              ..1. ....      SIESVC2C       X'20' SIESVC2C INTERCEPT ON SVC
                                            NUMBER IN SVC2N
              ...1 ....      SIESVC3C       X'10' SIESVC3C INTERCEPT ON SVC
                                            NUMBER IN SVC3N
    0041   65 Bitstring    1 SIESVC1N       Intercept SVC number first id
    0042   66 Bitstring    1 SIESVC2N       Intercept SVC number second id
    0043   67 Bitstring    1 SIESVC3N       Intercept SVC number third id
    0044   68 Bitstring    2 SIELCTLS (0)   LCTL/LCTLG interception controls
    0044   68 Bitstring    1 SIELCTB0       LCTL interception, CR0-CR7
              1... ....      SIELCTL0       X'80' SIELCTL0 INTERCEPT LCTL CR0
              .1.. ....      SIELCTL1       X'40' SIELCTL1 INTERCEPT LCTL CR1
              ..1. ....      SIELCTL2       X'20' SIELCTL2 INTERCEPT LCTL CR2
              ...1 ....      SIELCTL3       X'10' SIELCTL3 INTERCEPT LCTL CR3
              .... 1...      SIELCTL4       X'08' SIELCTL4 INTERCEPT LCTL CR4
              .... .1..      SIELCTL5       X'04' SIELCTL5 INTERCEPT LCTL CR5
              .... ..1.      SIELCTL6       X'02' SIELCTL6 INTERCEPT LCTL CR6
              .... ...1      SIELCTL7       X'01' SIELCTL7 INTERCEPT LCTL CR7
    0045   69 Bitstring    1 SIELCTB1       LCTL interception, CR8-CR15
              1... ....      SIELCTL8       X'80' SIELCTL8 INTERCEPT LCTL CR8
              .1.. ....      SIELCTL9       X'40' SIELCTL9 INTERCEPT LCTL CR9
              ..1. ....      SIELCTLA       X'20' SIELCTLA INTERCEPT LCTL
                                            CR10
              ...1 ....      SIELCTLB       X'10' SIELCTLB INTERCEPT LCTL
                                            CR11
              .... 1...      SIELCTLC       X'08' SIELCTLC INTERCEPT LCTL
                                            CR12
              .... .1..      SIELCTLD       X'04' SIELCTLD INTERCEPT LCTL
                                            CR13
              .... ..1.      SIELCTLE       X'02' SIELCTLE INTERCEPT LCTL
                                            CR14
              .... ...1      SIELCTLF       X'01' SIELCTLF INTERCEPT LCTL
                                            CR15
    0046   70 Signed       2 SIEICPUA       Virtual CPU address for
                                            interpretive execution (bits
                                            10-15 are used, bits 0-9 are
                                            reserved for IBM hardware)
    0048   72 Bitstring    4 SIEICTLS (0)   Interception controls
    0048   72 Bitstring    1 SIEICPT0       Interception controls, byte 0
              1... ....      SIEICPOP       X'80' SIEICPOP Intercept
                                            operation exception program
                                            interruptions
              .1.. ....      SIEICPRO       X'40' SIEICPRO Intercept
                                            privileged operation program
                                            interruptions
              ..1. ....      SIEICPRG       X'20' SIEICPRG Intercept program
                                            interruptions
              ...1 ....      SIEICFII       X'10' SIEICFII IC.3 Intercept
                                            Facility-indicating- instructions
              .... ...1      SIEICIPT       X'01' SIEICIPT Intercept
                                            Invalidate Page Table Entry
                                            instructions (IPTE) or CSP or
                                            IDTE or CSPG
    0049   73 Bitstring    1 SIEICPT1       Interception controls, byte 1
              .1.. ....      SIEICLPS       X'40' SIEICLPS Intercept Load PSW
                                            (LPSW), Load PSW Extended
                                            (LPSWE), and Extract PSW (EPSW)
                                            instructions
              ..1. ....      SIEICPTL       X'20' SIEICPTL Intercept Purge
                                            TLB (PTLB) and Purge ALB (PALB)
                                            instructions
              ...1 ....      SIEICSSM       X'10' SIEICSSM Intercept Set
                                            System Mask (SSM) instructions
              .... 1...      SIEICBSA       X'08' SIEICBSA Intercept Branch
                                            and Set Authority (BSA)
                                            instructions
              .... .1..      SIEICSTC       X'04' SIEICSTC Intercept Store
                                            Control (STCTL, STCTG)
                                            instructions
              .... ..1.      SIEICSTN       X'02' SIEICSTN Intercept Store
                                            Then And System Mask (STNSM)
                                            instructions
              .... ...1      SIEICSTO       X'01' SIEICSTO Intercept Store
                                            Then Or System Mask (STOSM)
                                            instructions
                       X'80'          Reserved for future IBM use
    004A   74 Bitstring    1 SIEICPT2       Interception controls, byte 2
              1... ....      SIEICSTK       X'80' SIEICSTK Intercept Store
                                            Clock (STCK) and Store Clock Fast
                                            (STCKF) instructions
              .1.. ....      SIEICISK       X'40' SIEICISK Intercept Insert
                                            Storage Key Extended (ISKE)
                                            instructions
              ..1. ....      SIEICSSK       X'20' SIEICSSK Intercept Set
                                            Storage Key Extended (SSKE)
                                            instructions
              ...1 ....      SIEICRRB       X'10' SIEICRRB Intercept Reset
                                            Reference Bit Extended (RRBE)
                                            instructions
              .... 1...      SIEICPC        X'08' SIEICPC Intercept Program
                                            Call (PC) instructions
              .... .1..      SIEICPT        X'04' SIEICPT Intercept Program
                                            Transfer (PT) and Program
                                            Transfer with Instance (PTI)
                                            instructions
              .... ..1.      SIEICTPT       X'02' SIEICTPT Intercept Test
                                            Protection (TPROT) instructions
              .... ...1      SIEICLSP       X'01' SIEICLSP Intercept Load
                                            Address Space Parameters (LASP)
                                            instructions
    004B   75 Bitstring    1 SIEICPT3       Interception controls, byte 3
              .1.. ....      SIEICSPT       X'40' SIEICSPT Intercept Set CPU
                                            Timer (SPT) and Store CPU Timer
                                            (STPT) instructions
              ..1. ....      SIEICSCK       X'20' SIEICSCK Intercept Set
                                            Clock Comparator (SCKC) and Store
                                            Clock Comparator (STCKC)
                                            instructions instruction
              .... 1...      SIEICPR        X'08' SIEICPR Intercept Program
                                            Return (PR) instruction
              .... .1..      SIEICBAK       X'04' SIEICBAK Intercept Branch
                                            and Stack (BAKR) instruction
              .... ..1.      SIEICPG        X'02' SIEICPG Intercept Page In
                                            (PGIN) and Page Out (PGOUT)
                                            instructions.
    004C   76 Bitstring    4 SIEECA (0)     Execution controls
    004C   76 Bitstring    1 SIEECA0        Execution controls, byte 0
              1... ....      SIEECEXT       X'80' SIEECEXT External
                                            Interruption Interpretation
                                            Assist
              .1.. ....      SIEECINT       X'40' SIEECINT Intervention
                                            Bypass Assist
              ..1. ....      SIEECWAI       X'20' SIEECWAI Guest Wait-State
                                            Assist
              ...1 ....      SIEECSGP       X'10' SIEECSGP SIGP
                                            Interpretation Assist
              .... 1...      SIEECALT       X'08' SIEECALT Alert monitoring
                                            bit
              .... .1..      SIEECIO2       X'04' SIEECIO2
                                            I/O-Interpretation-level-2
                                            activation bit
              .... ...1      SIEECMVP       X'01' SIEECMVP MVPG Facility
                                            enablement. When this bit is one,
                                            SIE will inter- pret the MVPG and
                                            IESBE opcodes.
    004D   77 Bitstring    1 SIEECA1        Execution controls, byte 1
              .... ..1.      SIEECVEC       X'02' SIEECVEC Vector Facility
                                            Enablement
    004E   78 Bitstring    1 SIEECA2        Execution controls, byte 2
    004F   79 Bitstring    1 SIEECA3        Execution controls, byte 3
              .... .1..      SIESIGA        X'04' SIESIGA Signal Adapter
                                            (SIGA) Assist
    0050   80 Bitstring    1 SIEICODE       Interception Event Code This
                                            field describes a guest condition
                                            detected by the
                                            interpretive-execution facility
                                            (usually), which requires
                                            software intervention or
                                            simulation. [VMDBK only: It is
                                            also used by software to indicate
                                            that there exists a description
                                            of guest conditions by software,
                                            in VMDNTMOD, that requires
                                            sortware intervention for
                                            tracing.]
              00000000       SIEENDOP       0 SIEENDOP RESERVED FOR IBM
                                            SOFTWARE USE SIxENDOP is used to
                                            indicate that the guest machine
                                            is between instuctions, or
                                            currently executing in emulation
                                            mode
              00000004       SIEICNTC       4 SIEICNTC INSTRUCTION
                                            INTERCEPTION. A GUEST INSTRUCTION
                                            WAS FOUND BY EMULATION HARDWARE
                                            WHICH IS NOT EMULATED, OR WHICH
                                            WAS REQUESTED FOR INTERCEPTION IN
                                            THE INTERCEPTION CONTROLS.
              00000008       SIEICPNT       8 SIEICPNT PROGRAM INTERRUPT
                                            INTERCEPTION
              0000000C       SIEICBOT       12 SIEICBOT BOTH INSTRUCTION AND
                                            PROGRAM INTERRUPT INTERCEPTIONS
              00000010       SIEICPEX       16 SIEICPEX PENDING EXTERNAL
                                            INTERRUPT
              00000014       SIEICXNT       20 SIEICXNT EXTERNAL INTERRUPT
                                            INTERCEPTION
              00000018       SIEICPIO       24 SIEICPIO PENDING I/O INTERRUPT
                                            INTERCEPT
              0000001C       SIEICWT        28 SIEICWT WAIT STATE
                                            INTERCEPTION
              00000020       SIEICVAL       32 SIEICVAL VALIDITY INTERCEPTION
              00000024       SIEIMISC       36 SIEIMISC SOFTWARE USE ONLY
                                            Used to indicate that a software
                                            event has occurred which is not
                                            one of the other codes. [VMDBK
                                            only: the condition is further
                                            described in the VMDNTMOD field.]
              00000028       SIEICSTP       40 SIEICSTP STOP INTERCEPTION
              0000002C       SIEICOUO       44 SIEICOUO OPERATION EXCEPTION
                                            INTERCEPTION
              00000030       SIEICALT       48 SIEICALT Alert interception
              00000038       SIEICPIX       56 SIEICPIX PARTIAL
                                            INSTRUCTION-EXECUTION
                                            INTERCEPTION
              0000003C       SIEICIOR       60 SIEICIOR I/O INTERRUPTION
                                            INTERCEPTION
              00000040       SIEICION       64 SIEICION I/O INSTRUCTION
                                            INTERCEPTION
              00000044       SIEICRUN       68 SIEICRUN Expedite-Run
                                            processing Interception
              00000048       SIEICTMR       72 SIEICTMR Expedite-Timer
                                            processing Interception
              00000003       SIEIMLT4       X'03' SIEIMLT4 To ensure field is
                                            multiple of 4
    0051   81 Bitstring    1 SIEICFLG       Instruction interception status
              .11. ....      SIEICEXL       X'60' SIEICEXL In SIE the
                                            interception status is one byte,
                                            x'51'. The XILC is bits 1 and 2
                                            of that byte. A value in those
                                            bits of 2 indicates the
                                            interception was for an EX type
                                            instruction. A value of 3 in
                                            those bits indicates the
                                            interception was for an EXRL type
                                            instruction. ICEXL and ICEXS
                                            describe this scenario.
              .1.. ....      SIEICEXS       X'40' SIEICEXS The intercepted
                                            Execute-type instruction has an
                                            instruction length of 6 if bits 1
                                            and 2 are on (a value of 3) and
                                            ICEX is on. The Execute-type
                                            instruction has an instruction
                                            length of 4 if bit 1 is on and
                                            bit 2 is off (a value of 2) and
                                            if ICEX is on. These two bits are
                                            only set if the
                                            Execute-Extensions Facility is
                                            installed.
              .... ..1.      SIEICIF        X'02' SIEICIF INSTRUCTION FETCH
                                            EVENT (P.E.R)
              .... ...1      SIEICEX        X'01' SIEICEX The intercepted
                                            instruction was the subject of an
                                            execute-type instruction
    0052   82 Signed       2 SIEIHCPU       Host CPU address that last
                                            entered emulation mode for this
                                            state description
    0054   84 Signed       2 *              Reserved for IBM use
    0056   86 Bitstring    6 SIEIPARM (0)   Interception parameter (A & B)
    0056   86 Signed       2 SIEIPA (0)     Interception parameter A Bits
                                            0-15
    0056   86 Signed       2 SIEINST (0)    Interception parameter bit 0-15
    0056   86 Bitstring    1 SIEINSTO       Interception parameter bits 0-7
                                            First byte of the OPCODE
              00000056       SIEIPA0        SIEINSTO
    0057   87 Bitstring    1 SIEINSTE       Interception parameter bit 8-15
              .1.1 .111      SIEIPA1        SIEINSTE SIEIPA1 Second byte of
                                            the OPCODE for extended opcode
                                            instruction or R1R2 field or
                                            immediate data field or length
                                            field
    0058   88 Signed       4 SIEIPB (0)     Interception parameter B Bits
                                            16-47 For instruction
                                            interception, this field contains
                                            bytes 2 and beyond of the
                                            instruction text, if the
                                            instruction is that long
    0058   88 Signed       2 SIEIPBH0 (0)   Halfword 0 of IPB
    0058   88 Bitstring    1 SIEIPB0        Byte 0 of IPB
    0059   89 Bitstring    1 SIEIPB1        Byte 1 of IPB
    005A   90 Signed       2 SIEIPBH1 (0)   Halfword 1 of IPB
    005A   90 Bitstring    1 SIEIPB2        Byte 2 of IPB
    005B   91 Bitstring    1 SIEIPB3        Byte 3 of IPB
    005C   92 Signed       4 SIEIBM3        Reserved for IBM hardware use
    0060   96 Bitstring    1 SIERCPB0       Function-Progress Flags
              .1.. ....      SIESKAIP       X'40' SIESKAIP Storage key assist
                                            in progress
    0061   97 Bitstring    3 SIEECB (0)     Execution Controls B
    0061   97 Bitstring    1 SIEECBB0       Execution Controls B (ECB byte 0)
              1... ....      SIEQEBSM       X'80' SIEQEBSM (00) QEBSM
                                            Interpretation Active
              .1.. ....      SIEECGSF       X'40' SIEECGSF (01)
                                            Guarded-storage facility
              ...1 ....      SIEECTX        X'10' SIEECTX (03) Transactional
                                            Exection
    0062   98 Bitstring    1 SIEECBB1 (0)   Execution Controls B (ECB byte 1)
    0062   98 Bitstring    1 SIERCPB2       Byte two, flags for assists
              ..1. ....      SIEECIEP       X'20' SIEECIEP (10) Instruction
                                            Execution Protection facility
              ...1 ....      SIERCPBY       X'10' SIERCPBY (11) RCP Bypass
                                            (B) for guest
    0063   99 Bitstring    1 SIEECBB2       Execution Controls B (ECB byte 2)
              .... 1...      SIEECB20       X'08' SIEECB20 (20) Reserved for
                                            IBM Use
              .... .1..      SIEECB21       X'04' SIEECB21 (21) Reserved for
                                            IBM Use
    0064  100 Address      4 SIEISCAA       System control area address
              SIEISCAA       SIEISCAM       X'FFFFFFF0' SIEISCAM SCA address
                                            mask
    0068  104 Bitstring    2 *              Reserved for IBM hardware
    006A  106 Bitstring    1 SIEIBM5        Reserved for IBM hardware
    006B  107 Bitstring    1 *              Reserved for IBM hardware
    006C  108 Signed       4 SIETODPR (0)   TOD Programmable Register
    006C  108 Signed       2 *              TODPR high half
    006E  110 Signed       2 SIETODPF       TOD Programmable Field
    0070  112 Address      4 SIEGISA        GISA Absolute Address
    0074  116 Bitstring    4 SIEIOPCT (0)   I/O Interpretation Control 2
    0074  116 Bitstring    1 SIEAZN         Active zone number
    0075  117 Bitstring    1 *              Reserved for IBM hardware use
    0076  118 Signed       2 SIEDVSCS (0)   IRB DS mask
    0076  118 Bitstring    1 SIEDVST        Device status byte of the IRB DS
                                            mask - the contents of this field
                                            are ANDed with the device status
                                            byte of the IRB by TSCH to see if
                                            type B information is present
              1... ....      CSWATTN        X'80' CSWATTN ATTENTION
              .1.. ....      CSWSM          X'40' CSWSM STATUS MODIFIER
              ..1. ....      CSWCUE         X'20' CSWCUE CONTROL UNIT END
              ...1 ....      CSWBUSY        X'10' CSWBUSY BUSY
              .... 1...      CSWCE          X'08' CSWCE CHANNEL END
              .... .1..      CSWDE          X'04' CSWDE DEVICE END
              .... ..1.      CSWUC          X'02' CSWUC UNIT CHECK
              .... ...1      CSWUE          X'01' CSWUE UNIT EXCEPTION
              .... 11..      CSWCEDE        X'0C' CSWCEDE CHANNEL END AND
                                            DEVICE END
              .... 111.      CSWCDEUC       X'0E' CSWCDEUC CHANNEL END,DEVICE
                                            END,UNIT CHECK
              ..1. 11..      CSWCEDC        X'2C' CSWCEDC CHANNEL END,DEVICE
                                            END,AND CUE
              .1.1 ....      CSWSMBSY       X'50' CSWSMBSY CONTROL UNIT BUSY
              .111 ....      CSWCBS         X'70' CSWCBS CONTROL UNIT BUSY
                                            AND END
              1... .1..      CSWDEA         X'84' CSWDEA DEVICE END AND
                                            ATTENTION
    0077  119 Bitstring    1 SIESCST        Subchannel status byte of the IRB
                                            DS mask - the contents of this
                                            field are ANDed with the
                                            subchannel status byte of the IRB
                                            by TSCH to see if type B
                                            information is present
              1... ....      CSWPCI         X'80' CSWPCI PROGRAM CONTROLLED
                                            INTERRUPTION Command Mode only
              .1.. ....      CSWIL          X'40' CSWIL INCORRECT LENGTH
                                            INDICATION Command Mode only
              ..1. ....      CSWPRG         X'20' CSWPRG CHANNEL PROGRAM
                                            CHECK
              ...1 ....      CSWPROT        X'10' CSWPROT STORAGE PROTECTION
                                            CHECK
              .... 1...      CSWCDC         X'08' CSWCDC CHANNEL DATA CHECK
              .... .1..      CSWCCC         X'04' CSWCCC CHANNEL CONTROL
                                            CHECK
              .... ..1.      CSWIFCC        X'02' CSWIFCC INTERFACE CONTROL
                                            CHECK
              .... ...1      CSWCHC         X'01' CSWCHC CHANNEL CHAINING
                                            CHECK Command Mode only
              .... 111.      CSWHCE         X'0E' CSWHCE CDC+CCC+IFCC
                                            HARDWARE ERRORS
              ..11 ...1      CSWPCE         X'31' CSWPCE PRG+CHC+PROT PROGRAM
                                            ERRORS
    0078  120 Signed       4 SIERSVD3 (0)   Reserved for IBM hardware
    0078  120 Bitstring    1 SIEAZM         Alert generating zone mask
    0079  121 Bitstring    2 SIEIBM2        Reserved for IBM hardware
    007B  123 Bitstring    1 *              Reserved for IBM hardware
    007C  124 Signed       4 *              Reserved for IBM hardware
    0080  128 Signed       8 SIEGMSOR       Guest real main-storage origin in
                                            host address space
    0088  136 Signed       8 SIEGMSLM       Guest real main-storage limit in
                                            host address space Bits 0-43 of
                                            this field, padded on the right
                                            with 20 *ones*, is the highest
                                            host virtual address to which the
                                            guest has access. Thus, the
                                            actual guest storage size is
                                            (GMSLM+1M-GMSOR).
              00FFFFFF       SIEGMSMKH      X'FFFFFFFF' Mask for significant
                                            bits of GMSOR/GMSLM -- high half
              00F00000       SIEGMSMKL      X'FFF00000' Ditto -- low half
    0090  144 Bitstring   16 SIEGPSW (0)    Guest PSW (zArch guests)
    0090  144 Bitstring    8 SIEPSW (0)     Guest PSW (ESA/390 guests)
    0090  144 Signed       4 SIEPSW0F (0)   Bytes 0:3 of guest PSW
    0090  144 Bitstring    1 SIEPSW0B (0)   Byte 0 of guest PSW
              1111 11..      PSWIOMSK       X'FC' PSWIOMSK CHANNEL MASK,
                                            CHANNELS 0-5
              .... ..1.      PSWIOSMB       X'02' PSWIOSMB I/O SUMMARY MASK,
                                            CHANNEL 6-15
              .... ...1      PSWEXSMB       X'01' PSWEXSMB EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0090  144 Bitstring    1 SIEPSW0        Byte 0 of guest PSW
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0091  145 Bitstring    1 SIEPSW1        Byte 1 of guest PSW
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0092  146 Signed       2 SIEPSW2H (0)   Bytes 2:3 of guest PSW
    0092  146 Bitstring    1 SIEPSW2        Byte 2 of guest PSW
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0093  147 Bitstring    1 SIEPSW3        Reserved for IBM hardware
              1... ....      PSWRTI         X'80' PSWRTI Run-time
                                            instrumentation
              .... ...1      PSWEA          X'01' PSWEA Extended Addressing
                                            Mode
    0094  148 Signed       4 SIEPSW4F (0)   Bytes 4:7 of guest PSW
    0094  148 Bitstring    1 SIEPSW4B (0)   Byte 4 of guest PSW
              11.. ....      PSWILCBC       X'C0' PSWILCBC INSTRUCTION LENGTH
                                            CODE (ILC)
              1... ....      PSWILCB4       X'80' PSWILCB4 BC MODE ILC, 4
                                            BYTE LENGTH
              .1.. ....      PSWILCB2       X'40' PSWILCB2 BC MODE ILC, 2
                                            BYTE LENGTH
              ..11 ....      PSWCONDB       X'30' PSWCONDB PSW CONDITION CODE
              ..1. ....      PSWCONB2       X'20' PSWCONB2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCONB1       X'10' PSWCONB1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSKB       X'0F' PSWPMSKB
                                            FIXOB+DECOB+EXUNB+SIGNB PROGRAM
                                            MASK
              .... 1...      PSWFIXOB       X'08' PSWFIXOB FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECOB       X'04' PSWDECOB DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUNB       X'02' PSWEXUNB EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGNB       X'01' PSWSIGNB SIGNIFICANCE
                                            INTERRUPT MASK Equate to define
                                            the open storage key associated
                                            with the Storage-Protection
                                            Override facility
              .... 1..1      KEYOPEN        9 KEYOPEN Access-control bits for
                                            the open storage key. Equates for
                                            storage key processing. May be
                                            used to process storage key
                                            information in ISKE/SSKE operand
                                            format.
              1111 ....      KEYACC         X'F0' KEYACC Storage key access
                                            control
              .... 1...      KEYFETCH       X'08' KEYFETCH Storage key
                                            fetch-protection control
              1111 1...      KEYACCF        KEYACC+KEYFETCH KEYACCF Storage
                                            key access and fetch
              .... .1..      KEYREF         X'04' KEYREF Storage key
                                            reference bit
              .... ..1.      KEYCHG         X'02' KEYCHG Storage key change
                                            bit
              .... .11.      KEYRC          KEYREF+KEYCHG KEYRC Storage key
                                            reference and change
              1111 111.      KEYISOL        KEYACCF+KEYRC KEYISOL Isolate
                                            entire 7 bit storage key Equates
                                            for SSKE M3 mask field option
                                            bits
              .... 1...      SSKENQ         8 SSKENQ SSKE Non-Quiescing
              .... .1..      SSKEMR         4 SSKEMR SSKE Reference bit
                                            update bypass
              .... ..1.      SSKEMC         2 SSKEMC SSKE Change bit update
                                            bypass
              .... ...1      SSKEMB         1 SSKEMB SSKE Multiple 4K blocks
                                            !IC Codes used as operand to SAC
                                            instruction
              .... ....      SACPRIM        X'000' SACPRIM Primary-space mode
              SIEPSW4B       SACSECO        X'100' SACSECO Secondary-space
                                            mode
              SIEPSW4B       SACAR          X'200' SACAR Access-register mode
              SIEPSW4B       SACHOME        X'300' SACHOME Home-space mode
                                            Codes used in register operand to
                                            IDTE instruction
              SIEPSW4B       IDTEG2         X'2000' IDTEG2 IDTE G2
              SIEPSW4B       IDTECBA        X'0800' IDTECBA
                                            IDTE-clearing-by-ASCE Codes used
                                            to locate instances of SAM* (Set
                                            Address Mode) instructions SAM31
                                            and SAM64 (used for cross
                                            reference as HCPXREF operands)
              ...1 1111      SAM31          31 SAM31 Cross reference Set
                                            Addressing Mode entry into 31-bit
                                            addressing mode
              .1.. ....      SAM64          64 SAM64 Cross reference Set
                                            Addressing Mode entry into 64-bit
                                            addressing mode Equates to help
                                            deal with virtual addresses.
              SIEPSW4B       DATSXM         X'7FF00000' DATSXM Isolate
                                            segment-index field of a virtual
                                            address.
              SIEPSW4B       DATPXM         X'000FF000' DATPXM Isolate
                                            page-index field of a virtual
                                            address.
              SIEPSW4B       DATBXM         X'00000FFF' DATBXM Isolate
                                            byte-index field of a virtual
                                            address. Equates to use in NILL
                                            instructions to convert one
                                            64-bit address to another.
              SIEPSW4B       PTE2PTO        X'F800' PTE2PTO Convert PTE addr
                                            to PTO addr
              SIEPSW4B       PTE2PGM        X'F000' PTE2PGM Convert PTE addr
                                            to PGMBK addr
              SIEPSW4B       PTO2PGM        X'F000' PTO2PGM Convert PTO addr
                                            to PGMBK addr
              SIEPSW4B       STD2STO        X'F000' STD2STO Convert STD addr
                                            to STO addr
              SIEPSW4B       STE2STO        X'F000' STE2STO Convert STE addr
                                            to STO addr
              SIEPSW4B       STE2PTO        X'F800' STE2PTO Convert STE
                                            contents to PTO addr
              SIEPSW4B       STE2PGM        X'F000' STE2PGM Convert STE
                                            contents to PGMBK Equates to use
                                            in NILF instructions to convert
                                            one 64-bit address to another.
              SIEPSW4B       STE2SFAA       X'FFF00000' STE2SFAA Convert
                                            Format-1 STE contents to Segment
                                            Frame Absolute Address Equates
                                            related to access-list
                                            designations.
              SIEPSW4B       ALD0ALOM       X'7FFFFF80' ALD0ALOM Isolate
                                            access-list origin
              .111 1111      ALD0ALLM       X'0000007F' ALD0ALLM Isolate
                                            access-list length
              .... ..11      ALD0ALNS       3 ALD0ALNS Bits to shift right an
                                            ALEN to get the associated ALL
                                            value.
              1... ....      ALD0ALUN       128 ALD0ALUN Number of bytes in
                                            an "access-list unit", the number
                                            of bytes in the smallest
                                            variation of the size of an
                                            access list.
              .... .111      ALD0ALUS       7 ALD0ALUS Number of bits to
                                            shift left in order to multiply
                                            by ALD0ALUN.
              1... ....      ALDMIN         ALD0ALUN ALDMIN Length of
                                            smallest access list, in bytes.
              SIEPSW4B       ALDMAX         4096*4 ALDMAX Length of maximum
                                            access list, in bytes. Equates
                                            related to ASTEO-words:
              SIEPSW4B       ASWASTEOM      X'7FFFFFC0' ASWASTEOM Isolate
                                            ASTE origin Equates related to
                                            DUCTO-words:
              SIEPSW4B       DUWDUCTOM      X'7FFFFFC0' DUWDUCTOM Isolate
                                            DUCT origin SIGP CODES
                                            DEFINITIONS SIGNAL PROCESSOR
                                            CODES
              .... ...1      SIGPSENS       001 SIGPSENS SIGP SENSE
              .... ..1.      SIGPEXTC       002 SIGPEXTC SIGP EXTERNAL CALL
              .... ..11      SIGPEMER       003 SIGPEMER SIGP EMERGENCY
                                            SIGNAL
              .... .1..      SIGPSTRT       004 SIGPSTRT SIGP START
              .... .1.1      SIGPSTOP       005 SIGPSTOP SIGP STOP
              .... .11.      SIGPRSTR       006 SIGPRSTR SIGP RESTART
              .... .111      SIGPIPR        007 SIGPIPR SIGP INITIAL PROGRAM
                                            RESET
              .... 1...      SIGPPR         008 SIGPPR SIGP PROGRAM RESET
              .... 1..1      SIGPSSTT       009 SIGPSSTT SIGP STOP AND STORE
                                            STATUS
              .... 1.11      SIGPICPU       011 SIGPICPU SIGP INITIAL CPU
                                            RESET
              .... 11..      SIGPCPU        012 SIGPCPU SIGP CPU RESET
              .... 11.1      SIGPSPFX       013 SIGPSPFX SIGP SET PREFIX
              .... 111.      SIGPSSTS       014 SIGPSSTS SIGP STORE STATUS AT
                                            ADDRESS
              ...1 ...1      SIGPSXST       017 SIGPSXST SIGP Store Extended
                                            Status At Address
              ...1 ..1.      SIGPSARC       018 SIGPSARC SIGP Set
                                            Architecture
              ...1 .1.1      SIGPSRST       021 SIGPSRST SIGP Sense Running
                                            STatus
              ...1 .11.      SIGPSMT        022 SIGPSMT SIGP Set
                                            Multi-threading
              ...1 .111      SIGPSASA       023 SIGPSASA SIGP Store
                                            Additional Status at Address
    0094  148 Bitstring    1 SIEPSW4        Byte 4 of guest PSW
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0095  149 Bitstring    3 SIEPSW57       Bytes 5:7 of guest PSW
    0098  152 Address      8 SIEPSWIA       Bytes 8:15 of guest PSW (zArch
                                            instruction address)
    00A0  160 Bitstring   16 SIEGG145 (0)   Guest GPR 14 and GPR 15
    00A0  160 Signed       8 SIEGG14        Guest GPR 14 for SIE use only
    00A8  168 Signed       8 SIEGG15        Guest GPR 15 for SIE use only
    00B0  176 Dbl-Word     8 *              Reserved for IBM hardware
    00B8  184 Bitstring    1 SIEHSTID       Host Program ID
    00B9  185 Bitstring    1 *              Reserved for IBM hardware
    00BA  186 Bitstring    6 SIEESB (0)     Expanded-storage boundaries (for
                                            non-RRF guest)
    00BA  186 Bitstring    3 SIEXSO         Expanded-storage origin
    00BD  189 Bitstring    3 SIEXSL         Expanded-storage limit
    00C0  192 Bitstring   52 SIEUZP0        Interruption parameters Guest
                                            Prefix Storage Area bytes 128-175
                                            (x80-xAF) or, Guest Prefix
                                            Storage Area bytes 184-195
                                            (xB8-xC3) or, parameters for
                                            partial- execution interception
                                            depending on the event
    00F4  244 Bitstring    6 SIEIBM1        Reserved for IBM hardware
    00FA  250 Bitstring    2 SIEIEF         Migration Emulation Controls
    00FC  252 Signed       4 SIEIBM4        Reserved for IBM hardware
    0100  256 Bitstring  128 SIEGCRS (0)    Guest Control registers 0-15 If
                                            SIxMODEX.SIxESAME is NOT on then
                                            the 16 32-bit control registers
                                            are in the rightmost word of each
                                            doubleword register area
    0100  256 Signed       8 SIEGCR0 (0)    zArch Guest Control register 0
    0100  256 Bitstring    1 SIEGCR00       Guest CR0 byte 0
    0101  257 Bitstring    1 SIEGCR01       Guest CR0 byte 1
    0102  258 Bitstring    1 SIEGCR02       Guest CR0 byte 2
    0103  259 Bitstring    1 SIEGCR03       Guest CR0 byte 3
    0104  260 Bitstring    1 SIEGCR04       Guest CR0 byte 4
    0105  261 Bitstring    1 SIEGCR05       Guest CR0 byte 5
    0106  262 Bitstring    1 SIEGCR06       Guest CR0 byte 6
    0107  263 Bitstring    1 SIEGCR07       Guest CR0 byte 7
    0108  264 Signed       8 SIEGCR1 (0)    zArch Guest Control register 1
    0108  264 Bitstring    7 *
    010F  271 Bitstring    1 SIEGCR17       Guest CR1 byte 7
    0110  272 Signed       8 SIEGCR2 (0)    zArch Guest Control register 2
    0110  272 Bitstring    7 *
    0117  279 Bitstring    1 SIEGCR27       Guest CR2 byte 7
    0118  280 Signed       8 SIEGCR3        zArch Guest Control register 3
    0120  288 Signed       8 SIEGCR4        zArch Guest Control register 4
    0128  296 Signed       8 SIEGCR5 (0)    zArch Guest Control register 5
    0128  296 Bitstring    4 *
    012C  300 Bitstring    1 SIEGCR54       Guest CR5 byte 4
    012D  301 Bitstring    3 *
    0130  304 Signed       8 SIEGCR6 (0)    zArch Guest Control register 6
    0130  304 Bitstring    4 *
    0134  308 Bitstring    1 SIEGCR64       Guest CR6 byte 4
    0135  309 Bitstring    3 *
    0138  312 Signed       8 SIEGCR7        zArch Guest Control register 7
    0140  320 Signed       8 SIEGCR8 (0)    zArch Guest Control register 8
    0140  320 Bitstring    1 SIEGCR80       z/Arch guest CR8 Byte 0
    0141  321 Bitstring    1 SIEGCR81       z/Arch guest CR8 Byte 1
    0142  322 Signed       2 SIEGCR8E (0)   Enhanced-Monitor Mask
    0142  322 Bitstring    1 SIEGCR82       z/Arch guest CR8 Byte 2
    0143  323 Bitstring    1 SIEGCR83       z/Arch guest CR8 Byte 3
              ..1. ....      SIEEMC10       X'20' SIEEMC10 Enhanced-Mon Class
                                            10
    0144  324 Bitstring    2 SIEGCR8A       Guest CR8 bytes 4+5, EAX
    0146  326 Bitstring    2 SIEGCR8M       Guest CR8 bytes 6+7, Monitor Mask
    0148  328 Signed       8 SIEGCR9 (0)    zArch Guest Control register 9
    0148  328 Bitstring    4 *
    014C  332 Bitstring    1 SIEGCR94       Guest CR9 byte 4
    014D  333 Bitstring    1 SIEGCR95       Guest CR9 byte 5
    014E  334 Bitstring    2 *
    0150  336 Signed       8 SIEGCR10       zArch Guest Control register 10
    0158  344 Signed       8 SIEGCR11       zArch Guest Control register 11
    0160  352 Signed       8 SIEGCR12 (0)   zArch Guest Control register 12
    0160  352 Bitstring    7 *
    0167  359 Bitstring    1 SIEGCRC7       Guest CR12 byte 7
    0168  360 Signed       8 SIEGCR13 (0)   zArch Guest Control register 13
    0168  360 Bitstring    7 *
    016F  367 Bitstring    1 SIEGCRD7       Guest CR13 byte 7
    0170  368 Signed       8 SIEGCR14 (0)   zArch Guest Control register 14
    0170  368 Bitstring    4 *
    0174  372 Bitstring    1 SIEGCRE4       Guest CR14 byte 4
    0175  373 Bitstring    1 SIEGCRE5       Guest CR14 byte 5
    0176  374 Bitstring    2 *
    0178  376 Signed       8 SIEGCR15       zArch Guest Control register 15
    0180  384 Bitstring  128 SIEHWRSV (0)   Reserved for IBM hardware
    0180  384 Signed       8 SIEBEAR        Breaking-Event-Address Register
    0188  392 Bitstring    8 *              Reserved for IBM hardware
    0190  400 Bitstring    8 SIESDNXD       State-Description-Annex
                                            Designation
              SIESDNXD       SIESDNXO       SIESDNXD SIESDNXO SDNX origin
              SIESDNXD       SIESDNXC       00001 SIESDNXD+7,1 SDNX
                                            characteristic (bits 60-63)
              SIESDNXD       SIESDNXM       X'FFF0' SIESDNXM Mask to remove
                                            SDNXC from low halfword
    0198  408 Bitstring    8 *              Reserved for IBM hardware
    01A0  416 Signed       4 SIEFLD         Facility List Designation for
                                            STFLE
    01A4  420 Bitstring   36 *              Reserved for IBM hardware
    01C8  456 Bitstring    4 SIEECD (0)     Execution Controls D
    01C8  456 Bitstring    1 SIEECDB0       ECD byte 0
              ..1. ....      SIEECHRM       X'20' SIEECHRM Host Register
                                            Management
    01C9  457 Bitstring    1 SIEECDB1       ECD byte 1
              ..1. ....      SIEECD10       X'20' SIEECD10 Reserved
    01CA  458 Bitstring    1 SIEECDB2       ECD byte 2
    01CB  459 Bitstring    1 SIEECDB3       ECD byte 3
    01CC  460 Bitstring   18 *              Reserved for IBM use
    01DE  478 Bitstring    8 SIEPPARM       Guest Program Parameter
    01E6  486 Bitstring    2 *              Reserved for IBM hardware
    01E8  488 Signed       8 SIEITDBA       Interception TDB
    01F0  496 Bitstring    8 *              Reserved for IBM hardware
    01F8  504 Signed       8 SIEGVRD        Guest-Vector-Register Designation
              00000200       SIEBLEN        *-SIEBK Block size in bytes
              00000040       SIEDWLEN       ((*-SIEBK)+7)/8 Block size in
                                            doublewords
                  Redefine interception parameters for validity
                  interception.
    0056   86 Bitstring    4 SIEVIRSN (0)   Validity interception reason code
    0056   86 Bitstring    1 SIEVIWHO       "Who" recognized the validity
                                            interception? How many levels
                                            deep in interpretive execution,
                                            and what component?
    0057   87 Bitstring    1 SIEVIWHN       "When" was the condition
                                            encountered (SIE entry, exit,
                                            instruction interpretation,
                                            etc.)?
    0058   88 Signed       2 SIEVIWHY       "Why" did the validity inter-
                                            ception occur? What was the
                                            specific defect in the guest
                                            definition or host state?
    005A   90 Bitstring    2 SIEVIRSV       Reserved; zeroes stored on
                                            validity interception
                  Redefine Guest Prefix Area 128-239 (x80-xAF)
    00C0  192 Signed       4 SIEEXMSF       MSF Data Block Addr-Class 21 EXT
    00C4  196 Signed       4 SIEIEXCF (0)   External Interrupt CPU and Code
    00C4  196 Signed       2 SIEIEXCA       External Interrupt CPU address
    00C6  198 Signed       2 SIEIEXCD (0)   External Interrupt Code
    00C6  198 Bitstring    1 SIEIEXCL       EXTERNAL INTERRUPTION CLASS CODE
              00000000       EXTICL00       00 EXTICL00 CLASS 00 EXTERNAL
                                            INTERRUPTS (INTERRUPT KEY,
                                            INTERVAL TIMER)
              00000010       EXTICL10       16 EXTICL10 CLASS 10 EXTERNAL
                                            INTERRUPTS (TIMER, COMPARATOR,
                                            TOD SYNCH)
              00000012       EXTICL12       18 EXTICL12 CLASS 12 EXTERNAL
                                            INTERRUPTS (MULTI-CPU SIGNALS)
              00000014       EXTICL14       20 EXTICL14 CLASS 14 EXTERNAL
                                            INTERRUPTS (ETR INTERRUPTS)
              00000020       EXTICL20       32 EXTICL20 Class 20 external
                                            interrupts (Time zone transition)
              00000024       EXTICL24       36 EXTICL24 CLASS 24 EXTERNAL
                                            INTERRUPTS (SERVICE SIGNALS)
              00000026       EXTICL26       38 EXTICL26 CLASS 26 EXTERNAL
                                            INTERRUPTS (ESA/XC INTERRUPTS)
              00000040       EXTICL40       64 EXTICL40 CLASS 40 EXTERNAL
                                            INTERRUPTS (VMCF AND IUCV
                                            COMMUNICATION)
    00C7  199 Bitstring    1 SIEIEXCT       EXTERNAL INTERRUPTION TYPE CODE
              00000040       EXTIKEY        64 EXTIKEY CODE X'0040' INTERRUPT
                                            KEY
              00000080       EXTITMR        128 EXTITMR CODE X'0080' 370
                                            INTERVAL TIMER
              00000004       EXTICKC        04 EXTICKC CODE X'1004' CLOCK
                                            COMPARATOR
              00000005       EXTICPU        05 EXTICPU CODE X'1005' CPU TIMER
              00000000       EXTIMALF       00 EXTIMALF CODE X'1200'
                                            MALFUNCTION ALERT
              00000001       EXTIEMGS       01 EXTIEMGS CODE X'1201'
                                            EMERGENCY SIGNAL
              00000002       EXTICALL       02 EXTICALL CODE X'1202' EXTERNAL
                                            CALL
              00000006       EXTIETR        06 EXTIETR CODE X'1406' ETR
                                            INTERRUPT
              00000007       EXTIMEAS       07 EXTIMEAS Code X'1407'
                                            Measurement Alert
              00000004       EXTITZCH       04 EXTITZCH CODE X'2004' Time
                                            Zone Change
              00000001       EXTISVSG       01 EXTISVSG CODE X'2401' SERVICE
                                            SIGNAL
              00000002       EXTIPVM        02 EXTIPVM CODE X'2402' PVM
                                            LOGICAL DEVICE
              00000003       EXTIXC         03 EXTIXC CODE X'2603' ESA/XC and
                                            other VM external interrupts
              00000000       EXTIIUCV       00 EXTIIUCV CODE X'4000' IUCV
                                            INTERRUPTION
              00000001       EXTIVMCF       01 EXTIVMCF CODE X'4001' VMCF
                                            INTERRUPTION
    00C8  200 Signed       2 SIESVCIL       SVC Instruction Length Code
    00CA  202 Signed       2 SIESVCNT       SVC Interrupt Code
    00CC  204 Signed       4 SIEIPRCD (0)   Program ILC and Interrupt Code
    00CC  204 Signed       2 SIEIPRCL       Program Instruction Length Code
    00CE  206 Signed       2 SIEIPRCC (0)   Program Interrupt Code
              00000136       PRGIADCP       X'0136' PRGIADCP Addressing
                                            capability
              00000400       PRGITXHA       X'0400' PRGITXHA Host
                                            interrupting guest TX
              00000200       PRGITRXA       X'0200' PRGITRXA Transaction
                                            aborted by PRG intrpt
              00000600       PRGITXMD       PRGITXHA+PRGITRXA PRGITXMD TX
                                            modifiers combined
              00000680       PRGIHMOD       PRGITXHA+PRGITRXA+PRGIPER
                                            PRGIHMOD Prg intrpt modifiers
                                            used in host interruption
                                            handling
              0000F97F       PRGICHMD       X'FFFF'-PRGIHMOD PRGICHMD Mask
                                            used for clearing host
                                            interruption modifiers
    00CE  206 Bitstring    1 SIEIPRC0       Program interrupt code byte 0
    00CF  207 Bitstring    1 SIEIPRC1       Program interrupt code byte 1
              00000000       PRGICCLR       X'00' PRGICCLR USED TO CLEAR
                                            PRGICODE
              00000001       PRGIOPER       X'01' PRGIOPER OPERATION
              00000002       PRGIPRIV       X'02' PRGIPRIV PRIVILEGED
                                            OPERATION
              00000003       PRGIEXEC       X'03' PRGIEXEC EXECUTE
              00000004       PRGIPROT       X'04' PRGIPROT PROTECTION
              00000005       PRGIADDR       X'05' PRGIADDR ADDRESSING
              00000006       PRGISPEC       X'06' PRGISPEC SPECIFICATION
              00000007       PRGIDATA       X'07' PRGIDATA DATA
              00000008       PRGIFXDV       X'08' PRGIFXDV FIXED POINT
                                            OVERFLOW
              00000009       PRGIFDIV       X'09' PRGIFDIV FIXED POINT DIVIDE
              0000000A       PRGIDECO       X'0A' PRGIDECO DECIMAL OVERFLOW
              0000000B       PRGIDDIV       X'0B' PRGIDDIV DECIMAL DIVIDE
              0000000C       PRGIEXPO       X'0C' PRGIEXPO EXPONENT OVERFLOW
              0000000D       PRGIEXPU       X'0D' PRGIEXPU EXPONENT UNDERFLOW
              0000000E       PRGISGNF       X'0E' PRGISGNF SIGNIFICANCE
              0000000F       PRGIFPDV       X'0F' PRGIFPDV FLOATING POINT
                                            DIVIDE
              00000010       PRGISEG        X'10' PRGISEG SEGMENT TRANSLATION
              00000011       PRGIPAGE       X'11' PRGIPAGE PAGE TRANSLATION
              00000012       PRGITSPC       X'12' PRGITSPC TRANSLATION
                                            SPECIFICATION
              00000013       PRGISPOP       X'13' PRGISPOP SPECIAL OPERATION
              00000014       PRGIPPF        X'14' PRGIPPF PSEUDO-PAGE-FAULT
                                            (SOFTWARE ONLY)
              00000015       PRGIOPND       X'15' PRGIOPND OPERAND (370/XA
                                            ONLY)
              00000016       PRGITRAC       X'16' PRGITRAC TRACE TABLE FULL
                                            (370/XA ONLY)
              00000017       PRGIASNT       X'17' PRGIASNT ASN TRANSLATION
                                            SPECIFICATION EXCEPTION
              00000018       PRGITRCX       X'18' PRGITRCX Transaction
                                            constraint exception
              0000001A       PRGIBVOL       x'1A' PRGIBVOL Block-Volatility
                                            exception
              0000001B       PRGIVECT       x'1B' PRGIVECT Vector-Processing
                                            exception
              0000001C       PRGISPSW       X'1C' PRGISPSW SPACE SWITCH EVENT
              0000001E       PRGIUNOP       X'1E' PRGIUNOP UNNORMALIZED
                                            OPERAND EXCEPTION
              0000001F       PRGIPCTR       X'1F' PRGIPCTR PC-TRANSLATION
                                            SPECIFICATION
              00000020       PRGIAFXT       X'20' PRGIAFXT AFX TRANSLATION
              00000021       PRGIASXT       X'21' PRGIASXT ASX TRANSLATION
              00000022       PRGILXTR       X'22' PRGILXTR LX TRANSLATION
              00000023       PRGIEXTR       X'23' PRGIEXTR EX TRANSLATION
              00000024       PRGIPRIA       X'24' PRGIPRIA PRIMARY AUTHORITY
              00000025       PRGISECA       X'25' PRGISECA SECONDARY
                                            AUTHORITY
              00000026       PRGILFXTS      X'26' PRGILFXTS LFX translation
                                            specification
              00000027       PRGILSXTS      X'27' PRGILSXTS LSX translation
                                            specification
              00000028       PRGIALTS       X'28' PRGIALTS ALET SPECIFICATION
              00000029       PRGIALNT       X'29' PRGIALNT ALEN TRANSLATION
              0000002A       PRGIALES       X'2A' PRGIALES ALE SEQUENCE
              0000002B       PRGIASTV       X'2B' PRGIASTV ASTE VALIDITY
              0000002C       PRGIASTS       X'2C' PRGIASTS ASTE SEQUENCE
              0000002D       PRGIEXTA       X'2D' PRGIEXTA EXTENDED AUTHORITY
              0000002E       PRGILSTES      X'2E' PRGILSTES LSTE Sequence
              0000002F       PRGIASTI       X'2F' PRGIASTI ASTE Instance
                                            number
              00000030       PRGISTKF       X'30' PRGISTKF STACK FULL
              00000031       PRGISTKE       X'31' PRGISTKE STACK EMPTY
              00000032       PRGISTKS       X'32' PRGISTKS STACK
                                            SPECIFICATION
              00000033       PRGISTKT       X'33' PRGISTKT STACK TYPE
              00000034       PRGISTKO       X'34' PRGISTKO STACK OPERATION
              00000035       PRGIHIX1       X'35' PRGIHIX1 Host-indicated
                                            exception, #1
              00000036       PRGIHIX2       X'36' PRGIHIX2 Host-indicated
                                            exception, #2
              00000038       PRGIASCT       X'38' PRGIASCT ASCE type
              00000039       PRGIRFT        X'39' PRGIRFT Region first
                                            translation
              0000003A       PRGIRST        X'3A' PRGIRST Region second
                                            translation
              0000003B       PRGIRTT        X'3B' PRGIRTT Region third
                                            translation
              00000040       PRGIMC         X'40' PRGIMC MONITOR CALL
              0000007F       PRGICMSK       X'7F' PRGICMSK MASK TO ISOLATE
                                            PROGRAM CHECK
              00000080       PRGIPER        X'80' PRGIPER PROGRAM EVENT
                                            RECORDING, POSSIBLY WITH ANOTHER
                                            EXCEPTION CODE .
    00D0  208 Signed       4 SIEITRAD (0)   390: Translation Exception ID 390
                                            & zArch: Data exception code
    00D0  208 Bitstring    1 SIESSCTL       390: Space-switch event control
              1... ....      SIESSON        X'80' SIESSON 390: Space-sw-ctrl
                                            bit was on
    00D1  209 Bitstring    1 SIESSCT2       390: When a space-switch event
                                            occurs, the space-switch event
                                            control bit is saved in the
                                            high-order bit of SIxSSCTL, and
                                            the remaining bits of SIxSSCTL
                                            and SIxSSCT2 are set to zero
    00D2  210 Signed       2 SIEOPASN (0)   390: Old PASN - set for space-
                                            switch event program interrupt
    00D2  210 Bitstring    1 *              Reserved for IBM hardware use
    00D3  211 Bitstring    1 SIEADDSP (0)   Address space flag indicates
                                            where STD/ASCE value come from
              00000000       SIEPRSTD       00 SIEPRSTD STD/ASCE is obtained
                                            from CR1
              00000001       SIEARSTD       01 SIEARSTD STD/ASCE is obtained
                                            from ART
              00000002       SIESESTD       02 SIESESTD STD/ASCE is obtained
                                            from CR7
              00000003       SIEHOSTD       03 SIEHOSTD STD/ASCE is obtained
                                            from CR13
    00D3  211 Bitstring    1 SIEITRA3       390: Low byte of TEID (contains
                                            suppression-on-protection bits,
                                            STD ID)
    00D0  208 Signed       4 SIEFPARM (0)   Interruption parameter
    00D0  208 Bitstring    3 *
    00D3  211 Bitstring    1 SIEDXCOD       Data-exception code
    00D4  212 Signed       2 SIEIMNCL       Monitor Class
    00D6  214 Signed       2 SIEPERCL (0)   PER class code
    00D6  214 Bitstring    1 SIEPERCD       PER event code identifier
    00D7  215 Bitstring    1 SIEPERZF       PER interrupt code
              1... ....      SIEATM31       X'80' SIEATM31 ATMID PSW bit 31
              .1.. ....      SIEATMID       X'40' SIEATMID Addressing and
                                            translation mode identification
                                            (ATMID) validity bit
              ..1. ....      SIEATM32       X'20' SIEATM32 ATMID PSW bit 32
              ...1 ....      SIEATM05       X'10' SIEATM05 ATMID PSW bit 05
              .... 1...      SIEATM16       X'08' SIEATM16 ATMID PSW bit 16
              .... .1..      SIEATM17       X'04' SIEATM17 ATMID PSW bit 17
              .... ..1.      SIEPSTD1       X'02' SIEPSTD1 STD ID bit 1
              .... ...1      SIEPSTD2       X'01' SIEPSTD2 STD ID bit 2
              1111 1111      SIEATM         SIEATM31+SIEATMID+SIEATM32+SIEATM
                                            05+SIEATM16+SIEATM17+SI
                                            EPSTD1+SIEPSTD2 Mask to reset ATM
                                            bits
              .... ....      SIEPRSEG       X'00' SIEPRSEG STD ID bits both
                                            off. This is Primary Segment
                                            Table Designation obtained from
                                            CR-1
              .... ...1      SIEARSEG       X'01' SIEARSEG STD ID bits =
                                            '01'x. This is AR specified
              .... ..1.      SIESESEG       X'02' SIESESEG STD ID bits =
                                            '10'x. This is Secondary Segment
                                            Table Designation obtained from
                                            CR-7
              .... ..11      SIEHOSEG       X'03' SIEHOSEG STD ID bits both
                                            on. This is Home Segment Table
                                            Designation obtained from CR-13
    00D8  216 Dbl-Word     8 SIEGPERA (0)   zArch: PER Address
    00D8  216 Signed       4 SIEGPERL (0)   zArch: Left half PER address
    00D8  216 Signed       4 SIEPERAD       390: PER Address
    00DC  220 Signed       4 SIEGPERR (0)   zArch: Right half PER address
    00DC  220 Signed       4 SIEIMNCD       390: Monitor code (guest prefix
                                            156-159 (x9C-x9F))
    00E0  224 Bitstring    1 SIEXCPAR       Exception Access Identification
              ..1. ....      PRGXCPRI       X'20' PRGXCPRI Primary-tran
                                            problem (not Access Register
                                            related)
              ...1 ....      PRGXCSEC       X'10' PRGXCSEC Secondary-tran
                                            problem (not Access Register
                                            related)
              .... 1111      PRGXCREG       X'0F' PRGXCREG Access-register
                                            number
    00E1  225 Bitstring    1 SIEPERAR       PER Access Identification
    00E2  226 Bitstring    1 SIEOPRID       Operand access identification
    00E3  227 Bitstring    1 *              Reserved for IBM hardware
    00E4  228 Signed       4 *              Reserved for IBM hardware
    00E8  232 Signed       4 SIEXCPAL (0)   Exception ALET (corresponds to
                                            prefix offset 168-171; used only
                                            by VM/ESA during simulation for
                                            ESA/XC guests)
              000000E8       SIEIOPRM       * I/O interruption parameters
                                            (redefined below)
    00E8  232 Signed       8 SIEGTRAD (0)   zArch: Translation exception ID
    00E8  232 Signed       4 SIEGTRAH       zArch: High word of TEID
    00EC  236 Signed       4 SIEGTRAL (0)   zArch: Low word of TEID
    00EC  236 Bitstring    1 SIEGSSCT       zArch: Space-switch event ctrl
              1... ....      SIEGSSON       X'80' SIEGSSON zArch:
                                            Space-sw-ctrl bit was on
    00ED  237 Bitstring    1 SIEGSSC2       zArch: When a space-sw event
                                            occurs, the space-switch event
                                            control bit is saved in the
                                            high-order bit of SIxGSSCT, and
                                            the remaining bits of SIxGSSCT
                                            and SIxGSSC2 are set to zero
    00EE  238 Signed       2 SIEGOPAS (0)   zArch: Old PASN - set for space-
                                            switch event program interrupt
                                            Codes defined for SIEGTRA6 by
                                            HCPEQUAT@VRKNQKU
    00EE  238 Bitstring    1 SIEGTRA6       zArch: Byte 6 of TEID Contains
                                            Access-Exception Fetch/ Store
                                            Indication.
    00EF  239 Bitstring    1 SIEGTRA7       zArch: Low byte of TEID (contains
                                            suppression-on- protection bits,
                                            ASCE ID)
                  Redefine Interruption Parameters area for
                  intercepted I/O interrpution
    00E8  232 Signed       4 SIEIOSID (0)   I/O interruption subchannel
                                            number
    00E8  232 Signed       2 SIEIOINT       I/O interruption constant 0001
    00EA  234 Signed       2 SIEIORNM       I/O interruption subchannel
                                            number
    00EC  236 Signed       4 SIEINPRM       I/O interruption parm
    00F0  240 Signed       4 SIEHIIDW (0)   Host Interruption Identification
                                            Word
    00F0  240 Bitstring    1 SIEIVISC       00VISC000
    00F1  241 Bitstring    1 SIEIZONE       ZONE
    00F2  242 Bitstring    1 SIEISCHI       I0000000 INTERRUPT INTERLOCK CNTL
              1... ....      SIESCHI1       X'80' SIESCHI1 INTERRUPT
                                            INTERLOCK IS ON
    00F3  243 Bitstring    1 *              RESERVED
                  Redefine Interruption Parameters area for
                  intercepted monitor-event interruption
    00E8  232 Signed       8 SIEGMNCD       zArch: Monitor code (guest prefix
                                            176-187 (xB0-xB7))
                  Redefine Interruption Parameters area for
                  Move Page partial-execution interception
    00C0  192 Address      8 SIEGDPTE (0)   Destination operand host DAT
                                            table entry address If host
                                            EDAT-1 is not enabled, contains
                                            the address of the host PTE at
                                            which the translation process for
                                            the destination operand
                                            terminated. If host EDAT-1 is
                                            enabled, contains the address of
                                            the host PTE, STE, or RTE at
                                            which the translation process for
                                            the destination operand
                                            terminated. This could either be
                                            an invalid table entry or a valid
                                            leaf table entry.
    00C0  192 Signed       4 *
    00C4  196 Address      4 SIEDPTE        Dest host PTE addr, low half
    00C8  200 Address      8 SIEGSPTE (0)   Source operand host DAT table
                                            entry address If host EDAT-1 is
                                            not enabled, contains the address
                                            of the host PTE at which the
                                            translation process for the
                                            source operand terminated. If
                                            host EDAT-1 is enabled, contains
                                            the address of the host PTE, STE,
                                            or RTE at which the translation
                                            process for the source operand
                                            terminated. This could either be
                                            an invalid table entry or a valid
                                            leaf table entry.
    00C8  200 Signed       4 *
    00CC  204 Address      4 SIESPTE        Source host PTE addr, low half
                  Redefine Interruption Parameters area for
                  QDIO Enhanced Buffer State Management (QEBSM)
    00C0  192 Bitstring    3 SIEQPEI (0)    Entire EQBSM PEI Code
    00C0  192 Bitstring    1 SIEQCODE       PEI Reason Code
    00C1  193 Bitstring    1 SIEQSBIX       Storage Block Index (SBIX)
    00C2  194 Bitstring    1 SIEQLCK        Lock Indicators
              1... ....      SIEQSD1        X'80' SIEQSD1 QIOBK/QSD is Locked
              .1.. ....      SIEQSD2        X'40' SIEQSD2 QIOBK/QSD for
                                            Format 1, 2 or 3 output queue is
                                            locked
              ..1. ....      SIEQSD3        X'20' SIEQSD3 QIOBK/QSD for
                                            Format 2 completion queue is
                                            locked
                Redefinition of SIxGCRS for ESA/390 Guest
    0100  256 Signed       4 *              Unused for ESA/390 guest
    0104  260 Signed       4 SIECR0 (0)     ESA/390 guest's CR0
    0104  260 Bitstring    1 SIECR0B0       ESA/390 guest CR0 Byte 0
    0105  261 Bitstring    1 SIECR0B1       ESA/390 guest CR0 Byte 1
    0106  262 Bitstring    1 SIECR0B2       ESA/390 guest CR0 Byte 2
    0107  263 Bitstring    1 SIECR0B3       ESA/390 guest CR0 Byte 2
    0108  264 Signed       4 *              Unused for ESA/390 guest
    010C  268 Signed       4 SIECR1 (0)     ESA/390 guest's CR1
    010C  268 Bitstring    1 SIECR1B0       ESA/390 guest CR1 Byte 0 370
                                            Guest Segment Table Length
              1... ....      CR1SSXA        X'80' CR1SSXA 370/XA SPACE SWITCH
                                            EVENT MASK
    010D  269 Bitstring    3 SIECR1SO (0)   370 Guest STO Value
    010D  269 Bitstring    1 SIECR1B1       ESA/390 guest CR1 Byte 1
    010E  270 Bitstring    1 SIECR1B2       ESA/390 guest CR1 Byte 2
    010F  271 Bitstring    1 SIECR1B3       ESA/390 guest CR1 Byte 2
              .... ...1      CR1SS370       X'01' CR1SS370 370 SPACE SWITCH
                                            EVENT MASK
    0110  272 Signed       4 *              Unused for ESA/390 guest
    0114  276 Signed       4 SIECR2 (0)     ESA/390 guest's CR2
    0114  276 Signed       2 SIECR2IM (0)   370 GUEST CHANNEL MASK
    0114  276 Bitstring    1 SIECR2B0       ESA/390 guest CR2 Byte 0
    0115  277 Bitstring    1 SIECR2B1       ESA/390 guest CR2 Byte 0
    0116  278 Bitstring    1 SIECR2B2       ESA/390 guest CR2 Byte 0
    0117  279 Bitstring    1 SIECR2B3       ESA/390 guest CR2 Byte 0
    0118  280 Signed       4 *              Unused for ESA/390 guest
    011C  284 Signed       4 SIECR3 (0)     ESA/390 guest's CR3
    011C  284 Signed       2 SIECR3KM (0)   PSW-KEY mask
    011C  284 Bitstring    1 SIECR3B0       ESA/390 guest CR3 Byte 0
    011D  285 Bitstring    1 SIECR3B1       ESA/390 guest CR3 Byte 1
    011E  286 Signed       2 SIECR3SA (0)   Secondary ASN
    011E  286 Bitstring    1 SIECR3B2       ESA/390 guest CR3 Byte 2
    011F  287 Bitstring    1 SIECR3B3       ESA/390 guest CR3 Byte 3
    0120  288 Signed       4 *              Unused for ESA/390 guest
    0124  292 Signed       4 SIECR4 (0)     ESA/390 guest's CR4
    0124  292 Signed       2 SIECR4AX (0)   Guest control register 4 - HWORD
                                            0 extended authorization index
                                            (AX)
    0124  292 Bitstring    1 SIECR4B0       ESA/390 guest CR4 Byte 0
    0125  293 Bitstring    1 SIECR4B1       ESA/390 guest CR4 Byte 1
    0126  294 Signed       2 SIECR4PA (0)   Guest control register 4 - HWORD
                                            1 Primary address space number
                                            (PASN)
    0126  294 Bitstring    1 SIECR4B2       ESA/390 guest CR4 Byte 2
    0127  295 Bitstring    1 SIECR4B3       ESA/390 guest CR4 Byte 3
    0128  296 Signed       4 *              Unused for ESA/390 guest
    012C  300 Signed       4 SIECR5 (0)     ESA/390 guest's CR5
    012C  300 Bitstring    1 SIECR5B0       ESA/390 guest CR5 Byte 0
    012D  301 Bitstring    1 SIECR5B1       ESA/390 guest CR5 Byte 1
    012E  302 Bitstring    1 SIECR5B2       ESA/390 guest CR5 Byte 2
    012F  303 Bitstring    1 SIECR5B3       ESA/390 guest CR5 Byte 3
    0130  304 Signed       4 *              Unused for ESA/390 guest
    0134  308 Signed       4 SIECR6 (0)     ESA/390 guest's CR6
    0134  308 Bitstring    1 SIECR6B0       ESA/390 guest CR6 Byte 0
    0135  309 Bitstring    1 SIECR6B1       ESA/390 guest CR6 Byte 1
    0136  310 Bitstring    1 SIECR6B2       ESA/390 guest CR6 Byte 2
    0137  311 Bitstring    1 SIECR6B3       ESA/390 guest CR6 Byte 3
    0138  312 Signed       4 *              Unused for ESA/390 guest
    013C  316 Signed       4 SIECR7 (0)     ESA/390 guest's CR7
    013C  316 Bitstring    1 SIECR7B0       ESA/390 guest CR7 Byte 0
    013D  317 Bitstring    1 SIECR7B1       ESA/390 guest CR7 Byte 1
    013E  318 Bitstring    1 SIECR7B2       ESA/390 guest CR7 Byte 2
    013F  319 Bitstring    1 SIECR7B3       ESA/390 guest CR7 Byte 3
    0140  320 Signed       4 *              Unused for ESA/390 guest
    0144  324 Signed       4 SIECR8 (0)     ESA/390 guest's CR8
    0144  324 Signed       2 SIECR8AX (0)   Extended authorization index
    0144  324 Bitstring    1 SIECR8B0       ESA/390 guest CR8 Byte 0
    0145  325 Bitstring    1 SIECR8B1       ESA/390 guest CR8 Byte 1
    0146  326 Signed       2 SIECR8MM (0)   MONITOR CALL EVENT MASK
    0146  326 Bitstring    1 SIECR8B2       ESA/390 guest CR8 Byte 2
    0147  327 Bitstring    1 SIECR8B3       ESA/390 guest CR8 Byte 3
              ..1. ....      SIEMCL10       X'20' SIEMCL10 Monitor call class
                                            for data from guest to CP
    0148  328 Signed       4 *              Unused for ESA/390 guest
    014C  332 Signed       4 SIECR9 (0)     ESA/390 guest's CR9
    014C  332 Bitstring    1 SIECR9B0       ESA/390 guest CR9 Byte 0
    014D  333 Bitstring    1 SIECR9B1       ESA/390 guest CR9 Byte 1
    014E  334 Bitstring    2 SIECR9GM       PER General-register alteration
                                            mask
    0150  336 Signed       4 *              Unused for ESA/390 guest
    0154  340 Signed       4 SIECR10        ESA/390 guest's CR10
    0158  344 Signed       4 *              Unused for ESA/390 guest
    015C  348 Signed       4 SIECR11        ESA/390 guest's CR11
    0160  352 Signed       4 *              Unused for ESA/390 guest
    0164  356 Signed       4 SIECR12 (0)    ESA/390 guest's CR12
    0164  356 Bitstring    1 SIECRCB0       ESA/390 guest CR12 Byte 0
              1... ....      CRCBRCTL       X'80' CRCBRCTL BRANCH TRACE
                                            CONTROL BIT. WHEN ON, BALR, BASR,
                                            BASSM, BAKR AND BSG INST MAY BE
                                            TRACED BY THE HARDWARE. Note that
                                            for zArch, this bit is moved to
                                            GCRC0.0 of a 64-bit CRC with a
                                            label of CRCBTCTL.
    0165  357 Bitstring    1 SIECRCB1       ESA/390 guest CR12 Byte 1
    0166  358 Bitstring    1 SIECRCB2       ESA/390 guest CR12 Byte 2
    0167  359 Bitstring    1 SIECRCB3       ESA/390 guest CR12 Byte 3
    0168  360 Signed       4 *              Unused for ESA/390 guest
    016C  364 Signed       4 SIECR13 (0)    ESA/390 guest's CR13
    016C  364 Bitstring    1 SIECRDB0       ESA/390 guest CR13 Byte 0
    016D  365 Bitstring    1 SIECRDB1       ESA/390 guest CR13 Byte 1
    016E  366 Bitstring    1 SIECRDB2       ESA/390 guest CR13 Byte 2
    016F  367 Bitstring    1 SIECRDB3       ESA/390 guest CR13 Byte 3
    0170  368 Signed       4 *              Unused for ESA/390 guest
    0174  372 Signed       4 SIECR14 (0)    ESA/390 guest's CR14
    0174  372 Bitstring    1 SIECREB0       ESA/390 guest CR14 Byte 0
    0175  373 Bitstring    1 SIECREB1       ESA/390 guest CR14 Byte 1
    0176  374 Bitstring    1 SIECREB2       ESA/390 guest CR14 Byte 2
    0177  375 Bitstring    1 SIECREB3       ESA/390 guest CR14 Byte 3
    0178  376 Signed       4 *              Unused for ESA/390 guest
    017C  380 Signed       4 SIECR15 (0)    ESA/390 guest's CR15 MACHINE
                                            CHECK EXTENDED LOG ADDR
    017C  380 Bitstring    1 SIECRFB0       ESA/390 guest CR15 Byte 0
    017D  381 Bitstring    1 SIECRFB1       ESA/390 guest CR15 Byte 1
    017E  382 Bitstring    1 SIECRFB2       ESA/390 guest CR15 Byte 2
    017F  383 Bitstring    1 SIECRFB3       ESA/390 guest CR15 Byte 3
                 End of Control Register redefinitions
                  End of the SIxBK

SIEBK Storage Layout | Top of page

    *** SIEBK - SIE STATE DESCRIPTOR BLOCK
    *
    *     +------+------+------+------+---------------------------+
    *   0 |:NTVCT|:STATC|:MODEX|:MODE |         SIEPREFX          |
    *     +------+------+------+------+---------------------------+
    *   8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  18 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  20 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  28 |                       SIECPUTM                        |
    *     +-------------------------------------------------------+
    *  30 |                        SIECKC                         |
    *     +-------------------------------------------------------+
    *  38 |                       SIEEPOCH                        |
    *     +------+------+------+------+------+------+-------------+
    *  40 |:SVCTL|:SVC1N|:SVC2N|:SVC3N|:LCTB0|:LCTB1|  SIEICPUA   |
    *     +------+------+------+------+------+------+------+------+
    *  48 |:ICPT0|:ICPT1|:ICPT2|:ICPT3|:ECA0 |:ECA1 |:ECA2 |:ECA3 |
    *     +------+------+------+------+------+------+------+------+
    *  50 |:ICODE|:ICFLG|  SIEIHCPU   |/////////////|:INSTO|:INSTE|
    *     +------+------+------+------+-------------+------+------+
    *  58 |:IPB0 |:IPB1 |:IPB2 |:IPB3 |         SIEIBM3           |
    *     +------+------+------+------+---------------------------+
    *  60 |:RCPB0|:ECBB0|:RCPB2|:ECBB2|         SIEISCAA          |
    *     +------+------+------+------+-------------+-------------+
    *  68 |/////////////|:IBM5 |//////|/////////////|  SIETODPF   |
    *     +-------------+------+------+------+------+------+------+
    *  70 |         SIEGISA           |SIEAZN|//////|:DVST |:SCST |
    *     +------+-------------+------+------+------+------+------+
    *  78 |SIEAZM|  SIEIBM2    |//////|///////////////////////////|
    *     +------+-------------+------+---------------------------+
    *  80 |                       SIEGMSOR                        |
    *     +-------------------------------------------------------+
    *  88 |                       SIEGMSLM                        |
    *     +------+------+------+------+------+--------------------+
    *  90 |:PSW0 |:PSW1 |:PSW2 |:PSW3 |:PSW4 |     SIEPSW57       |
    *     +------+------+------+------+------+--------------------+
    *  98 |                       SIEPSWIA                        |
    *     +-------------------------------------------------------+
    *  A0 |                       SIEGG14                         |
    *     +-------------------------------------------------------+
    *  A8 |                       SIEGG15                         |
    *     +-------------------------------------------------------+
    *  B0 |///////////////////////////////////////////////////////|
    *     +------+------+--------------------+--------------------+
    *  B8 |:HSTID|//////|      SIEXSO        |      SIEXSL        |
    *     +------+------+--------------------+--------------------+
    *  C0 |                                                       |
    *     =                       SIEUZP0                         =
    *     |                           +---------------------------+
    *     |                           |         SIEIBM1-          |
    *     +-------------+-------------+---------------------------+
    *  F8 |   -(0F4)    |   SIEIEF    |         SIEIBM4           |
    *     +------+------+------+------+------+------+------+------+
    * 100 |:GCR00|:GCR01|:GCR02|:GCR03|:GCR04|:GCR05|:GCR06|:GCR07|
    *     +------+------+------+------+------+------+------+------+
    * 108 |////////////////////////////////////////////////|:GCR17|
    *     +------------------------------------------------+------+
    * 110 |////////////////////////////////////////////////|:GCR27|
    *     +------------------------------------------------+------+
    * 118 |                       SIEGCR3                         |
    *     +-------------------------------------------------------+
    * 120 |                       SIEGCR4                         |
    *     +---------------------------+------+--------------------+
    * 128 |///////////////////////////|:GCR54|////////////////////|
    *     +---------------------------+------+--------------------+
    * 130 |///////////////////////////|:GCR64|////////////////////|
    *     +---------------------------+------+--------------------+
    * 138 |                       SIEGCR7                         |
    *     +------+------+------+------+-------------+-------------+
    * 140 |:GCR80|:GCR81|:GCR82|:GCR83|  SIEGCR8A   |  SIEGCR8M   |
    *     +------+------+------+------+------+------+-------------+
    * 148 |///////////////////////////|:GCR94|:GCR95|/////////////|
    *     +---------------------------+------+------+-------------+
    * 150 |                       SIEGCR10                        |
    *     +-------------------------------------------------------+
    * 158 |                       SIEGCR11                        |
    *     +------------------------------------------------+------+
    * 160 |////////////////////////////////////////////////|:GCRC7|
    *     +------------------------------------------------+------+
    * 168 |////////////////////////////////////////////////|:GCRD7|
    *     +---------------------------+------+------+------+------+
    * 170 |///////////////////////////|:GCRE4|:GCRE5|/////////////|
    *     +---------------------------+------+------+-------------+
    * 178 |                       SIEGCR15                        |
    *     +-------------------------------------------------------+
    * 180 |                       SIEBEAR                         |
    *     +-------------------------------------------------------+
    * 188 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 190 |                       SIESDNXD                        |
    *     +-------------------------------------------------------+
    * 198 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 1A0 |          SIEFLD           |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    * 1A8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 1C8 |:ECDB0|:ECDB1|:ECDB2|:ECDB3|///////////////////////////|
    *     +------+------+------+------+///////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     |/////////////////////////////////////////+-------------+
    *     |/////////////////////////////////////////|   (1DE)-    |
    *     +-----------------------------------------+-------------+
    * 1E0 |               -SIEPPARM                 |/////////////|
    *     +-----------------------------------------+-------------+
    * 1E8 |                       SIEITDBA                        |
    *     +-------------------------------------------------------+
    * 1F0 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 1F8 |                       SIEGVRD                         |
    *     +-------------------------------------------------------+
    * 200
    *
    *** SIEBK - SIE STATE DESCRIPTOR BLOCK

    *** Overlay for SIEIPARM in SIEBK
    *
    *                                               +------+------+
    *  50 ...                                    56 |:VIWHO|:VIWHN|
    *     +-------------+-------------+-------------+------+------+
    *  58 |  SIEVIWHY   |  SIEVIRSV   | 5C
    *     +-------------+-------------+
    *
    *** Overlay for SIEIPARM in SIEBK

    *** Overlay for SIEUZP0 in SIEBK
    *
    *     +---------------------------+-------------+------+------+
    *  C0 |         SIEEXMSF          |  SIEIEXCA   |:IEXCL|:IEXCT|
    *     +-------------+-------------+-------------+------+------+
    *  C8 |  SIESVCIL   |  SIESVCNT   |  SIEIPRCL   |:IPRC0|:IPRC1|
    *     +------+------+------+------+-------------+------+------+
    *  D0 |:SSCTL|:SSCT2|//////|:ITRA3| D4
    *     +------+------+------+------+
    *
    *** Overlay for SIEUZP0 in SIEBK

    *** Overlay for SIEITRAD in SIEBK
    *
    *     +--------------------+------+-------------+------+------+
    *  D0 |////////////////////|:DXCOD|  SIEIMNCL   |:PERCD|:PERZF|
    *     +--------------------+------+-------------+------+------+
    *  D8 |         SIEPERAD          |         SIEIMNCD          |
    *     +------+------+------+------+---------------------------+
    *  E0 |:XCPAR|:PERAR|:OPRID|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    *  E8 |         SIEGTRAH          |:GSSCT|:GSSC2|:GTRA6|:GTRA7|
    *     +---------------------------+------+------+------+------+
    *  F0
    *
    *** Overlay for SIEITRAD in SIEBK

    *** Overlay for SIEIOPRM in SIEBK
    *
    *     +-------------+-------------+---------------------------+
    *  E8 |  SIEIOINT   |  SIEIORNM   |         SIEINPRM          |
    *     +------+------+------+------+---------------------------+
    *  F0 |:IVISC|:IZONE|:ISCHI|//////| F4
    *     +------+------+------+------+
    *
    *** Overlay for SIEIOPRM in SIEBK

    *** Overlay for SIEIOPRM in SIEBK
    *
    *     +-------------------------------------------------------+
    *  E8 |                       SIEGMNCD                        |
    *     +-------------------------------------------------------+
    *  F0
    *
    *** Overlay for SIEIOPRM in SIEBK

    *** Overlay for SIEUZP0 in SIEBK
    *
    *     +---------------------------+---------------------------+
    *  C0 |///////////////////////////|         SIEDPTE           |
    *     +---------------------------+---------------------------+
    *  C8 |///////////////////////////|         SIESPTE           |
    *     +---------------------------+---------------------------+
    *  D0
    *
    *** Overlay for SIEUZP0 in SIEBK

    *** Overlay for SIEUZP0 in SIEBK
    *
    *     +------+------+------+
    *  C0 |:QCODE|:QSBIX|:QLCK | C3
    *     +------+------+------+
    *
    *** Overlay for SIEUZP0 in SIEBK

    *** Overlay for SIEGCRS in SIEBK
    *
    *     +---------------------------+------+------+------+------+
    * 100 |///////////////////////////|:CR0B0|:CR0B1|:CR0B2|:CR0B3|
    *     +---------------------------+------+------+------+------+
    * 108 |///////////////////////////|:CR1B0|:CR1B1|:CR1B2|:CR1B3|
    *     +---------------------------+------+------+------+------+
    * 110 |///////////////////////////|:CR2B0|:CR2B1|:CR2B2|:CR2B3|
    *     +---------------------------+------+------+------+------+
    * 118 |///////////////////////////|:CR3B0|:CR3B1|:CR3B2|:CR3B3|
    *     +---------------------------+------+------+------+------+
    * 120 |///////////////////////////|:CR4B0|:CR4B1|:CR4B2|:CR4B3|
    *     +---------------------------+------+------+------+------+
    * 128 |///////////////////////////|:CR5B0|:CR5B1|:CR5B2|:CR5B3|
    *     +---------------------------+------+------+------+------+
    * 130 |///////////////////////////|:CR6B0|:CR6B1|:CR6B2|:CR6B3|
    *     +---------------------------+------+------+------+------+
    * 138 |///////////////////////////|:CR7B0|:CR7B1|:CR7B2|:CR7B3|
    *     +---------------------------+------+------+------+------+
    * 140 |///////////////////////////|:CR8B0|:CR8B1|:CR8B2|:CR8B3|
    *     +---------------------------+------+------+------+------+
    * 148 |///////////////////////////|:CR9B0|:CR9B1|  SIECR9GM   |
    *     +---------------------------+------+------+-------------+
    * 150 |///////////////////////////|         SIECR10           |
    *     +---------------------------+---------------------------+
    * 158 |///////////////////////////|         SIECR11           |
    *     +---------------------------+------+------+------+------+
    * 160 |///////////////////////////|:CRCB0|:CRCB1|:CRCB2|:CRCB3|
    *     +---------------------------+------+------+------+------+
    * 168 |///////////////////////////|:CRDB0|:CRDB1|:CRDB2|:CRDB3|
    *     +---------------------------+------+------+------+------+
    * 170 |///////////////////////////|:CREB0|:CREB1|:CREB2|:CREB3|
    *     +---------------------------+------+------+------+------+
    * 178 |///////////////////////////|:CRFB0|:CRFB1|:CRFB2|:CRFB3|
    *     +---------------------------+------+------+------+------+
    * 180
    *
    *** Overlay for SIEGCRS in SIEBK

SIEBK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    ALDMAX         0094 SIEPSW4B
    ALDMIN         0094 80
    ALD0ALLM       0094 7F
    ALD0ALNS       0094 03
    ALD0ALOM       0094 SIEPSW4B
    ALD0ALUN       0094 80
    ALD0ALUS       0094 07
    ASWASTEOM      0094 SIEPSW4B
    CRCBRCTL       0164 80
    CR1SSXA        010C 80
    CR1SS370       010F 01
    CSWATTN        0076 80
    CSWBUSY        0076 10
    CSWCBS         0076 70
    CSWCCC         0077 04
    CSWCDC         0077 08
    CSWCDEUC       0076 0E
    CSWCE          0076 08
    CSWCEDC        0076 2C
    CSWCEDE        0076 0C
    CSWCHC         0077 01
    CSWCUE         0076 20
    CSWDE          0076 04
    CSWDEA         0076 84
    CSWHCE         0077 0E
    CSWIFCC        0077 02
    CSWIL          0077 40
    CSWPCE         0077 31
    CSWPCI         0077 80
    CSWPRG         0077 20
    CSWPROT        0077 10
    CSWSM          0076 40
    CSWSMBSY       0076 50
    CSWUC          0076 02
    CSWUE          0076 01
    DATBXM         0094 SIEPSW4B
    DATPXM         0094 SIEPSW4B
    DATSXM         0094 SIEPSW4B
    DUWDUCTOM      0094 SIEPSW4B
    EXTICALL       00C7 00000002
    EXTICKC        00C7 00000004
    EXTICL00       00C6 00000000
    EXTICL10       00C6 00000010
    EXTICL12       00C6 00000012
    EXTICL14       00C6 00000014
    EXTICL20       00C6 00000020
    EXTICL24       00C6 00000024
    EXTICL26       00C6 00000026
    EXTICL40       00C6 00000040
    EXTICPU        00C7 00000005
    EXTIEMGS       00C7 00000001
    EXTIETR        00C7 00000006
    EXTIIUCV       00C7 00000000
    EXTIKEY        00C7 00000040
    EXTIMALF       00C7 00000000
    EXTIMEAS       00C7 00000007
    EXTIPVM        00C7 00000002
    EXTISVSG       00C7 00000001
    EXTITMR        00C7 00000080
    EXTITZCH       00C7 00000004
    EXTIVMCF       00C7 00000001
    EXTIXC         00C7 00000003
    IDTECBA        0094 SIEPSW4B
    IDTEG2         0094 SIEPSW4B
    KEYACC         0094 F0
    KEYACCF        0094 F8
    KEYCHG         0094 02
    KEYFETCH       0094 08
    KEYISOL        0094 FE
    KEYOPEN        0094 09
    KEYRC          0094 06
    KEYREF         0094 04
    PRGIADCP       00CE 00000136
    PRGIADDR       00CF 00000005
    PRGIAFXT       00CF 00000020
    PRGIALES       00CF 0000002A
    PRGIALNT       00CF 00000029
    PRGIALTS       00CF 00000028
    PRGIASCT       00CF 00000038
    PRGIASNT       00CF 00000017
    PRGIASTI       00CF 0000002F
    PRGIASTS       00CF 0000002C
    PRGIASTV       00CF 0000002B
    PRGIASXT       00CF 00000021
    PRGIBVOL       00CF 0000001A
    PRGICCLR       00CF 00000000
    PRGICHMD       00CE 0000F97F
    PRGICMSK       00CF 0000007F
    PRGIDATA       00CF 00000007
    PRGIDDIV       00CF 0000000B
    PRGIDECO       00CF 0000000A
    PRGIEXEC       00CF 00000003
    PRGIEXPO       00CF 0000000C
    PRGIEXPU       00CF 0000000D
    PRGIEXTA       00CF 0000002D
    PRGIEXTR       00CF 00000023
    PRGIFDIV       00CF 00000009
    PRGIFPDV       00CF 0000000F
    PRGIFXDV       00CF 00000008
    PRGIHIX1       00CF 00000035
    PRGIHIX2       00CF 00000036
    PRGIHMOD       00CE 00000680
    PRGILFXTS      00CF 00000026
    PRGILSTES      00CF 0000002E
    PRGILSXTS      00CF 00000027
    PRGILXTR       00CF 00000022
    PRGIMC         00CF 00000040
    PRGIOPER       00CF 00000001
    PRGIOPND       00CF 00000015
    PRGIPAGE       00CF 00000011
    PRGIPCTR       00CF 0000001F
    PRGIPER        00CF 00000080
    PRGIPPF        00CF 00000014
    PRGIPRIA       00CF 00000024
    PRGIPRIV       00CF 00000002
    PRGIPROT       00CF 00000004
    PRGIRFT        00CF 00000039
    PRGIRST        00CF 0000003A
    PRGIRTT        00CF 0000003B
    PRGISECA       00CF 00000025
    PRGISEG        00CF 00000010
    PRGISGNF       00CF 0000000E
    PRGISPEC       00CF 00000006
    PRGISPOP       00CF 00000013
    PRGISPSW       00CF 0000001C
    PRGISTKE       00CF 00000031
    PRGISTKF       00CF 00000030
    PRGISTKO       00CF 00000034
    PRGISTKS       00CF 00000032
    PRGISTKT       00CF 00000033
    PRGITRAC       00CF 00000016
    PRGITRCX       00CF 00000018
    PRGITRXA       00CE 00000200
    PRGITSPC       00CF 00000012
    PRGITXHA       00CE 00000400
    PRGITXMD       00CE 00000600
    PRGIUNOP       00CF 0000001E
    PRGIVECT       00CF 0000001B
    PRGXCPRI       00E0 20
    PRGXCREG       00E0 0F
    PRGXCSEC       00E0 10
    PSWAMODE       0092 40
    PSWASMSK       0092 C0
    PSWBA          0094 80
    PSWCONB1       0094 10
    PSWCONB2       0094 20
    PSWCOND        0092 30
    PSWCONDB       0094 30
    PSWCOND1       0092 10
    PSWCOND2       0092 20
    PSWDECO        0092 04
    PSWDECOB       0094 04
    PSWEA          0093 01
    PSWECMD        0091 08
    PSWEXSM        0090 01
    PSWEXSMB       0090 01
    PSWEXUN        0092 02
    PSWEXUNB       0094 02
    PSWFIXO        0092 08
    PSWFIXOB       0094 08
    PSWHIADR       0094 7F
    PSWHMODE       0092 C0
    PSWILCBC       0094 C0
    PSWILCB2       0094 40
    PSWILCB4       0094 80
    PSWIOMSK       0090 FC
    PSWIOSM        0090 02
    PSWIOSMB       0090 02
    PSWKEY         0091 F0
    PSWMAPPD       0091 01
    PSWMCHK        0091 04
    PSWPERA        0090 40
    PSWPMODE       0092 00
    PSWPMSK        0092 0F
    PSWPMSKB       0094 0F
    PSWPROB        0091 01
    PSWRTI         0093 80
    PSWSIGN        0092 01
    PSWSIGNB       0094 01
    PSWSMODE       0092 80
    PSWTRAN        0090 04
    PSWWAIT        0091 02
    PSW31AMF       0094 00
    PSW31BT        0094 80
    PTE2PGM        0094 SIEPSW4B
    PTE2PTO        0094 SIEPSW4B
    PTO2PGM        0094 SIEPSW4B
    SACAR          0094 SIEPSW4B
    SACHOME        0094 SIEPSW4B
    SACPRIM        0094 00
    SACSECO        0094 SIEPSW4B
    SAM31          0094 1F
    SAM64          0094 40
    SIEADDSP       00D3
    SIEARSEG       00D7 01
    SIEARSTD       00D3 00000001
    SIEATM         00D7 FF
    SIEATMID       00D7 40
    SIEATM05       00D7 10
    SIEATM16       00D7 08
    SIEATM17       00D7 04
    SIEATM31       00D7 80
    SIEATM32       00D7 20
    SIEAZM         0078
    SIEAZN         0074
    SIEBEAR        0180
    SIEBLEN        01F8 00000200
    SIECKC         0030
    SIECPUTM       0028
    SIECPUTN       0028 80
    SIECPUT0       0028
    SIECRCB0       0164
    SIECRCB1       0165
    SIECRCB2       0166
    SIECRCB3       0167
    SIECRDB0       016C
    SIECRDB1       016D
    SIECRDB2       016E
    SIECRDB3       016F
    SIECREB0       0174
    SIECREB1       0175
    SIECREB2       0176
    SIECREB3       0177
    SIECRFB0       017C
    SIECRFB1       017D
    SIECRFB2       017E
    SIECRFB3       017F
    SIECR0         0104
    SIECR0B0       0104
    SIECR0B1       0105
    SIECR0B2       0106
    SIECR0B3       0107
    SIECR1         010C
    SIECR1B0       010C
    SIECR1B1       010D
    SIECR1B2       010E
    SIECR1B3       010F
    SIECR1SO       010D
    SIECR10        0154
    SIECR11        015C
    SIECR12        0164
    SIECR13        016C
    SIECR14        0174
    SIECR15        017C
    SIECR2         0114
    SIECR2B0       0114
    SIECR2B1       0115
    SIECR2B2       0116
    SIECR2B3       0117
    SIECR2IM       0114
    SIECR3         011C
    SIECR3B0       011C
    SIECR3B1       011D
    SIECR3B2       011E
    SIECR3B3       011F
    SIECR3KM       011C
    SIECR3SA       011E
    SIECR4         0124
    SIECR4AX       0124
    SIECR4B0       0124
    SIECR4B1       0125
    SIECR4B2       0126
    SIECR4B3       0127
    SIECR4PA       0126
    SIECR5         012C
    SIECR5B0       012C
    SIECR5B1       012D
    SIECR5B2       012E
    SIECR5B3       012F
    SIECR6         0134
    SIECR6B0       0134
    SIECR6B1       0135
    SIECR6B2       0136
    SIECR6B3       0137
    SIECR7         013C
    SIECR7B0       013C
    SIECR7B1       013D
    SIECR7B2       013E
    SIECR7B3       013F
    SIECR8         0144
    SIECR8AX       0144
    SIECR8B0       0144
    SIECR8B1       0145
    SIECR8B2       0146
    SIECR8B3       0147
    SIECR8MM       0146
    SIECR9         014C
    SIECR9B0       014C
    SIECR9B1       014D
    SIECR9GM       014E
    SIEDPTE        00C4
    SIEDVSCS       0076
    SIEDVST        0076
    SIEDWLEN       01F8 00000040
    SIEDXCOD       00D3
    SIEECA         004C
    SIEECALT       004C 08
    SIEECA0        004C
    SIEECA1        004D
    SIEECA2        004E
    SIEECA3        004F
    SIEECB         0061
    SIEECBB0       0061
    SIEECBB1       0062
    SIEECBB2       0063
    SIEECB20       0063 08
    SIEECB21       0063 04
    SIEECD         01C8
    SIEECDB0       01C8
    SIEECDB1       01C9
    SIEECDB2       01CA
    SIEECDB3       01CB
    SIEECD10       01C9 20
    SIEECEXT       004C 80
    SIEECGSF       0061 40
    SIEECHRM       01C8 20
    SIEECIEP       0062 20
    SIEECINT       004C 40
    SIEECIO2       004C 04
    SIEECMVP       004C 01
    SIEECSGP       004C 10
    SIEECTX        0061 10
    SIEECVEC       004D 02
    SIEECWAI       004C 20
    SIEEMC10       0143 20
    SIEENDOP       0050 00000000
    SIEEPOCH       0038
    SIEESAME       0002 08
    SIEESB         00BA
    SIEEXMSF       00C0
    SIEEXRUN       0001 01
    SIEEXTMR       0001 02
    SIEFLD         01A0
    SIEFPARM       00D0
    SIEGCRC7       0167
    SIEGCRD7       016F
    SIEGCRE4       0174
    SIEGCRE5       0175
    SIEGCRS        0100
    SIEGCR0        0100
    SIEGCR00       0100
    SIEGCR01       0101
    SIEGCR02       0102
    SIEGCR03       0103
    SIEGCR04       0104
    SIEGCR05       0105
    SIEGCR06       0106
    SIEGCR07       0107
    SIEGCR1        0108
    SIEGCR10       0150
    SIEGCR11       0158
    SIEGCR12       0160
    SIEGCR13       0168
    SIEGCR14       0170
    SIEGCR15       0178
    SIEGCR17       010F
    SIEGCR2        0110
    SIEGCR27       0117
    SIEGCR3        0118
    SIEGCR4        0120
    SIEGCR5        0128
    SIEGCR54       012C
    SIEGCR6        0130
    SIEGCR64       0134
    SIEGCR7        0138
    SIEGCR8        0140
    SIEGCR8A       0144
    SIEGCR8E       0142
    SIEGCR8M       0146
    SIEGCR80       0140
    SIEGCR81       0141
    SIEGCR82       0142
    SIEGCR83       0143
    SIEGCR9        0148
    SIEGCR94       014C
    SIEGCR95       014D
    SIEGDPTE       00C0
    SIEGG14        00A0
    SIEGG145       00A0
    SIEGG15        00A8
    SIEGISA        0070
    SIEGMNCD       00E8
    SIEGMSLM       0088
    SIEGMSMKH      0088 00FFFFFF
    SIEGMSMKL      0088 00F00000
    SIEGMSOR       0080
    SIEGOPAS       00EE
    SIEGPE         0003 01
    SIEGPERA       00D8
    SIEGPERL       00D8
    SIEGPERR       00DC
    SIEGPSW        0090
    SIEGSPTE       00C8
    SIEGSSCT       00EC
    SIEGSSC2       00ED
    SIEGSSON       00EC 80
    SIEGTRAD       00E8
    SIEGTRAH       00E8
    SIEGTRAL       00EC
    SIEGTRA6       00EE
    SIEGTRA7       00EF
    SIEGVRD        01F8
    SIEHIIDW       00F0
    SIEHOSEG       00D7 03
    SIEHOSTD       00D3 00000003
    SIEHSTID       00B8
    SIEHWRSV       0180
    SIEIBM1        00F4
    SIEIBM2        0079
    SIEIBM3        005C
    SIEIBM4        00FC
    SIEIBM5        006A
    SIEICALT       0050 00000030
    SIEICBAK       004B 04
    SIEICBOT       0050 0000000C
    SIEICBSA       0049 08
    SIEICEX        0051 01
    SIEICEXL       0051 60
    SIEICEXS       0051 40
    SIEICFII       0048 10
    SIEICFLG       0051
    SIEICIF        0051 02
    SIEICION       0050 00000040
    SIEICIOR       0050 0000003C
    SIEICIPT       0048 01
    SIEICISK       004A 40
    SIEICLPS       0049 40
    SIEICLSP       004A 01
    SIEICNTC       0050 00000004
    SIEICODE       0050
    SIEICOUO       0050 0000002C
    SIEICPC        004A 08
    SIEICPEX       0050 00000010
    SIEICPG        004B 02
    SIEICPIO       0050 00000018
    SIEICPIX       0050 00000038
    SIEICPNT       0050 00000008
    SIEICPOP       0048 80
    SIEICPR        004B 08
    SIEICPRG       0048 20
    SIEICPRO       0048 40
    SIEICPT        004A 04
    SIEICPTL       0049 20
    SIEICPT0       0048
    SIEICPT1       0049
    SIEICPT2       004A
    SIEICPT3       004B
    SIEICPUA       0046
    SIEICRRB       004A 10
    SIEICRUN       0050 00000044
    SIEICSCK       004B 20
    SIEICSPT       004B 40
    SIEICSSK       004A 20
    SIEICSSM       0049 10
    SIEICSTC       0049 04
    SIEICSTK       004A 80
    SIEICSTN       0049 02
    SIEICSTO       0049 01
    SIEICSTP       0050 00000028
    SIEICTLS       0048
    SIEICTMR       0050 00000048
    SIEICTPT       004A 02
    SIEICVAL       0050 00000020
    SIEICWT        0050 0000001C
    SIEICXNT       0050 00000014
    SIEIEF         00FA
    SIEIEXCA       00C4
    SIEIEXCD       00C6
    SIEIEXCF       00C4
    SIEIEXCL       00C6
    SIEIEXCT       00C7
    SIEIHCPU       0052
    SIEIMISC       0050 00000024
    SIEIMLT4       0050 00000003
    SIEIMNCD       00DC
    SIEIMNCL       00D4
    SIEINPRM       00EC
    SIEINST        0056
    SIEINSTE       0057
    SIEINSTO       0056
    SIEINTWD       0000
    SIEIOINT       00E8
    SIEIOPCT       0074
    SIEIOPRM       00E8 000000E8
    SIEIORNM       00EA
    SIEIOSID       00E8
    SIEIPA         0056
    SIEIPARM       0056
    SIEIPA0        0056 00000056
    SIEIPA1        0057 57
    SIEIPB         0058
    SIEIPBH0       0058
    SIEIPBH1       005A
    SIEIPB0        0058
    SIEIPB1        0059
    SIEIPB2        005A
    SIEIPB3        005B
    SIEIPEXT       0000 01
    SIEIPRCC       00CE
    SIEIPRCD       00CC
    SIEIPRCL       00CC
    SIEIPRC0       00CE
    SIEIPRC1       00CF
    SIEIPSTP       0000 04
    SIEIPVIO       0000 02
    SIEIPWAI       0000 10
    SIEIPXTC       0000 08
    SIEISCAA       0064
    SIEISCAM       0064 SIEISCAA
    SIEISCHI       00F2
    SIEITDBA       01E8
    SIEITRAD       00D0
    SIEITRA3       00D3
    SIEIVISC       00F0
    SIEIZONE       00F1
    SIELCTB0       0044
    SIELCTB1       0045
    SIELCTLA       0045 20
    SIELCTLB       0045 10
    SIELCTLC       0045 08
    SIELCTLD       0045 04
    SIELCTLE       0045 02
    SIELCTLF       0045 01
    SIELCTLS       0044
    SIELCTL0       0044 80
    SIELCTL1       0044 40
    SIELCTL2       0044 20
    SIELCTL3       0044 10
    SIELCTL4       0044 08
    SIELCTL5       0044 04
    SIELCTL6       0044 02
    SIELCTL7       0044 01
    SIELCTL8       0045 80
    SIELCTL9       0045 40
    SIEMCDS        0002 01
    SIEMCL10       0147 20
    SIEMODE        0003
    SIEMODEX       0002
    SIENTVCT       0000
    SIEOPASN       00D2
    SIEOPRID       00E2
    SIEPERAD       00D8
    SIEPERAR       00E1
    SIEPERCD       00D6
    SIEPERCL       00D6
    SIEPERZF       00D7
    SIEPPARM       01DE
    SIEPREFX       0004
    SIEPRSEG       00D7 00
    SIEPRSTD       00D3 00000000
    SIEPSTD1       00D7 02
    SIEPSTD2       00D7 01
    SIEPSW         0090
    SIEPSWIA       0098
    SIEPSW0        0090
    SIEPSW0B       0090
    SIEPSW0F       0090
    SIEPSW1        0091
    SIEPSW2        0092
    SIEPSW2H       0092
    SIEPSW3        0093
    SIEPSW4        0094
    SIEPSW4B       0094
    SIEPSW4F       0094
    SIEPSW57       0095
    SIEQCODE       00C0
    SIEQEBSM       0061 80
    SIEQLCK        00C2
    SIEQPEI        00C0
    SIEQSBIX       00C1
    SIEQSD1        00C2 80
    SIEQSD2        00C2 40
    SIEQSD3        00C2 20
    SIERCPBY       0062 10
    SIERCPB0       0060
    SIERCPB2       0062
    SIERRF         0002 80
    SIERSCB        0001 40
    SIERSVD3       0078
    SIERUNNING     0001 80
    SIESCHI1       00F2 80
    SIESCST        0077
    SIESDNXC       0190 SIESDNXD
    SIESDNXD       0190
    SIESDNXM       0190 SIESDNXD
    SIESDNXO       0190 SIESDNXD
    SIESDSC        0000
    SIESESEG       00D7 02
    SIESESTD       00D3 00000002
    SIESIGA        004F 04
    SIESKAIP       0060 40
    SIESPTE        00CC
    SIESSCTL       00D0
    SIESSCT2       00D1
    SIESSON        00D0 80
    SIESTATC       0001
    SIESVCIL       00C8
    SIESVCNN       0040 80
    SIESVCNT       00CA
    SIESVCTL       0040
    SIESVC1C       0040 40
    SIESVC1N       0041
    SIESVC2C       0040 20
    SIESVC2N       0042
    SIESVC3C       0040 10
    SIESVC3N       0043
    SIETODPF       006E
    SIETODPR       006C
    SIEUZP0        00C0
    SIEVIRSN       0056
    SIEVIRSV       005A
    SIEVIWHN       0057
    SIEVIWHO       0056
    SIEVIWHY       0058
    SIEVR          0003 08
    SIEXCPAL       00E8
    SIEXCPAR       00E0
    SIEXSL         00BD
    SIEXSO         00BA
    SIE2NDVR       0002 20
    SIE2NDVV       0002 40
    SIGPCPU        0094 0C
    SIGPEMER       0094 03
    SIGPEXTC       0094 02
    SIGPICPU       0094 0B
    SIGPIPR        0094 07
    SIGPPR         0094 08
    SIGPRSTR       0094 06
    SIGPSARC       0094 12
    SIGPSASA       0094 17
    SIGPSENS       0094 01
    SIGPSMT        0094 16
    SIGPSPFX       0094 0D
    SIGPSRST       0094 15
    SIGPSSTS       0094 0E
    SIGPSSTT       0094 09
    SIGPSTOP       0094 05
    SIGPSTRT       0094 04
    SIGPSXST       0094 11
    SSKEMB         0094 01
    SSKEMC         0094 02
    SSKEMR         0094 04
    SSKENQ         0094 08
    STD2STO        0094 SIEPSW4B
    STE2PGM        0094 SIEPSW4B
    STE2PTO        0094 SIEPSW4B
    STE2SFAA       0094 SIEPSW4B
    STE2STO        0094 SIEPSW4B

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:31:47 EDT.
Copyright IBM Corporation, 1990, 2020