Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLDDL

Prolog
Control Block Contents
Cross Reference

#### MRSCLDDL Prolog

     DSECT NAME - SCLDDL
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLDDL
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler Domain
                        Record 5 - Drop User From Dispatch List
     DESCRIPTION - Indicates conditions after this user has been
                   dropped from the dispatch list.  A separate
                   record is generated for each VMDBK in the
                   virtual MP complex.
     NOTES:
          - To give a fuller picture of time consumed, three
            sets of used processor time are reported in this
            monitor record.  When multithreading is enabled on
            the system, all three are also reported in the Type
            1 and F accounting records. Timer field names
            ending with _MT1 are MT-1 Equivalent times. Timer
            field names ending with _PRO are Prorated Core
            Times.  Timer field names without an _MT1 or _PRO
            suffix contain Raw Time values.
          - Raw Time is tracked for ALL users for their entire
            session.  Raw Time is the CPU time each virtual CPU
            spent dispatched on a thread and is the CPU Timer
            information provided directly by the hardware.
          - MT-1 Equivalent Time is tracked for ALL users for
            their entire session. This calculated CPU time
            approximates the time that would have been spent
            if the workload had been run with multithreading
            disabled, that is, with all core resources available
            to one thread.  When a user is running on a system
            where multithreading is not installed or not
            enabled, MT-1 Equivalent Time consumed will be
            identical to Raw Time.  However, if a guest has
            relocated from an MT-enabled system to an
            MT-disabled system, the cumulative raw and MT-1
            Equivalent times reported in monitor records may
            differ due to the prior execution in the MT
            environment.
          - Prorated Core Time charges for core utilization in
            a way suitable to core-based software licensing.
            Time is charged by dividing the time the core was
            dispatched evenly among the threads dispatched in
            that interval. Since Prorated Core Time is not
            always calculated, additional information
            is reported regarding the Prorated Core Time values:
            * The _VMAPRCAL bit indicates whether the Prorated
              Core Time values in this record are valid.
            When the user is relocated to any other system
            (even a Multithreading aware/enabled system),
            Prorated Core Time is reset. This means:
            * the _VMAPRCAL bit is set based on whether the
              source system will be calculating prorated core
              time or not.
            * all _VMAxxxxx_PRO fields are reset to PFXTMMAX.

#### MRSCLDDL Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure   300  SCLDDL                 Start of monitor record
       0   0  Character     0  SCLDDL_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Character     8  SCLDDL_VMDUSER         Userid
      28  1C  Character     8  SCLDDL_VMDSVMID        VMDBK name for the last
                                                      successful IUCV, VMCF or
                                                      APPC/VM Send for this virtual
                                                      machine. Valid in base VMDBK
                                                      only.
      36  24  Bitstring     1  SCLDDL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLDDL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF, or
                                                      APPC.
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      37  25  Character     0  SCLDDL_VMDSVMW2        back-up byte to the
                                                      VMDSVMWT byte. Copied here so
                                                      that they will persist longer
                                                      than they would in VMDSVMWT.
                                                      Valid in base VMDBK only.
      37  25  Bitstring     1  SCLDDL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLDDL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF, or
                                                      APPC.
      38  26  Character     0  SCLDDL_VMDRDYCM        Flag byte set by IUCV,
                                                      VMCF, or APPC whenever
                                                      IUCV/VMCF/APPC makes an
                                                      external interrupt pending in
                                                      a virtual machine. It is sort
                                                      of a "reference bit" that
                                                      tells the scheduler that
                                                      IUCV/VMCF/APPC has been
                                                      active recently. Valid in
                                                      base VMDBK only.
      38  26  Bitstring     1  SCLDDL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLDDL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF, or
                                                      APPC.
      39  27  Bitstring     1  SCLDDL_CALFLAG1        Flag Byte 1
              1... ....        SCLDDL_VMDLRGST         User was preemptied due to
                                                      its large storage requirement
              .1.. ....        SCLDDL_CALBASE          If on, this is the base
                                                      VMDBK. VMDBASE
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      40  28  Unsigned      4  SCLDDL_VMDWSSPR        This user's projected
                                                      working working set size.
                                                      This is the scheduler's
                                                      estimate of the amount of
                                                      storage this user will
                                                      require to be resident as it
                                                      runs during its next stay in
                                                      the dispatch list. It is
                                                      based upon the user's past
                                                      behavior and, in some cases,
                                                      on the behavior of similar
                                                      types of users.
      44  2C  Unsigned      4  SCLDDL_VMDPGRTE        Number of pages per second
                                                      which this user read in
                                                      during its last stay in the
                                                      dispatch list.
      48  30  Unsigned      4  SCLDDL_VMDRPLIM        Resident page growth limit
      52  34  Unsigned      4  SCLDDL_VMDCTPVR        Cardinal count of resident
                                                      pages in private address
                                                      spaces belonging to this
                                                      user. This monitor field is
                                                      actually the sum of VMDCTPVR
                                                      + VMDCTPVG which is the
                                                      resident pages above and
                                                      below the 2GB line. To get
                                                      the count of resident pages
                                                      below the 2GB line, subtract
                                                      SCLDDL_VMDCTPVG from
                                                      SCLDDL_VMDCTPVR.
      56  38  Character     8  SCLDDL_VMDVTIME        Total Raw Time that this
                                                      user was running, doing
                                                      productive work. It does not
                                                      include any time that CP
                                                      spends on behalf of that user
                                                      doing such things as
                                                      instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format. The
                                                      complement of SCLDDL_VMDVTIME
                                                      is the accumulated time in
                                                      TOD clock units.
      64  40  Character     8  SCLDDL_VMDTTIME        Total Raw Time which has
                                                      been expended on this VMDBK.
                                                      This includes time which the
                                                      VMDBK spent doing its own
                                                      work and also time which CP
                                                      spent doing work on behalf of
                                                      the VMDBK. It is in CPU timer
                                                      format. The complement of
                                                      SCLDDL_VMDTTIME is the
                                                      elapsed time in TOD clock
                                                      units.
      72  48  Character     8  SCLDDL_VMDDPRTY        The user's dispatch list
                                                      priority. This is based on
                                                      the user's SHARE, its time
                                                      spent in the eligible list
                                                      and SHARES of all other
                                                      dispatch list users. It is
                                                      then adjusted by such factors
                                                      as interactive bias, paging
                                                      bias and limits on how large
                                                      or small this priority is
                                                      allowed to be. It represents
                                                      the relative order in which
                                                      this user will be selected to
                                                      be dispatched.
      80  50  Character     8  SCLDDL_VMDOPRTY        The user's dispatch
                                                      priority before adjustment
                                                      for factors such as
                                                      interactive bias and paging
                                                      bias
      88  58  Unsigned      4  SCLDDL_VMDRTHRU        This user's 'required
                                                      throughput' or 'resource
                                                      access' in the dispatch list.
                                                      This is the amount of time
                                                      while the user is in the
                                                      dispatch list that it should
                                                      be offered access to system
                                                      resources, considering its
                                                      SHARE and the time it spent
                                                      in the eligible list.
      92  5C  Unsigned      4  *                      Reserved for IBM use - was
                                                      SCLDDL_VMDCTXBK
      96  60  Unsigned      4  *                      Reserved for IBM use - was
                                                      SCLDDL_VMDFLREO
     100  64  Unsigned      4  *                      Reserved for IBM use - was
                                                      SCLDDL_VMDCTORF
     104  68  Unsigned      4  SCLDDL_CALCPPST        Cumulative count of pages
                                                      reclaimed from this user's
                                                      addr spaces while they were
                                                      private.
     108  6C  Bitstring     1  SCLDDL_CALRSTAT        Reason(s) the dispatched
                                                      VMDBK is not being run
              1... ....        *
              .1.. ....        SCLDDL_VMDCFWT          VMDBK is in console
                                                      function wait. Either a
                                                      console function is active,
                                                      or the virtual machine is
                                                      waiting for the remaining
                                                      VMDBKs in the configuration
                                                      to enter console function
                                                      mode.
              ..1. ....        SCLDDL_VMDSIMWT         CP is simulating some
                                                      hardware function for the
                                                      guest such as instructions,
                                                      interrupts, and timer
                                                      updates. Virtual machine is
                                                      prevented from running to
                                                      avoid potential conflicts
                                                      with the simulations.
              ...1 ....        SCLDDL_VMDIOWT          Instruction waiting for
                                                      I/O status for completion.
                                                      (May be cancelled without
                                                      loss of system integrity.)
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     109  6D  Bitstring     1  SCLDDL_VMDSTATE        Scheduler/Dispatcher State.
                                                      X'63' = Review-suspended.
                                                      VMDBK is in transition to the
                                                      suspended state. X'58' =
                                                      Review-idle. VMDBK is in
                                                      transition to the idle state.
                                                      X'4D' = VMDBK has been
                                                      selected by dispatcher for
                                                      processing. X'42' = VMDBK is
                                                      ready for selection by
                                                      dispatcher once it goes to
                                                      the dispatch list. X'37' =
                                                      Test-idle. VMDBK is ready for
                                                      selection by the dispatcher
                                                      but should be dropped from
                                                      the dispatch list when
                                                      selected the next time. X'2C'
                                                      = VMDBK is suspended,
                                                      probably waiting for a
                                                      short-term event to occur.
                                                      X'00' = VMDBK is idle. No
                                                      work is available.
     110  6E  Bitstring     1  SCLDDL_CALOSTAT        Virtual machine operating
                                                      status
              1... ....        SCLDDL_VMDSYSOP         User is primary system
                                                      operator
              .1.. ....        SCLDDL_VMDUSRCT         User is counted as being
                                                      logged on
              ..1. ....        *
              ...1 ....        SCLDDL_VMDFORCE         User is to be logged off.
                                                      This may be requested by CP,
                                                      a forced logoff, or user's
                                                      logoff command.
              .... 1...        SCLDDL_VMDUFORC         User is forced to logoff
                                                      the system
              .... .1..        SCLDDL_VMDDISC          User is running
                                                      disconnected
              .... ..1.        SCLDDL_VMDAUTOL         AUTOLOG/XAUTOLOG in
                                                      progress. User has been
                                                      automatically logged on. This
                                                      bit is set off when the
                                                      user's IPL statement is
                                                      processed, or (if there is no
                                                      IPL to process) when the user
                                                      enters a LOGON command from a
                                                      terminal to RECONNECT.
              .... ...1        SCLDDL_VMDXAUTO         The original command was
                                                      XAUTOLOG. Valid for the base
                                                      VMDBK only.
     111  6F  Bitstring     1  SCLDDL_VMDSACTL        Dispatch list control bits.
                                                      These are used to signal the
                                                      dispatcher that the currently
                                                      dispatched user requires
                                                      scheduler intervention,
                                                      either due to having reached
                                                      a resource consumption limit
                                                      or some other reason. At
                                                      dispatch list drop time,
                                                      these bits can indicate why
                                                      the user was dropped.
     112  70  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SCLDDL_VMDCWSS)
     116  74  Unsigned      1  SCLDDL_VMDSACTX        An extension byte to
                                                      VMDSACTL. It describes
                                                      additional reasons why the
                                                      user required scheduler
                                                      intervention, given that the
                                                      'other resources' bit is on
                                                      in VMDSACTL.
     117  75  Bitstring     1  SCLDDL_CALQSTAT        Scheduling status of user
              1... ....        SCLDDL_VMDHOTRQ         Hot Shot scheduling
                                                      requested
              .1.. ....        SCLDDL_VMDHOTST         Hot Shot user scheduling
                                                      granted
              ..1. ....        SCLDDL_VMDLOADU         Loading user designation
              ...1 ....        SCLDDL_VMDIABIA         Interactive bias is in
                                                      effect
              .... 1...        *
              .... .1..        SCLDDL_VMDLKSHT         "Lockshot" scheduling in
                                                      effect for this user. Set
                                                      only in the base VMDBK.
              .... ..1.        *
              .... ...1        SCLDDL_VMDNULL          User is logging off
     118  76  Unsigned      2  SCLDDL_VMDCPUAD        Virtual processor address
     120  78  Unsigned      4  SCLDDL_VMDCTCRT        Count of CP
                                                      critical-processes this VMDBK
                                                      is responsible for. VMDBK
                                                      must not wait in eligible
                                                      list while this count is
                                                      greater than 0. Valid only in
                                                      base VMDBK.
     124  7C  Unsigned      4  SCLDDL_VMDRELSH        This virtual CPU's RELATIVE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Set to zero when this VMDBK
                                                      has an ABSOLUTE share value,
                                                      or has a virtual processor
                                                      dedicated to it, or is in the
                                                      process of being logged off.
     128  80  Unsigned      4  SCLDDL_VMDABSSH        This virtual CPU's ABSOLUTE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Unit of value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Set to zero when this VMDBK
                                                      has a RELATIVE share value.
     132  84  Bitstring     1  SCLDDL_CALSHARF        Set Share flags
              1... ....        SCLDDL_VMDMXSHA         Max share is Absolute if
                                                      ON. Max share is Relative if
                                                      OFF.
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        SCLDDL_VMDLIMTH         Max share is Limithard if
                                                      ON. Max share is Limitsoft if
                                                      OFF.
              .... ...1        *
     133  85  Unsigned      1  *                      Reserved and available for
                                                      IBM use.
     134  86  Signed        2  SCLDDL_VMDSLCNT        Count of minor time slices
                                                      that have expired since the
                                                      start of current transaction.
     136  88  Unsigned      4  SCLDDL_VMDMXSHR        The virtual CPU's Max share
                                                      of the system, as set in the
                                                      user's directory or via the
                                                      SET SHARE command. This value
                                                      is set to zero if no Max
                                                      share exists. If the Max
                                                      share is Absolute, then the
                                                      unit of the value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Check SCLDDL_VMDMXSHA to
                                                      determine if Max share is
                                                      absolute or relative.
     140  8C  Character     8  SCLDDL_SRMATOD         Artificial TOD. This TOD
                                                      only advances at the rate the
                                                      system is running user work.
                                                      Applies to real primary
                                                      processor on which user is
                                                      dispatched.
     148  94  Character     8  SCLDDL_SRMATOD2        Artificial TOD2. This TOD
                                                      only advances with each CPU's
                                                      user time and each CPU's wait
                                                      time. Applies to real primary
                                                      processor on which user is
                                                      dispatched.
     156  9C  Unsigned      4  SCLDDL_VMDCTPVG        Count of private address
                                                      space resident pages in DPA
                                                      owned by this virtual machine
                                                      which are above the 2GB line.
                                                      Valid only in base VMDBK. To
                                                      get total resident pages
                                                      under the 2GB line, subtract
                                                      this field from
                                                      SCLDDL_VMDCTPVR.
     160  A0  Bitstring     1  SCLDDL_VMDCFGEM        Virtual configuration
                                                      indicators. Valid in base
                                                      VMDBK only
              1... ....        *
              .1.. ....        SCLDDL_VMDCPUAF         User requested CPU
                                                      Affinity
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     161  A1  Bitstring     1  SCLDDL_VMDPUST         CPU Status flag
              1... ....        SCLDDL_VMDAFSUP         CPU Affinity suppressed
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     162  A2  Character     2  *                      Reserved for IBM use
     164  A4  Character     8  SCLDDL_VMDVTMP         Total raw virtual time for
                                                      the user on primary
                                                      processor.
     172  AC  Character     8  SCLDDL_VMDTTMP         Total raw virtual and
                                                      simulation time for the user
                                                      on primary processor.
     180  B4  Character     8  SCLDDL_VMDVTMS         Total raw virtual time for
                                                      the user on secondary
                                                      processor.
     188  BC  Character     8  SCLDDL_VMDTTMS         Total raw virtual and
                                                      simulation time for the user
                                                      on secondary processor.
     196  C4  Character     8  SCLDDL_VMDTTIME_MT1    Total MT-1 Equivalent time
                                                      which has been expended on
                                                      this VMDBK. This includes
                                                      time which the VMDBK spent
                                                      doing its own work and also
                                                      time which CP spent doing
                                                      work on behalf of the VMDBK.
                                                      It is in CPU timer format.
     204  CC  Character     8  SCLDDL_VMDVTIME_MT1    Total MT-1 Equivalent time
                                                      that this user was running
                                                      and doing productive work. It
                                                      does NOT include any time
                                                      that CP spends on behalf of
                                                      that user doing such things
                                                      as instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format.
     212  D4  Character     8  SCLDDL_VMDVTMP_MT1     MT-1 Equivalent virtual
                                                      time for the user on primary
                                                      processor
     220  DC  Character     8  SCLDDL_VMDTTMP_MT1     MT-1 Equivalent total
                                                      virtual and simulation time
                                                      for the user on primary
                                                      processor.
     228  E4  Character     8  SCLDDL_VMDVTMS_MT1     MT-1 Equivalent total
                                                      virtual time for the user on
                                                      secondary processor.
     236  EC  Character     8  SCLDDL_VMDTTMS_MT1     MT-1 Equivalent total
                                                      virtual and simulation time
                                                      for the user on secondary
                                                      processor.
     244  F4  Character     8  SCLDDL_VMATTIME_PRO    Total Prorated Core Time
                                                      which has been expended on
                                                      this VMDBK. This includes
                                                      time which the VMDBK spent
                                                      doing its own work and also
                                                      time which CP spent doing
                                                      work on behalf of the VMDBK.
                                                      It is in CPU timer format.
                                                      See the notes above.
     252  FC  Character     8  SCLDDL_VMAVTIME_PRO    Total Prorated Core Time
                                                      that this user was running
                                                      and doing productive work. It
                                                      does NOT include any time
                                                      that CP spends on behalf of
                                                      that user doing such things
                                                      as instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format. See the
                                                      notes above.
     260 104  Character     8  SCLDDL_VMAVTMP_PRO     Total Prorated Core virtual
                                                      time for user on primary
                                                      processor. See the notes
                                                      above.
     268 10C  Character     8  SCLDDL_VMATTMP_PRO     Total Prorated Core virtual
                                                      and simulation time for the
                                                      user on primary processor.
                                                      See the notes above.
     276 114  Character     8  SCLDDL_VMAVTMS_PRO     Total Prorated Core virtual
                                                      time for user on secondary
                                                      processor. See the notes
                                                      above.
     284 11C  Character     8  SCLDDL_VMATTMS_PRO     Total Prorated Core virtual
                                                      and simulation time for the
                                                      user on secondary processor.
                                                      See the notes above.
     292 124  Unsigned      4  *                      Reserved for IBM use
     296 128  Bitstring     1  SCLDDL_PROBITS         Prorated Core Time bits
                                                      needed to understand those
                                                      fields.
              1... ....        SCLDDL_VMAPRCAL         Indicates whether the
                                                      Prorated Core Time values in
                                                      this record are valid (only
                                                      use if valid): 0 = values not
                                                      valid 1 = values are valid
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     297 129  Bitstring     1  *                      Reserved for IBM use
     298 12A  Unsigned      2  *                      Reserved for IBM use
     300 12C  Character     0  SCLDDL_END

#### MRSCLDDL Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SCLDDL                     0    300
    SCLDDL_CALBASE            27           40
    SCLDDL_CALCPPST           68      4
    SCLDDL_CALFLAG1           27      1
    SCLDDL_CALOSTAT           6E      1
    SCLDDL_CALQSTAT           75      1
    SCLDDL_CALRSTAT           6C      1
    SCLDDL_CALSHARF           84      1
    SCLDDL_END               12C      0
    SCLDDL_MRHDR               0      0
    SCLDDL_PROBITS           128      1
    SCLDDL_SRMATOD            8C      8
    SCLDDL_SRMATOD2           94      8
    SCLDDL_VMAPRCAL          128           80
    SCLDDL_VMATTIME_PRO       F4      8
    SCLDDL_VMATTMP_PRO       10C      8
    SCLDDL_VMATTMS_PRO       11C      8
    SCLDDL_VMAVTIME_PRO       FC      8
    SCLDDL_VMAVTMP_PRO       104      8
    SCLDDL_VMAVTMS_PRO       114      8
    SCLDDL_VMDABSSH           80      4
    SCLDDL_VMDAFSUP           A1           80
    SCLDDL_VMDAUTOL           6E           02
    SCLDDL_VMDCFGEM           A0      1
    SCLDDL_VMDCFWT            6C           40
    SCLDDL_VMDCPUAD           76      2
    SCLDDL_VMDCPUAF           A0           40
    SCLDDL_VMDCTCRT           78      4
    SCLDDL_VMDCTPVG           9C      4
    SCLDDL_VMDCTPVR           34      4
    SCLDDL_VMDDISC            6E           04
    SCLDDL_VMDDPRTY           48      8
    SCLDDL_VMDFORCE           6E           10
    SCLDDL_VMDHOTRQ           75           80
    SCLDDL_VMDHOTST           75           40
    SCLDDL_VMDIABIA           75           10
    SCLDDL_VMDIOWT            6C           10
    SCLDDL_VMDLIMTH           84           02
    SCLDDL_VMDLKSHT           75           04
    SCLDDL_VMDLOADU           75           20
    SCLDDL_VMDLRGST           27           80
    SCLDDL_VMDMXSHA           84           80
    SCLDDL_VMDMXSHR           88      4
    SCLDDL_VMDNULL            75           01
    SCLDDL_VMDOPRTY           50      8
    SCLDDL_VMDPGRTE           2C      4
    SCLDDL_VMDPUST            A1      1
    SCLDDL_VMDRDYCM           26      0
    SCLDDL_VMDRELSH           7C      4
    SCLDDL_VMDRPLIM           30      4
    SCLDDL_VMDRTHRU           58      4
    SCLDDL_VMDSACTL           6F      1
    SCLDDL_VMDSACTX           74      1
    SCLDDL_VMDSIMWT           6C           20
    SCLDDL_VMDSLCNT           86      2
    SCLDDL_VMDSTATE           6D      1
    SCLDDL_VMDSVMID           1C      8
    SCLDDL_VMDSVMWF           24           80
    SCLDDL_VMDSVMWF           25           80
    SCLDDL_VMDSVMWF           26           80
    SCLDDL_VMDSVMWT           24      1
    SCLDDL_VMDSVMWT           25      1
    SCLDDL_VMDSVMWT           26      1
    SCLDDL_VMDSVMW2           25      0
    SCLDDL_VMDSYSOP           6E           80
    SCLDDL_VMDTTIME           40      8
    SCLDDL_VMDTTIME_MT1       C4      8
    SCLDDL_VMDTTMP            AC      8
    SCLDDL_VMDTTMP_MT1        DC      8
    SCLDDL_VMDTTMS            BC      8
    SCLDDL_VMDTTMS_MT1        EC      8
    SCLDDL_VMDUFORC           6E           08
    SCLDDL_VMDUSER            14      8
    SCLDDL_VMDUSRCT           6E           40
    SCLDDL_VMDVTIME           38      8
    SCLDDL_VMDVTIME_MT1       CC      8
    SCLDDL_VMDVTMP            A4      8
    SCLDDL_VMDVTMP_MT1        D4      8
    SCLDDL_VMDVTMS            B4      8
    SCLDDL_VMDVTMS_MT1        E4      8
    SCLDDL_VMDWSSPR           28      4
    SCLDDL_VMDXAUTO           6E           01

    This information is
    based on z/VM V7R2.0.

    Last updated on 08 August 2020 at 16:09:51.

    Copyright IBM Corporation, 1990, 2020