###
Performance Toolkit for VM Data Areas
for z/VM V7R2.0

Programming Interface Information: This page documents intended Programming Interfaces that allow the customer to write programs to obtain the services of z/VM.

#### SEGTSYS

APAR VM66285

Prolog

Control Block Contents
SEGTSYS DSECT
SEGTSYS2 DSECT
SEGTLPAR DSECT
SEGTRDEV DSECT
SEGTCPDV DSECT
SEGTWKLD DSECT
SEGTNHIP DSECT
SEGTVSWI DSECT
SEGTNSRV DSECT
SEGTNUSR DSECT
SEGTAPPL DSECT
SEGTPRC DSECT
SEGTMDC DSECT
SEGTCHN DSECT
SEGTLCHN DSECT
SEGTFCHN DSECT
SEGTDCAC DSECT
SEGTCTLU DSECT
SEGTVDSK DSECT
SEGTSPLK DSECT
SEGTWAIT DSECT
SEGTCPC DSECT
SEGTSSI DSECT
SEGTSCSI DSECT
SEGTLGR DSECT
SEGTCPUP DSECT
SEGTADAP DSECT
SEGTASEG DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### SEGTSYS Prolog

     NAME       : FCXOMY
     DESCRIPTION: SEGOUT DCSS Content Data Definition
     DSECT      : SEGTSYS

#### SEGTSYS Control Block Content

#### SEGTSYS DSECT - System Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTSYS        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 ACTUSER        Number of users who had any
                                            activity since the last sampling
                                            interval.
    0004    4 Signed       4 AVGUSER        Average number of users logged
                                            on.
    0008    8 Dbl-Word     8 AVLFRAMS       The number of frames currently on
                                            the available list below the 2GB
                                            line.
    0010   16 Dbl-Word     8 AVLFRA2G       The number of frames currently on
                                            the available list above the 2GB
                                            line.
    0018   24 Dbl-Word     8 AVLHGHTH       The high threshold for the
                                            available list replenishment
                                            subsystem below 2GB line.
                                            (No longer available in
                                            z/VM 6.3)
    0020   32 Dbl-Word     8 AVLHGH2G       The high threshold for the
                                            available list replenishment
                                            subsystem above 2GB line.
    0028   40 Dbl-Word     8 AVLLMEAN       The average number of page frames
                                            on the available list below the
                                            2GB line. (Mean Avail List from
                                            Paging Log Screen)
    0030   48 Dbl-Word     8 AVLLME2G       The average number of page frames
                                            on the available list above the
                                            2GB line. (Mean Avail List from
                                            Paging Log Screen)
    0038   56 Dbl-Word     8 AVLLOWTH       The low threshold for the
                                            available list replenishment
                                            subsystem below 2GB.
                                            (No longer available in
                                            z/VM 6.3)
    0040   64 Dbl-Word     8 AVLLOW2G       The low threshold for the
                                            available list replenishment
                                            subsystem above 2GB.
    0048   72 Signed       4 AVLWAIT        The number of tasks that cannot
                                            be executed because they are
                                            waiting for a frame.
    004C   76 Signed       4 CPBUSY         Percentage of CPU utilized by CP.
                                            (General CPU screen, %CP
                                            aggregated across processors.)
    0050   80 Signed       4 CPUBUSY        Total CPU utilization (CP and
                                            virtual combined) If you are
                                            running multiple processors, this
                                            value is the sum of CPU
                                            utilization for all processors
                                            and can be > 100% (General CPU
                                            screen, %CPU aggregated across
                                            processors)
    0054   84 Signed       4 CPUNUM         Number of active processors.
                                            (General CPU screen PROC
                                            attribute, reported as a total of
                                            processors instead of by
                                            processor.)
    0058   88 Signed       4 DEVIOSCS       This number represents the
                                            system-wide I/O paging rate.
                                            Related statistics appear
                                            elsewhere by DASD volume.
                                            (General Storage Utilization,
                                            page read and page write rates.
                                            Could also come from Paging Log
                                            data screen, which is considered
                                            historical information.)
    005C   92 Signed       4 DIALUSER       Number of users who are dialed to
                                            VM. (General CPU screen, # of
                                            dialled users.)
    0060   96 Dbl-Word     8 DPAFRAMS       The number of frames allocated to
                                            the dynamic paging area.
    0068  104 Dbl-Word     8 DSCNFAIL       The number of times the demand
                                            scan was invoked and could not
                                            replenish the available list to
                                            its threshold. (No longer
                                            available in z/VM 6.3)
    0070  112 Dbl-Word     8 ELIGUSER       Average number of users waiting
                                            in the eligible list. (General
                                            CPU screen, Eligible VMDBKs)
    0078  120 Dbl-Word     8 EXPUSER1       The number of short running users
                                            in the eligible list for the E1
                                            queue.
    0080  128 Dbl-Word     8 EXPUSER2       The number of medium-running
                                            users in the eligible list for
                                            the E2 queue.
    0088  136 Dbl-Word     8 EXPUSER3       The number of long-running users
                                            in the eligible list for the E3
                                            queue.
    0090  144 Dbl-Word     8 EXTFRAMS       The number of frames used by
                                            free-storage management.
    0098  152 Dbl-Word     8 EXTWAIT        The number of deferred pages
                                            waiting for a frame
    00A0  160 Dbl-Word     8 FSTRREQS       The total number of free-storage
                                            requests during the reporting
                                            interval.
    00A8  168 Dbl-Word     8 FSTRRETS       The total number of free-storage
                                            releases during the reporting
                                            interval.
    00B0  176 Dbl-Word     8 LPARBSYS       Percentage of time this LPAR was
                                            busy based on the number of
                                            available logical processors.
    00B8  184 Dbl-Word     8 NTRVRATE       This number represents the
                                            average number of non-trivial
                                            transactions processed per second
                                            during the reporting interval.
    00C0  192 Dbl-Word     8 PAGERATE       The number of pages per second
                                            being read in by the system.
    00C8  200 Signed       4 PAGINDEX       The system resource weight for
                                            paging. Used by the scheduler to
                                            decide how much of a bottleneck
                                            the paging resources are.
    00CC  204 Signed       4 PCTPAGE        This number represents the
                                            average system-wide percent of
                                            paging space in use. Related
                                            statistics appear elsewhere by
                                            DASD volume.
    00D0  208 Signed       4 PCTSPOL        Represents the percent of SPOOL
                                            space in use for the entire
                                            system.
    00D4  212 Signed       4 PCTTDSK        Represents the percent of
                                            temporary disk space in use for
                                            the entire system.
    00D8  216 Signed       4 RESELWAT       Percentage of 'in-queue' users
                                            found in an 'eligible list', i.e.
                                            waiting for a constrained
                                            resource, during the measuring
                                            interval. (% elig. (resource
                                            wait).)
    00E0  224 Dbl-Word     8 SINGFLTS       The average number of page faults
                                            per second for single-page reads
                                            during the reporting interval.
    00E8  232 Dbl-Word     8 SYSDPAP        This statistic represents the
                                            percentage of real storage
                                            available to the Dynamic Paging
                                            Area (Can be derived from General
                                            Storage Utilization screen. Total
                                            DPA size.)
    00F0  240 Dbl-Word     8 SYSITR         System Internal Throughput Rate
                                            (ITR) The number of transactions
                                            executed on the system per second
                                            of total CPU time
    00F8  248 Dbl-Word     8 TRVRATE        This number represents the total
                                            number of trivial transactions
                                            processed during the reporting
                                            interval.
    0100  256 Dbl-Word     8 TVRATIO        Ratio of total CPU time to
                                            virtual CPU time. (User resource
                                            screen, T/V ratio for user
                                            system.)
    0108  264 Signed       4 USERQ          Average number of users in queue
                                            waiting to be dispatched.
                                            (General CPU screen, # of in
                                            queue users.)
    010C  268 Signed       4 WAITIOP        This statistic represents the
                                            percent of all virtual machines
                                            in an I/O wait state.
    0110  272 Signed       4 WAITPAGP       This statistic represents the
                                            percent of all virtual machines
                                            in a page wait state.
    0118  280 Dbl-Word     8 TOTSTOR        Total main storage size. Note
                                            that this is the real storage size,
                                            including HSA (Hardware Storage
                                            Area) frames and that less
                                            storage may actually be used by
                                            your system if less storage has
                                            been defined during system
                                            generation.
    0120  288 Dbl-Word     8 OFFSTORF       Total main storage that is
                                            offline.
    0128  296 Dbl-Word     8 SYSSTORF       Storage size defined for the
                                            VM system.
    0130  304 Dbl-Word     8 SHARSTOR       The amount of main storage
                                            currently used by shared segments.
    0138  312 Dbl-Word     8 FSTORSUB       Storage taken up by subpools.
    0140  320 Signed       4 SSTORUTL       The percentage of subpool free
                                            storage which is currently in use.
    0148  328 Dbl-Word     8 LOCKPAGS       The amount of DPA storage which
                                            consists of pages which have been
                                            locked (includes CP FREE storage
                                            space).
    0150  336 Dbl-Word     8 TRTABSZ        Storage occupied by CP trace
                                            tables.
    0158  344 Dbl-Word     8 PAGSTOR        The size of the pageable part
                                            of the DPA (that is, total DPA size
                                            minus locked pages, minus trace
                                            table).
    0160  352 Signed       4 STORUTIL       The percentage of pageable
                                            storage which is used up by the
                                            working sets of currently active
                                            users. Due to rounding can be
                                            slightly above 100 percent.
    0164  356 Signed       4 TSKWFRCT       The number of CP tasks which
                                            are waiting for a page frame.
    0168  360 Signed       4 TSKWPGRT       The number of CP tasks which
                                            were found to be waiting for a
                                            page, per second.
    0170  368 Dbl-Word     8 STBYSTOR       Real machine standby storage
                                            size. Standby storage is a
                                            calculated value based on the
                                            amount of installed storage that
                                            is not currently claimed by active
                                            logical partitions and the
                                            RESERVED storage specified for
                                            this partition.
    0178  376 Dbl-Word     8 RESVSTOR       Real machine reserved storage
                                            size.
    0180  384 Dbl-Word     8 TOTXSTAV       Total size of expanded storage.
                                            (DCSS in bytes)
    0188  392 Dbl-Word     8 TOTXSTUS       Size dedicated to specific
                                            virtual machines. (DCSS in bytes)
    0190  400 Dbl-Word     8 TOTXSTCP       Expanded storage size
                                            allocated for CP use.
    0198  408 Signed       4 CPXSTORE       Percentage of CP partition
                                            currently in use.
    01A0  416 Dbl-Word     8 XSTMIGLW       The minimum XSTORE size which
                                            is to be kept free for
                                            allocation of new blocks. Used
                                            XSTORE blocks will be migrated
                                            to DASD if less free XSTORE
                                            space is available. (DCSS in
                                            bytes)
    01A8  424 Dbl-Word     8 XSTALLOC       The rate at which XSTORE pages
                                            were allocated.
    01B0  432 Dbl-Word     8 XSTBLKAG       The average age of XSTORE pages
                                            in the CP partition.
    01B8  440 Dbl-Word     8 XSTBLKMG       The average age of XSTORE pages
                                            at migration. If the average age
                                            at migration is low and near to
                                            the average age of all XSTORE
                                            blocks in storage, the size of
                                            the CP partition is probably too
                                            small.
              000001C0       SYSDLEN        *-SEGTSYS

#### SEGTSYS2 DSECT - System Data 2

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTSYS2       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Dbl-Word     8 VDSKSYSL       The system limit set for maximum
                                            storage utilization by virtual disks
                                            in blocks.
    0008    8 Dbl-Word     8 VDSKUSRL       The maximum number of VDISK
                                            blocks that can be defined per user.
    0010   16 Dbl-Word     8 VDSKMSF        The number of main storage page
                                            frames used by virtual disks.
    0018   24 Dbl-Word     8 VDSKXSF        The number of expanded storage
                                            blocks used by virtual disks.
    0020   32 Dbl-Word     8 VDSKMPG        The number of virtual disk
                                            pages that have been migrated
                                            to DASD.
    0028   40 Dbl-Word     8 PGMVBL2G       The rate at which pages were
                                            moved below the 2GB line for
                                            translation. The field is
                                            available only for VM systems
                                            running in 64-bit mode.
    0030   48 Dbl-Word     8 FSTPGIRT       The rate at which pages were
                                            paged in using fast path logic.
    0038   56 Dbl-Word     8 LNGPGIRT       The rate at which pages were
                                            paged in using long path logic.
    0040   64 Dbl-Word     8 LNGPGORT       The rate at which pages were
                                            paged out using long path logic.
    0048   72 Dbl-Word     8 PAGEWRRT       The number of pages per
                                            second being written by the system.
    0050   80 Signed       4 PGRDBLKF       Average blocking factor for
                                            page read operations, that is,
                                            average number of pages read with
                                            a single read operation. Both the
                                            page read and page write blocking
                                            factors are indicators of the
                                            efficiency  of block paging (the
                                            higher the number, the greater the
                                            efficiency). Due to the page-in
                                            logic employed, the page read
                                            blocking factor will usually turn
                                            out to be about half the page write
                                            blocking factor.
    0054   84 Signed       4 PGWRBLKF       Average blocking factor for
                                            page write operations.
    0058   88 Signed       4 MIGOBLKF       Average blocking factor for
                                            migrating pages out from XSTORE
                                            to DASD. Both the page read and
                                            page write blocking factors  are
                                            indicators of the efficiency of
                                            block paging (the higher the
                                            number, the greater the efficiency).
                                            Due to the page-in logic employed,
                                            the page read blocking factor will
                                            usually turn out to be about half
                                            the page write blocking factor.
    0060   96 Dbl-Word     8 PAGSSCH        Number of I/O operations per
                                            second for moving pages between
                                            main storage and paging devices.
                                            This number will, due to the
                                            block paging logic, will usually
                                            be considerably lower than the
                                            number of pages transferred.
    0068  104 Dbl-Word     8 SPRDRATE       The rate at which pages were
                                            read from SPOOL devices.
    0070  112 Dbl-Word     8 SPWRRATE       The rate at which pages were
                                            written out to SPOOL devices.
    0078  120 Dbl-Word     8 TOTREAL        Total main storage size,
                                            including any offline frames.
    0080  128 Dbl-Word     8 STRAGESZ       Target amount of storage in
                                            the age list.
    0088  136 Dbl-Word     8 STRAGINC       Current amount of storage in
                                            the age list.
    0090  144 Dbl-Word     8 STRRSVPG       Total amount of storage
                                            reserved via the SET RESERVED
                                            command.
    0098  152 Dbl-Word     8 STRRSDMX       The maximum amount of storage
                                            that can be reserved, in bytes,
                                            via the SET RESERVED command.
    00A0  160 Dbl-Word     8 SMCR2GDC       Count of deferred frame requests
                                            that are waiting for an available
                                            frame that can be located anywhere.
                                            This count plus requests waiting
                                            <2G plus requests waiting >2G
                                            is the total wait count.
    00A8  168 Dbl-Word     8 SMCRFRQW       Count of deferred frame requests
                                            that are waiting for an available
                                            frame that can be located only <2G.
                                            This count plus requests waiting
                                            anywhere plus requests waiting >2G
                                            is the total wait count.
    00B0  176 Dbl-Word     8 SMCRCT2G       Count of deferred frame requests
                                            that are waiting for an available
                                            frame that can be located only >2G.
                                            This count plus requests waiting
                                            anywhere plus requests waiting <2G
                                            is the total wait count.
    00B8  184 Dbl-Word     8 EMPSINGL       Count of times that the single
                                            frames available list for frames
                                            <2G was empty, per second.
    00C0  192 Dbl-Word     8 EMPCONTL       Count of times that the
                                            continguous frames available list
                                            for frames <2G was empty, per second.
    00C8  200 Dbl-Word     8 EMPSINGG       Count of times that the single
                                            frames available list for frames
                                            >2G was empty, per second.
    00D0  208 Dbl-Word     8 EMPCONTG       Count of times that the
                                            continguous frames available list
                                            for frames >2G was empty, per second.
              000000D8       SYS2DLEN       *-SEGTSYS2

#### SEGTLPAR DSECT - LPAR Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTLPAR       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 LPARNUM        Assigned logical partition
                                            number. (LPAR load screen,
                                            partition #.)
    0004    4 Character    8 LPARNAME       Assigned name of the logical
                                            partition. (LPAR load screen,
                                            partition name.)
    0010   16 Dbl-Word     8 LPARBUSY       Average percentage of time that
                                            logical processors were busy,
                                            defined as the percentage of
                                            elapsed time during which real
                                            processors were assigned to
                                            logical processors. Note that the
                                            value will also include wait time
                                            in the system that is running in
                                            the partition if 'wait completion'
                                            has been enabled for the
                                            processor.
    0018   24 Dbl-Word     8 LPARLOAD       Total amount of time that all of
                                            the logical processors for this
                                            LPAR were busy during the
                                            reporting interval.
    0020   32 Signed       4 LPARLPCT       Number of logical processors
                                            assigned to this LPAR. (LPAR load
                                            screen, #Proc.)
    0028   40 Dbl-Word     8 LPARMSPC       Percentage of elapsed time
                                            that the logical processor was
                                            'suspended', i.e. could not give
                                            service to the guest system due
                                            to LPAR management time and
                                            contention for real processors,
                                            where the 'suspended' time is
                                            calculated as the difference
                                            between elapsed time and the sum
                                            of processor busy time and
                                            voluntary wait time for the same
                                            processor as seen by the VM
                                            system that is active in the
                                            partition. (Deleted with APAR
                                            VM65697)
    0030   48 Dbl-Word     8 LPAROVER       Amount of logical CPU busy which
                                            was due to LP dispatching
                                            overhead.
    0038   56 Dbl-Word     8 LPAROVHD       Average percentage of elapsed
                                            time that the logical processors
                                            spent for LPAR mgmt. This
                                            information is available only on
                                            systems with the LPAR management
                                            time facility (LPAR load screen,
                                            %Ovhd.)
    0040   64 Signed       4 LPARSTAT       Status of the logical partition
                                            during the reporting interval.
                                            Can be enumerations 2=ACTIVE or
                                            1=INACTIVE or 0=inactive. The
                                            partition that was used to
                                            collect the LPAR data will have
                                            an asterisk (*) appended (for
                                            example, "ACTIVE*").
    0044   68 Signed       4 LPARWAIT       Status of the WAIT bit for the
                                            logical processors within this
                                            LPAR. If any LP has the WAIT bit
                                            ON, this field will contain
                                            enumerations 1="YES" or 0=NO.
                                            (LPAR load screen, Wait Char.)
    0048   72 Signed       4 LPARWGHT       Average weight of all logical
                                            processors defined for this LPAR.
                                            The weight values for dedicated
                                            processors will be 1000. (LPAR
                                            load screen, Weight.)
    0050   80 Dbl-Word     8 PHYSBUSY       This is the sum of the %Load
                                            values for all active logical paritions with
                                            normal processors plus the General LPAR
                                            management (if available), i.e. it gives you the
                                            overall load for normal processors in the
                                            processor complex and does not include the load
                                            of partitions with IFL or ICF processors.
    0058   88 Character    4 LPARUPID       The user partition ID number
                                            for the logical partition.
    005C   92 Signed       4 LPARCAP        Enumerated value reflecting the
                                            capping definition for the partition. It can be
                                            Yes (2) if capping has been set on for the partition
                                            indicating that CPU cycles are to be allocated only
                                            up to the specified maximum, or No (1) if capping
                                            is not active.
    0060   96 Dbl-Word     8 LPARLGLD       Logical processor load as seen
                                            by the guest VM system, based on processor busy
                                            time seen by the guest system and the sum of wait
                                            time and processor busy time perceived by the
                                            guest VM system. This is the logic used for the
                                            the calculation of the 'INDICATE LOAD' output.
                                            Note, however, that the resulting value depends
                                            not only on the actual activity of the guest
                                            system (the processor time used), but also on the
                                            activity of systems in other logical partitions of
                                            the same physical system. The 'suspended' time
                                            (see %Susp value) will increase if there is more
                                            contention for the real processors, thus causing
                                            less voluntary wait time. Less voluntary wait
                                            time in turn will result in a higher 'Logical
                                            processor load' being calculated, even if the
                                            actual CPU time used by the processor is the same.
                                            (Deleted with APAR VM65697)
    0068  104 Dbl-Word     8 LPARVMLD       Processor load as seen by the
                                            guest VM system, based on processor busy time
                                            seen by the guest system and elapsed time.
                                            (Deleted with APAR VM65697)
    0070  112 Signed       4 LPARPTYP       The CPU type of the logical
                                            processors defined for the partition, as follows:
                                            CP: Central Processor, ICF: Internal Coupling
                                            Facility Processor, IFL: Integrated Facility for
                                            Linux Processor, ZIIP: IBM System z9 Integrated
                                            Information Processor (zIIP), ZAAP: IBM z/Series
                                            Application Assist Processor (zAAP), Special:
                                            other.
    0074  120 Dbl-Word     8 LPARTCAP       The maximum amount of core
                                            power of this type the partition is permitted
                                            to use, where a value of 100 represents one
                                            whole physical core worth of power.
    007C  128 Signed       4 LPARMTDP       The multithreading depth for
                                            the specified logical core of this partition.
    0080  132 Character    8 LPARGCPN       The group capping name
                                            assigned to this partition.
    0088  140 Dbl-Word     8 LPARGCPV       The group capping value
                                            assigned to this partition.
              00000090       LPADLEN        *-SEGTLPAR

#### SEGTRDEV DSECT - Device Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTRDEV       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 DEVADDR        Real address of device. (CP Owned
                                            Device screen, Page or SPOOL
                                            device address.)
    0004    4 Character    8 DEVTYPE        Type of device (for example: 3370
                                            or 3380). (CP Owned Device
                                            screen, Device type.)
    0010   16 Dbl-Word     8 CONNTIME       Average time this device was in
                                            CONNECT state during the
                                            interval. (General I/O device
                                            screen: Pend, Disc, Conn.)
    0018   24 Signed       4 DASDBUSY       Percentage of time the device was
                                            found busy. (Detailed I/O device
                                            info., Device Busy.)
    0020   32 Dbl-Word     8 DASDQUE        Average number of I/Os queued on
                                            the device. (General I/O device
                                            screen, Req. Queued.)
    0028   40 Dbl-Word     8 DASIOREQ       Number of I/Os started on this
                                            device.
    0030   48 Dbl-Word     8 DEVIOSEC       I/Os per second to this device
                                            (I/O rate). (General I/O device
                                            screen: I/O Rate.)
    0038   56 Dbl-Word     8 DISCTIME       Average time this device was in
                                            DISCONNECT state during the
                                            reporting interval. (Genl I/O
                                            device screen: Pend, Disc, Conn.)
    0040   64 Dbl-Word     8 PENDTIME       Average time this device was in
                                            PENDING state during the
                                            reporting interval. (General I/O
                                            device screen: Pend, Disc, Conn.)
    0048   72 Dbl-Word     8 SERVTIME       Average service time for this
                                            device in milliseconds.
    0050   80 Character    8 VOLSER         Volume serial number if DASD
                                            device. (CP Owned Device screen,
                                            Device volume serial.)
              00000058       DEVDLEN        *-SEGTRDEV

#### SEGTCPDV DSECT - CP-Owned Device Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTCPDV       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 DEVADDRX       Real address of CP-owned DASD.
                                            (CP Owned Device screen, Page or
                                            SPOOL device address)
    0004    4 Signed       4 ALLOCCNT       The number of cylinders or blocks
                                            allocated for the CP-owned
                                            extent. (CP Owned Device screen,
                                            number of Page or SPOOL slots
                                            allocated, by volume.)
    0008    8 Signed       4 AVAILSLT       The number of slots available on
                                            the CP-Owned device at the time
                                            the sample was taken. (CP Owned
                                            Device screen, Page or SPOOL slot
                                            availability by volume.)
    000C   12 Signed       4 CPRESRV1       Reserved
    0010   16 Character    8 DEVTYPEX       Type of DASD (for example: 3370
                                            or 3380). (CP Owned Device
                                            screen, Device type.)
    0018   24 Signed       4 PAGETYPE       Type of PAGING (for example
                                            enumerations 0=PAGING,
                                            1=SPOOLING, 3=PREFERRED). (CP
                                            Owned Device screen, Paging
                                            type.)
    001C   28 Signed       4 ENDCYL         End extent allocated on CP-owned
                                            device (cylinder or block
                                            number). (CP Owned Volume screen,
                                            Extent Information.)
    0020   32 Signed       4 PERFULL        Percentage of space on the
                                            CP-Owned volume in use at the
                                            time the sample was taken. (CP
                                            Owned Volume screen, Used %.)
    0024   36 Signed       4 STARTCYL       The starting cylinder or block
                                            number for the CP-Owned device
                                            extent (cylinder or block
                                            number). (CP Owned Volume screen,
                                            Extent Information.)
    0028   40 Signed       4 TOTUSLOT       The number of used slots on the
                                            CP-Owned dev. at the time the
                                            sample was taken. (CP Owned
                                            Device screen, Page or SPOOL
                                            slots used by volume.)
    002C   44 Signed       4 CPRESRV2       Reserved
    0030   48 Character    8 VOLSERX        Volume serial number of CP-owned
                                            DASD. (CP Owned Device screen,
                                            Device volume serial.)
              00000038       CPODLEN        *-SEGTCPDV

#### SEGTWKLD DSECT - Workload Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTWKLD       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 WORKLOAD       Userid or group name.
    0008    8 Dbl-Word     8 CPPCT          Percent of total CPU used by the
                                            system to manage this workload.
                                            (User resource usage details
                                            screen, Superv. CPU.)
    0010   16 Dbl-Word     8 CPSECS         Total CP seconds used by this
                                            workload (to nearest second).
    0018   24 Dbl-Word     8 CPUPCT         Percent of total CPU utilized by
                                            this workload (User resource
                                            usage details screen, Total CPU.)
    0020   32 Dbl-Word     8 CPUSECS        Total CPU seconds used by this
                                            workload (to nearest second).
    0028   40 Dbl-Word     8 SESSTIME       Total time this workload was
                                            logged on (to nearest second), or
                                            aggregation of group.
    0030   48 Dbl-Word     8 VIRTPCT        Percent of virtual CPU
                                            utilization for the workload
                                            specified. (User resource usage
                                            details screen, Emulat. CPU.)
    0038   56 Dbl-Word     8 VIRTSECS       Total virtual CPU seconds used by
                                            this workload (to nearest
                                            second).
    0040   64 Dbl-Word     8 PAGERATW       The rate of page-ins and
                                            page-outs for this workload (in
                                            pages/sec.). (User resource usage
                                            screen, Page fault rate.)
    0048   72 Dbl-Word     8 PAGREADS       Number of page reads over the
                                            specified period of time. (User
                                            resource usage screen, Page Read
                                            rate.)
    0050   80 Dbl-Word     8 PAGWRTS        Number of page writes over the
                                            specified period of time. (User
                                            resource usage screen, Page write
                                            rate.)
    0058   88 Dbl-Word     8 RESPAGES       The current number of pages
                                            physically in main storage for
                                            this workload below 2GB
    0060   96 Dbl-Word     8 RESPAG2G       The current number of pages
                                            physically in main storage for
                                            this workload above 2GB
    0068  104 Dbl-Word     8 STORSIZE       Average storage size for this
                                            workload.
    0070  112 Dbl-Word     8 WKLXATT        The number of megabytes of
                                            expanded storage attached to this
                                            workload.
    0078  120 Dbl-Word     8 WKLXMOV        The number of expanded pages
                                            moved for this workload.
    0080  128 Dbl-Word     8 WKLXPAG        The number of expanded storage
                                            blocks allocated to this workload
                                            by CP for paging.
    0088  136 Dbl-Word     8 WSS            A user's projected working set
                                            size. This value is calculated
                                            each time a user drops from queue
                                            and is based on the number of
                                            pages referenced during the last
                                            stay in queue. (Projected Working
                                            set from User details.)
    0090  144 Character    8 GROUP          Name of group this workload
                                            belongs to. (Primarily used to
                                            determine which VMs are Linux
                                            guest hosts.)
    0098  152 Signed       4 WKVCPU         The number of virtual processors
                                            in the virtual machine.
    009C  156 Signed       4 WKRESV1        Reserved for alignment.
                                            configuration.
    00A0  160 Dbl-Word     8 WKLDDSOW       The number of non-base address
                                            spaces owned by the virtual machine.
    00A8  168 Dbl-Word     8 WKLDPGST       The rate at which pages were
                                            stolen from the virtual machine's
                                            address spaces while they were
                                            private.
    00B0  176 Dbl-Word     8 WKLDB2G        The rate at which page frames
                                            were moved below the 2GB line for
                                            translation.
    00B8  184 Dbl-Word     8 WKLDXRD        The rate at which page frames
                                            were moved from XSTORE to main
                                            storage.
    00C0  192 Dbl-Word     8 WKLDXWR        The rate at which page frames
                                            were migrated out from main storage
                                            to XSTORE.
    00C8  200 Dbl-Word     8 WKLDXMG        The rate at which page frames
                                            were migrated out from XSTORE to
                                            DASD.
    00D0  208 Dbl-Word     8 WKLDRVPG       The number of reserved pages
                                            for the user.
    00D8  216 Dbl-Word     8 WKLDPGLK       The number of pages locked in
                                            the user's private address spaces
                                            below the 2GB line.
    00E0  224 Dbl-Word     8 WKLDPGLG       The number of private pages
                                            that are locked above the 2GB line.
    00E8  232 Dbl-Word     8 WKLDDASD       The number of page slots used
                                            on system paging areas on DASD.
    00F0  240 Dbl-Word     8 WKLDSHR        Absolute share or relative
                                            share value for the user.
    00F8  248 Signed       4 WKLDSHRM       No limit-This is the default
                                            share setting. It allows z/VM to
                                            adjust the users share value
                                            according to system load with no
                                            restrictions. Maximum-This means that
                                            a maximum share value has been set
                                            for the user. The Share value shown
                                            is the actual value, not the maximum.
                                            Limit Hard-This means that the share
                                            value for the user can never exceed
                                            the maximum value. Absolute-This means
                                            that the user will receive a targetted
                                            minimum of the system resources.
                                            Dedicated-This means the user is
                                            running on a dedicated processor, and
                                            the share setting has no meaning.
    0100  256 Dbl-Word     8 WKLDTVRT       Ratio of total to virtual
                                            (emulation) CPU time used.
    0108  264 Dbl-Word     8 WKLDSIO        Total virtual I/O rate per
                                            second in the selected interval.
    0110  272 Dbl-Word     8 WKLDDAIO       Virtual I/O rate to disks.
    0118  280 Dbl-Word     8 WKLDAVIO       Rate of I/Os which were
                                            avoided because the requested
                                            blocks could be found in the
                                            minidisk cache.
    0120  288 Dbl-Word     8 WKLDDI98       Diagnose X'98' rate.
                                            Diagnose X'98' allows virtual
                                            machines to execute I/O
                                            very efficiently, bypassing
                                            normal CCW translation logic.
    0128  296 Dbl-Word     8 WKLDURIO       Rate of start requests to
                                            virtual UR devices.
    0130  304 Dbl-Word     8 WKLDACTV       Time, in minutes, that the
                                            user was found to have been
                                            active (the whole length of a
                                            sample interval will be counted as
                                            'active' time if the user
                                            consumed some virtual CPU time
                                            or executed any I/Os during the
                                            interval).
    0138  312 Dbl-Word     8 WKLDSPGS       The total number of pages
                                            spooled for the user.
    0140  320 Dbl-Word     8 WKLDSPGR       Spool read and write rate
                                            per second.
    0148  328 Dbl-Word     8 WKLDMDCI       The number of minidisk cache
                                            inserts per second. Note that
                                            for long monitor intervals this
                                            number may not be exact.
    0150  326 Dbl-Word     8 CPUPOOL
              00000158       WKLDLEN        *-SEGTWKLD

#### SEGTNHIP DSECT - Network Hipersocket Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTNHIP       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 CHANPATH       The Hex channel path identifier.
                                            (Hipersocket Channel Activity
                                            Screen.)
    0004    4 Signed       4 SHRD           Sharing indicator for the channel
                                            enumerations 1=YES - shared with
                                            other LPARs, 0=NO - Dedicated
                                            channel. (Hipersocket Channel
                                            Activity Screen.)
    0008    8 Dbl-Word     8 XFERTMSG       Number of messages sent per
                                            second for the whole system.
                                            (Hipersocket Channel Activity
                                            Screen.)
    0010   16 Dbl-Word     8 XFERTDUN       Number of data units sent per
                                            second for the whole system
                                            (Hipersocket Channel Activity
                                            Screen.)
    0018   24 Dbl-Word     8 FAILRBFS       Number of sends per second that
                                            failed due to no receiver buffer
                                            for the whole system.(Hipersocket
                                            Chan Activity Screen)
    0020   32 Dbl-Word     8 XFERMSGS       Number of messages sent per
                                            second for this partition.
                                            (Hipersocket Channel Activity
                                            Screen.)
    0028   40 Dbl-Word     8 XFERDUNI       Number of data units sent per
                                            second for this partition.
                                            (Hipersocket Channel Activity
                                            Screen.)
    0030   48 Dbl-Word     8 FAILRBFR       Number of sends per second that
                                            failed due to no receiver buffer
                                            for this partition. (Hipersocket
                                            Channel Activity Screen.)
    0038   56 Dbl-Word     8 FAILSOTH       Number of sends per second that
                                            failed due to other problems for
                                            this partition. (Hipersocket
                                            Channel Activity Screen.)
              00000040       HIPDLEN        *-SEGTNHIP

#### SEGTVSWI DSECT - Network Virtual Switch Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTVSWI       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 ADDR           Real Device Address. (Virtual
                                            Switch Activity Screen.)
    0004    4 Character    8 USERID         The user id of the virtual
                                            machine the device is currently
                                            attached to. (Virtual Switch
                                            Activity Screen.)
    000C   12 Signed       4 QSV            The queue storage value (Values 1
                                            - 8 ). (Virtual Switch Activity
                                            Screen.)
    0010   16 Signed       4 TIMEOUT        The timeout value for the virtual
                                            switch in seconds. (Virtual
                                            Switch Activity Screen.)
    0018   24 Dbl-Word     8 XMITBYTS       Number of bytes transmitted per
                                            second. (Virtual Switch Activity
                                            Screen.)
    0020   32 Dbl-Word     8 XMITPCKT       Number of packets transmitted per
                                            second. (Virtual Switch Activity
                                            Screen.)
    0028   40 Dbl-Word     8 XMITPCKD       Number of outbound packets
                                            discarded per second. (Virtual
                                            Switch Activity Screen.)
    0030   48 Dbl-Word     8 RCVBYTES       Number of bytes received per
                                            second. (Virtual Switch Activity
                                            Screen.)
    0038   56 Dbl-Word     8 RCVPCKTS       Number of packets received per
                                            second. (Virtual Switch Activity
                                            Screen.)
    0040   64 Dbl-Word     8 DISCPCKD       Number of inbound packets
                                            discarded per second. (Virtual
                                            Switch Activity Screen.)
    0048   72 Character    8 VLLID          The name of the Virtual
                                            Switch. A Virtual Switch is given a 16-byte
                                            identification, or LAN ID, when it is
                                            created. The VSWITCH LAN ID consists of two
                                            8-byte character fields: OWNER||NAME. The
                                            OWNER is always SYSTEM. This column is the
                                            NAME component of the LAN ID.
    0050   80 Dbl-Word     8 VSWRT          Number of write signals
                                            issued per second.
    0058   88 Dbl-Word     8 VSRED          Number of read signals
                                            issued per second.
    0060   96 Dbl-Word     8 VSSYN          Number of sync signals
                                            issued per second.
    0068  104 Dbl-Word     8 VSPCR          Number of interrupts, such
                                            as PCI and AI, received per second.
    0070  112 Dbl-Word     8 VSPCI          Number of interrupts, such
                                            as PCI and AI, that resulted in
                                            input queue processing per
                                            second.
    0078  120 Character    8 VSGVGRP        Name of the link aggregation
                                            port group in use for this VSWITCH.
    0080  128 Character   17 VSGVMAC        The LAN management MAC address.
    0091  145 Character   45 VSGVIPA        The LAN management IP address.
                                            This address is used by clients
                                            involved in switch management.
                                            For example, a Network Management
                                            System can request Bridge MIB
                                            information from an SNMP agent
                                            using this address. If an SNMP
                                            agent has not been assigned, the
                                            IP address field will contain
                                            blanks.
    00BE  190 Character    8 VSGVMGI        The LAN management IP userid.
                                            This is the userid of the z/VM
                                            TCP/IP stack that has assigned
                                            an SNMP agent to the virtual
                                            switch in its HOME statement. If
                                            an SNMP agent has not been
                                            assigned, the userid field will
                                            contain blanks.
    00C8  200 Signed       4 VSGVLAY        The session layer, 2 or 3.
    00D0  208 Dbl-Word     8 VSEVLIN        The load balancing interval.
                                            This is the number of seconds
                                            between load balancing operations.
    00D8  216 Dbl-Word     8 VSEVREQ        Number of lock requests made
                                            for the network lock, per
                                            second.
    00E0  224 Dbl-Word     8 VSEVLDE        Number of times per second
                                            that CP waited for the
                                            network lock.
    00E8  232 Dbl-Word     8 VSEVTXD        Number of times per second
                                            that CP waited for any lock
                                            when sending data on this
                                            VSWITCH port.
    00F0  240 Dbl-Word     8 VSEVRXD        Number of times per second
                                            that CP waited for any lock
                                            when receiving data on this
                                            VSWITCH port.
    00F8  248 Dbl-Word     8 VSEVMTX        Number of marker PDUs sent
                                            to this port. This is the total
                                            value for the monitor interval
    0100  256 Dbl-Word     8 VSEVMRX        Number of marker responses
                                            received. This is the total value
                                            for the monitor interval.
    0108  264 Dbl-Word     8 VSEVMKR        Number of marker response
                                            PDUs sent to this port in response
                                            to receiving a marker PDU from the
                                            partner port. This is the total for
                                            the monitor interval.
    0110  272 Dbl-Word     8 VSEVMTO        Number of times timed out
                                            waiting for a marker response PDU
                                            for a marker request sent by CP
                                            to a partner port. This is the total
                                            for the monitor interval.
    0118  280 Dbl-Word     8 VSEVLAX        Number of LACP PDUs sent
                                            on this port. This is the total
                                            value for the monitor interval.
    0120  288 Dbl-Word     8 VSEVLAR        Number of LACP PDUs
                                            received on this port. This is
                                            total value for the monitor
                                            interval.
    0128  296 Dbl-Word     8 VSEVIBF        Number of input
                                            buffers processed per second.
    0130  304 Dbl-Word     8 VSEVIQO        Number of input
                                            queue overflows per second.
    0138  312 Dbl-Word     8 VSEVOBF        Number of output
                                            buffers processed per second.
    0140  320 Dbl-Word     8 VSEVOQO        Number of output
                                            queue overflows per second.
    0148  328 Character    8 VSEVLVL        OSA device microcode level.
    0150  336 Character    4 VSGVOPN        The OSA port number specified
                                            on the RDEV parameter of the DEFINE
                                            VSWITCH command.
    0154  340 Signed       4 VSGVISO        Determines if guests on the
                                            virtual switch can communicate
                                            between themselves and other hosts
                                            and/or LPARs that share the same
                                            OSA-Express port with the virtual
                                            switch. Valid values are: ON
                                            prohibits guest from sending traffic
                                            to other guests on the same virtual
                                            switch by discarding traffic that is
                                            destined for another guest port on the
                                            virtual switch. In addition, no direct
                                            LPAR communications sharing the same
                                            OSA port is permitted with the guest
                                            ports of the virtual switch. All
                                            traffic from the virtual switch
                                            destined for any sharing host/LPARs
                                            on the same OSA port will be dropped.
                                            Any traffic destined for the virtual
                                            switch guest ports from hosts/LPARs
                                            sharing the same OSA port will also
                                            be dropped. OFF allows guest ports
                                            to communicate with each other and
                                            with any hosts and/or LPARs that
                                            share the same OSA port.
    0158  344 Signed       4 VSGCONF        The access type for the
                                            virtual switch. Possible values are:
                                            USER Specifies that the virtual switch
                                            will be on a user ID basis.
                                            Authorization and configuration will be
                                            for the user. Use SET VSWITCH GRANT and
                                            REVOKE commands for authorization.
                                            Port numbers for guests will be assigned
                                            CP. PORT Specifies that the virtual
                                            switch will be port based. All
                                            connections will be on a port basis.
                                            Each port must be configured with the
                                            SET VSWITCH PORTNUMBER command. This
                                            configuration will allow a guest to
                                            have multiple unique access ports
                                            connected to the same VSWITCH instance.
    015C  348 Signed       4 VSGBPBR        The configured bridge port
                                            role. Possible roles are:
    0160  352 Signed       4 VSGBPBS        The current state of the
                                            bridge port. Possible states are:
                                            Undefined Inactive Standby Active
    0164  356 Signed       4 VSGBPBC        The state of the bridge port
                                            connection. Possible states are:
                                            VSWITCH defined Controller not
                                            available Operator intervention
                                            required Diconnected VDEVs attached
                                            to controller Initialization in
                                            progress Device not ready Device
                                            ready Devices being detached
                                            VSWITCH delete pending VSWITCH
                                            failover recovering AUTOSTART in
                                            progress
    0168  360 Character    4 VSGBMFS        Maximum Frame Size for the
                                            bridge port in kilobytes.
    016C  364 Character    8 VSGBLPA        When BPBSTATE is Active of
                                            Standby, this is the LPAR name
                                            acting as the active bridge
                                            port connection.
    0174  372 Signed       4 VSWRES1        Reserved
              00000178       VSWDLEN        *-SEGTVSWI

#### SEGTNSRV DSECT - Network Server (TCP/IP Stack) Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTNSRV       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 SRVRNAME       Name of the TCP/IP Server.
    0008    8 Dbl-Word     8 CONNOINI       The rate per second at which TCP
                                            connection open requests were
                                            initiated. (General TCP/IP
                                            Activity Log.)
    0010   16 Dbl-Word     8 CONNOACP       The rate per second at which TCP
                                            connection open requests were
                                            accepted. (General TCP/IP
                                            Activity Log.)
    0018   24 Dbl-Word     8 CONNOFAI       The rate per second for TCP
                                            connection open failures.
                                            (General TCP/IP Activity Log.)
    0020   32 Dbl-Word     8 CONNRSET       The reset rate per second for TCP
                                            Connections. (General TCP/IP
                                            Activity Log.)
    0028   40 Dbl-Word     8 READREQ        The read requests per second.
                                            (TCP/IP I/O Activity Log.)
    0030   48 Dbl-Word     8 WRITEREQ       The write requests per second.
                                            (TCP/IP I/O Activity Log.)
    0038   56 Dbl-Word     8 BYTESREC       The number of bytes received per
                                            second. (TCP/IP I/O Activity
                                            Log.)
    0040   64 Dbl-Word     8 BYTEXMIT       The number of bytes transmitted
                                            per second. (TCP/IP I/O Activity
                                            Log.)
    0048   72 Dbl-Word     8 SEGSRECV       The TCP segments received rate
                                            per second. (General TCP/IP
                                            Activity Log.)
    0050   80 Dbl-Word     8 SEGSXMIT       The TCP segments transmit rate
                                            per second. (General TCP/IP
                                            Activity Log.)
    0058   88 Dbl-Word     8 SEGSRXMI       The rate at which TCP segments
                                            were retransmitted, per second.
                                            (General TCP/IP Activity Log.)
    0060   96 Dbl-Word     8 SEGSRCVE       The rate at which TCP segments
                                            were received that had errors,
                                            per second. (General TCP/IP
                                            Activity Log.)
    0068  104 Dbl-Word     8 SEGSXMIR       The rate at which TCP segments
                                            were transmitted that included a
                                            reset, in seconds. (General
                                            TCP/IP Activity Log.)
    0070  112 Dbl-Word     8 ARPRECV        The ARP requests received rate
                                            per second. (General TCP/IP
                                            Activity Log.)
    0078  120 Dbl-Word     8 ARPREPLY       The rate at which ARP replies
                                            were transmitted, in seconds.
                                            (General TCP/IP Activity Log.)
    0080  128 Dbl-Word     8 ARPREQXM       The rate at which ARP requests
                                            were transmitted, per second.
                                            (General TCP/IP Activity Log.)
    0088  136 Dbl-Word     8 ACTBLKPL       Activity control block pool
                                            level. (TCP/IP Buffer Pool Log.)
    0090  144 Dbl-Word     8 CLNBLKPL       Client control block pool level.
                                            (TCP/IP Buffer Pool Log.)
    0098  152 Dbl-Word     8 ENVREGPL       Regular envelope pool level.
                                            (TCP/IP Buffer Pool Log.)
    00A0  160 Dbl-Word     8 ENVLARGE       Large envelope pool level.
                                            (TCP/IP Buffer Pool Log.)
    00A8  168 Dbl-Word     8 RAWBLKIP       Raw IP control block pool.
                                            (TCP/IP Buffer Pool Log.)
    00B0  176 Dbl-Word     8 SOCKBLKL       Socket control block pool level.
                                            (TCP/IP Buffer Pool Log.)
    00B8  184 Dbl-Word     8 BSDSOCKB       BSD-style socket control block
                                            pool level. (TCP/IP Buffer Pool
                                            Log.)
    00C0  192 Dbl-Word     8 TCPBLKPL       TCP control block pool level.
                                            (TCP/IP Buffer Pool Log.)
    00C8  200 Dbl-Word     8 UDPBLKPL       UDP control block pool level.
                                            (TCP/IP Buffer Pool Log.)
    00D0  208 Dbl-Word     8 REGBUFPL       Regular data buffer pool level.
                                            (TCP/IP Buffer Pool Log.)
    00D8  216 Dbl-Word     8 SMLBUFPL       Small data buffer pool level.
                                            (TCP/IP Buffer Pool Log.)
    00E0  224 Dbl-Word     8 TNYBUFPL       Tiny data buffer pool level.
                                            (TCP/IP Buffer Pool Log.)
    00E8  232 Dbl-Word     8 SACBLKPL       Segment acknowledgement control
                                            block pool. (TCP/IP Buffer Pool
                                            Log.)
    00F0  240 Dbl-Word     8 FIXPAGPL       Fixed Page Storage Pool. (TCP/IP
                                            Buffer Pool Log.)
              000000F8       TCPDLEN        *-SEGTNSRV

#### SEGTNUSR DSECT - Network User Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTNUSR       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 SRVRNAMU       Name of the TCP/IP Server the
                                            user is connected to.
    0008    8 Character    8 USERNAME       The userid of the virtual machine
                                            that handled the local side of
                                            the connection. (TCP/IP User
                                            Activity Log.)
    0010   16 Dbl-Word     8 TCPCSESS       The number of completed TCP
                                            sessions. (TCP/IP User Activity
                                            Log.)
    0018   24 Dbl-Word     8 UDPCSESS       The number of completed UDP
                                            sessions. (TCP/IP User Activity
                                            Log.)
    0020   32 Dbl-Word     8 TIMESESS       The average session duration
                                            (elapsed time from open to
                                            close). (TCP/IP User Activity
                                            Log.)
    0028   40 Dbl-Word     8 TOTTCPIN       The number of bytes received
                                            during TCP sessions. (TCP/IP User
                                            Activity Log.)
    0030   48 Dbl-Word     8 TOTTCPOU       The number of bytes sent during
                                            TCP sessions. (TCP/IP User
                                            Activity Log.)
    0038   56 Dbl-Word     8 TOTUDPIN       The number of bytes received
                                            during UDP sessions. (TCP/IP User
                                            Activity Log.)
    0040   64 Dbl-Word     8 TOTUPDOU       The number of bytes sent during
                                            UDP sessions. (TCP/IP User
                                            Activity Log.)
    0048   72 Dbl-Word     8 TRIPTSTH       The smoothed round trip time, in
                                            seconds. (TCP/IP User Activity
                                            Log.)
    0050   80 Dbl-Word     8 TRIPTVAR       The smoothed round trip time
                                            variance, in seconds. (TCP/IP
                                            User Activity Log.)
    0058   88 Dbl-Word     8 TOTSEGS        The total numbers of segments.
                                            (TCP/IP User Activity Log.)
    0060   96 Dbl-Word     8 UACKSEGS       The maximum number of
                                            unacknowledged segments. (TCP/IP
                                            User Activity Log.)
    0068  104 Dbl-Word     8 MAXIBUFQ       The maximum input buffer queue
                                            size. (TCP/IP User Activity Log.)
    0070  112 Dbl-Word     8 MAXOBUFQ       The maximum output buffer queue
                                            size. (TCP/IP User Activity Log.)
              00000078       NUSRDLEN       *-SEGTNUSR

#### SEGTAPPL DSECT - LINUX Appldata Area

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTAPPL       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 LUSERID        Userid of the LINUX guest machine
                                            (Linux summary CPU activity
                                            screen: userid)
    0008    8 Signed       4 VIRTCPU        The number of virtual CPUs
                                            defined for the guest (Linux
                                            summary CPU activity screen: Virt
                                            CPUs)
    0010   16 Dbl-Word     8 TOTCPU         Percent total CPU utilitzation
                                            (Linux summary CPU activity
                                            screen: totCPU)
    0018   24 Dbl-Word     8 USERCPU        Percent user mode CPU
                                            utilitzation (Linux summary CPU
                                            activity screen: user)
    0020   32 Dbl-Word     8 KERNLCPU       Percent kernel mode CPU
                                            utilitzation (Linux summary CPU
                                            activity screen: kernel)
    0028   40 Dbl-Word     8 NICECPU        Percent nice mode CPU
                                            utilitzation (Linux summary CPU
                                            activity screen: nice)
    0030   48 Dbl-Word     8 IRQ            Percent IRQ interrupts (Linux
                                            summary CPU activity screen: IRQ)
    0038   56 Dbl-Word     8 SOFTIRQ        Percent soft IRQ interrupts
                                            (Linux summary CPU activity
                                            screen: SoftIRQ)
    0040   64 Dbl-Word     8 IOWAIT         Percent waiting for I/O (Linux
                                            summary CPU activity screen:
                                            IOWait)
    0048   72 Dbl-Word     8 IDLE           Percent CPU idle (Linux summary
                                            CPU activity screen: Idle)
    0050   80 Signed       4 RUNABLE        The number of runable processes
                                            at sampling (Linux summary CPU
                                            activity screen: Runabl)
    0054   84 Signed       4 WAITING        The number of processes waiting
                                            for I/O (Linux summary CPU
                                            activity screen: Waiting)
    0058   88 Signed       4 TOTPROC        The total number of processes at
                                            sample time (Linux summary CPU
                                            activity screen: Total)
    0060   96 Dbl-Word     8 RUN1MIN        The average number of processes
                                            found running during the last 1
                                            minute (Linux summary CPU
                                            activity screen: 1_min)
    0068  104 Dbl-Word     8 RUN5MIN        The average number of processes
                                            found running during the last 5
                                            minutes (Linux summary CPU
                                            activity screen: 5_min)
    0070  112 Dbl-Word     8 RUN15MIN       The average number of processes
                                            found running during the last 15
                                            minutes (Linux summary CPU
                                            activity screen: 15_min)
    0078  120 Dbl-Word     8 TOTMAIN        The total main memory size in
                                            MBytes (Linux summary CPU memory
                                            screen: M_Total)
    0080  128 Dbl-Word     8 PERCMAIN       Main memory utilization in
                                            percentage (Linux summary CPU
                                            memory screen: %M_User)
    0088  136 Dbl-Word     8 TOTHIGH        The total high memory size in
                                            MBytes (Linux summary CPU memory
                                            screen: H_Total)
    0090  144 Dbl-Word     8 PERCHIGH       High memory utilization in
                                            percentage (Linux summary CPU
                                            memory screen: %H_User)
    0098  152 Dbl-Word     8 SHARED         Memory, in MBytes, that is usable
                                            by more than one process. (Linux
                                            summary CPU memory screen:
                                            Shared)
    00A0  160 Dbl-Word     8 BUFFREE        Memory, in MBytes, reserved for
                                            buffers and free cache (Linux
                                            summary CPU memory screen:
                                            Buffers/CAFree)
    00A8  168 Dbl-Word     8 CACHUSED       Memory, in MBytes, used for
                                            buffers. The LINUX buffer cache
                                            is a disk cache intended to
                                            relieve processes from having to
                                            wait for relatively slow disks to
                                            retrieve or store data. (Linux
                                            summary CPU memory screen: Cache
                                            Used)
    00B0  176 Dbl-Word     8 TOTSWAP        The size of the maximum available
                                            swap space in MBytes (Linux
                                            summary CPU memory screen:
                                            S_Total)
    00B8  184 Dbl-Word     8 PERCSWAP       Percentage of swap space useable
                                            swap space (Linux summary CPU
                                            memory screen: %SUSed)
    00C0  192 Dbl-Word     8 SWAPIN         Swap in rate, in 4KB pgs/second
                                            (Linux summary CPU memory screen:
                                            In)
    00C8  200 Dbl-Word     8 SWAPOUT        Swap out rate, in 4KB pgs/second
                                            (Linux summary CPU memory screen:
                                            Out)
    00D0  208 Dbl-Word     8 PGALLOC        Page allocation rate (Linux
                                            summary CPU memory screen:
                                            Allocates)
    00D8  216 Dbl-Word     8 PGFTMAJ        Page faults (major) (Linux
                                            summary CPU memory screen: Major)
    00E0  224 Dbl-Word     8 PGFTMIN        Page faults (minor) (Linux
                                            summary CPU memory screen: Minor)
    00E8  232 Dbl-Word     8 BLKREAD        Block I/O data read rate in
                                            KB/sec (Linux summary CPU memory
                                            screen: I/O Read)
    00F0  240 Dbl-Word     8 BLKWRITE       Block I/O data write rate in
                                            KB/sec (Linux summary CPU memory
                                            screen: I/O Write)
    00F8  248 Dbl-Word     8 INTERFCS       Number of networking interfaces
                                            defined (Linux summary CPU
                                            networking screen: Interfaces)
    0100  256 Dbl-Word     8 PKTRECV        Number of packets received per
                                            second (Linux summary CPU
                                            networking screen: Packets
                                            P_recv)
    0108  264 Dbl-Word     8 PKTSENT        Number of packets sent per second
                                            (Linux summary CPU networking
                                            screen: Packets P_Xmit)
    0110  272 Dbl-Word     8 BYTRECV        Number of bytes received per
                                            second (Linux summary CPU
                                            networking screen: Bytes B_recv)
    0118  280 Dbl-Word     8 BYTSENT        Number of bytes sent per second
                                            (Linux summary CPU networking
                                            screen: Bytes B_Xmit)
    0120  288 Dbl-Word     8 BADPACK        Bad packets received per second
                                            (Linux summary CPU networking
                                            screen: BadPac Recvd)
    0128  296 Dbl-Word     8 XMITERR        Packet transmit problems per
                                            second (Linux summary CPU
                                            networking screen: Packet X_mit)
    0130  304 Dbl-Word     8 NSPBUFF        No space found in Linux buffers
                                            per second (Linux summary CPU
                                            networking screen: No Space
                                            Buffer)
    0138  312 Dbl-Word     8 NSPLINX        No space available in Linux per
                                            second (Linux summary CPU
                                            networking screen: No Space
                                            Linux)
    0140  320 Dbl-Word     8 XMITCOLL       Collisions while transmitting per
                                            second (Linux summary CPU
                                            networking screen: Transmit
                                            Collisn)
    0148  328 Dbl-Word     8 STEALTM        Percent time hypervisor in
                                            control
    0150  336 Character   16 LNXPRDID       Linux Kernel Product ID
    0160  352 Signed       4 LNXFLAG        APPLDATA internal flag field.
                                            X'01' means data has been normalized
    0168  360 Dbl-Word     8 LNXTIME        TOD when APPLDATA was written
              00000170       APPLDLEN       *-SEGTAPPL

#### SEGTPRC DSECT - Processor Data Area

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTPRC        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 LPENUM         Assigned logical partition
                                            number. (LPAR load screen, partition#.)
    0004    4 Character    8 LPENAME        Assigned name of the logical
                                            partition. (LPAR load screen, partition name.)
    000C   12 Signed       4 LPENUPID       The user partition ID number
                                            for the logical partition.
    0010   16 Signed       4 LPENLPCT       Number of logical processors
                                            assigned to this LPAR. (LPAR load screen, #Proc.)
    0014   20 Signed       4 LPENCAP        Enumerated value reflecting the
                                            capping definition for the partition. It can be
                                            Yes (2) if capping has been set on for the
                                            partition, indicating that CPU cycles are to be
                                            allocated only up to  the specified maximum, or
                                            No (1) if capping is not active.
    0018   24 Signed       4 LPENWGHT       Average weight for all logical
                                            processors defined for this LPAR. The weight
                                            values for dedicated processors will be 1000.
                                            (LPAR load screen, Weight.)
    001C   28 Signed       4 LPENWAIT       Status of the WAIT bit for the
                                            logical processors within this LPAR. If any LP
                                            has the WAIT bit ON, this field will contain
                                            enumerations 1=YES or 0=NO. (LPAR load screen,
                                            Wait Char.)
    0020   32 Dbl-Word     8 LPENLOAD       Total amount of time that all
                                            of the logical processors for this LPAR were
                                            busy during the reported interval.
    0028   40 Signed       4 LPENSTAT       Status of the logical partition
                                            during the reporting interval. Can be enumerations
                                            2=ACTIVE or 1=INACTIVE or 0=inactive. The partition
                                            that was used to collect the LPAR data will have an
                                            asterisk (*) appended, for example ACTIVE).
    002C   44 Signed       4 LPENPTYP       The CPU type of the logical
                                            processors defined for the partition as follows:
                                            CP: Central Processor, ICF: Internal Coupling
                                            Facility Processor, IFL: Integrated Facility for
                                            Linux Processor, ZIIP: IBM System z9 Integrated
                                            Information Processor (zIIP), ZAAP: IBM zSeries
                                            Application Assist Processor (zAAP), Special: other.
    0030   48 Signed       4 LPENCPU        The CPU identification character
                                            allocated to each of the logical processors which
                                            were defined. (CPU)
    0038   56 Dbl-Word     8 LPENMSPC       Percentage of elapsed time that
                                            the logical processor was suspended, i.e. could
                                            not give Service to the guest system due to LPAR
                                            management time and contention for real processors,
                                            where the suspended time is calculated as the
                                            difference between elapsed time and the sum of
                                            processor busy time and voluntary wait time for
                                            the same processor as seen by the VM system that is
                                            active in the partition.
    0040   64 Dbl-Word     8 LPENOVHD       Average percentage of elapsed
                                            time that the logical processor spent for LPAR
                                            mgmt. This information is available only on
                                            systems with the LPAR management time facility
                                            (LPAR load screen, %Ovhd.)
    0048   72 Dbl-Word     8 LPENBUSY       Average percentage of time that
                                            logical processors were busy, defined as the
                                            percentage of elapsed time during which real
                                            processors were assigned to logical processors.
                                            Note that the value will also include wait time
                                            in the system that is running in the partition
                                            if 'wait completion' has been enabled for the
                                            processor.
    0050   80 Dbl-Word     8 LPENOVER       Amount of logical CPU busy
                                            which was due to LP dispatching overhead.
    0058   88 Dbl-Word     8 LPENPHYS       This is the sum of the %Load
                                            values for all active logical partitions with
                                            normal processors plus the General LPAR
                                            management overhead (if available), i.e. it
                                            gives you the overall load for normal processors
                                            in the complex and does not include the load
                                            of partitions with IFL or ICF processors.
    0060   96 Dbl-Word     8 LPENLGLD       Logical processor load as seen
                                            by the guest VM system, based on processor busy
                                            time seen by the guest system and the sum of
                                            wait time and processor busy time perceived by
                                            the guest VM system. This is the logic used for
                                            the calculation of the 'INDICATE LOAD' output.
                                            Note, however, that the resulting value depends
                                            not only on the actual activity of the guest
                                            system (the processor time used), but also on
                                            the activity of the systems in other logical
                                            partitions of the same physical system: The
                                            'suspended' time (see %Susp value) will
                                            increase if there is more contention for the
                                            real processors, thus causing less voluntary
                                            wait time. Less voluntary wait time in turn
                                            will result in a higher 'Logical processor
                                            load' being calculated, even if the actual CPU
                                            time used by a processor is the same.
    0068  104 Dbl-Word     8 LPENVMLD       Processor load as seen by the
                                            guest VM system, based on processor busy time
                                            seen by the guest system and elapsed time.
    0070  112 Dbl-Word     8 LPENTCAP       The maximum amount of core
                                            power of this type the partition is permitted
                                            to use, where a value of 100 represents one
                                            whole physical core worth of power.
    0078  120 Signed       4 LPENMTDP       The multithreading depth for
                                            the specified logical core of this partition
    007C  124 Character    8 LPENGCPN       The group capping name assigned
                                            to this partition
    0088  136 Dbl-Word     8 LPENGCPV       The group capping value assigned
                                            to this partition
    0090  144 Character    4 LPENCPUH       The CPU identification character
                                            allocated to each of the logical
                                            processors which were defined (CPU)
    0094  148 Signed       4 LPENRSV1       Reserved (double word aligned)
              00000098       PROCDLEN       *-SEGTPRC

#### SEGTMDC DSECT - Minidisk Cache

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTMDC        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Dbl-Word     8 PARTSIZE       The size of the CP partition in
                                            expanded storage, in blocks
    0008    8 Dbl-Word     8 MAXCACHE       The maximum number of expanded
                                            storage blocks that can be used for minidisk
                                            caching
    0010   16 Dbl-Word     8 ACTCACHE       The number of expanded storage
                                            blocks used for minidisk caching at the end of
                                            the interval
    0018   24 Dbl-Word     8 FAIRSHR        The fair share limit for the
                                            minidisk cache, i.e. the maximum number of blocks
                                            any one user is allowed to insert into the
                                            minidisk cache per fair share interval
    0020   32 Dbl-Word     8 MDCRDRAT       The number of read requests
                                            per second
    0028   40 Dbl-Word     8 FULLRDHT       The percentage of requests
                                            which were full hits, i.e. where all the
                                            requested blocks were found in the cache
    0030   48 Dbl-Word     8 PGINRT         The rate at which minidisk
                                            cache blocks are moved from expanded storage
                                            to central storage
    0038   56 Dbl-Word     8 PGOUTRT        The rate at which minidisk
                                            cache blocks are moved from central storage
                                            to expanded storage
    0040   64 Dbl-Word     8 BLKLIFE        The estimated average age,
                                            in seconds, of a minidisk cache block, based on
                                            Little's Law (cache size divided by PGOUT rate).
                                            Dots will be shown if the age cannot be
                                            calculated because the PGOUT rate is zero.
    0048   72 Dbl-Word     8 FRSHRXRT       The rate, per second, that
                                            blocks could not be moved into the minidisk
                                            cache because their user's fair share limit was
                                            exceeded
    0050   80 Dbl-Word     8 INTINSRT       Insertions per second into
                                            the in-transit waiting queue (which keeps track
                                            of users requesting blocks which are already on
                                            their way to the minidisk cache)
    0058   88 Dbl-Word     8 INVREQRT       The number of requests per
                                            second to invalidate minidisk cache blocks, due
                                            to an I/O to a virtual device via a non-cachable
                                            I/O interface
    0060   96 Dbl-Word     8 BLKINVRT       The number of blocks per
                                            second which were invalidated following an
                                            invalidation request
    0068  104 Dbl-Word     8 IDEALFRM       The ideal number of main
                                            storage page frames in the minidisk cache
                                            (based on average age of a page in DPA,
                                            determined by arbiter)
    0070  112 Dbl-Word     8 ACTFRL2G       The actual number of main
                                            storage page frames used for the minidisk
                                            cache below the 2G line
    0078  120 Dbl-Word     8 ACTFRG2G       The actual number of main
                                            storage page frames used for the minidisk
                                            cache above the 2G line. The field is only
                                            available for z/VM systems running in 64-bit
                                            mode.
    0080  128 Dbl-Word     8 MINFRMS        The minimum number of
                                            main storage pages to be used for the minidisk
                                            cache
    0088  136 Dbl-Word     8 MAXFRMS        The maximum number of
                                            main storage pages to be used for the minidisk
                                            cache
    0090  144 Dbl-Word     8 PGDELRT        The number of main storage
                                            pages deleted from the cache per second
    0098  152 Dbl-Word     8 STINVRT        The number of times the
                                            steal function was invoked to steal main
                                            storage pages from cache per second
    00A0  160 Dbl-Word     8 MDCBIAS        The bias for minidisk cache
                                            usage of real storage. A number less than 1 is
                                            a bias against minidisk cache; a number greater
                                            than 1 is a bias for minidisk cache.
    00A8  168 Dbl-Word     8 IDEALXST       The ideal number of expanded
                                            storage blocks in the minidisk cache (based on
                                            average age of an XSTORE block, as determined by
                                            arbiter)
    00B0  176 Dbl-Word     8 ACTXST         The actual number of expanded
                                            storage blocks used for the minidisk cache
    00B8  184 Dbl-Word     8 MINXST         The minimum number of expanded
                                            storage blocks to be used for the minidisk cache
    00C0  192 Dbl-Word     8 MAXXST         The maximum number of expanded
                                            storage blocks to be used for the minidisk cache
    00C8  200 Dbl-Word     8 PGDELXST       The number of XSTORE pages
                                            deleted from the cache per second
    00D0  208 Dbl-Word     8 STINVXST       The number of times the steal
                                            function was invoked to steal expanded storage
                                            pages from the cache per second
    00D8  216 Dbl-Word     8 MDCBSXST       The bias for minidisk cache
                                            use of expanded storage. A number less than 1 is
                                            a bias against minidisk cache; a number greater
                                            than 1 is a bias for minidisk cache.
    00E0  224 Dbl-Word     8 AGEXST         The average age of paging
                                            XSTORE blocks
    00E8  232 Dbl-Word     8 DASDONE        Successfully translated CCWs
                                            per second for DASD devices
    00F0  240 Dbl-Word     8 DASDABRT       Aborted translation attempts
                                            per second for DASD devices
    00F8  248 Dbl-Word     8 DASDNELG       Number of CCWs which were
                                            found to be not eligible for translation, per
                                            second for DASD devices
    0100  256 Dbl-Word     8 DASDTOT        Total number of CCWs handled
                                            per second for DASD devices
    0108  264 Dbl-Word     8 NETDONE        Successfully translated CCWs
                                            per second for network devices
    0110  272 Dbl-Word     8 NETABRT        Aborted translation attempts
                                            per second for network devices
    0118  280 Dbl-Word     8 NETNELG        Number of CCWs which were
                                            found to be not eligible for translation, per
                                            second for network devices
    0120  288 Dbl-Word     8 NETTOT         Total number of CCWs handled
                                            per second for network devices
    0128  296 Dbl-Word     8 MDCWRRTE       The number of write operations
                                            per second to the minidisk cache.
    0130  304 Dbl-Word     8 MDCRDHRT       The number of read operations
                                            per second to cached minidisks
                                            where the block to be read was
                                            already in the minidisk cache.
              00000138       MDCDLEN        *-SEGTMDC

#### SEGTCHN DSECT - Channel

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTCHN        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 CHPID          The hexadecimal 'channel path
                                            identifier'
    0004    4 Character    8 CHMODGRP       Description of the channel
                                            model group, as found in the Store-Channel-Path
                                            description.
    000C   12 Character    4 CHMODQ         The hexadecimal channel model
                                            group qualifier. Note that a valid qualifier is
                                            available only on systems with the extended
                                            channel measurement facility.
    0010   16 Dbl-Word     8 CHPRCBSY       The percentage of 'busy'
                                            conditions found, calculated for the last interval.
                                            For FICON channels the 'busy' value is
                                            calculated as the percentage of actual work unit
                                            utilization compared to the maximum possible
                                            value. Channel 'busy' percentages cannot be
                                            calculated for Hipersocket channels.
    0018   24 Dbl-Word     8 CHAVGBSY       The percentage of 'busy'
                                            conditions found, calculated for the whole period
                                            since the last RESET, or since Performance Toolkit
                                            was last invoked. For FICON channels the 'busy'
                                            value is calculated as the percentage of actual
                                            work unit utilization compared to the maximum
                                            possible value. Channel 'busy' percentages
                                            cannot be calculated for Hipersocket channels.
    0020   32 Dbl-Word     8 CHBSY0         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 0-10.
    0028   40 Dbl-Word     8 CHBSY1         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 11-20.
    0030   48 Dbl-Word     8 CHBSY2         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 21-30.
    0038   56 Dbl-Word     8 CHBSY3         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 31-40.
    0040   64 Dbl-Word     8 CHBSY4         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 41-50.
    0048   72 Dbl-Word     8 CHBSY5         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 51-60.
    0050   80 Dbl-Word     8 CHBSY6         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 61-70.
    0058   88 Dbl-Word     8 CHBSY7         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 71-80.
    0060   96 Dbl-Word     8 CHBSY8         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 81-90.
    0068  104 Dbl-Word     8 CHBSY9         Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals
                                            was found in the range 91-100.
              00000070       CHNDLEN        *-SEGTCHN

#### SEGTLCHN DSECT - LPAR Channel

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTLCHN       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 LCHPID         The hexadecimal 'channel path
                                            identifier'
    0004    4 Character    8 LCHGRP         Description of the channel
                                            model group, as found in the Store-Channel-Path
                                            description.
    000C   12 Character    4 LCHGRPQ        The hexadecimal channel model
                                            group qualifier. Note that a valid qualifier is
                                            available only on systems with the extended
                                            channel measurement facility.
    0010   16 Character    4 LCHSHR         Shared indicator for the channel.
                                            It can be either YES for channels shared with other
                                            logical partitions, or NO for channels dedicated to
                                            this logical partition.
    0018   24 Dbl-Word     8 LCHPRBSY       The percentage of 'busy'
                                            conditions found, calculated for the last interval.
    0020   32 Dbl-Word     8 LCHAVGBS       The percentage of 'busy'
                                            conditions found, calculated for the whole period
                                            since the last RESET, or since Performance Toolkit
                                            was last invoked.
    0028   40 Dbl-Word     8 LCHBSY0        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 0-10.
    0030   48 Dbl-Word     8 LCHBSY1        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 11-20.
    0038   56 Dbl-Word     8 LCHBSY2        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 21-30.
    0040   64 Dbl-Word     8 LCHBSY3        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 31-40.
    0048   72 Dbl-Word     8 LCHBSY4        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 41-50.
    0050   80 Dbl-Word     8 LCHBSY5        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 51-60.
    0058   88 Dbl-Word     8 LCHBSY6        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 61-70.
    0060   96 Dbl-Word     8 LCHBSY7        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 71-80.
    0068  104 Dbl-Word     8 LCHBSY8        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 81-90.
    0070  112 Dbl-Word     8 LCHBSY9        Channel load distribution for
                                            each of the active channels. It shows the
                                            relative frequency with which the channel busy
                                            percentage of separate measurement intervals was
                                            found in the range 91-100.
              00000078       LCHNDLEN       *-SEGTLCHN

#### SEGTFCHN DSECT - FICON Channel

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTFCHN       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 FCHPID         The hexadecimal 'channel path
                                            identifier'
    0004    4 Character    4 FCHSHR         Shared indicator for the channel.
                                            It can be either YES for channels shared with
                                            other logical partitions, or NO for channels
                                            dedicated to this logical partition.
    0008    8 Dbl-Word     8 FCHBUS         The bus cycles utilization for
                                            the whole system.
    0010   16 Dbl-Word     8 FCHWRK         The work units utilization for
                                            the whole system.
    0018   24 Dbl-Word     8 FCHDUW         The data units write utilization
                                            for the whole system.
    0020   32 Dbl-Word     8 FCHDUR         The data units read utilization
                                            for the whole system.
    0028   40 Dbl-Word     8 FCHLWRK        The work units utilization for
                                            for the own logical partition.
    0030   48 Dbl-Word     8 FCHLDUW        The data units write utilization
                                            for the own logical partition.
    0038   56 Dbl-Word     8 FCHLDUR        The data units read utilization
                                            for the own logical partition.
    0040   56 Dbl-Word     8 FCHWRT         The total number of bytes
                                            written per second, for the whole system.
    0048   64 Dbl-Word     8 FCHRD          The total number of bytes
                                            read per second, for the whole system.
              00000050       FCHNDLEN       *-SEGTFCHN

#### SEGTDCAC DSECT - DASD Cache

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTDCAC       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 DCACDIR        3880-13/23 storage director
                                            ID. For IBM DASD subsystems the last
                                            two hexadecimal digits of the SSID
                                            will be inserted.
    0004    4 Character    4 DCACADDR       Disk device number.
    0008    8 Character    8 DCACLABL       Disk label.
    0010   16 Character    8 DCACTYP        Device type and model. For
                                            alias parallel access volumes of an
                                            IBM DASD Subsystem, the device type
                                            is replacesd by the string PAV.
    0018   24 Character    4 DCACPAV        This is the base address for
                                            any Parallel Access Volumes.
    001C   28 Character    4 DCACSID        Storage controller subsystem
                                            identifier.
    0020   32 Signed       4 DCACSTC        Caching status, A=Caching is
                                            activated, D=Caching is deactivated,
                                            P=Deactivate is pending.
    0024   36 Signed       4 DCACSTF        Status of DASD fast write,
                                            A=DASD fast write is activated, D= DASD fast
                                            write is deactivated, P=DASD fast write
                                            deactivate is pending.
    0028   40 Signed       4 DCACDPS        Duplex indicator 0=No
                                            duplex, 1=Disk is primary device
                                            of a dual copy pair, 2=Disk is
                                            secondary device of a dual pair.
    002C   44 Signed       4 DCACDUST       Status of duplex. A=Duplex
                                            pair available, P=Duplex pair
                                            pending, F=Failed duplex, S=Duplex
                                            has been suspended.
    0030   48 Dbl-Word     8 DCACOVIO       Sum of NORMAL, SEQUENTIAL
                                            and FAST WRITE (for IBM DASD
                                            subsystems only) I/O requests
                                            per second (READ+WRITE).
    0038   56 Dbl-Word     8 DCACOVRD       Overall percentage of READ
                                            requests (NORMAL, SEQUENTIAL
                                            and FAST WRITE) to the total
                                            I/O activity of the device.
    0040   64 Dbl-Word     8 DCACOVRH       Overall percentage of READ
                                            hits, i.e. the percentage of
                                            READ requests which did not
                                            need DASD access (NORMAL,
                                            SEQUENTIAL and FAST WRITE).
    0048   72 Dbl-Word     8 DCACDWRH       Ratio of WRITE hits to
                                            WRITE requests. On 3880 control
                                            units this refers to 'write
                                            normal' hits, and on IBM DASD
                                            subsystems to DASD fast write
                                            hits.
    0050   80 Dbl-Word     8 DCACOVIC       Number of INHIBIT CACHE
                                            LOAD requests per second.
    0058   88 Dbl-Word     8 DCACOVBC       Number of BYPASS CACHE
                                            requests per second.
    0060   96 Dbl-Word     8 DCACNDIO       Number of Normal I/O
                                            requests per second.
    0068  104 Dbl-Word     8 DCACNRDR       Percentage of Normal READ
                                            requests.
    0070  112 Dbl-Word     8 DCACNRDH       Normal READ percentage, i.e.
                                            the percentage of READ requests
                                            which did not need DASD access.
    0078  120 Dbl-Word     8 DCACSDIO       Number of Fast-Write I/O
                                            requests per second over this
                                            storage director.
    0080  128 Dbl-Word     8 DCACSRDR       Percentage of Fast-Write
                                            READ requests.
    0088  136 Dbl-Word     8 DCACSRDH       Fast-Write READ percentage,
                                            i.e. the percentage of READ
                                            requests which did not need
                                            DASD access.
    0090  144 Dbl-Word     8 DCACFDIO       Number of Sequential I/O
                                            requests per second over this
                                            storage director.
    0098  152 Dbl-Word     8 DCACFRDR       Percentage of Sequential
                                            READ requests.
    00A0  160 Dbl-Word     8 DCACFRDH       Sequential READ percentage,
                                            i.e. the percentage of READ
                                            requests which did not need
                                            DASD access.
    00A8  168 Dbl-Word     8 DCACCIO        Total I/O rate for the disk
                                            as it is perceived by the cache
                                            control unit, i.e. where multiple
                                            systems are connected to one
                                            control unit the total I/O
                                            activity from all systems is
                                            shown.
    00B0  176 Dbl-Word     8 DCACSSC        I/O rate as indicated by
                                            subchannel measurement block
                                            data for the system which does
                                            the monitoring, i.e. only the I/O
                                            activity for that system is
                                            included. Where V=R guest systems
                                            can set up their own subchannel
                                            measurement blocks for dedicated
                                            disks, SIE assisted I/O activity
                                            to such disks will not be
                                            included either.
    00B8  184 Dbl-Word     8 DCACRNR        Nonsequential read rate
                                            (read normal + read CFW)
    00C0  192 Dbl-Word     8 DCACRSR        Sequential read rate
                                            (read sequential)
    00C8  200 Dbl-Word     8 DCACWRR        Total write fast write
                                            rate (CFW + DFW).
    00D0  208 Dbl-Word     8 DCACPRD        Percentage of cachable
                                            read operations, based on
                                            total I/O activity.
    00D8  216 Dbl-Word     8 DCACHTO        Percentage of total hits
                                            (read + CFW + DFW), based on
                                            the sum of all cachable read
                                            and write operations.
    00E0  224 Dbl-Word     8 DCACHRD        Percentage of read hits,
                                            based on the sum of all
                                            cachable read operations.
    00E8  232 Dbl-Word     8 DCACHWR        Percentage of write hits,
                                            (DASD FW + cache FW), based on
                                            the sum of all DASD and cache
                                            fast write write operations.
    00F0  240 Dbl-Word     8 DCACHDW        Percentage of DASD fast
                                            write hits, based on the sum
                                            of all DASD fast write write
                                            operations.
    00F8  248 Dbl-Word     8 DCACHCW        Percentage of cache fast
                                            write hits, based on the sum
                                            of all cache fast write write
                                            operations.
    0100  256 Dbl-Word     8 DCACPDF        Percentage of DASD fast
                                            write operations, based on the
                                            total write activity.
    0108  264 Dbl-Word     8 DCACPCF        Percentage of cache fast
                                            write operations, based on
                                            total write activity.
    0110  272 Dbl-Word     8 DCACSGN        Percent of non-sequential
                                            DASD to cache transfer
                                            operations.
    0118  280 Dbl-Word     8 DCACSGS        Percent of sequential DASD
                                            to cache transfer operations.
    0120  288 Dbl-Word     8 DCACDSG        Percent of cache to DASD
                                            transfer operations.
    0128  296 Dbl-Word     8 DCACDFB        Percent of DASD fast write
                                            operations which were forced
                                            to bypass the cache and access
                                            DASD directly due to non-volatile
                                            storage constraints.
    0130  304 Dbl-Word     8 DCACICL        Percentage of I/O operations
                                            which bypassed caching voluntarily.
    0138  312 Dbl-Word     8 DCACTMO        Number of timeouts that
                                            occurred while waiting for data
                                            from the control unit (status = -2).
    0140  320 Signed       4 DCACCAFG       Flag for validity of bytes
                                            read and written fields (pcardrt,
                                            pcawrrt, pcabrd and pcabwr)
    0148  328 Dbl-Word     8 DCACRDRT       Rate at which bytes are
                                            read
    0150  336 Dbl-Word     8 DCACWRRT       Rate at which bytes are
                                            written
    0158  344 Signed       4 DCACBRD        Total bytes read in 128K
                                            blocks
    015C  348 Signed       4 DCACBWR        Total bytes written in
                                            128K blocks
              00000160       DCACDLEN       *-SEGTDCAC

#### SEGTCTLU DSECT - Control Unit Cache

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTCTLU       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 CTLSID         The control unit's subsystem
                                            identifier.
    0004    4 Character    8 CTLTYP         The control unit type and model.
    0010   16 Dbl-Word     8 CTLCST         The size of configured cache
                                            storage, in Megabytes.
    0018   24 Dbl-Word     8 CTLAST         The amount of cache storage which
                                            is available, in Megabytes.
    0020   32 Dbl-Word     8 CTLCNV         The size of configured
                                            non-volatile storage, in
                                            Megabytes.
    0028   40 Dbl-Word     8 CTLANV         The amount of non-volatile
                                            storage which is available,
                                            in Megabytes.
    0030   48 Dbl-Word     8 CTLCIO         The total I/O activity as it
                                            is perceived by the cache control
                                            unit, i.e. where multiple systems
                                            are connected to one control unit
                                            the total I/O activity from all
                                            systems is shown.
    0038   56 Dbl-Word     8 CTLSSC         The total I/O activity as
                                            determined from count fields in
                                            the subchannel measurement blocks
                                            of the system which does the
                                            monitoring, i.e. only the I/O
                                            requests from that system.
                                            Where V=R guest systems can set
                                            up their own subchannel
                                            measurement blocks for dedicated
                                            disks, SIE assisted I/O activity
                                            to such disks will not be included
                                            either. Since the busy percentage
                                            and all of the service time
                                            components are calculated from
                                            subchannel measurement data, the
                                            same restrictions apply also to
                                            the next six fields.
    0040   64 Dbl-Word     8 CTLBSY         Average busy percentage for
                                            all connected disks.
    0048   72 Dbl-Word     8 CTLFPT         Average 'fucntion pending' time
                                            (msec). This is the average
                                            time an I/O request remained
                                            pending in the I/O subsystem due
                                            to path busy conditions.
    0050   80 Dbl-Word     8 CTLDST         Average 'disconnected' time.
                                            This is the average time that the
                                            device remained disconnected from
                                            the channel while executing I/O
                                            requests. For DASD it includes the
                                            time spent for executing the SEEK
                                            and SET SECTOR orders and also any
                                            re-connect misses. High values may
                                            indicate overloaded paths, or many
                                            long SEEKs to data at opposite ends
                                            of the device. The value also includes
                                            the 'device-active-only' time where
                                            that information is available.
    0058   88 Dbl-Word     8 CTLCNT         Average 'connected' time (msec).
                                            This is the average time that the
                                            device was connected to the channel
                                            while executing I/O requests, i.e.
                                            receiving commands or actually
                                            transferring data. It includes also
                                            the search time.
    0060   96 Dbl-Word     8 CTLSRV         Average service time, i.e.
                                            the sum of function pending,
                                            disconnected and connected time.
    0068  104 Dbl-Word     8 CTLRSP         Device response time. This
                                            is the device service time plus
                                            the time during which an I/O
                                            request was waiting to be started.
                                            It is calculated based on the
                                            average I/O request queue length
                                            and the I/O rate.
    0070  112 Dbl-Word     8 CTLRNR         Total non-sequential read
                                            rate, per second.
    0078  120 Dbl-Word     8 CTLRSR         Total sequential read rate,
                                            per second.
    0080  128 Dbl-Word     8 CTLWRR         Total fast-write write rate,
                                            per second.
    0088  136 Dbl-Word     8 CTLPRD         Average percentage of read
                                            operations, based on the sum of
                                            read and write operations.
    0090  144 Dbl-Word     8 CTLPDF         Average percentage of DASD
                                            fast-write write operations,
                                            based on the sum of all write
                                            operations.
    0098  152 Dbl-Word     8 CTLPCF         Average percentage of cache
                                            fast-write write operations,
                                            based on the sum of all write
                                            operations.
    00A0  160 Dbl-Word     8 CTLHRD         Average read hits percentage.
    00A8  168 Dbl-Word     8 CTLHWR         Average write hits percentage,
                                            for DASD and cache fast write
                                            operations.
    00B0  176 Dbl-Word     8 CTLHDW         Average DASD fast-write hit
                                            percentage.
    00B8  184 Dbl-Word     8 CTLHCW         Average cache fast-write hit
                                            percentage.
              000000C0       CTLUDLEN       *-SEGTCTLU

#### SEGTVDSK DSECT - Virtual Disk

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTVDSK       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 VDSUID         Userid of the owner of the
                                            VDISK.
    0008    8 Character    4 VDSDEVNM       The virtual device number of
                                            the VDISK.
    0010   16 Dbl-Word     8 VDSSIZE        The size of the VDISK, expressed
                                            as the number of 512-byte blocks
                                            for which it was defined.
    0018   24 Dbl-Word     8 VDSLINK        The number of LINKs to the
                                            virtual disk.
    0020   32 Dbl-Word     8 VDSIOS         The virtual I/O rate to the
                                            virtual disk.
    0028   40 Dbl-Word     8 VDSSTLS        The number of pages stolen per
                                            second.
    0030   48 Dbl-Word     8 VDSPRDS        The number of pages read from
                                            DASD per second.
    0038   56 Dbl-Word     8 VDSPWRT        The number of pages written to
                                            DASD per second.
    0040   64 Dbl-Word     8 VDSXRDS        The number of pages moved from
                                            expanded storage to central
    0048   72 Dbl-Word     8 VDSXWRS        The number of pages moved from
                                            central storage to expanded
                                            storage, per second.
    0050   80 Dbl-Word     8 VDSXMIG        The number of pages migrated
                                            from expanded storage to DASD, per
                                            second.
    0058   88 Dbl-Word     8 VDSPRES        The number of pages resident
                                            in central storage.
    0060   96 Dbl-Word     8 VDSPLOK        The number of locked pages.
    0068  104 Dbl-Word     8 VDSPXST        The number of XSTOR blocks
                                            occupied by the data space.
    0070  112 Dbl-Word     8 VDSPNPS        The number of slots occupied
                                            on auxillary storage.
    0078  120 Character   24 VDSNAME        The name of the data space.
    0090  144 Signed       4 VDSPRIV        Indicates whether this virtual
                                            disk is a private vdisk, or a
                                            shared vdisk
    0098  152 Dbl-Word     8 VDSIBR         The number of
                                            Invalid-but-Resident (IBR)
                                            pages for this virtual disk
              000000A0       VDSKDLEN       *-SEGTVDSK

#### SEGTSPLK DSECT - Spin Lock

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTSPLK       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 LOKNAME        The name of the lock.
    0008    8 Dbl-Word     8 LOKTLCT        The total exclusive and shared
                                            spin lock calls per second.
    0010   16 Dbl-Word     8 LOKTLTM        The total average microseconds
                                            spent spinning on both exclusive and
                                            shared spin locks.
    0018   24 Dbl-Word     8 LOKTLPC        The percentage of total elapsed
                                            time spent in both exclusive and shared
                                            spin locks.
    0020   32 Dbl-Word     8 LOKEXCT        The total exclusive spin lock
                                            calls per second.
    0028   40 Dbl-Word     8 LOKEXTM        The average total microseconds
                                            spent spinning on exclusive spin locks.
    0030   48 Dbl-Word     8 LOKEXPC        The percentage of total elapsed
                                            time spent in exclusive spin locks.
    0038   56 Dbl-Word     8 LOKSHCT        The total shared spin lock calls
                                            per second.
    0040   64 Dbl-Word     8 LOKSHTM        The average total microseconds
                                            spent spinning on shared spin locks.
    0048   72 Dbl-Word     8 LOKSHPC        The percentage of total elapsed
                                            time spent in shared spin locks.
              00000050       SPLKDLEN       *-SEGTSPLK

#### SEGTWAIT DSECT - Resource Constraint Analysis

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTWAIT       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 WAITWKLD       Userid or group name.
    0008    8 Signed       4 WAITACT        Percent of samples during
                                            which the user was found to be
                                            active, either consuming CPU or
                                            waiting for some service.
    000C   12 Signed       4 WAITRUN        Percent of active samples
                                            during which the user was found
                                            to be running on a real processor.
    0010   16 Signed       4 WAITCPU        Percent of active samples
                                            during which the user was found
                                            to be waiting to run on the real CPU.
    0014   20 Signed       4 WAITLDG        Percent of active samples
                                            during which the user was found
                                            in loading state, i.e. with a very
                                            high page read rate.
    0018   24 Signed       4 WAITPGW        Percent of active samples
                                            during which the user was found
                                            in page wait state.
    001C   28 Signed       4 WAITIOW        Percent of active samples
                                            during which the user was found
                                            in I/O wait state.
    0020   32 Signed       4 WAITSIM        Percent of active samples
                                            during which the user was found
                                            in instruction simulation wait,
                                            i.e. waiting for CP to complete
                                            simulation of a privileged
                                            instruction.
    0024   36 Signed       4 WAITTIW        Percent of active samples
                                            during which the user was found
                                            in test idle wait, i.e. waiting to
                                            be dropped from the dispatch list.
    0028   40 Signed       4 WAITCFW        Percent of active samples
                                            during which the user was found
                                            in console function wait, i.e.
                                            waiting for CP to execute one of
                                            the console function commands
                                            which allow a user to alter the
                                            state and configuration of the
                                            virtual machine (e.g. LINK,
                                            ATTACH, and DETACH).
    002C   44 Signed       4 WAITSVTI       Percent of active samples
                                            during which the user was found
                                            in both SVM wait and test idle wait.
                                            SVM wait state indicates that the
                                            user was waiting for the completion
                                            of a communication with a service
                                            virtual machine.
    0030   48 Signed       4 WAITSVEL       Percent of active samples
                                            during which the user was found
                                            in both SVM wait and in the
                                            eligible list (resource wait).
    0034   52 Signed       4 WAITSVDM       Percent of active samples
                                            during which the user was found
                                            in both SVM wait and in the
                                            dormant list. (This status is
                                            counted as active since the
                                            machine is actually waiting
                                            for something, and not just
                                            idle).
    0038   56 Signed       4 WAITIOA        Percent of active measurements
                                            during which the user was found
                                            waiting for something other
                                            than the above while an I/O
                                            operation started by this
                                            machine had not yet completed.
    003C   60 Signed       4 WAITPACT       Percent of page active wait,
                                            i.e. the virtual machine has
                                            loaded a wait PSW while waiting
                                            for the completion of a page read
                                            operation. This state is to be
                                            expected for guest systems
                                            running with PAGEX ON.
    0040   64 Signed       4 WAITLIML       Percent of active measurements
                                            during which the user was found
                                            in the limit list, i.e. in the
                                            dispatch list waiting for CPU but
                                            prevented from running by a
                                            maximum share setting.
    0044   68 Signed       4 WAITOTH        Percent of active measurements
                                            during which the user was found in
                                            other states.
    0048   72 Signed       4 WAITUIQ0       Percent of active measurements
                                            during which the user was found in
                                            Q0 ( in the dispatch list as class
                                            0 user).
    004C   76 Signed       4 WAITUIQ1       Percent of active measurements
                                            during which the user was found in
                                            Q1 ( in the dispatch list as class
                                            1 user).
    0050   80 Signed       4 WAITUIQ2       Percent of active measurements
                                            during which the user was found in
                                            Q2 ( in the dispatch list as class
                                            2 user).
    0054   84 Signed       4 WAITUIQ3       Percent of active measurements
                                            during which the user was found in
                                            Q3 ( in the dispatch list as class
                                            3 user).
    0058   88 Signed       4 WAITELIG       Percent of active measurements
                                            during which the user was found in
                                            the eligible list ( any class).
    005C   92 Signed       4 WAITRSV1       Reserved for alignment.
              00000060       WAITDLEN       *-SEGTWAIT

#### SEGTCPC DSECT - The CPU type of the logical processors

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTCPC        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 CPCBLTYP       The CPU type of the logical
                                            processors defined for the
                                            partition, as follows:
                                            CP: Central Processor,
                                            ICF: Internal Coupling Facility
                                                 processor
                                            IFL: Integrated Facility for Linux
                                                 processor
                                            ZIIP: IBM System z9 Integrated
                                                 Information Processor (zIIP)
                                            ZAAP: IBM zSeries Application Assist
                                                  Processor (zAAP)
                                            Special: other
    0004    4 Signed       4 CPCBNUM        The number of physical
                                            processors of this type.
    0008    8 Signed       4 CPCBWT         The total weight of processors
                                            of this type. This value is
                                            derived by summing the weight
                                            of each processor type once in
                                            in each LPAR.
    000C   12 Signed       4 CPCBDED        The total number of dedicated
                                            processors of this type.
    0010   16 Signed       4 CPCBLPTM       For this physical processor
                                            type, the percent of physical
                                            capacity used actually running
                                            logical processors of the
                                            corresponding type. The value ranges
                                            from 0% to n*100%, where n is the
                                            number of physical processors of
                                            this type.
    0014   20 Signed       4 CPCBOVHD       For this physical processor
                                            type, the percent of physical
                                            capacity used doing LPAR management
                                            activities that are directly
                                            chargeable or attributable to the
                                            actions of logical processors
                                            of the corresponding type. The
                                            value ranges from 0% to n*100%,
                                            where n is the number of physical
                                            processors of this type.
    0018   24 Signed       4 CPCBMGTM       For this physical processor
                                            type, the percent of physical
                                            capacity used doing LPAR management
                                            activities that are not directly
                                            chargeable or attributable to the
                                            actions of logical processors
                                            of the corresponding type. The
                                            value ranges from 0% to n*100%,
                                            where n is the number of physical
                                            processors of this type.
    001C   28 Signed       4 CPCBSUM        For this physical processor
                                            type, the sum of %LPBUSY, %LPOVHD,
                                            and %NCOVHD. This is the totatl
                                            capacity used for this processor
                                            type.
              00000020       CPCDLEN        *-SEGTCPC

.

#### SEGTSSI DSECT - SSI Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTSSI        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 SSISLOT        The slot used in the SSI used
                                            by this member
    0004    4 Character    8 SSISYSID       The name of the member in the
                                            SSI
    000C   12 Signed       4 SSIRES1        Reserved
              00000010       SSIDLEN        *-SEGTSSI

#### SEGTSCSI DSECT - SCSI Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTSCSI       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    4 SCZDVNO        The real emulated FBA device
                                            (EDEV) number.
    0004    4 Signed       4 SCZBYTS        Number of bytes in a block
                                            for this DASD.
    0008    8 Dbl-Word     8 SCZKBRT        The transfer rate (kilobytes per
                                            second) of the device. Note
                                            that the transfer rate is only
                                            meaningful for devices which support
                                            discrete seeks. SCSI DASD do not
                                            support discrete seeks and return
                                            a value of 0 for this field.
    0010   16 Dbl-Word     8 SCZXFRT        The number of data transfers per
                                            second to and from this device.
    0018   24 Dbl-Word     8 SCZSKRT        The number of seek operations
                                            per second associated with the
                                            device. Note that the transfer rate
                                            is only meaningful for devices
                                            which support discrete seeks. SCSI
                                            DASD do not support discrete seeks
                                            and return a value of 0 for this field.
    0020   32 Signed       4 SCZPCCT        The device-busy time over
                                            the selected interval. This is a
                                            function of the time the device is
                                            connected to the channel over the
                                            selected interval.
    0024   36 Character    4 SCZEATT        The value of this device's
                                            EDEV attribute.
    0028   40 Signed       4 SCZBKRD        Number of blocks read
    002C   44 Signed       4 SCZBKWR        Number of blocks written
    0030   48 Dbl-Word     8 SCZBKRT        Number of blocks read per
                                            second during the selected
                                            interval
    0038   56 Dbl-Word     8 SCZBKWT        Number of blocks written
                                            per second during the selected
                                            interval
    0040   64 Signed       4 SCZP1RD        Number of blocks read on
                                            path 1
    0044   68 Signed       4 SCZP1WR        Number of blocks written
                                            on path 1
    0048   72 Dbl-Word     8 SCZP1RT        Number of blocks read on
                                            path 1 per second
    0050   80 Dbl-Word     8 SCZP1WT        Number of blocks written
                                            on path 1 per second
    0058   88 Signed       4 SCZP2RD        Number of blocks read on
                                            path 2
    005C   92 Signed       4 SCZP2WR        Number of blocks written
                                            on path 2
    0060   96 Dbl-Word     8 SCZP2RT        Number of blocks read on
                                            path 2 per second
    0068  104 Dbl-Word     8 SCZP2WT        Number of blocks written
                                            on path 2 per second
    0070  112 Signed       4 SCZP3RD        Number of blocks read on
                                            path 3
    0074  116 Signed       4 SCZP3WR        Number of blocks written
                                            on path 3
    0078  120 Dbl-Word     8 SCZP3RT        Number of blocks read on
                                            path 3 per second
    0080  128 Dbl-Word     8 SCZP3WT        Number of blocks written
                                            on path 3 per second
    0088  136 Signed       4 SCZP4RD        Number of blocks read on
                                            path 4
    008C  140 Signed       4 SCZP4WR        Number of blocks written
                                            on path 4
    0090  144 Dbl-Word     8 SCZP4RT        Number of blocks read on
                                            path 4 per second
    0098  152 Dbl-Word     8 SCZP4WT        Number of blocks written
                                            on path 4 per second
    00A0  160 Signed       4 SCZP5RD        Number of blocks read on
                                            path 5
    00A4  164 Signed       4 SCZP5WR        Number of blocks written
                                            on path 5
    00A8  168 Dbl-Word     8 SCZP5RT        Number of blocks read on
                                            path 5 per second
    00B0  176 Dbl-Word     8 SCZP5WT        Number of blocks written
                                            on path 5 per second
    00B8  184 Signed       4 SCZP6RD        Number of blocks read on
                                            path 6
    00BC  188 Signed       4 SCZP6WR        Number of blocks written
                                            on path 6
    00C0  192 Dbl-Word     8 SCZP6RT        Number of blocks read on
                                            path 6 per second
    00C8  200 Dbl-Word     8 SCZP6WT        Number of blocks written
                                            on path 6 per second
    00D0  208 Signed       4 SCZP7RD        Number of blocks read on
                                            path 7
    00D4  212 Signed       4 SCZP7WR        Number of blocks written
                                            on path 7
    00D8  216 Dbl-Word     8 SCZP7RT        Number of blocks read on
                                            path 7 per second
    00E0  224 Dbl-Word     8 SCZP7WT        Number of blocks written
                                            on path 7 per second
    00E8  232 Signed       4 SCZP8RD        Number of blocks read on
                                            path 8
    00EC  236 Signed       4 SCZP8WR        Number of blocks written
                                            on path 8
    00F0  240 Dbl-Word     8 SCZP8RT        Number of blocks read on
                                            path 8 per second
    00F8  248 Dbl-Word     8 SCZP8WT        Number of blocks written
                                            on path 8 per second
              00000100       SCSIDLEN       *-SEGTSCSI

#### SEGTLGR DSECT - LGR Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTLGR        SEGOUT DCSS Content Data
                                            Definition
    0000    0 Signed       4 LGREVTT        Time that the live guest
                                            relocation completed
    0004    4 Character    8 LGRISSR        The userid that initiated the
                                            live guest relocation
    000C   12 Character    8 LGRUSER        The userid for which this
                                            relocation was attempted
    0014   20 Character    8 LGRSRC         The z/VM system from which
                                            the userid was moved
    001C   28 Character    8 LGRDEST        The z/VM system to which
                                            the userid was moved
    0024   36 Signed       4 LGRFINCD       The finishing code for the
                                            relocation
    0028   40 Dbl-Word     8 LGRRELOT       The amount of time the entire
                                            live guest relocation took
    0030   48 Dbl-Word     8 LGRQUIES       The amount of time it took to
                                            quiesce the userid prior to
                                            relocation
    0038   56 Dbl-Word     8 LGRPASS        Number of memory passes made
                                            during the relocation
    0040   64 Dbl-Word     8 LGRPG1P        Number of guest pages
                                            transferred in the first pass
    0048   72 Dbl-Word     8 LGRPGIP        Average number of guest
                                            pages transferred during pass
                                            2 through pass n-2
    0050   80 Dbl-Word     8 LGRPGN1P       Number of guest pages
                                            transferred in the next to
                                            last pass
    0058   88 Dbl-Word     8 LGRPGNP        Number of guest pages
                                            transferred in the final pass
    0060   96 Dbl-Word     8 LGRPGTOT       The total number of pages
                                            moved for the guest
    0068  104 Dbl-Word     8 LGRVDEV        Count of transferred virtual
                                            devices
    0070  112 Dbl-Word     8 LGRAIOS        Count of active I/O operations
                                            relocated
    0078  120 Dbl-Word     8 LGRCNQDI       Count of non-QDIO type I/O
                                            operations cleared
    0080  128 Dbl-Word     8 LGRCQDIO       Count of QDIO type operations
                                            cleared
    0088  136 Signed       4 LGRROPT1       Synchronous/Asynchronous,
                                            Immediate, Max Quiesce No Limit
                                            and Max_Relocation No Limit
    008C  140 Signed       4 LGRROPT2       Force Architecture, Domain
                                            and Storage
    0090  144 Signed       4 LGRSOPT1       Relocation Off, CPU Affinity
                                            Supressed, CPU Affinity Changed
                                            and Source System Record used
    0094  148 Signed       4 LGRRES1         Reserved
              00000098       LGRDLEN        *-SEGTLGR

#### SEGTCPUP DSECT - CPU Pool Data

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTCPUP       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Dbl-Word     8 CPUPPOOL       The Name of the CPU Pool
    0008    8 Signed       4 CPUPTYPE       The type of CPUs in the CPU
                                            Pool. It can be either CP or
                                            IFL.
    000C   12 Signed       4 CPUPAFF        CPU affinity setting for the
                                            core type limited by this
                                            CPU pool. It can be either
                                            ON or SUP.
    0010   16 Dbl-Word     8 CPUPLVAL       CPU pool maximum share from
                                            the DEFINE or SET CPUPOOL
                                            command. It is a percentage
                                            for a LIMITHARD limit or the
                                            number of CPU/Cores for a
                                            CAPACITY limit.
    0018   24 Signed       4 CPUPLTYP       The type of CPU pool limiting.
                                            This is % for a LIMITHARD limit.
                                            It is CPU or CORES for a
                                            CAPACITY LIMIT.
    001C   28 Signed       4 CPUPMEMS       The number of members currently
                                            in the CPU pool.
    0020   32 Dbl-Word     8 CPUPCPU        The total time consumed by CPU
                                            pool members, as a percentage.
                                            A value of 100 represents one
                                            physical CPU's worth of power.
                                            When SMT is disabled this value
                                            is based on raw CPU time if CP is
                                            running 6.3 without CP APAR VM65680.
                                            When SMT is enabled, this value is
                                            based on prorated core CPU time if CP
                                            is running 6.3 with CP APAR VM65680
                                            or any release after 6.3.
    0028   40 Dbl-Word     8 CPUPLRAT       The rate of times, per minute,
                                            the CPU pool has been limited
                                            during the interval.
    0030   48 Dbl-Word     8 CPUPPUSE       The amount of available CPU
                                            pool space used by members,
                                            expressed as a percent. It is
                                            either the %CPU used divided by the
                                            limit, if the limit is expressed in
                                            percent, or the %CPU divided by the
                                            number of cores, if the limit is
                                            expressed in cores.
    0038   56 Dbl-Word     8 CPUPMXCR       The maximum size of the CPU
                                            pool, expressed in cores. If the
                                            limit is expressed in percent, then
                                            this is the number of CPUs of the
                                            same type as the pool that are in
                                            the LPAR multiplied by the limit.
              00000040       CPUPDLEN       *-SEGTCPUP

#### SEGTADAP DSECT - Data Area Prefix

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTADAP       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 DAPEYEC        Eyecatcher "KVLDAPAA" or
                                            "KVLDAPAB"
    0008    8 Character    8 DAPSYSID       Sysid
    0010   16 Signed       4 DAPSTAMP (2)   Observation Time Stamp (sec
                                            units)
    0018   24 Character    8 DAPLPARN       LPAR Partition Name
    0020   32 Signed       4 SYSDOFF        System Data offset.
    0024   36 Signed       4 SYSDCNT        The number of System elements.
    0028   40 Signed       4 WKLDOFF        Workload Data offset.
    002C   44 Signed       4 WKLDCNT        The number of Workload elements.
    0030   48 Signed       4 LPADOFF        LPAR Data offset.
    0034   52 Signed       4 LPADCNT        The number of LPAR elements.
    0038   56 Signed       4 CPODOFF        CP-Owned Device Data offset.
    003C   60 Signed       4 CPODCNT        The number of CPOwned elements.
    0040   64 Signed       4 DEVDOFF        Device Data offset.
    0044   68 Signed       4 DEVDCNT        The number of Device elements.
    0048   72 Signed       4 HIPDOFF        Network Hiersocket Data offset.
    004C   76 Signed       4 HIPDCNT        The number of Network Hiper
                                            elements.
    0050   80 Signed       4 VSWDOFF        Network Virtual Switch Data
                                            offset.
    0054   84 Signed       4 VSWDCNT        The number of Network Virtual
                                            Switch elements.
    0058   88 Signed       4 TCPDOFF        Network Server (TCP/IP Stack)
                                            Data offset
    005C   92 Signed       4 TCPDCNT        The number of Network TCP/IP
                                            elements.
    0060   96 Signed       4 NUSRDOFF       Network User Data offset.
    0064  100 Signed       4 NUSRDCNT       The number of Network User
                                            elements.
    0068  104 Signed       4 LINXDOFF       LINUX APPLDATA offset
    006C  108 Signed       4 LINXDCNT       LINUX rows
    0070  112 Signed       4 LPENDOFF       Processor offset
    0074  116 Signed       4 LPENDCNT       Processor rows
    0078  120 Signed       4 MDCDOFF        Minidisk cache offset
    007C  124 Signed       4 MDCDCNT        Minidisk cache rows
    0080  128 Signed       4 CHANDOFF       Channel offset
    0084  132 Signed       4 CHANDCNT       Channel rows
    0088  136 Signed       4 LCHNDOFF       LPAR Channel offset
    008C  140 Signed       4 LCHNDCNT       LPAR Channel rows
    0090  144 Signed       4 FCHNDOFF       FICON Channel offset
    0094  148 Signed       4 FCHNDCNT       FICON Channel rows
    0098  152 Signed       4 DCANDOFF       DASD cache offset
    009C  156 Signed       4 DCANDCNT       DASD cache rows
    00A0  160 Signed       4 CTLNDOFF       Control Unit cache offset
    00A4  164 Signed       4 CTLNDCNT       Control Unit cache rows
    00A8  168 Signed       4 VDKNDOFF       Virtual Disk offset
    00AC  172 Signed       4 VDKNDCNT       Virtual Disk rows
    00B0  176 Signed       4 SPNNDOFF       Spin Locks offset
    00B4  180 Signed       4 SPNNDCNT       Spin Locks rows
    00B8  184 Signed       4 WAINDOFF       Resource constraint Analysis
                                            offset.
    00BC  188 Signed       4 WAINDCNT       Resource constraint Analysis
                                            rows.
    00C0  192 Signed       4 SYS2DOFF       System2 Data offset.
    00C4  196 Signed       4 SYS2DCNT       The number of System2 elements.
    00C8  200 Signed       4 CPCDOFF        CPC Data offset.
    00CC  204 Signed       4 CPCDCNT        The number of CPC elements.
    00D0  208 Signed       4 SSIDOFF        SSI Data offset.
    00D4  212 Signed       4 SSIDCNT        The number of SSI elements.
    00D8  216 Signed       4 SCSIDOFF       SCSI Data offset.
    00DC  220 Signed       4 SCSIDCNT       The number of SCSI elements.
    00E0  224 Signed       4 LGRDOFF        LGR Data offset.
    00E4  228 Signed       4 LGRDCNT        The number of LGR elements.
    00E8  232 Signed       4 CPUPDOFF       CPU Pool Data offset.
    00EC  236 Signed       4 CPUPDCNT       The number of CPU Pool elements.
    00F0  240 Signed       4 DATAEND        ending addr of data area
    00F4  244 Character    8 DAPSSINM       SSI Cluster name
    00FC  252 Signed       4 RESRVED1       Double-word alignment. Future
                                            use.
              00000100       DAPLEN         *-SEGTADAP DSCCOUT

#### SEGTASEG DSECT - Segment Prefix

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SEGTASEG       SEGOUT DCSS Content Data
                                            Definition
    0000    0 Character    8 PTKEYEC        Eyecatcher "KVLPTK00"
    0008    8 Character    8 PTKVERS        Performance Toolkit version
                                            string.
    0010   16 Character    8 PTKLEVEL       Performance Toolkit service level
                                            string.
    0018   24 Character    8 ZVMVERS        zVM version string.
    0020   32 Character    8 ZVMLEVEL       zVM service level string.
    0028   40 Signed       4 INTRVLTM       Sample interval at time of
                                            segment update.
    002C   44 Signed       4 UPDTIMEA (2)   TOD clock PTK begins writing Data
                                            Area A
    0034   52 Signed       4 UPDSTRTA       Integer counter incremented at
                                            start of update to data area A.
    0038   56 Signed       4 UPDENDA        Integer counter incremented at
                                            end of update to data area A.
    003C   60 Signed       4 LOCKDATA       Data Area A lock.
    0040   64 Signed       4 DAPAOFF        Data Area A offset.
    0044   68 Signed       4 DAPACNT        Data Area A length.
    0048   72 Signed       4 UPDTIMEB (2)   TOD clock PTK begins writing Data
                                            Area B
    0050   80 Signed       4 UPDSTRTB       Integer counter incremented at
                                            start of update to data area B.
    0054   84 Signed       4 UPDENDB        Integer counter incremented at
                                            end of update to data area B.
    0058   88 Signed       4 LOCKDATB       Data Area B lock.
    005C   92 Signed       4 DAPBOFF        Data Area B offset.
    0060   96 Signed       4 DAPBCNT        Data Area B length.
    0064  100 Character    8 SEGUSER        Userid of Owning VM
    006C  108 Signed       4 SEGFREE1       Reserved
              00000070       SEGLEN         *-SEGTASEG

#### SEGTSYS Storage Layout

    *** SEGTSYS - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         ACTUSER           |         AVGUSER           |
    *     +---------------------------+---------------------------+
    *   8 |                       AVLFRAMS                        |
    *     +-------------------------------------------------------+
    *  10 |                       AVLFRA2G                        |
    *     +-------------------------------------------------------+
    *  18 |                       AVLHGHTH                        |
    *     +-------------------------------------------------------+
    *  20 |                       AVLHGH2G                        |
    *     +-------------------------------------------------------+
    *  28 |                       AVLLMEAN                        |
    *     +-------------------------------------------------------+
    *  30 |                       AVLLME2G                        |
    *     +-------------------------------------------------------+
    *  38 |                       AVLLOWTH                        |
    *     +-------------------------------------------------------+
    *  40 |                       AVLLOW2G                        |
    *     +---------------------------+---------------------------+
    *  48 |         AVLWAIT           |          CPBUSY           |
    *     +---------------------------+---------------------------+
    *  50 |         CPUBUSY           |          CPUNUM           |
    *     +---------------------------+---------------------------+
    *  58 |         DEVIOSCS          |         DIALUSER          |
    *     +---------------------------+---------------------------+
    *  60 |                       DPAFRAMS                        |
    *     +-------------------------------------------------------+
    *  68 |                       DSCNFAIL                        |
    *     +-------------------------------------------------------+
    *  70 |                       ELIGUSER                        |
    *     +-------------------------------------------------------+
    *  78 |                       EXPUSER1                        |
    *     +-------------------------------------------------------+
    *  80 |                       EXPUSER2                        |
    *     +-------------------------------------------------------+
    *  88 |                       EXPUSER3                        |
    *     +-------------------------------------------------------+
    *  90 |                       EXTFRAMS                        |
    *     +-------------------------------------------------------+
    *  98 |                       EXTWAIT                         |
    *     +-------------------------------------------------------+
    *  A0 |                       FSTRREQS                        |
    *     +-------------------------------------------------------+
    *  A8 |                       FSTRRETS                        |
    *     +-------------------------------------------------------+
    *  B0 |                       LPARBSYS                        |
    *     +-------------------------------------------------------+
    *  B8 |                       NTRVRATE                        |
    *     +-------------------------------------------------------+
    *  C0 |                       PAGERATE                        |
    *     +---------------------------+---------------------------+
    *  C8 |         PAGINDEX          |         PCTPAGE           |
    *     +---------------------------+---------------------------+
    *  D0 |         PCTSPOL           |         PCTTDSK           |
    *     +---------------------------+---------------------------+
    *  D8 |         RESELWAT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  E0 |                       SINGFLTS                        |
    *     +-------------------------------------------------------+
    *  E8 |                       SYSDPAP                         |
    *     +-------------------------------------------------------+
    *  F0 |                        SYSITR                         |
    *     +-------------------------------------------------------+
    *  F8 |                       TRVRATE                         |
    *     +-------------------------------------------------------+
    * 100 |                       TVRATIO                         |
    *     +---------------------------+---------------------------+
    * 108 |          USERQ            |         WAITIOP           |
    *     +---------------------------+---------------------------+
    * 110 |         WAITPAGP          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 118 |                       TOTSTOR                         |
    *     +-------------------------------------------------------+
    * 120 |                       OFFSTORE                        |
    *     +-------------------------------------------------------+
    * 128 |                       SYSSTORE                        |
    *     +-------------------------------------------------------+
    * 130 |                       SHARSTOR                        |
    *     +-------------------------------------------------------+
    * 138 |                       FSTORSUB                        |
    *     +---------------------------+---------------------------+
    * 140 |         SSTORUTL          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 148 |                       LOCKPAGS                        |
    *     +-------------------------------------------------------+
    * 150 |                       TRTABSZ                         |
    *     +-------------------------------------------------------+
    * 158 |                       PAGSTOR                         |
    *     +---------------------------+---------------------------+
    * 160 |         STORUTIL          |        TSKWFRCT           |
    *     +---------------------------+---------------------------+
    * 168 |         TSKWPGRT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 170 |                       STBYSTOR                        |
    *     +-------------------------------------------------------+
    * 178 |                       RESVSTOR                        |
    *     +-------------------------------------------------------+
    * 180 |                       TOTXSTAV                        |
    *     +-------------------------------------------------------+
    * 188 |                       TOTXSTUS                        |
    *     +-------------------------------------------------------+
    * 190 |                       TOTXSTCP                        |
    *     +---------------------------+---------------------------+
    * 198 |         CPXSTORE          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1A0 |                       XSTMIGLW                        |
    *     +-------------------------------------------------------+
    * 1A8 |                       XSTALLOC                        |
    *     +-------------------------------------------------------+
    * 1B0 |                       XSTBLKAG                        |
    *     +-------------------------------------------------------+
    * 1B8 |                       XSTBLKMG                        |
    *     +-------------------------------------------------------+
    * 1C0
    *
    *** SEGTSYS - SEGOUT DCSS Content Data Definition

    *** SEGTSYS2 - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       VDSKSYSL                        |
    *     +-------------------------------------------------------+
    *   8 |                       VDSKUSRL                        |
    *     +-------------------------------------------------------+
    *  10 |                       VDSKMSF                         |
    *     +-------------------------------------------------------+
    *  18 |                       VDSKXSF                         |
    *     +-------------------------------------------------------+
    *  20 |                       VDSKMPG                         |
    *     +-------------------------------------------------------+
    *  28 |                       PGMVBL2G                        |
    *     +-------------------------------------------------------+
    *  30 |                       FSTPGIRT                        |
    *     +-------------------------------------------------------+
    *  38 |                       LNGPGIRT                        |
    *     +-------------------------------------------------------+
    *  40 |                       LNGPGORT                        |
    *     +-------------------------------------------------------+
    *  48 |                       PAGEWRRT                        |
    *     +---------------------------+---------------------------+
    *  50 |         PGRDBLKF          |        PGWRBLKF           |
    *     +---------------------------+---------------------------+
    *  58 |         MIGOBLKF          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  60 |                       PAGSSCH                         |
    *     +-------------------------------------------------------+
    *  68 |                       SPRDRATE                        |
    *     +-------------------------------------------------------+
    *  70 |                       SPWRRATE                        |
    *     +-------------------------------------------------------+
    *  78 |                       TOTREAL                         |
    *     +-------------------------------------------------------+
    *  80 |                       STRAGESZ                        |
    *     +-------------------------------------------------------+
    *  88 |                       STRAGINC                        |
    *     +-------------------------------------------------------+
    *  90 |                       STRRSVPG                        |
    *     +-------------------------------------------------------+
    *  98 |                       STRRSDMX                        |
    *     +-------------------------------------------------------+
    *  A0 |                       SMCR2GDC                        |
    *     +-------------------------------------------------------+
    *  A8 |                       SMCRFRQW                        |
    *     +-------------------------------------------------------+
    *  B0 |                       SMCRCT2G                        |
    *     +-------------------------------------------------------+
    *  B8 |                       EMPSINGL                        |
    *     +-------------------------------------------------------+
    *  C0 |                       EMPCONTL                        |
    *     +-------------------------------------------------------+
    *  C8 |                       EMPSINGG                        |
    *     +-------------------------------------------------------+
    *  D0 |                       EMPCONTG                        |
    *     +-------------------------------------------------------+
    *  D8
    *
    *** SEGTSYS2 - SEGOUT DCSS Content Data Definition

    *** SEGTLPAR - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         LPARNUM           |        LPARNAME           |
    *     +---------------------------+---------------------------+
    *   8 |         LPARNAME cont'd   |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                       LPARBUSY                        |
    *     +-------------------------------------------------------+
    *  18 |                       LPARLOAD                        |
    *     +---------------------------+---------------------------+
    *  20 |         LPARLPCT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  28 |                       LPARMSPC                        |
    *     +-------------------------------------------------------+
    *  30 |                       LPAROVER                        |
    *     +-------------------------------------------------------+
    *  38 |                       LPAROVHD                        |
    *     +---------------------------+---------------------------+
    *  40 |         LPARSTAT          |         LPARWAIT          |
    *     +---------------------------+---------------------------+
    *  48 |         LPARWGHT          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  50 |                       PHYSBUSY                        |
    *     +---------------------------+---------------------------+
    *  58 |         LPARUPID          |         LPARCAP           |
    *     +---------------------------+---------------------------+
    *  60 |                       LPARLGLD                        |
    *     +-------------------------------------------------------+
    *  68 |                       LPARVMLD                        |
    *     +---------------------------+---------------------------+
    *  70 |         LPARPTYP          |         LPARTCAP          |
    *     +---------------------------+---------------------------+
    *  78 |         LPARTCAP cont'd   |         LPARMTDP          |
    *     +---------------------------+---------------------------+
    *  80 |                       LPARGCPN                        |
    *     +-------------------------------------------------------+
    *  88 |                       LPARGCPV                        |
    *     +-------------------------------------------------------+
    *  90
    *
    *** SEGTLPAR - SEGOUT DCSS Content Data Definition

    *** SEGTRDEV - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         DEVADDR           |         DEVTYPE           |
    *     +---------------------------+---------------------------+
    *   8 |         DEVTYPE cont'd    |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                       CONNTIME                        |
    *     +---------------------------+---------------------------+
    *  18 |         DASDBUSY          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  20 |                       DASDQUE                         |
    *     +-------------------------------------------------------+
    *  28 |                       DASIOREQ                        |
    *     +-------------------------------------------------------+
    *  30 |                       DEVIOSEC                        |
    *     +-------------------------------------------------------+
    *  38 |                       DISCTIME                        |
    *     +-------------------------------------------------------+
    *  40 |                       PENDTIME                        |
    *     +-------------------------------------------------------+
    *  48 |                       SERVTIME                        |
    *     +-------------------------------------------------------+
    *  50 |                        VOLSER                         |
    *     +-------------------------------------------------------+
    *  58
    *
    *** SEGTRDEV - SEGOUT DCSS Content Data Definition

    *** SEGTCPDV - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         DEVADDRX          |         ALLOCCNT          |
    *     +---------------------------+---------------------------+
    *   8 |         AVAILSLT          |         CPRESRV1          |
    *     +---------------------------+---------------------------+
    *  10 |                       DEVTYPEX                        |
    *     +---------------------------+---------------------------+
    *  18 |         PAGETYPE          |          ENDCYL           |
    *     +---------------------------+---------------------------+
    *  20 |         PERFULL           |         STARTCYL          |
    *     +---------------------------+---------------------------+
    *  28 |         TOTUSLOT          |         CPRESRV2          |
    *     +---------------------------+---------------------------+
    *  30 |                       VOLSERX                         |
    *     +-------------------------------------------------------+
    *  38
    *
    *** SEGTCPDV - SEGOUT DCSS Content Data Definition

    *** SEGTWKLD - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       WORKLOAD                        |
    *     +-------------------------------------------------------+
    *   8 |                        CPPCT                          |
    *     +-------------------------------------------------------+
    *  10 |                        CPSECS                         |
    *     +-------------------------------------------------------+
    *  18 |                        CPUPCT                         |
    *     +-------------------------------------------------------+
    *  20 |                       CPUSECS                         |
    *     +-------------------------------------------------------+
    *  28 |                       SESSTIME                        |
    *     +-------------------------------------------------------+
    *  30 |                       VIRTPCT                         |
    *     +-------------------------------------------------------+
    *  38 |                       VIRTSECS                        |
    *     +-------------------------------------------------------+
    *  40 |                       PAGERATW                        |
    *     +-------------------------------------------------------+
    *  48 |                       PAGREADS                        |
    *     +-------------------------------------------------------+
    *  50 |                       PAGWRTS                         |
    *     +-------------------------------------------------------+
    *  58 |                       RESPAGES                        |
    *     +-------------------------------------------------------+
    *  60 |                       RESPAG2G                        |
    *     +-------------------------------------------------------+
    *  68 |                       STORSIZE                        |
    *     +-------------------------------------------------------+
    *  70 |                       WKLXATT                         |
    *     +-------------------------------------------------------+
    *  78 |                       WKLXMOV                         |
    *     +-------------------------------------------------------+
    *  80 |                       WKLXPAG                         |
    *     +-------------------------------------------------------+
    *  88 |                       WSS                             |
    *     +-------------------------------------------------------+
    *  90 |                       GROUP                           |
    *     +---------------------------+---------------------------+
    *  98 |         WKVCPU            |           WKRESV1         |
    *     +---------------------------+---------------------------+
    *  A0 |                       WKLDDSOW                        |
    *     +-------------------------------------------------------+
    *  A8 |                       WKLDPGST                        |
    *     +-------------------------------------------------------+
    *  B0 |                       WKLDDB2G                        |
    *     +-------------------------------------------------------+
    *  B8 |                       WKLDXRD                         |
    *     +-------------------------------------------------------+
    *  C0 |                       WKLDXWR                         |
    *     +-------------------------------------------------------+
    *  C8 |                       WKLDXMG                         |
    *     +-------------------------------------------------------+
    *  D0 |                       WKLDRVPG                        |
    *     +-------------------------------------------------------+
    *  D8 |                       WKLDPGLK                        |
    *     +-------------------------------------------------------+
    *  E0 |                       WKLDPGLG                        |
    *     +-------------------------------------------------------+
    *  E8 |                       WKLDDASD                        |
    *     +-------------------------------------------------------+
    *  F0 |                       WKLDSHR                         |
    *     +---------------------------+---------------------------+
    *  F8 |         WKLDSHRM          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 100 |                       WKLDTVRT                        |
    *     +-------------------------------------------------------+
    * 108 |                       WKLDSIO                         |
    *     +-------------------------------------------------------+
    * 110 |                       WKLDDAIO                        |
    *     +-------------------------------------------------------+
    * 118 |                       WKLDAVIO                        |
    *     +-------------------------------------------------------+
    * 120 |                       WKLDDI98                        |
    *     +-------------------------------------------------------+
    * 128 |                       WKLDURIO                        |
    *     +-------------------------------------------------------+
    * 130 |                       WKLDACTV                        |
    *     +-------------------------------------------------------+
    * 138 |                       WKLDSPGS                        |
    *     +-------------------------------------------------------+
    * 140 |                       WKLDSPGR                        |
    *     +-------------------------------------------------------+
    * 148 |                       WKLDMDCI                        |
    *     +-------------------------------------------------------+
    * 150 |                       CPUPOOL                         |
    *     +-------------------------------------------------------+
    * 158
    *
    *** SEGTWKLD - SEGOUT DCSS Content Data Definition

    *** SEGTNHIP - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         CHANPATH          |           SHRD            |
    *     +---------------------------+---------------------------+
    *   8 |                       XFERTMSG                        |
    *     +-------------------------------------------------------+
    *  10 |                       XFERTDUN                        |
    *     +-------------------------------------------------------+
    *  18 |                       FAILRBFS                        |
    *     +-------------------------------------------------------+
    *  20 |                       XFERMSGS                        |
    *     +-------------------------------------------------------+
    *  28 |                       XFERDUNI                        |
    *     +-------------------------------------------------------+
    *  30 |                       FAILRBFR                        |
    *     +-------------------------------------------------------+
    *  38 |                       FAILSOTH                        |
    *     +-------------------------------------------------------+
    *  40
    *
    *** SEGTNHIP - SEGOUT DCSS Content Data Definition

    *** SEGTVSWI - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |           ADDR            |         USERID            |
    *     +---------------------------+---------------------------+
    *   8 |           USERID cont'd   |           QSV             |
    *     +---------------------------+---------------------------+
    *  10 |           TIMEOUT         |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  18 |                       XMITBYTS                        |
    *     +-------------------------------------------------------+
    *  20 |                       XMITPCKT                        |
    *     +-------------------------------------------------------+
    *  28 |                       XMITPCKD                        |
    *     +-------------------------------------------------------+
    *  30 |                       RCVBYTES                        |
    *     +-------------------------------------------------------+
    *  38 |                       RCVPCKTS                        |
    *     +-------------------------------------------------------+
    *  40 |                       DISCPCKD                        |
    *     +-------------------------------------------------------+
    *  48 |                       VLLID                           |
    *     +-------------------------------------------------------+
    *  50 |                       VSWRT                           |
    *     +-------------------------------------------------------+
    *  58 |                       VSRED                           |
    *     +-------------------------------------------------------+
    *  60 |                       VSSYN                           |
    *     +-------------------------------------------------------+
    *  68 |                       VSPCR                           |
    *     +-------------------------------------------------------+
    *  70 |                       VSPCI                           |
    *     +-------------------------------------------------------+
    *  78 |                       VSGVGRP                         |
    *     +-------------------------------------------------------+
    *  80 |                       VSGVMAC                         |
    *     +-------------------------------------------------------+
    *  88 |                       VSGVMAC cont'd                  |
    *     +------+------------------------------------------------+
    *  90 |      |                VSGVIPA                         |
    *     +------+------------------------------------------------+
    *  98 |                       VSGVIPA cont'd                  |
    *     +-------------------------------------------------------+
    *  A0 |                       VSGVIPA cont'd                  |
    *     +-------------------------------------------------------+
    *  A8 |                       VSGVIPA cont'd                  |
    *     +-------------------------------------------------------+
    *  B0 |                       VSGVIPA cont'd                  |
    *     +-----------------------------------------+-------------+
    *  B8 |             VSGVIPA cont'd              |  VSGVMGI    |
    *     +-----------------------------------------+-------------+
    *  C0 |             VSGVMGI cont'd              |/////////////|
    *     +---------------------------+-------------+-------------+
    *  C8 |           VSGVLAY         |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  D0 |                       VSEVLIN                         |
    *     +-------------------------------------------------------+
    *  D8 |                       VSEVREQ                         |
    *     +-------------------------------------------------------+
    *  E0 |                       VSEVLDE                         |
    *     +-------------------------------------------------------+
    *  E8 |                       VSEVTXD                         |
    *     +-------------------------------------------------------+
    *  F0 |                       VSEVRXD                         |
    *     +-------------------------------------------------------+
    *  F8 |                       VSEVMTX                         |
    *     +-------------------------------------------------------+
    * 100 |                       VSEVMRX                         |
    *     +-------------------------------------------------------+
    * 108 |                       VSEVMKR                         |
    *     +-------------------------------------------------------+
    * 110 |                       VSEVMTO                         |
    *     +-------------------------------------------------------+
    * 118 |                       VSEVLAX                         |
    *     +-------------------------------------------------------+
    * 120 |                       VSEVLAR                         |
    *     +-------------------------------------------------------+
    * 128 |                       VSEVIBF                         |
    *     +-------------------------------------------------------+
    * 130 |                       VSEVIQO                         |
    *     +-------------------------------------------------------+
    * 138 |                       VSEVOBF                         |
    *     +-------------------------------------------------------+
    * 140 |                       VSEVOQO                         |
    *     +-------------------------------------------------------+
    * 148 |                       VSEVLVL                         |
    *     +---------------------------+---------------------------+
    * 150 |           VSGVOPN         |           VSGVISO         |
    *     +---------------------------+---------------------------+
    * 158 |           VSGCONF         |           VSGBPBR         |
    *     +---------------------------+---------------------------+
    * 160 |           VSGBPBS         |           VSGBPBC         |
    *     +---------------------------+---------------------------+
    * 168 |           VSGBMFS         |           VSGBLPA         |
    *     +---------------------------+---------------------------+
    * 170 |           VSGBLPA cont'd  |           VSWRES1         |
    *     +---------------------------+---------------------------+
    * 178
    *
    *** SEGTVSWI - SEGOUT DCSS Content Data Definition

    *** SEGTNSRV - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       SRVRNAME                        |
    *     +-------------------------------------------------------+
    *   8 |                       CONNOINI                        |
    *     +-------------------------------------------------------+
    *  10 |                       CONNOACP                        |
    *     +-------------------------------------------------------+
    *  18 |                       CONNOFAI                        |
    *     +-------------------------------------------------------+
    *  20 |                       CONNRSET                        |
    *     +-------------------------------------------------------+
    *  28 |                       READREQ                         |
    *     +-------------------------------------------------------+
    *  30 |                       WRITEREQ                        |
    *     +-------------------------------------------------------+
    *  38 |                       BYTESREC                        |
    *     +-------------------------------------------------------+
    *  40 |                       BYTEXMIT                        |
    *     +-------------------------------------------------------+
    *  48 |                       SEGSRECV                        |
    *     +-------------------------------------------------------+
    *  50 |                       SEGSXMIT                        |
    *     +-------------------------------------------------------+
    *  58 |                       SEGSRXMI                        |
    *     +-------------------------------------------------------+
    *  60 |                       SEGSRCVE                        |
    *     +-------------------------------------------------------+
    *  68 |                       SEGSXMIR                        |
    *     +-------------------------------------------------------+
    *  70 |                       ARPRECV                         |
    *     +-------------------------------------------------------+
    *  78 |                       ARPREPLY                        |
    *     +-------------------------------------------------------+
    *  80 |                       ARPREQXM                        |
    *     +-------------------------------------------------------+
    *  88 |                       ACTBLKPL                        |
    *     +-------------------------------------------------------+
    *  90 |                       CLNBLKPL                        |
    *     +-------------------------------------------------------+
    *  98 |                       ENVREGPL                        |
    *     +-------------------------------------------------------+
    *  A0 |                       ENVLARGE                        |
    *     +-------------------------------------------------------+
    *  A8 |                       RAWBLKIP                        |
    *     +-------------------------------------------------------+
    *  B0 |                       SOCKBLKL                        |
    *     +-------------------------------------------------------+
    *  B8 |                       BSDSOCKB                        |
    *     +-------------------------------------------------------+
    *  C0 |                       TCPBLKPL                        |
    *     +-------------------------------------------------------+
    *  C8 |                       UDPBLKPL                        |
    *     +-------------------------------------------------------+
    *  D0 |                       REGBUFPL                        |
    *     +-------------------------------------------------------+
    *  D8 |                       SMLBUFPL                        |
    *     +-------------------------------------------------------+
    *  E0 |                       TNYBUFPL                        |
    *     +-------------------------------------------------------+
    *  E8 |                       SACBLKPL                        |
    *     +-------------------------------------------------------+
    *  F0 |                       FIXPAGPL                        |
    *     +-------------------------------------------------------+
    *  F8
    *
    *** SEGTNSRV - SEGOUT DCSS Content Data Definition

    *** SEGTNUSR - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       SRVRNAMU                        |
    *     +-------------------------------------------------------+
    *   8 |                       USERNAME                        |
    *     +-------------------------------------------------------+
    *  10 |                       TCPCSESS                        |
    *     +-------------------------------------------------------+
    *  18 |                       UDPCSESS                        |
    *     +-------------------------------------------------------+
    *  20 |                       TIMESESS                        |
    *     +-------------------------------------------------------+
    *  28 |                       TOTTCPIN                        |
    *     +-------------------------------------------------------+
    *  30 |                       TOTTCPOU                        |
    *     +-------------------------------------------------------+
    *  38 |                       TOTUDPIN                        |
    *     +-------------------------------------------------------+
    *  40 |                       TOTUPDOU                        |
    *     +-------------------------------------------------------+
    *  48 |                       TRIPTSTH                        |
    *     +-------------------------------------------------------+
    *  50 |                       TRIPTVAR                        |
    *     +-------------------------------------------------------+
    *  58 |                       TOTSEGS                         |
    *     +-------------------------------------------------------+
    *  60 |                       UACKSEGS                        |
    *     +-------------------------------------------------------+
    *  68 |                       MAXIBUFQ                        |
    *     +-------------------------------------------------------+
    *  70 |                       MAXOBUFQ                        |
    *     +-------------------------------------------------------+
    *  78
    *
    *** SEGTNUSR - SEGOUT DCSS Content Data Definition

    *** SEGTAPPL - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       LUSERID                         |
    *     +---------------------------+---------------------------+
    *   8 |         VIRTCPU           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                        TOTCPU                         |
    *     +-------------------------------------------------------+
    *  18 |                       USERCPU                         |
    *     +-------------------------------------------------------+
    *  20 |                       KERNLCPU                        |
    *     +-------------------------------------------------------+
    *  28 |                       NICECPU                         |
    *     +-------------------------------------------------------+
    *  30 |                         IRQ                           |
    *     +-------------------------------------------------------+
    *  38 |                       SOFTIRQ                         |
    *     +-------------------------------------------------------+
    *  40 |                        IOWAIT                         |
    *     +-------------------------------------------------------+
    *  48 |                         IDLE                          |
    *     +---------------------------+---------------------------+
    *  50 |         RUNABLE           |         WAITING           |
    *     +---------------------------+---------------------------+
    *  58 |         TOTPROC           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  60 |                       RUN1MIN                         |
    *     +-------------------------------------------------------+
    *  68 |                       RUN5MIN                         |
    *     +-------------------------------------------------------+
    *  70 |                       RUN15MIN                        |
    *     +-------------------------------------------------------+
    *  78 |                       TOTMAIN                         |
    *     +-------------------------------------------------------+
    *  80 |                       PERCMAIN                        |
    *     +-------------------------------------------------------+
    *  88 |                       TOTHIGH                         |
    *     +-------------------------------------------------------+
    *  90 |                       PERCHIGH                        |
    *     +-------------------------------------------------------+
    *  98 |                        SHARED                         |
    *     +-------------------------------------------------------+
    *  A0 |                       BUFFREE                         |
    *     +-------------------------------------------------------+
    *  A8 |                       CACHUSED                        |
    *     +-------------------------------------------------------+
    *  B0 |                       TOTSWAP                         |
    *     +-------------------------------------------------------+
    *  B8 |                       PERCSWAP                        |
    *     +-------------------------------------------------------+
    *  C0 |                        SWAPIN                         |
    *     +-------------------------------------------------------+
    *  C8 |                       SWAPOUT                         |
    *     +-------------------------------------------------------+
    *  D0 |                       PGALLOC                         |
    *     +-------------------------------------------------------+
    *  D8 |                       PGFTMAJ                         |
    *     +-------------------------------------------------------+
    *  E0 |                       PGFTMIN                         |
    *     +-------------------------------------------------------+
    *  E8 |                       BLKREAD                         |
    *     +-------------------------------------------------------+
    *  F0 |                       BLKWRITE                        |
    *     +-------------------------------------------------------+
    *  F8 |                       INTERFCS                        |
    *     +-------------------------------------------------------+
    * 100 |                       PKTRECV                         |
    *     +-------------------------------------------------------+
    * 108 |                       PKTSENT                         |
    *     +-------------------------------------------------------+
    * 110 |                       BYTRECV                         |
    *     +-------------------------------------------------------+
    * 118 |                       BYTSENT                         |
    *     +-------------------------------------------------------+
    * 120 |                       BADPACK                         |
    *     +-------------------------------------------------------+
    * 128 |                       XMITERR                         |
    *     +-------------------------------------------------------+
    * 130 |                       NSPBUFF                         |
    *     +-------------------------------------------------------+
    * 138 |                       NSPLINX                         |
    *     +-------------------------------------------------------+
    * 140 |                       XMITCOLL                        |
    *     +-------------------------------------------------------+
    * 148 |                       STEALTM                         |
    *     +-------------------------------------------------------+
    * 150 |                       LNXPRDID                        |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 160 |         LNXFLAG           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 168 |                       LNXTIME                         |
    *     +-------------------------------------------------------+
    * 170
    *
    *** SEGTAPPL - SEGOUT DCSS Content Data Definition

    *** SEGTPRC  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         LPENUM            |         LPENAME           |
    *     +---------------------------+---------------------------+
    *   8 |         LPENAME cont'd    |         LPENUPID          |
    *     +---------------------------+---------------------------+
    *  10 |         LPENLPCT          |         LPENCAP           |
    *     +---------------------------+---------------------------+
    *  18 |         LPENWGHT          |         LPENWAIT          |
    *     +---------------------------+---------------------------+
    *  20 |                       LPENLOAD                        |
    *     +---------------------------+---------------------------+
    *  28 |         LPENSTAT          |         LPENPTYP          |
    *     +---------------------------+---------------------------+
    *  30 |         LPENCPU           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  38 |                       LPENMSPC                        |
    *     +-------------------------------------------------------+
    *  40 |                       LPENOVHD                        |
    *     +-------------------------------------------------------+
    *  48 |                       LPENBUSY                        |
    *     +-------------------------------------------------------+
    *  50 |                       LPENOVER                        |
    *     +-------------------------------------------------------+
    *  58 |                       LPENPHYS                        |
    *     +-------------------------------------------------------+
    *  60 |                       LPENLGLD                        |
    *     +-------------------------------------------------------+
    *  68 |                       LPENVMLD                        |
    *     +-------------------------------------------------------+
    *  70 |                       LPENTCAP                        |
    *     +---------------------------+---------------------------+
    *  78 |         LPENMTDP          |         LPENGCPN          |
    *     +---------------------------+---------------------------+
    *  80 |         LPENGCPN cont'd   |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  88 |                       LPENGCPV                        |
    *     +---------------------------+---------------------------+
    *  90 |         LPENCPUH          |         LPENRSV1          |
    *     +---------------------------+---------------------------+
    *  98
    *
    *** SEGTPRC  - SEGOUT DCSS Content Data Definition

    *** SEGTMDC  - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       PARTSIZE                        |
    *     +-------------------------------------------------------+
    *   8 |                       MAXCACHE                        |
    *     +-------------------------------------------------------+
    *  10 |                       ACTCACHE                        |
    *     +-------------------------------------------------------+
    *  18 |                       FAIRSHR                         |
    *     +-------------------------------------------------------+
    *  20 |                       MDCRDRAT                        |
    *     +-------------------------------------------------------+
    *  28 |                       FULLRDHT                        |
    *     +-------------------------------------------------------+
    *  30 |                       PGINRT                          |
    *     +-------------------------------------------------------+
    *  38 |                       PGOUTRT                         |
    *     +-------------------------------------------------------+
    *  40 |                       BLKLIFE                         |
    *     +-------------------------------------------------------+
    *  48 |                       FRSHRXRT                        |
    *     +-------------------------------------------------------+
    *  50 |                       INTINSRT                        |
    *     +-------------------------------------------------------+
    *  58 |                       INVREQRT                        |
    *     +-------------------------------------------------------+
    *  60 |                       BLKINVRT                        |
    *     +-------------------------------------------------------+
    *  68 |                       IDEALFRM                        |
    *     +-------------------------------------------------------+
    *  70 |                       ACTFRL2G                        |
    *     +-------------------------------------------------------+
    *  78 |                       ACTFRG2G                        |
    *     +-------------------------------------------------------+
    *  80 |                       MINFRMS                         |
    *     +-------------------------------------------------------+
    *  88 |                       MAXFRMS                         |
    *     +-------------------------------------------------------+
    *  90 |                       PGDELRT                         |
    *     +-------------------------------------------------------+
    *  98 |                       STINVRT                         |
    *     +-------------------------------------------------------+
    *  A0 |                       MDCBIAS                         |
    *     +-------------------------------------------------------+
    *  A8 |                       IDEALXST                        |
    *     +-------------------------------------------------------+
    *  B0 |                       ACTXST                          |
    *     +-------------------------------------------------------+
    *  B8 |                       MINXST                          |
    *     +-------------------------------------------------------+
    *  C0 |                       MAXXST                          |
    *     +-------------------------------------------------------+
    *  C8 |                       PGDELXST                        |
    *     +-------------------------------------------------------+
    *  D0 |                       STINVXST                        |
    *     +-------------------------------------------------------+
    *  D8 |                       MDCBSXST                        |
    *     +-------------------------------------------------------+
    *  E0 |                       AGEXST                          |
    *     +-------------------------------------------------------+
    *  E8 |                       DASDONE                         |
    *     +-------------------------------------------------------+
    *  F0 |                       DASDABRT                        |
    *     +-------------------------------------------------------+
    *  F8 |                       DASDNELG                        |
    *     +-------------------------------------------------------+
    * 100 |                       DASDTOT                         |
    *     +-------------------------------------------------------+
    * 108 |                       NETDONE                         |
    *     +-------------------------------------------------------+
    * 110 |                       NETABRT                         |
    *     +-------------------------------------------------------+
    * 118 |                       NETNELG                         |
    *     +-------------------------------------------------------+
    * 120 |                       NETTOT                          |
    *     +-------------------------------------------------------+
    * 128 |                       MDCWRRTE                        |
    *     +-------------------------------------------------------+
    * 130 |                       MDCRDHRT                        |
    *     +-------------------------------------------------------+
    * 138
    *
    *** SEGTMDC  - SEGOUT DCSS Content Data Definition

    *** SEGTCHN  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         CHPID             |         CHMODGRP          |
    *     +---------------------------+---------------------------+
    *   8 |         CHMODGRP cont'd   |         CHMODQ            |
    *     +---------------------------+---------------------------+
    *  10 |                       CHPRCBSY                        |
    *     +-------------------------------------------------------+
    *  18 |                       CHAVGBSY                        |
    *     +-------------------------------------------------------+
    *  20 |                       CHBSY0                          |
    *     +-------------------------------------------------------+
    *  28 |                       CHBSY1                          |
    *     +-------------------------------------------------------+
    *  30 |                       CHBSY2                          |
    *     +-------------------------------------------------------+
    *  38 |                       CHBSY3                          |
    *     +-------------------------------------------------------+
    *  40 |                       CHBSY4                          |
    *     +-------------------------------------------------------+
    *  48 |                       CHBSY5                          |
    *     +-------------------------------------------------------+
    *  50 |                       CHBSY6                          |
    *     +-------------------------------------------------------+
    *  58 |                       CHBSY7                          |
    *     +-------------------------------------------------------+
    *  60 |                       CHBSY8                          |
    *     +-------------------------------------------------------+
    *  68 |                       CHBSY9                          |
    *     +-------------------------------------------------------+
    *  70
    *
    *** SEGTCHN  - SEGOUT DCSS Content Data Definition

    *** SEGTLCHN  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         LCHPID            |         LCHGRP            |
    *     +---------------------------+---------------------------+
    *   8 |         LCHGRP cont'd     |         LCHGRPQ           |
    *     +---------------------------+---------------------------+
    *  10 |         LCHSHR            |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  18 |                       LCHPRBSY                        |
    *     +-------------------------------------------------------+
    *  20 |                       LCHAVGBS                        |
    *     +-------------------------------------------------------+
    *  28 |                       LCHBSY0                         |
    *     +-------------------------------------------------------+
    *  30 |                       LCHBSY1                         |
    *     +-------------------------------------------------------+
    *  38 |                       LCHBSY2                         |
    *     +-------------------------------------------------------+
    *  40 |                       LCHBSY3                         |
    *     +-------------------------------------------------------+
    *  48 |                       LCHBSY4                         |
    *     +-------------------------------------------------------+
    *  50 |                       LCHBSY5                         |
    *     +-------------------------------------------------------+
    *  58 |                       LCHBSY6                         |
    *     +-------------------------------------------------------+
    *  60 |                       LCHBSY7                         |
    *     +-------------------------------------------------------+
    *  68 |                       LCHBSY8                         |
    *     +-------------------------------------------------------+
    *  70 |                       LCHBSY9                         |
    *     +-------------------------------------------------------+
    *  78
    *
    *** SEGTLCHN  - SEGOUT DCSS Content Data Definition

    *** SEGTFCHN  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         FCHPID            |         FCHSHR            |
    *     +---------------------------+---------------------------+
    *   8 |                       FCHBUS                          |
    *     +-------------------------------------------------------+
    *  10 |                       FCHWRK                          |
    *     +-------------------------------------------------------+
    *  18 |                       FCHDUW                          |
    *     +-------------------------------------------------------+
    *  20 |                       FCHDUR                          |
    *     +-------------------------------------------------------+
    *  28 |                       FCHLWRK                         |
    *     +-------------------------------------------------------+
    *  30 |                       FCHLDUW                         |
    *     +-------------------------------------------------------+
    *  38 |                       FCHLDUR                         |
    *     +-------------------------------------------------------+
    *  40 |                       FCHWRT                          |
    *     +-------------------------------------------------------+
    *  48 |                       FCHRD                           |
    *     +-------------------------------------------------------+
    *  50
    *
    *** SEGTFCHN  - SEGOUT DCSS Content Data Definition

    *** SEGTDCAC - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         DCACDIR           |         DCACADDR          |
    *     +---------------------------+---------------------------+
    *   8 |                       DCACLABL                        |
    *     +-------------------------------------------------------+
    *  10 |                       DCACTYP                         |
    *     +---------------------------+---------------------------+
    *  18 |         DCACPAV           |         DCACSID           |
    *     +---------------------------+---------------------------+
    *  20 |         DCACSTC           |         DCACSTF           |
    *     +---------------------------+---------------------------+
    *  28 |         DCACDPS           |         DCACDUST          |
    *     +---------------------------+---------------------------+
    *  30 |                       DCACOVIO                        |
    *     +-------------------------------------------------------+
    *  38 |                       DCACOVRD                        |
    *     +-------------------------------------------------------+
    *  40 |                       DCACOVRH                        |
    *     +-------------------------------------------------------+
    *  48 |                       DCACDWRH                        |
    *     +-------------------------------------------------------+
    *  50 |                       DCACOVIC                        |
    *     +-------------------------------------------------------+
    *  58 |                       DCACOVBC                        |
    *     +-------------------------------------------------------+
    *  60 |                       DCACNDIO                        |
    *     +-------------------------------------------------------+
    *  68 |                       DCACNRDR                        |
    *     +-------------------------------------------------------+
    *  70 |                       DCACNRDH                        |
    *     +-------------------------------------------------------+
    *  78 |                       DCACSDIO                        |
    *     +-------------------------------------------------------+
    *  80 |                       DCACSRDR                        |
    *     +-------------------------------------------------------+
    *  88 |                       DCACSRDH                        |
    *     +-------------------------------------------------------+
    *  90 |                       DCACFDIO                        |
    *     +-------------------------------------------------------+
    *  98 |                       DCACFRDR                        |
    *     +-------------------------------------------------------+
    *  A0 |                       DCACFRDH                        |
    *     +-------------------------------------------------------+
    *  A8 |                       DCACCIO                         |
    *     +-------------------------------------------------------+
    *  B0 |                       DCACSSC                         |
    *     +-------------------------------------------------------+
    *  B8 |                       DCACRNR                         |
    *     +-------------------------------------------------------+
    *  C0 |                       DCACRSR                         |
    *     +-------------------------------------------------------+
    *  C8 |                       DCACWRR                         |
    *     +-------------------------------------------------------+
    *  D0 |                       DCACPRD                         |
    *     +-------------------------------------------------------+
    *  D8 |                       DCACHTO                         |
    *     +-------------------------------------------------------+
    *  E0 |                       DCACHRD                         |
    *     +-------------------------------------------------------+
    *  E8 |                       DCACHWR                         |
    *     +-------------------------------------------------------+
    *  F0 |                       DCACHDW                         |
    *     +-------------------------------------------------------+
    *  F8 |                       DCACHCW                         |
    *     +-------------------------------------------------------+
    * 100 |                       DCACPDF                         |
    *     +-------------------------------------------------------+
    * 108 |                       DCACPCF                         |
    *     +-------------------------------------------------------+
    * 110 |                       DCACSGN                         |
    *     +-------------------------------------------------------+
    * 118 |                       DCACSGS                         |
    *     +-------------------------------------------------------+
    * 120 |                       DCACDSG                         |
    *     +-------------------------------------------------------+
    * 128 |                       DCACDFB                         |
    *     +-------------------------------------------------------+
    * 130 |                       DCACICL                         |
    *     +-------------------------------------------------------+
    * 138 |                       DCACTMO                         |
    *     +---------------------------+---------------------------+
    * 140 |         DCACCA            |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 148 |                       DCACRDRT                        |
    *     +-------------------------------------------------------+
    * 150 |                       DCACWRRT                        |
    *     +---------------------------+---------------------------+
    * 158 |         DCACBRD           |         DCACBWR           |
    *     +---------------------------+---------------------------+
    * 160
    *
    *** SEGTDCAC - SEGOUT DCSS Content Data Definition

    *** SEGTCTLU - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         CTLSID            |         CTLTYP            |
    *     +---------------------------+---------------------------+
    *   8 |     CTLTYP cont'd         |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                       CTLCST                          |
    *     +-------------------------------------------------------+
    *  18 |                       CTLAST                          |
    *     +-------------------------------------------------------+
    *  20 |                       CTLCNV                          |
    *     +-------------------------------------------------------+
    *  28 |                       CTLANV                          |
    *     +-------------------------------------------------------+
    *  30 |                       CTLCIO                          |
    *     +-------------------------------------------------------+
    *  38 |                       CTLSSC                          |
    *     +-------------------------------------------------------+
    *  40 |                       CTLBSY                          |
    *     +-------------------------------------------------------+
    *  48 |                       CTLFPT                          |
    *     +-------------------------------------------------------+
    *  50 |                       CTLDST                          |
    *     +-------------------------------------------------------+
    *  58 |                       CTLCNT                          |
    *     +-------------------------------------------------------+
    *  60 |                       CTLSRV                          |
    *     +-------------------------------------------------------+
    *  68 |                       CTLRSP                          |
    *     +-------------------------------------------------------+
    *  70 |                       CTLRNR                          |
    *     +-------------------------------------------------------+
    *  78 |                       CTLRSR                          |
    *     +-------------------------------------------------------+
    *  80 |                       CTLWRR                          |
    *     +-------------------------------------------------------+
    *  88 |                       CTLPRD                          |
    *     +-------------------------------------------------------+
    *  90 |                       CTLPDF                          |
    *     +-------------------------------------------------------+
    *  98 |                       CTLPCF                          |
    *     +-------------------------------------------------------+
    *  A0 |                       CTLHRD                          |
    *     +-------------------------------------------------------+
    *  A8 |                       CTLHWR                          |
    *     +-------------------------------------------------------+
    *  B0 |                       CTLHDW                          |
    *     +-------------------------------------------------------+
    *  B8 |                       CTLHCW                          |
    *     +-------------------------------------------------------+
    *  C0
    *
    *** SEGTCTLU - SEGOUT DCSS Content Data Definition

    *** SEGTVDSK - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       VDSUID                          |
    *     +---------------------------+---------------------------+
    *   8 |         VDSDEVNM          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                       VDSSIZE                         |
    *     +-------------------------------------------------------+
    *  18 |                       VDSLINK                         |
    *     +-------------------------------------------------------+
    *  20 |                       VDSIOS                          |
    *     +-------------------------------------------------------+
    *  28 |                       VDSSTLS                         |
    *     +-------------------------------------------------------+
    *  30 |                       VDSPRDS                         |
    *     +-------------------------------------------------------+
    *  38 |                       VDSPWRT                         |
    *     +-------------------------------------------------------+
    *  40 |                       VDSXRDS                         |
    *     +-------------------------------------------------------+
    *  48 |                       VDSXWRS                         |
    *     +-------------------------------------------------------+
    *  50 |                       VDSXMIG                         |
    *     +-------------------------------------------------------+
    *  58 |                       VDSPRES                         |
    *     +-------------------------------------------------------+
    *  60 |                       VDSPLOK                         |
    *     +-------------------------------------------------------+
    *  68 |                       VDSPXST                         |
    *     +-------------------------------------------------------+
    *  70 |                       VDSPNPS                         |
    *     +-------------------------------------------------------+
    *  78 |                       VDSNAME                         |
    *     +-------------------------------------------------------+
    *  80 |                       VDSNAME cont'd                  |
    *     +---------------------------+---------------------------+
    *  88 |     VDSNAME cont'd        |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  90 |          VDSPRIV          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  98 |                       VDSIBR                          |
    *     +-------------------------------------------------------+
    *  A0
    *
    *** SEGTVDSK - SEGOUT DCSS Content Data Definition

    *** SEGTSPLK - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       LOKNAME                         |
    *     +-------------------------------------------------------+
    *   8 |                       LOKTLCT                         |
    *     +-------------------------------------------------------+
    *  10 |                       LOKTLTM                         |
    *     +-------------------------------------------------------+
    *  18 |                       LOKTLPC                         |
    *     +-------------------------------------------------------+
    *  20 |                       LOKEXCT                         |
    *     +-------------------------------------------------------+
    *  28 |                       LOKEXTM                         |
    *     +-------------------------------------------------------+
    *  30 |                       LOKEXPC                         |
    *     +-------------------------------------------------------+
    *  38 |                       LOKSHCT                         |
    *     +-------------------------------------------------------+
    *  40 |                       LOKSHTM                         |
    *     +-------------------------------------------------------+
    *  48 |                       LOKSHPC                         |
    *     +-------------------------------------------------------+
    *  50
    *
    *** SEGTSPLK - SEGOUT DCSS Content Data Definition

    *** SEGTWAIT - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       WAITWKLD                        |
    *     +---------------------------+---------------------------+
    *   8 |         WAITACT           |         WAITRUN           |
    *     +---------------------------+---------------------------+
    *  10 |         WAITCPU           |         WAITLDG           |
    *     +---------------------------+---------------------------+
    *  18 |         WAITPGW           |         WAITIOW           |
    *     +---------------------------+---------------------------+
    *  20 |         WAITSIM           |         WAITTIW           |
    *     +---------------------------+---------------------------+
    *  28 |         WAITCFW           |         WAITSVTI          |
    *     +---------------------------+---------------------------+
    *  30 |         WAITSVEL          |         WAITSVDM          |
    *     +---------------------------+---------------------------+
    *  38 |         WAITIOA           |         WAITPACT          |
    *     +---------------------------+---------------------------+
    *  40 |         WAITLIML          |         WAITOTH           |
    *     +---------------------------+---------------------------+
    *  48 |         WAITUIQ0          |         WAITUIQ1          |
    *     +---------------------------+---------------------------+
    *  50 |         WAITUIQ2          |         WAITUIQ3          |
    *     +---------------------------+---------------------------+
    *  58 |         WAITELIG          |         WAITRSV1          |
    *     +---------------------------+---------------------------+
    *  60
    *
    *** SEGTWAIT - SEGOUT DCSS Content Data Definition

    *** SEGTCPC  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         CPCBLTYP          |         CPCBNUM           |
    *     +---------------------------+---------------------------+
    *   8 |         CPCBWT            |         CPCBDED           |
    *     +---------------------------+---------------------------+
    *  10 |         CPCBLPTM          |         CPCBOVHD          |
    *     +---------------------------+---------------------------+
    *  18 |         CPCBMGTM          |         CPCBSUM           |
    *     +---------------------------+---------------------------+
    *  20
    *
    *** SEGTCPC  - SEGOUT DCSS Content Data Definition

    *** SEGTSSI  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         SSISLOT           |         SSISYSID          |
    *     +---------------------------+---------------------------+
    *   8 |         SSISYSID cont'd   |         SSIRES1           |
    *     +---------------------------+---------------------------+
    *  10
    *
    *** SEGTSSI  - SEGOUT DCSS Content Data Definition

    *** SEGTSCSI - SEGOUT DCSS Content Data Definition
    *     +---------------------------+---------------------------+
    *   0 |         SCZDVNO           |         SCZBYTS           |
    *     +---------------------------+---------------------------+
    *   8 |                       SCZKBRT                         |
    *     +-------------------------------------------------------+
    *  10 |                       SCZXFRT                         |
    *     +-------------------------------------------------------+
    *  18 |                       SCZSKRT                         |
    *     +---------------------------+---------------------------+
    *  20 |         SCZPCCT           |         SCZEATT           |
    *     +---------------------------+---------------------------+
    *  28 |         SCZBKRD           |         SCZBKWR           |
    *     +---------------------------+---------------------------+
    *  30 |                       SCZBKRT                         |
    *     +-------------------------------------------------------+
    *  38 |                       SCZBKWT                         |
    *     +---------------------------+---------------------------+
    *  40 |         SCZP1RD           |         SCZP1WR           |
    *     +---------------------------+---------------------------+
    *  48 |                       SCZP1RT                         |
    *     +-------------------------------------------------------+
    *  50 |                       SCZP1WT                         |
    *     +---------------------------+---------------------------+
    *  58 |         SCZP2RD           |         SCZP2WR           |
    *     +---------------------------+---------------------------+
    *  60 |                       SCZP2RT                         |
    *     +-------------------------------------------------------+
    *  68 |                       SCZP2WT                         |
    *     +---------------------------+---------------------------+
    *  70 |         SCZP3RD           |         SCZP3WR           |
    *     +---------------------------+---------------------------+
    *  78 |                       SCZP3RT                         |
    *     +-------------------------------------------------------+
    *  80 |                       SCZP3WT                         |
    *     +---------------------------+---------------------------+
    *  88 |         SCZP4RD           |         SCZP4WR           |
    *     +---------------------------+---------------------------+
    *  90 |                       SCZP4RT                         |
    *     +-------------------------------------------------------+
    *  98 |                       SCZP4WT                         |
    *     +---------------------------+---------------------------+
    *  A0 |         SCZP5RD           |         SCZP5WR           |
    *     +---------------------------+---------------------------+
    *  A8 |                       SCZP5RT                         |
    *     +-------------------------------------------------------+
    *  B0 |                       SCZP5WT                         |
    *     +---------------------------+---------------------------+
    *  B8 |         SCZP6RD           |         SCZP6WR           |
    *     +---------------------------+---------------------------+
    *  C0 |                       SCZP6RT                         |
    *     +-------------------------------------------------------+
    *  C8 |                       SCZP6WT                         |
    *     +---------------------------+---------------------------+
    *  D0 |         SCZP7RD           |         SCZP7WR           |
    *     +---------------------------+---------------------------+
    *  D8 |                       SCZP7RT                         |
    *     +-------------------------------------------------------+
    *  E0 |                       SCZP7WT                         |
    *     +---------------------------+---------------------------+
    *  E8 |         SCZP8RD           |         SCZP8WR           |
    *     +---------------------------+---------------------------+
    *  F0 |                       SCZP8RT                         |
    *     +-------------------------------------------------------+
    *  F8 |                       SCZP8WT                         |
    *     +---------------------------+---------------------------+
    * 100
    *
    *** SEGTSCSI - SEGOUT DCSS Content Data Definition

    *** SEGTLGR  - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |         LGREVTT           |         LGRISSR           |
    *     +---------------------------+---------------------------+
    *   8 |         LGRISSR cont'd    |         LGRUSER           |
    *     +---------------------------+---------------------------+
    *  10 |         LGRUSER cont'd    |         LGRSRC            |
    *     +---------------------------+---------------------------+
    *  18 |         LGRSRC cont'd     |         LGRDEST           |
    *     +---------------------------+---------------------------+
    *  20 |         LGRDEST cont'd    |         LGRFINCD          |
    *     +---------------------------+---------------------------+
    *  28 |                       LGRRELOT                        |
    *     +-------------------------------------------------------+
    *  30 |                       LGRQUIES                        |
    *     +-------------------------------------------------------+
    *  38 |                       LGRPASS                         |
    *     +-------------------------------------------------------+
    *  40 |                       LGRPG1P                         |
    *     +-------------------------------------------------------+
    *  48 |                       LGRPGIP                         |
    *     +-------------------------------------------------------+
    *  50 |                       LGRPGN1P                        |
    *     +-------------------------------------------------------+
    *  58 |                       LGRPGNP                         |
    *     +-------------------------------------------------------+
    *  60 |                       LGRPGTOT                        |
    *     +-------------------------------------------------------+
    *  68 |                       LGRVDEV                         |
    *     +-------------------------------------------------------+
    *  70 |                       LGRAIOS                         |
    *     +-------------------------------------------------------+
    *  78 |                       LGRCNQDI                        |
    *     +-------------------------------------------------------+
    *  80 |                       LGRCQDIO                        |
    *     +---------------------------+---------------------------+
    *  88 |         LGRROPT1          |         LGRROPT2          |
    *     +---------------------------+---------------------------+
    *  90 |         LGRSOPT1          |         LGRRES1           |
    *     +---------------------------+---------------------------+
    *  98
    *
    *** SEGTLGR  - SEGOUT DCSS Content Data Definition

    *** SEGTCPUP - SEGOUT DCSS Content Data Definition
    *
    *     +---------------------------+---------------------------+
    *   0 |                       CPUPPOOL                        |
    *     +---------------------------+---------------------------+
    *   8 |         CPUPTYPE          |         CPUPAFF           |
    *     +---------------------------+---------------------------+
    *  10 |                       CPUPLVAL                        |
    *     +---------------------------+---------------------------+
    *  18 |         CPUPLTYP          |         CPUPMEMS          |
    *     +---------------------------+---------------------------+
    *  20 |                       CPUPCPU                         |
    *     +---------------------------+---------------------------+
    *  28 |                       CPUPLRAT                        |
    *     +---------------------------+---------------------------+
    *  30 |                       CPUPPUSE                        |
    *     +---------------------------+---------------------------+
    *  38 |                       CPUPMXCR                        |
    *     +---------------------------+---------------------------+
    *  40
    *** SEGTCPUP - SEGOUT DCSS Content Data Definition

    *** SEGTADAP - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       DAPEYEC                         |
    *     +-------------------------------------------------------+
    *   8 |                       DAPSYSID                        |
    *     +-------------------------------------------------------+
    *  10 |                       DAPSTAMP                        |
    *     +-------------------------------------------------------+
    *  18 |                       DAPLPARN                        |
    *     +---------------------------+---------------------------+
    *  20 |         SYSDOFF           |         SYSDCNT           |
    *     +---------------------------+---------------------------+
    *  28 |         WKLDOFF           |         WKLDCNT           |
    *     +---------------------------+---------------------------+
    *  30 |         LPADOFF           |         LPADCNT           |
    *     +---------------------------+---------------------------+
    *  38 |         CPODOFF           |         CPODCNT           |
    *     +---------------------------+---------------------------+
    *  40 |         DEVDOFF           |         DEVDCNT           |
    *     +---------------------------+---------------------------+
    *  48 |         HIPDOFF           |         HIPDCNT           |
    *     +---------------------------+---------------------------+
    *  50 |         VSWDOFF           |         VSWDCNT           |
    *     +---------------------------+---------------------------+
    *  58 |         TCPDOFF           |         TCPDCNT           |
    *     +---------------------------+---------------------------+
    *  60 |         NUSRDOFF          |         NUSRDCNT          |
    *     +---------------------------+---------------------------+
    *  68 |         LINXDOFF          |         LINXDCNT          |
    *     +---------------------------+---------------------------+
    *  70 |         LPENDOFF          |         LPENDCNT          |
    *     +---------------------------+---------------------------+
    *  78 |         MDCDOFF           |         MDCDCNT           |
    *     +---------------------------+---------------------------+
    *  80 |         CHANDOFF          |         CHANDCNT          |
    *     +---------------------------+---------------------------+
    *  88 |         LCHNDOFF          |         LCHNDCNT          |
    *     +---------------------------+---------------------------+
    *  90 |         FCHNDOFF          |         FCHNDCNT          |
    *     +---------------------------+---------------------------+
    *  98 |         DCANDOFF          |         DCANDCNT          |
    *     +---------------------------+---------------------------+
    *  A0 |         CTLNDOFF          |         CTLNDCNT          |
    *     +---------------------------+---------------------------+
    *  A8 |         VDKNDOFF          |         VDKNDCNT          |
    *     +---------------------------+---------------------------+
    *  B0 |         SPNNDOFF          |         SPNNDCNT          |
    *     +---------------------------+---------------------------+
    *  B8 |         WAINDOFF          |         WAINDCNT          |
    *     +---------------------------+---------------------------+
    *  C0 |         SYS2DOFF          |         SYS2DCNT          |
    *     +---------------------------+---------------------------+
    *  C8 |         CPCDOFF           |         CPCDCNT           |
    *     +---------------------------+---------------------------+
    *  D0 |         SSIDOFF           |         SSIDCNT           |
    *     +---------------------------+---------------------------+
    *  D8 |         SCSIDOFF          |         SCSIDCNT          |
    *     +---------------------------+---------------------------+
    *  E0 |         LGRDOFF           |         LGRDCNT           |
    *     +---------------------------+---------------------------+
    *  E8 |         CPUPDOFF          |         CPUPDCNT          |
    *     +---------------------------+---------------------------+
    *  F0 |         DATAEND           |         DAPSSINM          |
    *     +---------------------------+---------------------------+
    *  FC |         DAPSSINM cont'd   |         RESRVED1          |
    *     +---------------------------+---------------------------+
    * 100
    *
    *** SEGTADAP - SEGOUT DCSS Content Data Definition

    *** SEGTASEG - SEGOUT DCSS Content Data Definition
    *
    *     +-------------------------------------------------------+
    *   0 |                       PTKEYEC                         |
    *     +-------------------------------------------------------+
    *   8 |                       PTKVERS                         |
    *     +-------------------------------------------------------+
    *  10 |                       PTKLEVEL                        |
    *     +-------------------------------------------------------+
    *  18 |                       ZVMVERS                         |
    *     +-------------------------------------------------------+
    *  20 |                       ZVMLEVEL                        |
    *     +---------------------------+---------------------------+
    *  28 |         INTRVLTM          |        UPDTIMEA           |
    *     +---------------------------+---------------------------+
    *  30 |         UPDTIMEA cont'd   |         UPDSTRTA          |
    *     +---------------------------+---------------------------+
    *  38 |         UPDENDA           |         LOCKDATA          |
    *     +---------------------------+---------------------------+
    *  40 |         DAPAOFF           |         DAPACNT           |
    *     +---------------------------+---------------------------+
    *  48 |                       UPDTIMEB                        |
    *     +---------------------------+---------------------------+
    *  50 |         UPDSTRTB          |         UPDENDB           |
    *     +---------------------------+---------------------------+
    *  58 |         LOCKDATB          |         DAPBOFF           |
    *     +---------------------------+---------------------------+
    *  60 |         DAPBCNT           |         SEGUSER           |
    *     +---------------------------+---------------------------+
    *  68 |         SEGUSER cont'd    |         SEGFREE1          |
    *     +---------------------------+---------------------------+
    *  70
    *
    *** SEGTASEG - SEGOUT DCSS Content Data Definition

#### SEGTSYS Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    ACTBLKPL       0088
    ACTCACHE       0010
    ACTFRG2G       0078
    ACTFRL2G       0070
    ACTUSER        0000
    ACTXST         00B0
    ADDR           0000
    AGEXST         00E0
    ALLOCCNT       0004
    APPLDLEN       0170 00000368
    ARPRECV        0070
    ARPREPLY       0078
    ARPREQXM       0080
    AVAILSLT       0008
    AVGUSER        0004
    AVLFRAMS       0008
    AVLFRA2G       0010
    AVLHGHTH       0018
    AVLHGH2G       0020
    AVLLMEAN       0028
    AVLLME2G       0030
    AVLLOWTH       0038
    AVLLOW2G       0040
    AVLWAIT        0048
    BADPACK        0120
    BLKINVRT       0060
    BLKLIFE        0040
    BLKREAD        00E8
    BLKWRITE       00F0
    BSDSOCKB       00B8
    BUFFREE        00A0
    BYTESREC       0038
    BYTEXMIT       0040
    BYTRECV        0110
    BYTSENT        0118
    CACHUSED       00A8
    CHANDCNT       0084
    CHANDOFF       0080
    CHANPATH       0000
    CHAVGBSY       0018
    CHBSY0         0020
    CHBSY1         0028
    CHBSY2         0030
    CHBSY3         0038
    CHBSY4         0040
    CHBSY5         0048
    CHBSY6         0050
    CHBSY7         0058
    CHBSY8         0060
    CHBSY9         0068
    CHMODGRP       0004
    CHMODQ         000C
    CHNDLEN        0070 00000112
    CHPID          0000
    CHPRCBSY       0010
    CLNBLKPL       0090
    CONNOACP       0010
    CONNOFAI       0018
    CONNOINI       0008
    CONNRSET       0020
    CONNTIME       0010
    CPBUSY         004C
    CPCBDED        000C
    CPCDLEN        0020 00000032
    CPCDCNT        00CC
    CPCDOFF        00C8
    CPCBLPTM       0010
    CPCBLTYP       0000
    CPCBMGTM       0018
    CPCBNUM        0004
    CPCBOVHD       0014
    CPCBSUM        001C
    CPCBWT         0008
    CPODCNT        003C
    CPODLEN        0038 00000056
    CPODOFF        0038
    CPPCT          0008
    CPRESRV1       000C
    CPRESRV2       002C
    CPSECS         0010
    CPUBUSY        0050
    CPUNUM         0054
    CPUPAFF        000C
    CPUPCT         0018
    CPUPCPU        0020
    CPUPDCNT       00EC
    CPUPDLEN       0040 00000064
    CPUPDOFF       00E8
    CPUPLRAT       0028
    CPUPLTYP       0018
    CPUPMEMS       001C
    CPUPMXCR       0038
    CPUPLVAL       0010
    CPUPOOL        0150
    CPUPPOOL       0000
    CPUPPUSE       0030
    CPUPTYPE       0008
    CPUSECS        0020
    CPXSTORE       0198
    CTLANV         0028
    CTLAST         0018
    CTLBSY         0040
    CTLCIO         0030
    CTLCNT         0058
    CTLCNV         0020
    CTLCST         0010
    CTLDST         0050
    CTLFPT         0048
    CTLHCW         00B8
    CTLHDW         00B0
    CTLHRD         00A0
    CTLHWR         00A8
    CTLNDCNT       00A4
    CTLNDOFF       00A0
    CTLPCF         0098
    CTLPDF         0090
    CTLPRD         0088
    CTLRNR         0070
    CTLRSP         0068
    CTLRSR         0078
    CTLSID         0000
    CTLSRV         0060
    CTLSSC         0038
    CTLTYP         0004
    CTLUDLEN       00C0 00000192
    CTLWRR         0080
    DAPACNT        0044
    DAPAOFF        0040
    DAPBCNT        0060
    DAPBOFF        005C
    DAPEYEC        0000
    DAPLEN         0100 00000256
    DAPLPARN       0018
    DAPSSIMN       00EC
    DAPSTAMP       0010
    DAPSYSID       0008
    DASDABRT       00F0
    DASDBUSY       0018
    DASDNELG       00F8
    DASDONE        00E8
    DASDQUE        0020
    DASDTOT        0100
    DASIOREQ       0028
    DATAEND        00F0
    DCACADDR       0004
    DCACBRD        0158
    DCACBWR        015C
    DCACCAFG       0140
    DCACCIO        00A8
    DCACDFB        0128
    DCACDIR        0000
    DCACDLEN       0160 00000352
    DCACDPS        0028
    DCACDSG        0120
    DCACDUST       002C
    DCACDWRH       0048
    DCACFDIO       0090
    DCACFRDH       00A0
    DCACFRDR       0098
    DCACHCW        00F8
    DCACHDW        00F0
    DCACHRD        00E0
    DCACHTO        00D8
    DCACHWR        00E8
    DCACICL        0130
    DCACLABL       0008
    DCACNDIO       0060
    DCACNRDH       0070
    DCACNRDR       0068
    DCACOVBC       0058
    DCACOVIC       0050
    DCACOVIO       0030
    DCACOVRD       0038
    DCACOVRH       0040
    DCACPAV        0018
    DCACPCF        0108
    DCACPDF        0100
    DCACPRD        00D0
    DCACRDRT       0148
    DCACRNR        00B8
    DCACRSR        00C0
    DCACSDIO       0078
    DCACSGN        0110
    DCACSGS        0118
    DCACSID        001C
    DCACSRDH       0088
    DCACSRDR       0080
    DCACSSC        00B0
    DCACSTC        0020
    DCACSTF        0024
    DCACTMO        0138
    DCACTYP        0010
    DCACWRR        00C8
    DCACWRRT       0150
    DCANDCNT       009C
    DCANDOFF       0098
    DEVADDR        0000
    DEVADDRX       0000
    DEVDCNT        0044
    DEVDLEN        0058 00000088
    DEVDOFF        0040
    DEVIOSCS       0058
    DEVIOSEC       0030
    DEVTYPE        0004
    DEVTYPEX       0010
    DIALUSER       005C
    DISCPCKD       0040
    DISCTIME       0038
    DPAFRAMS       0060
    DSCNFAIL       0068
    ELIGUSER       0070
    EMPCONTG       00D0
    EMPCONTL       00C0
    EMPSINGG       00C8
    EMPSINGL       00B8
    ENDCYL         001C
    ENVLARGE       00A0
    ENVREGPL       0098
    EXPUSER1       0078
    EXPUSER2       0080
    EXPUSER3       0088
    EXTFRAMS       0090
    EXTWAIT        0098
    FAILRBFR       0030
    FAILRBFS       0018
    FAILSOTH       0038
    FAIRSHR        0018
    FCHBUS         0008
    FCHDUR         0020
    FCHDUW         0018
    FCHLDUR        0038
    FCHLDUW        0030
    FCHLWRK        0028
    FCHNDCNT       0094
    FCHNDLEN       0050 00000080
    FCHNDOFF       0090
    FCHPID         0000
    FCHRD          0048
    FCHSHR         0004
    FCHWRK         0010
    FCHWRT         0040
    FIXPAGPL       00F0
    FRSHRXRT       0048
    FSTORSUB       0138
    FSTPGIRT       0030
    FSTRREQS       00A0
    FSTRRETS       00A8
    FULLRDHT       0028
    GROUP          0090
    HIPDCNT        004C
    HIPDLEN        0040 00000064
    HIPDOFF        0048
    IDEALFRM       0068
    IDEALXST       00A8
    IDLE           0048
    INTERFCS       00F8
    INTINSRT       0050
    INTRVLTM       0028
    INVREQRT       0058
    IOWAIT         0040
    IRQ            0030
    KERNLCPU       0020
    LCHAVGBS       0020
    LCHBSY0        0028
    LCHBSY1        0030
    LCHBSY2        0038
    LCHBSY3        0040
    LCHBSY4        0048
    LCHBSY5        0050
    LCHBSY6        0058
    LCHBSY7        0060
    LCHBSY8        0068
    LCHBSY9        0070
    LCHGRP         0004
    LCHGRPQ        000C
    LCHNDCNT       008C
    LCHNDLEN       0078 00000120
    LCHNDOFF       0088
    LCHPID         0000
    LCHPRBSY       0018
    LCHSHR         0010
    LGRAIOS        0070
    LGRCNQDI       0078
    LGRCQDIO       0080
    LGRDCNT        00E4
    LGRDEST        001C
    LGRDLEN        0098 00000152
    LGRDOFF        00E0
    LGREVTT        0000
    LGRFINCD       0024
    LGRISSR        0004
    LGRPASS        0038
    LGRPG1P        0040
    LGRPGIP        0048
    LGRPGN1P       0050
    LGRPGNP        0058
    LGRPGTOT       0060
    LGRQUIES       0030
    LGRRELOT       0028
    LGRRES1        0094
    LGRROPT1       0088
    LGRROPT2       008C
    LGRSOPT1       0090
    LGRSRC         0014
    LGRUSER        000C
    LGRVDEV        0068
    LINXDCNT       006C
    LINXDOFF       0068
    LNGPGIRT       0038
    LNGPGORT       0040
    LNXFLAG        0160
    LNXPRDID       0150
    LNXTIME        0168
    LOCKDATA       003C
    LOCKDATB       0058
    LOCKPAGS       0148
    LOKEXCT        0020
    LOKEXPC        0030
    LOKEXTM        0028
    LOKNAME        0000
    LOKSHCT        0038
    LOKSHPC        0048
    LOKSHTM        0040
    LOKTLCT        0008
    LOKTLPC        0018
    LOKTLTM        0010
    LPADCNT        0034
    LPADLEN        0090 00000144
    LPADOFF        0030
    LPARBSYS       00B0
    LPARBUSY       0010
    LPARCAP        005C
    LPARGCPN       0080
    LPARGCPV       0088
    LPARLGLD       0060
    LPARLOAD       0018
    LPARLPCT       0020
    LPARMSPC       0028
    LPARMTDP       007C
    LPARNAME       0004
    LPARNUM        0000
    LPAROVER       0030
    LPAROVHD       0038
    LPARPTYP       0070
    LPARSTAT       0040
    LPARTCAP       0074
    LPARUPID       0058
    LPARVMLD       0068
    LPARWAIT       0044
    LPARWGHT       0048
    LPENAME        0004
    LPENBUSY       0048
    LPENCAP        0014
    LPENCPU        0030
    LPENCPUH       0090
    LPENDCNT       0074
    LPENDOFF       0070
    LPENGCPN       007C
    LPENGCPV       0088
    LPENLGLD       0060
    LPENLOAD       0020
    LPENLPCT       0010
    LPENMSPC       0038
    LPENMTDP       0078
    LPENOVER       0050
    LPENOVHD       0040
    LPENPHYS       0058
    LPENPTYP       002C
    LPENRSV1       0094
    LPENSTAT       0028
    LPENTCAP       0070
    LPENUM         0000
    LPENUPID       000C
    LPENVMLD       0068
    LPENWAIT       001C
    LPENWGHT       0018
    LUSERID        0000
    MAXCACHE       0008
    MAXIBUFQ       0068
    MAXOBUFQ       0070
    MDCBIAS        00A0
    MDCBSXST       00D8
    MDCDCNT        007C
    MDCDLEN        0138 00000312
    MDCDOFF        0078
    MDCRDHRT       0130
    MDCRDRAT       0020
    MDCWRRTE       0128
    MAXFRMS        0088
    MAXXST         00C0
    MIGOBLKF       0058
    MINFRMS        0080
    MINXST         00B8
    NETABRT        0110
    NETDONE        0108
    NETNELG        0118
    NETTOT         0120
    NICECPU        0028
    NSPBUFF        0130
    NSPLINX        0138
    NTRVRATE       00B8
    NUSRDCNT       0064
    NUSRDLEN       0078 00000120
    NUSRDOFF       0060
    OFFSTORF       0120
    PAGERATE       00C0
    PAGERATW       0040
    PAGETYPE       0018
    PAGEWRRT       0048
    PAGINDEX       00C8
    PAGREADS       0048
    PAGSSCH        0060
    PAGSTOR        0158
    PAGWRTS        0050
    PARTSIZE       0000
    PCTPAGE        00CC
    PCTSPOL        00D0
    PCTTDSK        00D4
    PENDTIME       0040
    PERCHIGH       0090
    PERCMAIN       0080
    PERCSWAP       00B8
    PERFULL        0020
    PGALLOC        00D0
    PGDELRT        0090
    PGDELXST       00C8
    PGFTMAJ        00D8
    PGFTMIN        00E0
    PGINRT         0030
    PGMVBL2G       0028
    PGOUTRT        0038
    PGRDBLKF       0050
    PGWRBLKF       0054
    PHYSBUSY       0050
    PKTRECV        0100
    PKTSENT        0108
    PROCDLEN       0098 00000152
    PTKEYEC        0000
    PTKLEVEL       0010
    PTKVERS        0008
    QSV            000C
    RAWBLKIP       00A8
    RCVBYTES       0030
    RCVPCKTS       0038
    READREQ        0028
    REGBUFPL       00D0
    RESELWAT       00D8
    RESPAGES       0058
    RESPAG2G       0060
    RESRVED1       00F4
    RESVSTOR       0178
    RUNABLE        0050
    RUN1MIN        0060
    RUN15MIN       0070
    RUN5MIN        0068
    SACBLKPL       00E8
    SCSIDCNT       00DC
    SCSIDLEN       0100 00000256
    SCSIDOFF       00D8
    SCZBKRD        0028
    SCZBKRT        0030
    SCZBKWR        002C
    SCZBKWT        0038
    SCZBYTS        0004
    SCZDVNO        0000
    SCZEATT        0024
    SCZKBRT        0008
    SCZP1RD        0040
    SCZP1RT        0048
    SCZP1WR        0044
    SCZP1WT        0050
    SCZP2RD        0058
    SCZP2RT        0060
    SCZP2WR        005C
    SCZP2WT        0068
    SCZP3RD        0070
    SCZP3RT        0078
    SCZP3WR        0074
    SCZP3WT        0080
    SCZP4RD        0088
    SCZP4RT        0090
    SCZP4WR        008C
    SCZP4WT        0098
    SCZP5RD        00A0
    SCZP5RT        00A8
    SCZP5WR        00A4
    SCZP5WT        00B0
    SCZP6RD        00B8
    SCZP6RT        00C0
    SCZP6WR        00BC
    SCZP6WT        00C8
    SCZP7RD        00D0
    SCZP7RT        00D8
    SCZP7WR        00D4
    SCZP7WT        00E0
    SCZP8RD        00E8
    SCZP8RT        00F0
    SCZP8WR        00EC
    SCZP8WT        00F8
    SCZPCCT        0020
    SCZSKRT        0018
    SCZXFRT        0010
    SEGFREE1       006C
    SEGLEN         0070 00000112
    SEGSRCVE       0060
    SEGSRECV       0048
    SEGSRXMI       0058
    SEGSXMIR       0068
    SEGSXMIT       0050
    SEGUSER        0064
    SERVTIME       0048
    SESSTIME       0028
    SHARED         0098
    SHARSTOR       0130
    SHRD           0004
    SINGFLTS       00E0
    SMCR2GDC       00A0
    SMCRCT2G       00B0
    SMCRFRQW       00A8
    SMLBUFPL       00D8
    SOCKBLKL       00B0
    SOFTIRQ        0038
    SPLKDLEN       0050 00000080
    SPNNDCNT       00B4
    SPNNDOFF       00B0
    SPRDRATE       0068
    SPWRRATE       0070
    SRVRNAME       0000
    SRVRNAMU       0000
    SSIDCNT        00D4
    SSIDLEN        0010 00000016
    SSIDOFF        00D0
    SSIRES1        000C
    SSISLOT        0000
    SSISYSID       0004
    SSTORUTL       0140
    STARTCYL       0024
    STBYSTOR       0170
    STEALTM        0148
    STINVRT        0098
    STINVXST       00D0
    STORSIZE       0068
    STORUTIL       0160
    STRAGESZ       0080
    STRRSDMX       0098
    STRRSVPG       0090
    STRAGINC       0088
    SWAPIN         00C0
    SWAPOUT        00C8
    SYSDCNT        0024
    SYS2DCNT       00C4
    SYS2DLEN       00D8 00000216
    SYS2DOFF       00C0
    SYSDLEN        01C0 00000448
    SYSDOFF        0020
    SYSDPAP        00E8
    SYSITR         00F0
    SYSSTORF       0128
    TCPBLKPL       00C0
    TCPCSESS       0010
    TCPDCNT        005C
    TCPDLEN        00F8 00000248
    TCPDOFF        0058
    TIMEOUT        0010
    TIMESESS       0020
    TNYBUFPL       00E0
    TOTCPU         0010
    TOTHIGH        0088
    TOTMAIN        0078
    TOTPROC        0058
    TOTREAL        0078
    TOTSEGS        0058
    TOTSTOR        0118
    TOTSWAP        00B0
    TOTTCPIN       0028
    TOTTCPOU       0030
    TOTUDPIN       0038
    TOTUPDOU       0040
    TOTUSLOT       0028
    TOTXSTAV       0180
    TOTXSTCP       0190
    TOTXSTUS       0188
    TRIPTSTH       0048
    TRIPTVAR       0050
    TRTABSZ        0150
    TRVRATE        00F8
    TSKWFRCT       0164
    TSKWPGRT       0168
    TVRATIO        0100
    UACKSEGS       0060
    UDPBLKPL       00C8
    UDPCSESS       0018
    UPDENDA        0038
    UPDENDB        0054
    UPDSTRTA       0034
    UPDSTRTB       0050
    UPDTIMEA       002C
    UPDTIMEB       0048
    USERCPU        0018
    USERID         0004
    USERNAME       0008
    USERQ          0108
    VDKNDCNT       00AC
    VDKNDOFF       00A8
    VDSDEVNM       0008
    VDSIBR         0098
    VDSIOS         0020
    VDSKDLEN       00A0 00000160
    VDSKMPG        0020
    VDSKMSF        0010
    VDSKSYSL       0000
    VDSKUSRL       0008
    VDSKXSF        0018
    VDSLINK        0018
    VDSNAME        0078
    VDSPLOK        0060
    VDSPNPS        0070
    VDSPRDS        0030
    VDSPRES        0058
    VDSPRIV        0090
    VDSPWRT        0038
    VDSPXST        0068
    VDSSIZE        0010
    VDSSTLS        0028
    VDSUID         0000
    VDSXMIG        0050
    VDSXRDS        0040
    VDSXWRS        0048
    VIRTCPU        0008
    VIRTPCT        0030
    VIRTSECS       0038
    VLLID          0048
    VOLSER         0050
    VOLSERX        0030
    VSEVIBF        0128
    VSEVIQO        0130
    VSEVLAR        0120
    VSEVLAX        0118
    VSEVLDE        00E0
    VSEVLIN        00D0
    VSEVLVL        0148
    VSEVMKR        0108
    VSEVMRX        0100
    VSEVMTO        0110
    VSEVMTX        00F8
    VSEVOBF        0138
    VSEVOQO        0140
    VSEVREQ        00D8
    VSEVRXD        00F0
    VSEVTXD        00E8
    VSGBLPA        016C
    VSGBMFS        0168
    VSGBPBC        0164
    VSGBPBR        015C
    VSGBPBS        0160
    VSGCONF        0158
    VSGVGRP        0078
    VSGVIPA        0091
    VSGVISO        0154
    VSGVLAY        00C8
    VSGVMAC        0080
    VSGVMGI        00BE
    VSGVOPN        0150
    VSPCI          0070
    VSPCR          0068
    VSRED          0058
    VSSYN          0060
    VSWDCNT        0054
    VSWDLEN        0178 00000376
    VSWDOFF        0050
    VSWRES1        0174
    VSWRT          0050
    WAINDCNT       00BC
    WAINDOFF       00B8
    WAITACT        0008
    WAITCFW        0028
    WAITCPU        0010
    WAITDLEN       0060 00000096
    WAITELIG       0058
    WAITING        0054
    WAITIOA        0038
    WAITIOP        010C
    WAITIOW        001C
    WAITLDG        0014
    WAITLIML       0040
    WAITOTH        0044
    WAITPACT       003C
    WAITPAGP       0110
    WAITPGW        0018
    WAITRSV1       0058
    WAITRUN        000C
    WAITSIM        0020
    WAITSVDM       0034
    WAITSVEL       0030
    WAITSVTI       002C
    WAITTIW        0024
    WAITUIQ0       0048
    WAITUIQ1       004C
    WAITUIQ2       0050
    WAITUIQ3       0054
    WAITWKLD       0000
    WKLDACTV       0130
    WKLDAVIO       0118
    WKLDB2G        00B0
    WKLDCNT        002C
    WKLDDAIO       0110
    WKLDDASD       00E8
    WKLDDI98       0120
    WKLDDSOW       00A0
    WKLDLEN        0158 00000344
    WKLDMDCI       0148
    WKLDOFF        0028
    WKLDPGLG       00E0
    WKLDPGLK       00D8
    WKLDPGST       00A8
    WKLDRVPG       00D0
    WKLDSHR        00F0
    WKLDSHRM       00F8
    WKLDSIO        0108
    WKLDSPGR       0140
    WKLDSPGS       0138
    WKLDTVRT       0100
    WKLDURIO       0128
    WKLDXMG        00C8
    WKLDXRD        00B8
    WKLDXWR        00C0
    WKLXATT        0070
    WKLXMOV        0078
    WKLXPAG        0080
    WKRESV1        009C
    WKVCPU         0098
    WORKLOAD       0000
    WRITEREQ       0030
    WSS            0088
    XFERDUNI       0028
    XFERMSGS       0020
    XFERTDUN       0010
    XFERTMSG       0008
    XMITBYTS       0018
    XMITCOLL       0140
    XMITERR        0128
    XMITPCKD       0028
    XMITPCKT       0020
    XSTALLOC       01A8
    XSTBLKAG       01B0
    XSTBLKMG       01B8
    XSTMIGLW       01A0
    ZVMLEVEL       0020
    ZVMVERS        0018

This information is based on z/VM V7R2.0. Last updated on 19 August 2021 at 10:27:00 EDT.
Copyright IBM Corporation, 2006, 2021