RSSBK | Back to Index page

| Prolog Control Block Contents RSSBK DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

RSSBK Prolog | Top of page

     NAME       : HCPRSSBK
     DESCRIPTION: RECORDING SYSTEM SERVICE BLOCK
     DSECT      : RSSBK
     FUNCTION   : MAPS OUT THE HEADER OF SYSTEM RECORDS ON THE
                  RECORDING QUEUE.
     LOCATED BY : RTHQUE
                  RSSNEXT CHAINED
     DELETED BY : HCPREC
     RELOCATION CONSIDERATIONS : None
     COMPATIBILITY AND MIGRATION CONCERNS : This control block gets checkpointed during SHUTDOWN and
                  will be read back in during a WARM start.  Therefore, if
                  the format of the block changes due to service being
                  applied before the warm start, code should be in place to
                  distinguish between the old and new format.  (See the
                  note below describing the RSSVERS field.)

RSSBK Control Block Content | Top of page

     RSSBK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      RSSBK          RECORDING SYSTEM SERVICE BLOCK
    0000    0 Address      4 RSSNEXT        Pointer to next RSSBK
    0004    4 Signed       2 RSSUSCNT       SYSTEM RECORD USE COUNT
    0006    6 Signed       2 RSSVN00M (0)   PLACE HOLDER (VERSION 00 INFO)
    0006    6 Signed       2 *              RESERVED
    0008    8 Bitstring    1 *              RESERVED
    0009    9 Bitstring    1 RSSRID         SYSTEM RECORD ID
              00000001       RSSRACNT       X'01' RSSRACNT Accounting record
              00000002       RSSRIOER       X'02' RSSRIOER EREP (LOGREC)
                                            record
              00000003       RSSRSYMP       X'03' RSSRSYMP Sympton record
              00000004       RSSRCNFG       X'04' RSSRCNFG Configuration
                                            record
              000000FF       RSSRTAB        X'FF' RSSRTAB Recording table (if
                                            set block mapped by the RTHBK not
                                            the RSSBK, RSSRID must remain at
                                            the same offset as RTHRID)
    000A   10 Signed       2 RSSFRESZ       RSSBK BLOCK SIZE IN DOUBLE WORDS
    000C   12 Bitstring    1 RSSFLAG        FLAGS DEFINED FOR RECORDING
                                            SYSTEM SERVICES
              1... ....      RSSRINIT       X'80' RSSRINIT RECORD INITIALIZED
                                            TO RECORDING TABLE
              .1.. ....      RSSRINC        X'40' RSSRINC RECORD INCOMPLETE
              ..1. ....      RSSNOMON       X'20' RSSNOMON Record not
                                            monitored by Free Storage Limit
                                            Detection function NOTES : The
                                            following field is used to
                                            indicate when the RSSBK format
                                            has changed and what that change
                                            was due to. Any code defined here
                                            should be checked in HCPRECKP
                                            when old format RSSBKs are read
                                            from the checkpoint cylinders.
                                            The old format RSSBKs should then
                                            be updated appropriately to the
                                            new format. Code should also be
                                            added to HCPRIUCF and HCPRECRI to
                                            set the code for any RSSBKs that
                                            are being newly created AFTER the
                                            format change. A new code should
                                            only need to be defined here when
                                            a change to the RSSBK causes it
                                            to be incompatible with a
                                            previous format (as in the case
                                            of the RSSMSGN field being
                                            expanded from a halfword to a
                                            fullword). Due to compatibility,
                                            the displacement of RSSVERS
                                            should NEVER change. Previous
                                            versions of this control block
                                            had this field marked 'RESERVED'
                                            and the field was known to be
                                            zero. Therefore, previous
                                            versions were version X'00'. In
                                            addition, RSSFLAG should never be
                                            moved. This field is used without
                                            regard to the version of the
                                            RSSBK.
    000D   13 Bitstring    1 RSSVERS        RSSBK VERSION INDICATOR
              00000000       RSSVN00        X'00' RSSVN00 For version 00,
                                            original format
              00000001       RSSVN01        X'01' RSSVN01 For version 01, the
                                            RSSMSGN field was expanded from a
                                            halfword to fullword
    000E   14 Signed       2 RSSDCNT        LENGTH OF RSSDATA IN BYTES
    0010   16 Signed       4 RSSMSGN        SYSTEM RECORD MESSAGE NUMBER
    0014   20 Signed       4 *              RESERVED
    0018   24 Character    1 RSSDATA (0)    START OF VARIABLE LENGTH SYSTEM
                                            RECORD DATA
              00000018       RSSBLEN        *-RSSBK RSSBK HEADER LENGTH IN
                                            BYTES
              00000003       RSSSIZE        (*-RSSBK+7)/8 RSSBK ENTRY IN
                                            DOUBLEWORDS
          The following mapping shows what the fields changed for the
          Version 01 RSSBK looked like in Version 00.  The following
          fields are used when updating Version 00 RSSBKs to Version
          01.
    0006    6 Signed       2 RSSV00MN       RSSMSGN FIELD (Version 00 Format)
    0010   16 Character    1 RSSV00DA (0)   RSSDATA FIELD (Version 00 Format)
              00000010       RSSV00HL       *-RSSBK Length of a Version 00
                                            Header

RSSBK Storage Layout | Top of page

    *** RSSBK - RECORDING SYSTEM SERVICE BLOCK
    *
    *     +---------------------------+-------------+-------------+
    *   0 |         RSSNEXT           |  RSSUSCNT   |/////////////|
    *     +------+------+-------------+------+------+-------------+
    *   8 |//////|RSSRID|  RSSFRESZ   |:FLAG |:VERS |  RSSDCNT    |
    *     +------+------+-------------+------+------+-------------+
    *  10 |         RSSMSGN           |///////////////////////////|
    *     +---------------------------+---------------------------+
    *
    *** RSSBK - RECORDING SYSTEM SERVICE BLOCK

    *** Overlay for RSSVN00M in RSSBK
    *
    *                                               +-------------+
    *   0 ...                                     6 |  RSSV00MN   |
    *                                               +-------------+
    *   8
    *
    *** Overlay for RSSVN00M in RSSBK

    *** Overlay for RSSMSGN in RSSBK
    *
    *
    *** Overlay for RSSMSGN in RSSBK

RSSBK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    RSSBLEN        0018 00000018
    RSSDATA        0018
    RSSDCNT        000E
    RSSFLAG        000C
    RSSFRESZ       000A
    RSSMSGN        0010
    RSSNEXT        0000
    RSSNOMON       000C 20
    RSSRACNT       0009 00000001
    RSSRCNFG       0009 00000004
    RSSRID         0009
    RSSRINC        000C 40
    RSSRINIT       000C 80
    RSSRIOER       0009 00000002
    RSSRSYMP       0009 00000003
    RSSRTAB        0009 000000FF
    RSSSIZE        0018 00000003
    RSSUSCNT       0004
    RSSVERS        000D
    RSSVN00        000D 00000000
    RSSVN00M       0006
    RSSVN01        000D 00000001
    RSSV00DA       0010
    RSSV00HL       0010 00000010
    RSSV00MN       0006

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:30:08 EDT.
Copyright IBM Corporation, 1990, 2020