VLCCACHE | Back to Index page

| Prolog Control Block Contents VLCCACHE DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

VLCCACHE Control Block Content | Top of page

     VLCCACHE DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      VLCCACHE       Virtual Network Interface Card block
    0000    0 Signed       2 VLCCAVID       VLAN ID
    0002    2 Signed       2 *              Reserved
    0004    4 Address      4 VLCCAPTR       Pointer to VLCBK
          Define the DSECT for the NICRX structure that will be used
          to contain the queue totals.   See HCPNICAQ & HCPNICCQ.

VLCCACHE Storage Layout | Top of page

    *** VLCCACHE - Virtual Network Interface Card block
    *
    *     +-------------+-------------+---------------------------+
    *   0 |  VLCCAVID   |/////////////|         VLCCAPTR          |
    *     +-------------+-------------+---------------------------+
    *   8
    *
    *** VLCCACHE - Virtual Network Interface Card block

VLCCACHE Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    VLCCAPTR       0004
    VLCCAVID       0000

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:29:23 EDT.
Copyright IBM Corporation, 1990, 2020