Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSYTRSG

Prolog
Control Block Contents
Cross Reference

#### MRSYTRSG Prolog

     DSECT NAME - SYTRSG
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSYTRSG
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 0 - System Domain
                        Record 3 - Real Storage Data (Global)
     DESCRIPTION - Real storage allocation and use. Provides
                   dynamically changing classes of usage.
                   Static classes of usage are provided in the
                   MONITOR domain.

#### MRSYTRSG Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure   604  SYTRSG                 Start of monitor record
       0   0  Character     0  SYTRSG_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meangingul. (SYTRSG_RSAFSTOR)
      24  18  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_SYSVRSZ)
      28  1C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_RSAFSYUD)
      32  20  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_RSAFVRUD)
      36  24  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_SYSRSVPG)
      40  28  Unsigned      4  SYTRSG_RSACPLOK        Cardinal count of frames
                                                      locked below 2G by the CP
                                                      LOCK REAL command. See
                                                      SYTRSG_RSACPLKG for the >2G
                                                      count.
      44  2C  Unsigned      4  SYTRSG_RSANONPG        Cardinal count of <2G
                                                      pageable frames in the system
                                                      that have been made
                                                      non-pageable. This includes
                                                      pages locked for I/O, CP LOCK
                                                      command, virtual system lock
                                                      functions, etc. See
                                                      SYTRSG_RSAPGABL and
                                                      SYTRSG_RSALGFRM.
      48  30  Unsigned      4  SYTRSG_RSAPGABL        Cardinal count of <2G
                                                      pageable frames in the
                                                      system. This includes those
                                                      that had been made
                                                      non-pageable (see
                                                      SYTRSG_RSANONPG). The size of
                                                      the dynamic area (DPA) or the
                                                      count of useable frames may
                                                      be calculated as follows:
                                                      RSAPGABL-RSANONPG+RSALGFRM+
                                                      RSAFNOTI.
                                                      See SYTRSG_RSALGFRM for the
                                                      >2G field for the count of
                                                      useable frames. NOTE: There
                                                      is no separate count for
                                                      pageable frames (RSAPAGBL)
                                                      and frames made non-pageable
                                                      (RSANONPG) >2G.
      52  34  Unsigned      4  SYTRSG_RSAAVAIL        Cardinal count of ALL
                                                      frames that are currently on
                                                      the <2G available lists. This
                                                      is a TOTAL VALUE
                                                      (Singles+Contig) as in
                                                      previous releases. See
                                                      SYTRSG_RSA2GAVL for the >2G
                                                      count.
      56  38  Unsigned      4  SYTRSG_RSAFRQWT        Cardinal count of deferred
                                                      tasks waiting for a frame.
                                                      This represents the number of
                                                      requests for real frames
                                                      which have not been satisfied
                                                      yet because no frames are
                                                      available. It includes tasks
                                                      waiting for frames <2G only,
                                                      task waiting for frames >2G
                                                      only, and tasks waiting for
                                                      frames that can be anywhere.
                                                      See also SYTRSG_RSA2GDCT and
                                                      SYTRSG_RSADefCTA2G which can
                                                      be subtracted from this count
                                                      to get the number of tasks
                                                      waiting for frames <2G only.
      60  3C  Unsigned      4  SYTRSG_RSAXTEND        Cardinal count of frames
                                                      missing from the free storage
                                                      reserved frames list.
      64  40  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_RSAXFREE)
      68  44  Unsigned      4  SYTRSG_RSASAVFR        Cardinal count of frames in
                                                      use for saveareas.
      72  48  Bitstring     1  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_CALSTAT)
      73  49  Bitstring     1  SYTRSG_CALFLAG1        Flags byte.
              1... ....        SYTRSG_TCMCACHE         Minidisk Caching is
                                                      enabled.
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      74  4A  Unsigned      2  SYTRSG_HCPSTPMB        Bias for minidisk cache use
                                                      of real storage. A decimal
                                                      point is assumed to the left
                                                      of the low order 2 digits.
                                                      For example, a value of
                                                      decimal 95 in this field
                                                      would be a bias setting of
                                                      .95 .
      76  4C  Unsigned      4  SYTRSG_SYS98XA         Cardinal number of pages
                                                      locked by Diagnose X'98' in
                                                      31-bit mode
      80  50  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (SYTRSG_SYS98370)
      84  54  Unsigned      4  SYTRSG_TCMMIDSZ        Maximum allowable number of
                                                      pages in mindisk cache (based
                                                      on average age of a page in
                                                      DPA). AKA "ideal main store
                                                      cache size", set by arbiter
                                                      logic in HCPSTP.
      88  58  Unsigned      4  SYTRSG_TCMMAIN         Current number of pages in
                                                      main storage being used as
                                                      track cache pages. For a
                                                      breakdown of pages below and
                                                      above the 2GB line, see
                                                      SYTRSG_TCMMNBLW and
                                                      SYTRSG_TCMMNABV.
      92  5C  Unsigned      4  SYTRSG_TCMMNMIN        Minimum number of main
                                                      storage pages used by cache
                                                      as set by user command
      96  60  Unsigned      4  SYTRSG_TCMMNMAX        Maximum number of main
                                                      storage pages used by cache
                                                      as set by user command
     100  64  Unsigned      4  SYTRSG_TCMMNDL         Number of main storage
                                                      pages deleted from cache
     104  68  Unsigned      4  SYTRSG_TCMSTLMN        Number of times the steal
                                                      function was invoked to steal
                                                      main storage pages from the
                                                      track cache
     108  6C  Unsigned      4  SYTRSG_SYSSCMAV        Number of SCMBKs that are
                                                      available. This field is
                                                      valid only when format-0
                                                      measurement blocks are being
                                                      used (MTRSYS_CALFLG2 <>
                                                      x'80').
     112  70  Unsigned      4  SYTRSG_TCMMNBLW        Number of pages in main
                                                      storage below 2GB in use as
                                                      track cache pages. For
                                                      ESA/390 systems this field
                                                      will be equal to
                                                      SYTRSG_TCMMAIN.
     116  74  Unsigned      4  SYTRSG_TCMMNABV        Number of pages in main
                                                      storage at or above 2GB in
                                                      use as track cache pages. For
                                                      ESA/390 systems this field
                                                      will be zero.
     120  78  Unsigned      4  SYTRSG_RSA2GDCT        Cardinal count of deferred
                                                      tasks waiting for a real
                                                      frame that can be located
                                                      anywhere which have not been
                                                      satisfied yet because no
                                                      frames are available. This
                                                      count is included in
                                                      SYTRSG_RSADFRQWT.
     124  7C  Unsigned      4  SYTRSG_SYSSCGCT        Number of SCGBKs currently
                                                      allocated. This field is
                                                      valid only when format-1
                                                      measurement blocks are being
                                                      used (MTRSYS_CALFLG2 =
                                                      x'80').
     128  80  Unsigned      8  SYTRSG_RSALGFRM        Cardinal count of >2G
                                                      useable frames. See
                                                      SYTRSG_RSAPGABL and
                                                      STYRSG_RSANONPG for the <2G
                                                      value. Only counts initialized
                                                      frames, for not initialized
                                                      frames, which are part of the
                                                      DPA see MTRMEM_RSAFNOTI.
     136  88  Unsigned      4  SYTRSG_RSACPLKG        Cardinal count of frames
                                                      locked above 2G by the CP
                                                      LOCK REAL command. See
                                                      SYTRSG_RSACPLOK for the <2G
                                                      count.
     140  8C  Unsigned      8  SYTRSG_RSA2GAVL        Cardinal count of ALL
                                                      frames that are currently on
                                                      the >2G available lists. This
                                                      is a TOTAL VALUE
                                                      (Singles+Contig) as in
                                                      previous releases. See
                                                      SYTRSG_RSAAVAIL for the <2G
                                                      count.
     148  94  Unsigned      4  SYTRSG_RSAFSB2G        Count of doublewords
                                                      assigned to subpool free
                                                      storage backed below 2G.
     152  98  Unsigned      4  SYTRSG_RSAFSA2G        Count of doublewords
                                                      assigned to subpool free
                                                      storage backed above 2G.
     156  9C  Unsigned      4  SYTRSG_RSAFSYUB        Count of doublewords of in
                                                      use subpool free storage
                                                      backed below 2G.
     160  A0  Unsigned      4  SYTRSG_RSAFSYUA        Count of doublewords of in
                                                      use subpool free storage
                                                      backed above 2G.
     164  A4  Unsigned      4  SYTRSG_RSASXCPL        Count of locked System
                                                      Execution Space alias pages
                                                      locked in logical via the CP
                                                      LOCK command.
     168  A8  Unsigned      4  SYTRSG_RSASXCLA        Count of locked System
                                                      Execution Space alias pages
                                                      locked in logical. RSASXCLA
                                                      >= RSASXCPL
     172  AC  Unsigned      4  SYTRSG_RSARFRST        Count of frames allocated
                                                      for real free storage <2G.
     176  B0  Unsigned      8  SYTRSG_RSARFRSG        Count of frames allocated
                                                      for real free storage >2G.
     184  B8  Unsigned      4  SYTRSG_RSASXBCT        Count of SXS pages on the
                                                      queue of SXS pages backed
                                                      below 2G.
     188  BC  Unsigned      4  SYTRSG_RSASXACT        Count of SXS pages on the
                                                      queue of SXS pages backed
                                                      above 2G.
     192  C0  Unsigned      4  SYTRSG_RSAAFRDB        Count of doublewords of
                                                      aligned real free storage
                                                      <2G. This count includes
                                                      active as well as inactive
                                                      aligned free storage.
     196  C4  Unsigned      8  SYTRSG_RSAAFRDW        Count of doublewords of
                                                      aligned real free storage
                                                      >2G. This count includes
                                                      active as well as inactive
                                                      aligned free storage.
     204  CC  Unsigned      4  SYTRSG_RSAAFRIB        Count of doublewords of in
                                                      use aligned real free storage
                                                      <2G. This count includes only
                                                      active aligned free storage.
     208  D0  Unsigned      8  SYTRSG_RSAAFRIU        Count of doublewords of in
                                                      use aligned real free storage
                                                      >2G. This count includes only
                                                      active aligned free storage.
     216  D8  Unsigned      8  SYTRSG_RSACALCT        Count of the total number
                                                      of frames on the cleared
                                                      available list.
     224  E0  Unsigned      8  SYTRSG_RSASNG2G        Cardinal count of ALL
                                                      Single frames that are
                                                      currently on the >2G
                                                      available list.
     232  E8  Unsigned      4  SYTRSG_RSASNGAV        Cardinal count of ALL
                                                      Single frames that are
                                                      currently on the <2G
                                                      available list.
     236  EC  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDB1
     240  F0  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDA1
     244  F4  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDD1
     248  F8  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDC1
     252  FC  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDB2
     256 100  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDA2
     260 104  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDD2
     264 108  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDC2
     268 10C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDBE
     272 110  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDAE
     276 114  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDDE
     280 118  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSALTDCE
     284 11C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMB1
     288 120  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMA1
     292 124  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMD1
     296 128  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMC1
     300 12C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMB2
     304 130  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMA2
     308 134  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMD2
     312 138  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMC2
     316 13C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMBE
     320 140  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMAE
     324 144  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMDE
     328 148  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADRMCE
     332 14C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGB1
     336 150  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGA1
     340 154  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGD1
     344 158  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGC1
     348 15C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGB2
     352 160  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGA2
     356 164  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGD2
     360 168  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGC2
     364 16C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGBE
     368 170  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGAE
     372 174  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGDE
     376 178  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSAELGCE
     380 17C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPB1
     384 180  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPA1
     388 184  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPD1
     392 188  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPC1
     396 18C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPB2
     400 190  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPA2
     404 194  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPD2
     408 198  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPC2
     412 19C  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPBE
     416 1A0  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPAE
     420 1A4  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPDE
     424 1A8  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSADSPCE
     428 1AC  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRB1
     432 1B0  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRA1
     436 1B4  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRD1
     440 1B8  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRC1
     444 1BC  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRB2
     448 1C0  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRA2
     452 1C4  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRD2
     456 1C8  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRC2
     460 1CC  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRBE
     464 1D0  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRAE
     468 1D4  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRDE
     472 1D8  Unsigned      4  *                      Reserved for IBM use - used
                                                      to be SYTRSG_RSASHRCE
     476 1DC  Unsigned      4  SYTRSG_RSARESAC        Count of resident PTRM
                                                      pages i.e. count of resident
                                                      PGMBK frames >= 2G
     480 1E0  Unsigned      4  SYTRSG_RSARESBC        Count of resident PTRM
                                                      pages i.e. count of resident
                                                      PGMBK frames < 2G
     484 1E4  Unsigned      4  SYTRSG_RSARSVPG        Cardinal count of all
                                                      frames reserved via the SET
                                                      RESERVED command. The field
                                                      replaces SYTRSG_SYSRSVPG.
     488 1E8  Unsigned      4  SYTRSG_RSADEFCTA2G     Cardinal count of deferred
                                                      tasks waiting for a real
                                                      frame that can be located
                                                      only >2G which have not been
                                                      satisfied yet because no
                                                      frames are available. This
                                                      count is included in
                                                      SYTRSG_RSADFRQWT.
     492 1EC  Unsigned      8  SYTRSG_RSAPIN0B        Cardinal count of the
                                                      system total pinned pages
                                                      class 0 below 2G
     500 1F4  Unsigned      8  SYTRSG_RSAPIN0A        Cardinal count of the
                                                      system total pinned pages
                                                      class 0 above 2G
     508 1FC  Unsigned      8  SYTRSG_RSAPIN1B        Cardinal count of the
                                                      system total pinned pages
                                                      class 1 below 2G
     516 204  Unsigned      8  SYTRSG_RSAPIN1A        Cardinal count of the
                                                      system total pinned pages
                                                      class 1 above 2G
     524 20C  Unsigned      4  SYTRSG_RSAPINWP        Cardinal percent of the
                                                      total pinned page count
                                                      compared to the DPA that
                                                      causes a warning message when
                                                      a pin request is made.
                                                      Default value of
                                                      X'FF' indicates no pin
                                                      checking should be
                                                      done.
     528 210  Unsigned      4  SYTRSG_RSAPINFP        Cardinal percent of the
                                                      total pinned page count
                                                      compared to the DPA that
                                                      causes a pin request to
                                                      fail. Default value of X'FF'
                                                      indicates no pin checking
                                                      should be done.
     532 214  Unsigned      4  SYTRSG_RSAPINWC        Cumulative count of the
                                                      times the warning percent was
                                                      exceeded when a pin request
                                                      was made.
     536 218  Unsigned      4  SYTRSG_RSAPINFC        Cumulative count of the
                                                      times a pin request failed
                                                      because the fail percent was
                                                      exceeded.
     540 21C  Unsigned      8  SYTRSG_RSAIOUSD        Cardinal current usage in
                                                      BYTES of the IOAT subpool
                                                      storage.
     548 224  Unsigned      4  SYTRSG_RSAIOWRNP       Cardinal percent of the
                                                      IOAT subpool current usage
                                                      compared to the size when a
                                                      warning message is issued.
     552 228  Unsigned      4  SYTRSG_RSAIOWRNC       Cumulative count of the
                                                      times an IOAT subpool warning
                                                      message was issued.
     556 22C  Unsigned      4  SYTRSG_RSAIOFALS       Cumulative count of the
                                                      times IOAT subpool memory was
                                                      not available.
     560 230  Unsigned      4  SYTRSG_RSAIOFAIL       Cumulative count of the
                                                      times memory was not
                                                      available from the IOAT
                                                      subpool and from the
                                                      available list.
     564 234  Character     8  SYTRSG_RSAFNOTI        Count of not initialized
                                                      FRMTES>=2G.
     572 23C  Unsigned      8  SYTRSG_SYSPERMA        Amount of permanent storage
                                                      in bytes that is currently
                                                      online.
     580 244  Unsigned      8  SYTRSG_SYSRECNF        Amount of reconfigurable
                                                      storage in bytes that is
                                                      currently online.
     588 24C  Character     8  SYTRSG_SYSGSTBY        The standby real storage
                                                      size in bytes
     596 254  Character     8  SYTRSG_SYSGSTRS        The reserved real storage
                                                      size in bytes
     604 25C  Character     0  SYTRSG_END

#### MRSYTRSG Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SYTRSG                     0    604
    SYTRSG_CALFLAG1           49      1
    SYTRSG_END               25C      0
    SYTRSG_HCPSTPMB           4A      2
    SYTRSG_MRHDR               0      0
    SYTRSG_RSAAFRDB           C0      4
    SYTRSG_RSAAFRDW           C4      8
    SYTRSG_RSAAFRIB           CC      4
    SYTRSG_RSAAFRIU           D0      8
    SYTRSG_RSAAVAIL           34      4
    SYTRSG_RSACALCT           D8      8
    SYTRSG_RSACPLKG           88      4
    SYTRSG_RSACPLOK           28      4
    SYTRSG_RSADEFCTA2G       1E8      4
    SYTRSG_RSAFNOTI          234      8
    SYTRSG_RSAFRQWT           38      4
    SYTRSG_RSAFSA2G           98      4
    SYTRSG_RSAFSB2G           94      4
    SYTRSG_RSAFSYUA           A0      4
    SYTRSG_RSAFSYUB           9C      4
    SYTRSG_RSAIOFAIL         230      4
    SYTRSG_RSAIOFALS         22C      4
    SYTRSG_RSAIOUSD          21C      8
    SYTRSG_RSAIOWRNC         228      4
    SYTRSG_RSAIOWRNP         224      4
    SYTRSG_RSALGFRM           80      8
    SYTRSG_RSANONPG           2C      4
    SYTRSG_RSAPGABL           30      4
    SYTRSG_RSAPINFC          218      4
    SYTRSG_RSAPINFP          210      4
    SYTRSG_RSAPINWC          214      4
    SYTRSG_RSAPINWP          20C      4
    SYTRSG_RSAPIN0A          1F4      8
    SYTRSG_RSAPIN0B          1EC      8
    SYTRSG_RSAPIN1A          204      8
    SYTRSG_RSAPIN1B          1FC      8
    SYTRSG_RSARESAC          1DC      4
    SYTRSG_RSARESBC          1E0      4
    SYTRSG_RSARFRSG           B0      8
    SYTRSG_RSARFRST           AC      4
    SYTRSG_RSARSVPG          1E4      4
    SYTRSG_RSASAVFR           44      4
    SYTRSG_RSASNGAV           E8      4
    SYTRSG_RSASNG2G           E0      8
    SYTRSG_RSASXACT           BC      4
    SYTRSG_RSASXBCT           B8      4
    SYTRSG_RSASXCLA           A8      4
    SYTRSG_RSASXCPL           A4      4
    SYTRSG_RSAXTEND           3C      4
    SYTRSG_RSA2GAVL           8C      8
    SYTRSG_RSA2GDCT           78      4
    SYTRSG_SYSGSTBY          24C      8
    SYTRSG_SYSGSTRS          254      8
    SYTRSG_SYSPERMA          23C      8
    SYTRSG_SYSRECNF          244      8
    SYTRSG_SYSSCGCT           7C      4
    SYTRSG_SYSSCMAV           6C      4
    SYTRSG_SYS98XA            4C      4
    SYTRSG_TCMCACHE           49           80
    SYTRSG_TCMMAIN            58      4
    SYTRSG_TCMMIDSZ           54      4
    SYTRSG_TCMMNABV           74      4
    SYTRSG_TCMMNBLW           70      4
    SYTRSG_TCMMNDL            64      4
    SYTRSG_TCMMNMAX           60      4
    SYTRSG_TCMMNMIN           5C      4
    SYTRSG_TCMSTLMN           68      4

    This information is
    based on z/VM V7R2.0.

    Last updated on 06 August 2021 at 17:52:46.

    Copyright IBM Corporation, 1990, 2021