Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLSQD

Prolog
Control Block Contents
Cross Reference

#### MRSCLSQD Prolog

     DSECT NAME - SCLSQD
     FUNCTION - Map a Monitor record.
     LOCATED BY -
               Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLSQD
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler Domain
                        Record 10 - SET QUICKDSP Changes
     DESCRIPTION - Record of changes made by a SET QUICKDSP command.
                   Generated only if the user who is the target of the
                   command is enabled for scheduler domain (not to be
                   confused with the user that issued the command).

#### MRSCLSQD Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure    32  SCLSQD                 Start of monitor record
       0   0  Character     0  SCLSQD_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Character     8  SCLSQD_VMDUSER         Userid
      28  1C  Bitstring     1  SCLSQD_CALFLAG1        Flag byte 1
              1... ....        *
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        SCLSQD_VMDQDSPU         When set on, user is
                                                      classified as QUICKDSP. Set
                                                      by the user's directory or by
                                                      the SET QUICKDSP command.
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      29  1D  Character     3  *                      Reserved for IBM use
      32  20  Character     0  SCLSQD_END

#### MRSCLSQD Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SCLSQD                     0     32
    SCLSQD_CALFLAG1           1C      1
    SCLSQD_END                20      0
    SCLSQD_MRHDR               0      0
    SCLSQD_VMDQDSPU           1C           08
    SCLSQD_VMDUSER            14      8

    This information is
    based on z/VM V7R2.0.

    Last updated on 08 August 2020 at 16:14:17.

    Copyright IBM Corporation, 1990, 2020