STCONFIG | Back to Index page

| Prolog Control Block Contents STCONFIG DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

STCONFIG Prolog | Top of page

    Name       :  HCPASCBK
    DSECT      :  STCONFIG
    Description:  ASCSTCFG stg config element mapping

STCONFIG Control Block Content | Top of page

     STCONFIG DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      STCONFIG       Address-Space-Control Block
    0000    0 Dbl-Word     8 STCEXTSA       Guest Absolute Address Extent
                                            start address
    0008    8 Dbl-Word     8 STCEXTEA       Guest Absolute Address Extent end
                                            address (highes byte)
    0010   16 Dbl-Word     8 STCNEXT (0)    Next storage config element
              00000010       STCLEN         *-STCONFIG Length of one config
                                            element

STCONFIG Storage Layout | Top of page

    *** STCONFIG - Address-Space-Control Block
    *
    *     +-------------------------------------------------------+
    *   0 |                       STCEXTSA                        |
    *     +-------------------------------------------------------+
    *   8 |                       STCEXTEA                        |
    *     +-------------------------------------------------------+
    *
    *** STCONFIG - Address-Space-Control Block

STCONFIG Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    STCEXTEA       0008
    STCEXTSA       0000
    STCLEN         0010 00000010
    STCNEXT        0010

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:27:00 EDT.
Copyright IBM Corporation, 1990, 2020