CSLPL | Back to Index page

| Prolog Control Block Contents CSLPL DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

CSLPL Prolog | Top of page

     NAME       : HCPCSLPL
     DESCRIPTION: Console macro parameter list
     DSECT      : CSLPL
     LOCATED BY : HCPCONSL passes the address in a register
     CREATED BY : The HCPCSLPL is created by the HCPCONSL macro
                  whenever a read or write is to be done.
     DELETED BY : The HCPCSLPL is deleted by the HCPCONSL macro
     REFERENCES : None.
     SERIALIZED : HCPCONSL gets free storage for each instance of this
                  control block, so only one processor will be looking at
                  any one instance of this control block at any one time.
     RELOCATION CONSIDERATIONS : As part of cross system SCIF
                  flag bytes CSLTYPE, CSLDFLG, CSLEFLG and CSLSFLG are
                  shipped to a remote member of the plex.  Any changes
                  to these flag bytes must be done in an upwardly
                  compatible manner.  The transport is initiated in
                  HCPCFR.

CSLPL Control Block Content | Top of page

     CSLPL DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      CSLPL          Console macro parameter list
    0000    0 Character    2 CSLCOMMN (0)   common part
    0000    0 Bitstring    2 CSLNEST        how many caller's register to go
                                            back
    0002    2 Character    1 CSLFUNDE (0)   start of variable length data
    0002    2 Character   12 CSLWRITE (0)
    0002    2 Signed       2 CSLDADDR       bddd of data
    0004    4 Bitstring    1 CSLDATA        data information flags
              1... ....      CSLNUM         X'80' CSLNUM repository entry
                                            number
              .1.. ....      CSLNUMRG       X'40' CSLNUMRG repository entry
                                            number
              ..1. ....      CSLIST         X'20' CSLIST list of repository
                                            numbers
              ...1 ....      CSLDLNRG       X'10' CSLDLNRG length of data is
                                            in a register
              .... 1...      CSLSUBDT       X'08' CSLSUBDT substitution data
                                            is passed
              .... .1..      CSLSUBRG       X'04' CSLSUBRG substitution data
                                            is in a register
              .... ..1.      CSLHLNRG       X'02' CSLHLNRG header length is
                                            in a register
              .... ...1      CSLVMDRG       X'01' CSLVMDRG VMDBK address is
                                            in a register
    0005    5 Bitstring    1 CSLTYPE        data type flags
              1... ....      CSLEMSG        X'80' CSLEMSG error message
              .1.. ....      CSLIMSG        X'40' CSLIMSG informational
                                            message
              ..1. ....      CSLFEMSG       X'20' CSLFEMSG full error message
              ...1 ....      CSLCRESP       X'10' CSLCRESP command response
              .... 1...      CSLRDISP       X'08' CSLRDISP input redisplay
              .... .1..      CSLWNG         X'04' CSLWNG warning message
              .... ..1.      CSLMSG         X'02' CSLMSG message to a user
              .... ...1      CSLMSGNH       X'01' CSLMSGNH message no-header
                                            to a user
    0006    6 Bitstring    1 CSLDFLG        destination flags
              1... ....      CSLALTVM       X'80' CSLALTVM alternate vmdbk is
                                            specified
              .1.. ....      CSLOPER        X'40' CSLOPER data to be sent to
                                            the operator
              ..1. ....      CSLTERM        X'20' CSLTERM send data to
                                            terminal(not over IUCV, Diag 8 to
                                            buff,etc )
              ...1 ....      CSLGSDBK       X'10' CSLGSDBK return data in a
                                            GSDBK
              .... 1...      CSLTRMA        X'08' CSLTRMA force data to
                                            terminal also
              .... .1..      CSLTRMO        X'04' CSLTRMO force data to
                                            terminal only
              .... ..1.      CSLINITP       X'02' CSLINITP initial logon
                                            prompt
              .... ...1      CSLISSUS       X'01' CSLISSUS issuer's userid is
                                            specified
    0007    7 Bitstring    1 CSLEFLG        data edit flags
              .1.. ....      CSLADTIM       X'40' CSLADTIM add timestamp to
                                            data
              ..1. ....      CSLSPTIM       X'20' CSLSPTIM suppress time
                                            stamp and cpu id
              ...1 ....      CSLBRITE       X'10' CSLBRITE hilight this data
              .... 1...      CSLCOLFM       X'08' CSLCOLFM error message in
                                            column format
              .... .1..      CSLBLNKS       X'04' CSLBLNKS do not delete
                                            trailing blanks
              .... ..1.      CSLOBSRV       X'02' CSLOBSRV message to
                                            observer
              .... ...1      CSLPRND        X'01' CSLPRND prompt with
                                            no-display read
    0008    8 Bitstring    1 CSLSFLG        screen control flags
              1... ....      CSLALARM       X'80' CSLALARM sound alarm
              .1.. ....      CSLHIPRI       X'40' CSLHIPRI this is high
                                            priority data, if user is in full
                                            screen, post an attention to the
                                            user
              ..1. ....      CSLNDISP       X'20' CSLNDISP do not display
                                            data (or spool for reads)
              ...1 ....      CSLCLEAR       X'10' CSLCLEAR clear screen prior
                                            to displaying data
              .... 1...      CSLIOCMP       X'08' CSLIOCMP return after users
                                            IO completed
              .... .1..      CSLSCRFL       X'04' CSLSCRFL return if data can
                                            fit on current screen
              .... ..1.      CSLDROP        X'02' CSLDROP drops the
                                            connection
              .... ...1      CSLIMMED       X'01' CSLIMMED if the user is in
                                            full screen, this message will
                                            break the user out of full
                                            screen.
    0009    9 Bitstring    1 CSLPFLG        Parameter address flag (address
                                            of address)
              1... ....      CSLDPTR        X'80' CSLDPTR parameter list
                                            points to address of data
              .1.. ....      CSLIPTR        X'40' CSLIPTR parameter list
                                            points to address of issuers
                                            USERID
              ..1. ....      CSLAPTR        X'20' CSLAPTR parameter list
                                            points to address of alternate
                                            VMDBK
              ...1 ....      CSLSPTR        X'10' CSLSPTR parameter list
                                            points to address of substitution
                                            data/reg
              .... 1...      CSLLPTR        X'08' CSLLPTR parameter list
                                            points to address of data length
              .... .1..      CSLHPTR        X'04' CSLHPTR parameter list
                                            points to address of header
                                            length
    000A   10 Signed       2 CSLISSID       bddd of the issuer's userid
    000C   12 Signed       2 CSLVMDBK       bddd of alternate VMDBK address
    000E   14 Address      2 CSLCMPID       bddd of 3-char component ID
    0010   16 Address      2 CSLSRCID       bddd of source id string
    0012   18 Character    1 CSLWTYDE (0)   start of variable length data
          Write Type dependent parts
    0012   18 Character    2 CSLSUBDA (0)
    0012   18 Signed       2 CSLSBDAT       bddd of substitution data
              00000014       CSLSSIZE       *-CSLPL
    0012   18 Character    2 CSLSUBR (0)
    0012   18 Signed       2 CSLSBREG       register containing substitution
                                            data
              00000014       CSLESIZE       *-CSLPL
    0012   18 Character    4 CSLBDAT (0)
    0012   18 Signed       2 CSLDLGTH       bddd of length of data being
                                            passed
    0014   20 Signed       2 CSLHDRSZ       bddd of length of message header
    0016   22 Character    1 CSLPRMDE (0)   start of variable length data
              00000016       CSLQSIZE       *-CSLPL
          Read dependent parts
          Any changes to the read fields should also be made to the
          prompted read fields.
    0002    2 Character    1 CSLREAD (0)
    0002    2 Bitstring    1 CSLRPARM       read data flags
              1... ....      CSLNODSP       X'80' CSLNODSP do not display or
                                            spool this data
              .1.. ....      CSLNOLED       X'40' CSLNOLED do not perform
                                            line editing
              ..1. ....      CSLUPPER       X'20' CSLUPPER translate input
                                            line to upper case
              ...1 ....      CSLCDRDR       X'10' CSLCDRDR data from a card
                                            reader
              00000003       CSLRSIZE       *-CSLPL
          Prompted read dependent parts
          Any changes to the prompted read fields should also be made
          to the read fields.
    0016   22 Character    1 CSLPREAD (0)
    0016   22 Bitstring    1 CSLRFLAG       read data flags
              1... ....      CSLNODIS       X'80' CSLNODIS do not display or
                                            spool this data
              .1.. ....      CSLPNLED       X'40' CSLPNLED do not perform
                                            line editing
              ..1. ....      CSLUPPR        X'20' CSLUPPR translate input
                                            line to upper case
              ...1 ....      CSLCARDR       X'10' CSLCARDR data from a card
                                            reader
              00000017       CSLPSIZE       *-CSLPL
          Labels for XRef Purposes only
              .... ....      CSLWRTEF       X'00' WRITE to console specified
              .... ....      CSLFRMTF       X'00' WRITE(format) to GSDBK
              .... ....      CSLREADF       X'00' READ func specified
              .... ....      CSLPRMPT       X'00' PROMPT func specified
              .... ....      CSLWAITF       X'00' WAIT func specified
              .... ....      CSLDATAK       X'00' DATA keyword specified
              .... ....      CSLCPDAT       X'00' DATATYPE NONE
              .... ....      CSLDSPCH       X'00' DESTINATION dispatched
              .... ....      CSLXNDSP       X'00' DISPLAY NO
              .... ....      CSLXNLED       X'00' LINEEDIT NO
              .... ....      CSLXUPPR       X'00' CASE UPPER
              .... ....      CSLXCRDR       X'00' DEVICE CARDRDR

CSLPL Storage Layout | Top of page

    *** CSLPL - Console macro parameter list
    *
    *     +-------------+
    *   0 |  CSLNEST    |
    *     +-------------+
    *
    *** CSLPL - Console macro parameter list

    *** Overlay for CSLFUNDE in CSLPL
    *
    *                   +-------------+------+------+------+------+
    *   0 ...         2 |  CSLDADDR   |:DATA |:TYPE |:DFLG |:EFLG |
    *     +------+------+-------------+------+------+------+------+
    *   8 |:SFLG |:PFLG |  CSLISSID   |  CSLVMDBK   |  CSLCMPID   |
    *     +------+------+-------------+-------------+-------------+
    *  10 |  CSLSRCID   |
    *     +-------------+
    *
    *** Overlay for CSLFUNDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *                   +-------------+
    *  10 ...        12 |  CSLSBDAT   | 14
    *                   +-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *                   +-------------+
    *  10 ...        12 |  CSLSBREG   | 14
    *                   +-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLWTYDE in CSLPL
    *
    *                   +-------------+-------------+
    *  10 ...        12 |  CSLDLGTH   |  CSLHDRSZ   |
    *                   +-------------+-------------+
    *
    *** Overlay for CSLWTYDE in CSLPL

    *** Overlay for CSLFUNDE in CSLPL
    *
    *                   +------+
    *   0 ...         2 |:RPARM| 3
    *                   +------+
    *
    *** Overlay for CSLFUNDE in CSLPL

    *** Overlay for CSLPRMDE in CSLPL
    *
    *                                               +------+
    *  10 ...                                    16 |:RFLAG| 17
    *                                               +------+
    *
    *** Overlay for CSLPRMDE in CSLPL

CSLPL Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    CSLADTIM       0007 40
    CSLALARM       0008 80
    CSLALTVM       0006 80
    CSLAPTR        0009 20
    CSLBDAT        0012
    CSLBLNKS       0007 04
    CSLBRITE       0007 10
    CSLCARDR       0016 10
    CSLCDRDR       0002 10
    CSLCLEAR       0008 10
    CSLCMPID       000E
    CSLCOLFM       0007 08
    CSLCOMMN       0000
    CSLCPDAT       0016 00
    CSLCRESP       0005 10
    CSLDADDR       0002
    CSLDATA        0004
    CSLDATAK       0016 00
    CSLDFLG        0006
    CSLDLGTH       0012
    CSLDLNRG       0004 10
    CSLDPTR        0009 80
    CSLDROP        0008 02
    CSLDSPCH       0016 00
    CSLEFLG        0007
    CSLEMSG        0005 80
    CSLESIZE       0012 00000014
    CSLFEMSG       0005 20
    CSLFRMTF       0016 00
    CSLFUNDE       0002
    CSLGSDBK       0006 10
    CSLHDRSZ       0014
    CSLHIPRI       0008 40
    CSLHLNRG       0004 02
    CSLHPTR        0009 04
    CSLIMMED       0008 01
    CSLIMSG        0005 40
    CSLINITP       0006 02
    CSLIOCMP       0008 08
    CSLIPTR        0009 40
    CSLISSID       000A
    CSLISSUS       0006 01
    CSLIST         0004 20
    CSLLPTR        0009 08
    CSLMSG         0005 02
    CSLMSGNH       0005 01
    CSLNDISP       0008 20
    CSLNEST        0000
    CSLNODIS       0016 80
    CSLNODSP       0002 80
    CSLNOLED       0002 40
    CSLNUM         0004 80
    CSLNUMRG       0004 40
    CSLOBSRV       0007 02
    CSLOPER        0006 40
    CSLPFLG        0009
    CSLPNLED       0016 40
    CSLPREAD       0016
    CSLPRMDE       0016
    CSLPRMPT       0016 00
    CSLPRND        0007 01
    CSLPSIZE       0016 00000017
    CSLQSIZE       0016 00000016
    CSLRDISP       0005 08
    CSLREAD        0002
    CSLREADF       0016 00
    CSLRFLAG       0016
    CSLRPARM       0002
    CSLRSIZE       0002 00000003
    CSLSBDAT       0012
    CSLSBREG       0012
    CSLSCRFL       0008 04
    CSLSFLG        0008
    CSLSPTIM       0007 20
    CSLSPTR        0009 10
    CSLSRCID       0010
    CSLSSIZE       0012 00000014
    CSLSUBDA       0012
    CSLSUBDT       0004 08
    CSLSUBR        0012
    CSLSUBRG       0004 04
    CSLTERM        0006 20
    CSLTRMA        0006 08
    CSLTRMO        0006 04
    CSLTYPE        0005
    CSLUPPER       0002 20
    CSLUPPR        0016 20
    CSLVMDBK       000C
    CSLVMDRG       0004 01
    CSLWAITF       0016 00
    CSLWNG         0005 04
    CSLWRITE       0002
    CSLWRTEF       0016 00
    CSLWTYDE       0012
    CSLXCRDR       0016 00
    CSLXNDSP       0016 00
    CSLXNLED       0016 00
    CSLXUPPR       0016 00

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:31:54 EDT.
Copyright IBM Corporation, 1990, 2020