Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRUSEACT

Prolog
Control Block Contents
Cross Reference

#### MRUSEACT Prolog

     DSECT NAME - USEACT
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRUSEACT
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 4 - User Domain
                        Record 3 - User Activity Data
     DESCRIPTION - User activity data.  Generated for each virtual
                   processor in a virtual configuration.
     NOTES -
          - For additional information about the format and meaning of
            the MRUSEACT_VMUTOPDA entries in this record, knowledge of
            system topology as reported by the STSI instruction is
            necessary.  For a description of system topology, refer to
            the following book:
              - Principles of Operation for the layout of the
                variable length STSI 15.1.x output which is
                documented in Chapter 10 under "STORE SYSTEM
                INFORMATION".  Anyone looking at the STSI data
                in this record should read about the format of
                the data and the CPU Topology Overview contained
                there. (SA22-7832-08)
          - To give a fuller picture of time consumed, three
            sets of used processor time are reported in this
            monitor record.  When multithreading is enabled on
            the system, all three are also reported in the Type
            1 and F accounting records. Timer field names
            ending with _MT1 are MT-1 Equivalent times. Timer
            field names ending with _PRO are Prorated Core
            Times.  Timer field names without an _MT1 or _PRO
            suffix contain Raw Time values.
          - Raw Time is tracked for ALL users for their entire
            session.  Raw Time is the CPU time each virtual CPU
            spent dispatched on a thread and is the CPU Timer
            information provided directly by the hardware.
          - MT-1 Equivalent Time is tracked for ALL users for
            their entire session. This calculated CPU time
            approximates the time that would have been spent
            if the workload had been run with multithreading
            disabled, that is, with all core resources available
            to one thread.  When a user is running on a system
            where multithreading is not installed or not
            enabled, MT-1 Equivalent Time consumed will be
            identical to Raw Time.  However, if a guest has
            relocated from an MT-enabled system to an
            MT-disabled system, the cumulative raw and MT-1
            Equivalent times reported in monitor records may
            differ due to the prior execution in the MT
            environment.
          - Prorated Core Time charges for core utilization in
            a way suitable to core-based software licensing.
            Time is charged by dividing the time the core was
            dispatched evenly among the threads dispatched in
            that interval. Since Prorated Core Time is not always
            calculated, additional information
            is reported regarding the Prorated Core Time values:
            * The _VMAPRCAL bit indicates whether the Prorated
              Core Time values in this record are valid.
              When the user is relocated to any other system
              (even a Multithreading aware/enabled system),
              Prorated Core Time is reset. This means:
              * the _VMAPRCAL bit is set based on whether the
                source system will be calculating prorated core
                time or not
              * all _VMAxxxxx_PRO fields are reset to PFXTMMAX.

#### MRUSEACT Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure   912+ USEACT                 Start of monitor record
       0   0  Character     0  USEACT_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Character     8  USEACT_VMDUSER         Userid
      28  1C  Unsigned      2  USEACT_VMDCPUAD        Processor ID/CPU address of
                                                      virtual processor
      30  1E  Bitstring     1  USEACT_VMDMODE         Guest machine mode. This is
                                                      as set for internal use by
                                                      CP. See USEACT_CALMODE for
                                                      the mode 'calculated' at.
      31  1F  Bitstring     1  USEACT_CALMODE         Architectural mode of the
                                                      virtual machine
              1... ....        *
              .1.. ....        USEACT_CALMESA          ESA architecture
              ..1. ....        USEACT_CALMXA           XA architecture
              ...1 ....        USEACT_CALM370          370 architecture
              .... 1...        USEACT_CALMXC           XC architecture
              .... .1..        USEACT_CALMESAM         Machine has entered
                                                      z/Arch mode.
              .... ..1.        USEACT_CALVARCH         Guest's virtual
                                                      architecture is not the same
                                                      as the system's real
                                                      architecture
              .... ...1        USEACT_CALMZONL         z/Architecture-only
      32  20  Bitstring     1  USEACT_VMDSLIST        Scheduling list that the
                                                      user is in: X'37' = Dispatch
                                                      List. X'21' = Eligible List.
                                                      X'0B' = Dormant List. X'00' =
                                                      user is not in any list.
      33  21  Unsigned      1  USEACT_VMDELIST        Class number (0,1,2,or 3)
                                                      of the scheduling list the
                                                      user is in
      34  22  Bitstring     1  USEACT_CALFLAG1        Flag byte
              1... ....        USEACT_CALBASE          If on, this is the base
                                                      VMDBK. VMDBASE
              .1.. ....        USEACT_VMDQDSPU         This user has the QUICKDSP
                                                      designation, as set or
                                                      defaulted by the SET QUICKDSP
                                                      command. When the user has
                                                      work to do, it will be added
                                                      to the dispatch list
                                                      immediately without waiting
                                                      in the eligible list.
              ..1. ....        USEACT_CALDIAL          This user is a dialed user
              ...1 ....        USEACT_CALSNA           This user is connected
                                                      through System Network
                                                      Architecture (SNA)
              .... 1...        USEACT_VMDNOINS         User is prevented from
                                                      inserting any tracks into the
                                                      minidisk cache. (set when SET
                                                      MDC INS OFF command is
                                                      issued)
              .... .1..        USEACT_VMDNOFSL         No MDC fair share limit
                                                      applies. Set at LOGON if the
                                                      NOMDCFS option is specified
                                                      on the OPTIONS statement in
                                                      the user's directory.
              .... ..1.        USEACT_VMDMASST         Collaborative Memory
                                                      Management assist enabled.
              .... ...1        USEACT_VMDMAACT         Collaborative Memory
                                                      Management assist is active,
                                                      i.e. in use by this virtual
                                                      machine. Note: This guest may
                                                      be in a pending off state if
                                                      either a global or per-user
                                                      SET MEMASSIST OFF has been
                                                      issued (SYSMASST or VMDMASST
                                                      is off). This indicates that
                                                      the system or user setting
                                                      was turned off after the
                                                      guest started using the
                                                      assist. The assist will
                                                      remain active
                                                      (USEACT_VMDMAACT=1) and
                                                      available to this guest until
                                                      the next virtual machine
                                                      reset or IPL.
      35  23  Bitstring     1  USEACT_VMDSTYPE        Storage type this virtual
                                                      machine resides in. X'00' =>
                                                      V=V. X'80' => Reserved and no
                                                      longer available. X'40' =>
                                                      V=F.
      36  24  Character     8  USEACT_VMDTTIME        Total Raw Time which has
                                                      been expended on this VMDBK.
                                                      This includes time which the
                                                      VMDBK spent doing its own work
                                                      and also time which CP spent
                                                      doing work on behalf of the
                                                      VMDBK. It is in CPU timer
                                                      format. The complement of
                                                      this field is the elapsed
                                                      time in TOD clock units.
      44  2C  Character     8  USEACT_VMDVTIME        Total Raw Time that this
                                                      user was running and doing
                                                      productive work. It does NOT
                                                      include any time that CP
                                                      spends on behalf of that user
                                                      doing such things as
                                                      instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format. The
                                                      complement of this field is
                                                      the elapsed time in TOD clock
                                                      units.
      52  34  Character     8  *                      Reserved for IBM use
                                                      Previous field is no longer
                                                      meaningful. (USEACT_VMDVFVTM)
      60  3C  Character     8  *                      Reserved for IBM use
                                                      Previous field is no longer
                                                      meaningful. (USEACT_VMDVFOTM)
      68  44  Unsigned      4  USEACT_VMDCTPVR        Cardinal count of resident
                                                      pages in private address
                                                      spaces belonging to this
                                                      user. This monitor field is
                                                      actually the sum of VMDCTPVR
                                                      + VMDCTPVG. To get the count
                                                      of resident pages below the
                                                      2GB line, subtract
                                                      USEACT_VMDCTPVG from
                                                      USEACT_VMDCTPVR.
      72  48  Unsigned      4  USEACT_VMDCTPVL        Cardinal count of locked
                                                      pages in private address
                                                      spaces <2G belonging to this
                                                      user. See USEACT_VMDCTPVLA
                                                      for the >2G value.
      76  4C  Unsigned      4  USEACT_VMDWSSPR        This user's projected
                                                      working set size. This is the
                                                      scheduler's estimate of the
                                                      amount of storage this user
                                                      will require to be resident
                                                      as it runs during its next
                                                      stay in the dispatch list. It
                                                      is based upon the user's past
                                                      behavior and in some cases,
                                                      on the behavior of similar
                                                      types of users.
      80  50  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_VMDCTXBK
      84  54  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALXSTOR
      88  58  Unsigned      4  USEACT_VMDCTFLT        Count of host segment and
                                                      page faults on guest pages
                                                      which occurred while running
                                                      this virtual CPU. It does not
                                                      include faults on RCP pages.
      92  5C  Unsigned      4  *                      Reserved for IBM use
                                                      Previous field is no longer
                                                      meaningful. (USEACT_VMDCTVFL)
      96  60  Unsigned      4  *                      Reserved for IBM use - was
                                                      USEACT_VMDFLREO
     100  64  Unsigned      4  *                      Reserved for IBM use - was
                                                      USEACT_VMDCTORF
     104  68  Unsigned      4  USEACT_CALCTPGS        Cardinal count of
                                                      non-preferred paging slots
                                                      for private address spaces
                                                      belonging to this user.
     108  6C  Unsigned      4  *                      Reserved for IBM use
     112  70  Unsigned      4  USEACT_VMDCTPWT        Count of outstanding paging
                                                      and spooling I/O's for this
                                                      user
     116  74  Unsigned      4  USEACT_CALCPPGR        Cumulative count of pages
                                                      read from DASD to main
                                                      storage for this user's
                                                      address spaces while they
                                                      were private.
     120  78  Unsigned      4  USEACT_CALCPPGW        Cumulative count of pages
                                                      written from main storage to
                                                      DASD for this user's address
                                                      spaces while they were
                                                      private.
     124  7C  Unsigned      4  USEACT_VMDCTSPR        Number of times I/O was
                                                      issued for a spool read
                                                      request
     128  80  Unsigned      4  USEACT_VMDCTSPW        Number of times I/O was
                                                      issued for a spool write
                                                      request
     132  84  Unsigned      4  USEACT_VMDPGSPL        Number of pages spooled for
                                                      this user. This includes the
                                                      pages spooled for the virtual
                                                      reader, printer, punch,
                                                      console, dump, and trace
                                                      files.
     136  88  Unsigned      4  USEACT_VMDVCSCT        Cumulative count of virtual
                                                      SSCH requests to
                                                      the virtual machine console
     140  8C  Unsigned      4  USEACT_VMDVDSCT        Cumulative count of virtual
                                                      SSCH requests the virtual
                                                      machine has issued to DASD
                                                      devices
     144  90  Unsigned      4  USEACT_VMDVUSCT        Cumulative count of virtual
                                                      SSCH requests to
                                                      virtual Unit Record devices
     148  94  Unsigned      4  USEACT_VMDVTSCT        Cumulative count of virtual
                                                      SSCH requests to
                                                      virtual channel-to-channel
                                                      adapters
     152  98  Unsigned      4  USEACT_VMDVOSCT        Cumulative count of virtual
                                                      SSCH requests to
                                                      devices other than console,
                                                      DASDs, CTCAs, and unit
                                                      records. (see
                                                      USEACT_VMDVCSCT,
                                                      USEACT_VMDVDSCT,
                                                      USEACT_VMDVUSCT, and
                                                      USEACT_VMDVTSCT)
     156  9C  Unsigned      4  USEACT_CALCPPST        Cumulative count of pages
                                                      reclaimed from this user's
                                                      address spaces while they
                                                      were private.
     160  A0  Unsigned      4  USEACT_VMDISEVM        Number of times IUCV data
                                                      was successfully transferred
                                                      by this virtual complex.
                                                      (SENDs and REPLYs with RC=0
                                                      when this virtual machine is
                                                      the source). Not valid in the
                                                      SYSTEM VMDBK. Valid only in
                                                      base VMDBK.
     164  A4  Unsigned      4  USEACT_VMDISTVM        Number of times IUCV data
                                                      was successfully transferred
                                                      to this virtual complex.
                                                      (SENDs and REPLYs with RC=0
                                                      when this virtual machine is
                                                      the target). Not valid in the
                                                      SYSTEM VMDBK. Valid only in
                                                      base VMDBK.
     168  A8  Unsigned      4  USEACT_VMDISUVM        Number of times IUCV data
                                                      was NOT successfully
                                                      transferred by this virtual
                                                      complex. (SENDs and REPLYs
                                                      with RC^=0 when this virtual
                                                      machine is the source). Not
                                                      valid in the SYSTEM VMDBK.
                                                      Valid only in base VMDBK.
     172  AC  Unsigned      4  USEACT_VMDVSEVM        Number of times VMCF data
                                                      was successfully transferred
                                                      by this virtual machine.
                                                      (SENDs SENDXs, SEND/RECEIVEs,
                                                      and REPLYs with RC=0 and this
                                                      virtual machine is source.)
     176  B0  Unsigned      4  USEACT_VMDVSTVM        Number of times VMCF data
                                                      was successfully transferred
                                                      to this virtual machine.
                                                      (SENDs SENDXs, SEND/RECEIVEs,
                                                      and REPLYs with RC=0 and this
                                                      virtual machine is target.)
     180  B4  Unsigned      4  USEACT_VMDVSUVM        Number of times VMCF data
                                                      was NOT successfully
                                                      transferred by this virtual
                                                      machine. (SENDs SENDXs,
                                                      SEND/RECEIVEs, and REPLYs
                                                      with RC^=0 and this virtual
                                                      machine is source.)
     184  B8  Signed        4  USEACT_CALIUCVS        Cardinal count of messages
                                                      on the IUCV SEND queue. The
                                                      SEND queue consists of
                                                      messages sent to this user
                                                      either by another user or by
                                                      a CP System Service. Note: A
                                                      zero value may mean that the
                                                      data could not be obtained as
                                                      well as that there weren't
                                                      any messages.
     188  BC  Signed        4  USEACT_CALIUCVR        Cardinal count of messages
                                                      on the IUCV RECEIVE queue
                                                      which consists of messages
                                                      this user has received from
                                                      other users or CP System
                                                      Services, but has not yet
                                                      replied to. Note: A zero
                                                      value may mean that the data
                                                      could not be obtained as well
                                                      as that there were not any
                                                      messages.
     192  C0  Signed        4  USEACT_CALIUCVY        Cardinal count of messages
                                                      on the IUCV REPLY queue which
                                                      consists of replies to
                                                      messages this user sent
                                                      either to other users or to
                                                      CP System Services. Note: A
                                                      zero value may mean that the
                                                      data could not be obtained as
                                                      well as that there were not
                                                      any messages.
     196  C4  Signed        4  USEACT_CALVMCF         Cardinal count of messages
                                                      on the VMCF queue. Note: A
                                                      zero value may mean that the
                                                      data could not be obtained as
                                                      well as that there were not
                                                      any messages.
     200  C8  Unsigned      4  USEACT_VMDX98CT        Cumulative number of times
                                                      Diagnose X'98' was issued by
                                                      this virtual machine
     204  CC  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALCPMIG
     208  D0  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALCPXWT
     212  D4  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALCPXRD
     216  D8  Unsigned      2  USEACT_VMDASMCT        Cardinal number of non-base
                                                      address spaces owned by this
                                                      user.
     218  DA  Bitstring     1  USEACT_CALSHARF        Set Share flags
              1... ....        USEACT_VMDMXSHA         Max share is Absolute if
                                                      ON. Max share is Relative if
                                                      OFF.
              .1.. ....        USEACT_VMDSTOP          This virtual CPU is in
                                                      soft stop
              ..1. ....        USEACT_VMDSTOPD         This virtual CPU is
                                                      stopped
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        USEACT_VMDLIMTH         Max Share is Limithard if
                                                      ON. Max Share is Limitsoft if
                                                      OFF.
              .... ...1        *
     219  DB  Bitstring     1  USEACT_LCLFLAGS        General flags
              1... ....        USEACT_RELO1            Indicates this is first
                                                      record since a live guest
                                                      relocation occurred
              .1.. ....        USEACT_VMDREOFL         Reorder is always off
              ..1. ....        USEACT_VMDVVECT         Vector regs in use
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     220  DC  Unsigned      4  USEACT_VMDBLKCT        Count of SSCH's issued by
                                                      BLOCKIO system service
                                                      (includes both read and write
                                                      requests)
     224  E0  Unsigned      4  USEACT_VMDMDCIA        Count of SSCH's avoided due
                                                      to Minidisk Cache read hit
     228  E4  Unsigned      4  *                      Reserved for IBM use
                                                      Previous field is no longer
                                                      meaningful. (USEACT_VMDCOPCT)
     232  E8  Unsigned      4  USEACT_VMDCTISO        Number of times ISOLATE
                                                      occurred for spaces owned by
                                                      this virtual system. Valid
                                                      only in base VMDBK
     236  EC  Unsigned      4  USEACT_VMDRELSH        This virtual CPU's RELATIVE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Set to zero when this VMDBK
                                                      has an ABSOLUTE share value,
                                                      or has a virtual processor
                                                      dedicated to it, or is in the
                                                      process of being logged off.
                                                      Note that if the
                                                      USEACT_VMDSTOP bit is ON,
                                                      this virtual CPU share value
                                                      should not be included when
                                                      calculating the user's share
                                                      value.
     240  F0  Unsigned      4  USEACT_VMDABSSH        This virtual CPU's ABSOLUTE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Unit of value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Set to zero when this VMDBK
                                                      has a RELATIVE share value.
                                                      Note that if the
                                                      USEACT_VMDSTOP bit is ON,
                                                      this virtual CPU share value
                                                      should not be included when
                                                      calculating the user's share
                                                      value.
     244  F4  Unsigned      4  USEACT_VMDSSIZE        Virtual machine size, in
                                                      bytes. This field is kept for
                                                      compatability reasons, but
                                                      may not be accurate for
                                                      z/Arch systems where larger
                                                      virtual machines are valid.
                                                      The preferred field is
                                                      USEACT_ASCDEFSZ
     248  F8  Unsigned      4  USEACT_VMDMXRVP        Number of pages reserved
                                                      for the user
     252  FC  Character     8  USEACT_VMDACTNO        User accounting number
     260 104  Character     8  USEACT_VMDGRPN         RACF ACI group name
     268 10C  Character     8  USEACT_CALTODON        Time at which the user
                                                      logged on for this session.
                                                      In time-of-day (TOD) clock
                                                      format. To get the user's
                                                      connect time, subtract this
                                                      time value from the time
                                                      stamp in the record header's
                                                      MRHDRTOD.
     276 114  Unsigned      4  USEACT_VMDVDISK        Cumulative count of virtual
                                                      SSCH requests to
                                                      virtual disk in storage.
     280 118  Unsigned      4  USEACT_VMDMXSHR        The virtual CPU's Max share
                                                      of the system, as set in the
                                                      user's directory or via the
                                                      SET SHARE command. This value
                                                      is set to zero if no Max
                                                      share exists. If the Max
                                                      share is Absolute, then the
                                                      unit of the value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Check USEACT_VMDMXSHA to
                                                      determine if Max share is
                                                      absolute or relative. Note
                                                      that if the USEACT_VMDSTOP
                                                      bit is ON, this virtual CPU
                                                      share value should not be
                                                      included when calculating the
                                                      user's share value.
     284 11C  Unsigned      4  USEACT_VMDTHRCT        Total number of times this
                                                      user was delayed doing I/O to
                                                      a throttled device
     288 120  Unsigned      2  USEACT_IUCTOTCN        Total number of connections
                                                      for IUCV. Valid only for base
                                                      VMDKBK
     290 122  Unsigned      2  USEACT_IUCMXCN         Maximum number of
                                                      connections from the MAXCONN
                                                      directory option or the
                                                      system default.
     292 124  Unsigned      4  USEACT_VMDCTPVG        Count of private address
                                                      space resident pages in DPA
                                                      owned by this virtual machine
                                                      which are >= 2G. Valid only
                                                      in base VMDBK.
     296 128  Character     8  USEACT_ASCDEFSZ        Defined storage size in
                                                      addressable bytes, minus one.
                                                      If DEF STOR CONFIG was used
                                                      to define multiple
                                                      discontiguous extents of
                                                      addressable defined storage,
                                                      this field contains the sum
                                                      of the sizes in bytes of all
                                                      of the individual extents
                                                      (minus one). The minus one
                                                      notation is used so that a
                                                      total size of 16 Exabytes may
                                                      be represented without
                                                      ambiguity (as
                                                      x'FFFFFFFF_FFFFFFFF').
     296 128  Character     4  USEACT_CALDEFHI        high four bytes
     300 12C  Character     4  USEACT_CALDEFLO        low four bytes
     304 130  Unsigned      4  USEACT_VMDMVB2G        Number of times page
                                                      translation moved a page on
                                                      behalf of this us user from a
                                                      frame with address >= 2GB to
                                                      one < 2GB. This field is only
                                                      valid in the base VMDBK.
     308 134  Bitstring     1  USEACT_IPQF0           I/O priority flag byte. See
                                                      CP SET IOPRIORITY command for
                                                      description of absolute and
                                                      relative ranges. Valid only
                                                      in base VMDBK.
              1... ....        USEACT_IPQRELRG         Using a relative range.
                                                      Valid only in base VMDBK.
              .1.. ....        USEACT_IPQABSRG         Using an absolute range.
                                                      Valid only in base VMDBK.
              ..1. ....        USEACT_IPQGSSC          Guest requested I/O
                                                      subsystem details which
                                                      includes I/O priority
                                                      facility status. This usually
                                                      indicates that the guest is
                                                      I/O priority aware. Valid
                                                      only in base VMDBK.
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     309 135  Unsigned      1  USEACT_IPQRQLO         I/O priority requested
                                                      range low value. See CP SET
                                                      IOPRIORITY command for
                                                      description of requested and
                                                      effective I/O priority
                                                      values. Valid only in base
                                                      VMDBK.
     310 136  Unsigned      1  USEACT_IPQRQHI         I/O priority requested
                                                      range high value. Valid only
                                                      in base VMDBK.
     311 137  Unsigned      1  USEACT_IPQEFLO         I/O priority effective
                                                      range low value. Valid only
                                                      in base VMDBK.
     312 138  Unsigned      1  USEACT_IPQEFHI         I/O priority effective
                                                      range high value. Valid only
                                                      in base VMDBK.
     313 139  Unsigned      1  USEACT_CALMNEST        When configuration-topology
                                                      facility is installed, this is
                                                      the selector 2 (x) value used
                                                      by CP on STSI 15.1.x to obtain
                                                      CPU topology information. When
                                                      the configuration-topology
                                                      facility is not installed,
                                                      this contains a value of 1.

                                                      This value is used to determine
                                                      the number of valid entries in
                                                      the USEACT_VMUPLTL,
                                                          USEACT_VMUVMTL, and
                                                          USEACT_VMUSTLTL arrays.
     314 13A  Character     2  *                      Reserved and available for
                                                      IBM use.
     316 13C  Unsigned      4  USEACT_IPQDSKIP        Count of times that a DASD
                                                      I/O request was
                                                      out-prioritized by another
                                                      virtual machine's I/O. Valid
                                                      only in base VMDBK.
     320 140  Unsigned      4  USEACT_VEBALERT        Number of alert
                                                      interruptions Collected only
                                                      for base VMDBK.
     324 144  Unsigned      4  USEACT_VEBTVSCT        Number of interceptions for
                                                      guest TVS instructions
                                                      Collected only for base
                                                      VMDBK.
     328 148  Unsigned      4  USEACT_VEBSVSCT        Number of interceptions for
                                                      guest SVS instructions
                                                      Collected only for base
                                                      VMDBK.
     332 14C  Unsigned      4  USEACT_VEBTPIAI        Number of adapter
                                                      interruptions delivered via
                                                      guest TPI Collected only for
                                                      base VMDBK.
     336 150  Unsigned      4  USEACT_VEBVIRAI        Number of adapter
                                                      interruptions stacked for
                                                      guest by CP Collected only
                                                      for base VMDBK.
     340 154  Unsigned      4  USEACT_VEBHDWAI        Number of adapter
                                                      interruptions delivered to
                                                      guest inside SIE Collected
                                                      only for base VMDBK.
     344 158  Character     8  USEACT_VMDCTPVLA       Cardinal count of locked
                                                      pages in private address
                                                      spaces >2G belonging to this
                                                      user. See USEACT_VMDCTPVL for
                                                      the <2G value.
     352 160  Unsigned      4  USEACT_VMDCTSHL        Count of shared address
                                                      space resident pages <2G.
                                                      Valid only in the SYSTEM
                                                      VMDBK.
     356 164  Character     8  USEACT_VMDCTSHLA       Count of shared address
                                                      space resident pages >2G.
                                                      Valid only in the SYSTEM
                                                      VMDBK.
     364 16C  Unsigned      4  USEACT_VMDUFOLKCT      Total count of times UFO
                                                      list lock has gone into the
                                                      formal spin routine when
                                                      attempting to get the lock in
                                                      exclusive mode
     368 170  Character     8  USEACT_VMDUFOLKTM      Total elapsed spin time on
                                                      UFO list lock when attempting
                                                      to get it in exclusive mode,
                                                      starting at zero and counting
                                                      up
     376 178  Unsigned      4  *                      Reserved for IBM use - was
                                                      USEACT_VMDTMORD
     380 17C  Unsigned      4  USEACT_VMDPBKCT        Count of PGMBKs that are
                                                      currently on the PGMBK List
     384 180  Unsigned      4  *                      Reserved for IBM use - was
                                                      USEACT_VMDCRPGM
     388 184  Unsigned      4  *                      Reserved for IBM use - was
                                                      USEACT_VMDCUPGM
                                                      last reorder
     392 188  Unsigned      1  USEACT_VMDPUTYP        CPU Type. Valid values:
                                                      X'00' - General Purpose (CP)
                                                      X'02' - zSeries Application
                                                      Assist (zAAP) X'03' -
                                                      Integrated Facility for Linux
                                                      (IFL) X'04' - Internal
                                                      Coupling Facility (ICF) X'05'
                                                      - zSeries Integrated
                                                      Information (zIIP)
     393 189  Bitstring     1  USEACT_VMDCFGEM        Virtual configuration
                                                      indicators. Valid in base
                                                      VMDBK only
              1... ....        *
              .1.. ....        USEACT_VMDCPUAF         User requested CPU
                                                      Affinity
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     394 18A  Bitstring     1  USEACT_VMDPUST         CPU Status flag
              1... ....        USEACT_VMDAFSUP         CPU Affinity suppressed
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     395 18B  Character     1  *                      Reserved for IBM use
     396 18C  Character     8  USEACT_VMDVTMP         Total raw virtual time for
                                                      user on primary processor
     404 194  Character     8  USEACT_VMDTTMP         Total raw virtual and
                                                      simulation time for the user
                                                      on primary processor
     412 19C  Character     8  USEACT_VMDVTMS         Total raw virtual time for
                                                      user on secondary processor
     420 1A4  Character     8  USEACT_VMDTTMS         Total raw virtual and
                                                      simulation time for the user
                                                      on secondary processor
     428 1AC  Unsigned      4  USEACT_VMDCACHN        Number of minidisk cache
                                                      inserts
     432 1B0  Unsigned      4  USEACT_VMDCTSTA        Count of times this virtual
                                                      CPU has been started by one
                                                      of the following methods:
                                                      -SIGP START -SIGP RESTART
                                                      -Begin Command
     436 1B4  Unsigned      4  USEACT_VMDCTSTO        Count of times this virtual
                                                      CPU has been stopped by one
                                                      of the following methods:
                                                      -SIGP STOP -SIGP STOP AND
                                                      STORE STATUS -SIGP INITIAL
                                                      CPU RESET -SIGP CPU RESET
                                                      -STOP Command
     440 1B8  Unsigned      4  USEACT_VMDLKTOT        Cumulative count of times
                                                      this user has issued the LINK
                                                      command. Valid only in base
                                                      VMDBK.
     444 1BC  Unsigned      4  USEACT_VMDLKPLX        Cumulative count of times
                                                      this user has issued the LINK
                                                      command and consulted with
                                                      the SSI. Valid only in base
                                                      VMDBK.
     448 1C0  Character     8  USEACT_VMDLKTOD        Total virtual time for LINK
                                                      commands to consult with the
                                                      SSI. Valid only in base
                                                      VMDBK.
     456 1C8  Unsigned      4  USEACT_VMDDTTOT        Cumulative count of times
                                                      this user has issued the
                                                      DETACH command. Valid only in
                                                      base VMDBK.
     460 1CC  Unsigned      4  USEACT_VMDDTPLX        Cumulative count of times
                                                      this user has issued the
                                                      DETACH command and consulted
                                                      with the SSI. Valid only in
                                                      base VMDBK.
     464 1D0  Character     8  USEACT_VMDDTTOD        Total virtual time for
                                                      DETACH commands to consult
                                                      with the SSI. Valid only in
                                                      base VMDBK.
     472 1D8  Unsigned      4  USEACT_VMDWKTOT        Cumulative count of times
                                                      this user has used WRKALLEG
                                                      (SET WRKALLEG, DASDOPT
                                                      WRKALLEG or MINIOPT
                                                      WRKALLEG). Valid only in base
                                                      VMDBK.
     476 1DC  Unsigned      4  USEACT_VMDWKPLX        Cumulative count of times
                                                      this user has used WRKALLEG
                                                      (SET WRKALLEG, DASDOPT
                                                      WRKALLEG or MINIOPT WRKALLEG)
                                                      and consulted with the SSI.
                                                      Valid only in base VMDBK.
     480 1E0  Character     8  USEACT_VMDWKTOD        Total virtual time for
                                                      WRKALLEG use to consult with
                                                      the SSI. Valid only in base
                                                      VMDBK.
     488 1E8  Character     8  USEACT_VMDRLLST        Time stamp of last
                                                      relocation of this user. Only
                                                      valid if USEACT_RELO1 is ON.
     496 1F0  Character     8  USEACT_RDMNAME         Name of the guest's
                                                      relocation domain
     504 1F8  Bitstring     4  USEACT_RDMMMASK        Relocation domain's member
                                                      mask - bit mask that
                                                      indicates the slots of SSI
                                                      members that are included in
                                                      this guest's domain. (Bit 0
                                                      means SSI slot 1)
     508 1FC  Unsigned      4  USEACT_VMUNRBAL        Cumulative count of the
                                                      number of configuration
                                                      rebalances.
                                                      Valid only in base VMDBK.
     512 200  Unsigned      1  USEACT_VMUTOPNE        Number of elements that fit
                                                      in the USEACT_VMUTOPDA array.
     513 201  Unsigned      1  USEACT_VMUTOPNS        The size in bytes of one
                                                      element of the USEACT_VMUTOPDA
                                                      array.
     514 202  Unsigned      1  USEACT_VMUTOPDX        Zero-based index into the
                                                      circular array called
                                                      USEACT_VMUTOPDA. This field
                                                      indicates which element is the
                                                      most recently updated of
                                                      the ten.  A value of zero
                                                      indicates the first array
                                                      element is the latest.  A
                                                      value of one indicates the
                                                      second element is the
                                                      latest and so on.
     515 203  Unsigned      1  USEACT_MAXTOPO         Maximum number of topology
                                                      levels currently architected.
                                                      The value should be used for
                                                      array size calculation for the
                                                      following fields:
                                                        USEACT_VMUPLTL,
                                                        USEACT_VMUVMTL,
                                                        USEACT_VMUSTLTL.
     516 204  Unsigned      2  USEACT_OFFPLTL         Offset within this record to
                                                      the USEACT_VMUPLTL array.
     518 206  Unsigned      2  USEACT_OFFVMTL         Offset within this record to
                                                      the USEACT_VMUVMTL array.
     520 208  Unsigned      2  USEACT_OFFSTLTL        Offset within this record to
                                                      the USEACT_VMUSTLTL array.
     522 20A  Unsigned      2  USEACT_OFFTOPDA        Offset within this record to
                                                      the USEACT_VMUTOPDA array.
     524 20C  Unsigned      4  USEACT_VMUREBAL        The value of RCCREBAL (the
                                                      count of the number of times
                                                      a rebalance was done on this
                                                      system) at the time of the
                                                      most recent rebalance.
     528 210  Unsigned      2  USEACT_VMDSTLFC        Steal weight factor. Used to
                                                      determine the level of aggressiveness
                                                      in reclaiming frames from this
                                                      user.
                                                      Valid only for the base VMDBK.
     530 212  Unsigned      2  USEACT_VMDSTFHW        Steal weight factor high wat
                                                      mark.
                                                      Valid only for the base VMDBK.
     532 214  Unsigned      4  USEACT_VMDUFACTC       The length (in frames)
                                                      of the active section of the UFO.
                                                      Valid only for the base VMDBK.
     536 218  Unsigned      4  USEACT_VMDUFIBRC       The length (in frames)
                                                      of the IBR section of the UFO.
                                                      Valid only for the base VMDBK.
     540 21C  Unsigned      4  USEACT_CALCTINS        Cardinal count of private
                                                      instantiated pages.
                                                      Valid only for the base VMDBK.
     544 220  Unsigned      4  USEACT_CALCTIBRB2G     Cardinal count of private
                                                      IBR pages on the UFO that are
                                                      backed by frames < 2G.
                                                      Valid only for the base VMDBK.
     548 224  Unsigned      4  USEACT_CALCTIBRA2G     Cardinal count of private
                                                      IBR pages on the UFO that are
                                                      backed by frames > 2G.
                                                      Valid only for the base VMDBK.
     552 228  Unsigned      4  USEACT_CALCTAGLB2G     Cardinal count of private
                                                      IBR pages on the global aging
                                                      list that are backed by frames
                                                      < 2G.
                                                      Valid only for the base VMDBK.
     556 22C  Unsigned      4  USEACT_CALCTAGLA2G     Cardinal count of private
                                                      IBR pages on the global aging
                                                      list that are backed by frames
                                                      > 2G.
                                                      Valid only for the base VMDBK.
     560 230  Unsigned      4  USEACT_CALCTRABISB2G   Cardinal count of priva
                                                      non-faulted pages read in by a
                                                      block read, made IBR, currently
                                                      on the UFO or the global aging
                                                      list, and backed by frames < 2G.
                                                      Valid only for the base VMDBK.
     564 234  Unsigned      4  USEACT_CALCTRABISA2G   Cardinal count of priva
                                                      non-faulted pages read in by a
                                                      block read, made IBR, currently
                                                      on the UFO or the global aging
                                                      list, and backed by frames > 2G.
                                                      Valid only for the base VMDBK.
     568 238  Unsigned      4  USEACT_CALCPINT        Cumulative count of private
                                                      instantiated pages.
                                                      Valid only for the base VMDBK.
     572 23C  Unsigned      4  USEACT_CALCPREL        Cumulative count of private
                                                      pages whose frames were reclaimed
                                                      without preserving page content
                                                      because of the guest page state
                                                      (that is, the collaborative
                                                      memory management state or because
                                                      the contents was released by the
                                                      guest via DIAG x10 or Diag x214)
                                                      Valid only for the base VMDBK.
     576 240  Unsigned      4  USEACT_CALCPINV        Cumulative count of private
                                                      pages made IBR.
                                                      Valid only for the base VMDBK.
     580 244  Unsigned      4  USEACT_CALCPPFI        Cumulative count of private
                                                      IBR pages revalidated while on
                                                      the UFO.
                                                      Valid only for the base VMDBK.
     584 248  Unsigned      4  USEACT_CALCPPFA        Cumulative count of private
                                                      IBR pages revalidated while on
                                                      the global aging list.
                                                      Valid only for the base VMDBK.
     588 24C  Unsigned      4  USEACT_CALCPFRY        Cumulative count of private
                                                      IBR pages on the global aging
                                                      list that were already backed on
                                                      auxiliary before the frames
                                                      needed to be reclaimed.
                                                      Valid only for the base VMDBK.
     592 250  Unsigned      4  USEACT_CALCPFNR        Cumulative count of private
                                                      IBR pages on the UFO list that
                                                      were written to auxiliary
                                                      storage immediately before
                                                      the frames were reclaimed.
                                                      Valid only for the base VMDBK.
     596 254  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALCPXRL
     600 258  Unsigned      4  USEACT_VMDDSRSV        Cumulative count of times
                                                      demand scan could not move any
                                                      frames from the UFO to the
                                                      global aging list because it
                                                      would violate the user's SET
                                                      RESERVED setting.
                                                      Valid only for the base VMDBK.
     604 25C  Unsigned      4  USEACT_VMDWASTE        Cumulative count of times
                                                      page faults occurred for private
                                                      pages on the global aging list
                                                      that were already written to
                                                      auxiliary storage.
                                                      Valid only for the base VMDBK.
     608 260  Unsigned      4  *                      Reserved for IBM use
                                                      - was USEACT_CALCTXBK
     612 264  Character     8  USEACT_LIMPOOL         CPU pool name that the user
                                                      is assigned to.
     620 26C  Character     8  USEACT_VMDTTIME_MT1    Total MT-1 Equivalent time
                                                      which has been expended on
                                                      this VMDBK.  This includes
                                                      time which the VMDBK spent
                                                      doing its own work and also
                                                      time which CP spent doing work
                                                      on behalf of the VMDBK. It is
                                                      in CPU timer format.
     628 274  Character     8  USEACT_VMDVTIME_MT1    Total MT-1 Equivalent time
                                                      that this user was running
                                                      and doing productive work.
                                                      It does NOT include any time
                                                      that CP spends on behalf of
                                                      that user doing such things
                                                      as instruction simulation or
                                                      page translation.  This is in
                                                      CPU timer format.
     636 27C  Character     8  USEACT_VMDVTMP_MT1     MT-1 Equivalent virtual
                                                      time for the user on primary
                                                      processor.
     644 284  Character     8  USEACT_VMDTTMP_MT1     MT-1 Equivalent total
                                                      virtual and simulation time for
                                                      the user on primary processor.
     652 28C  Character     8  USEACT_VMDVTMS_MT1     MT-1 Equivalent total
                                                      virtual time for the user on
                                                      secondary processor.
     660 294  Character     8  USEACT_VMDTTMS_MT1     MT-1 Equivalent total
                                                      virtual and simulation time for
                                                      the user on secondary processor.
     668 29C  Character     8  USEACT_VMATTIME_PRO    Total Prorated Core Time
                                                      which has been expended on this
                                                      VMDBK. This includes time which the
                                                      VMDBK spent doing its own work
                                                      and also time which CP spent
                                                      doing work on behalf of the
                                                      VMDBK. It is in CPU timer format.
                                                      See the notes above.
     676 2A4  Character     8  USEACT_VMAVTIME_PRO    Total Prorated Core Time
                                                      that this user was running and
                                                      doing productive work. It does not
                                                      include any time that CP spends
                                                      on behalf of that user doing such
                                                      things as instruction simulation
                                                      or page translation.  This is in
                                                      CPU timer format.
                                                      See the notes above.
     684 2AC  Character     8  USEACT_VMAVTMP_PRO     Total Prorated Core virtual
                                                      time for user on primary processor.
                                                      See the notes above.
     692 2B4  Character     8  USEACT_VMATTMP_PRO     Total Prorated Core virtual
                                                      and simulation time for the user
                                                      on primary processor.
                                                      See the notes above.
     700 2BC  Character     8  USEACT_VMAVTMS_PRO     Total Prorated Core virtual
                                                      time for user on secondary processor.
                                                      See the notes above.
     708 2C4  Character     8  USEACT_VMATTMS_PRO     Total Prorated Core virtual
                                                      and simulation time for the user
                                                      on secondary processor.
                                                      See the notes above.
     716 2CC  Unsigned      4  *                      Reserved for IBM use
     720 2D0  Bitstring     1  USEACT_PROBITS         Prorated Core Time bits needed
                                                      to understand those fields.
              1... ....        USEACT_VMAPRCAL        Indicates whether the Prorated
                                                      Core Time values in this record
                                                      are valid. (only use if valid)
                                                      0 = values not valid
                                                      1 = values are valid
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     721 2D1  Unsigned      1  *                      Reserved for IBM use
     722 2D2  Unsigned      2  *                      Reserved for IBM use

    HOST SHARE IPTE INTERLOCK STATISTICS

    There are two sets of IPTE Interlock statistics,
    each of which is stored as a self-consistent set.

    The first set is a quintuple relating to Interlock wait and
    acquisition times. It comprises:

       CAL_VMAIPTEI, VMAIIA, VMAIIADD, VMAIIWTM and VMAIIWTSSQ.

    Derived from this are two triples from which we can
    calculate the mean and variance of host interlock
    acquisition wait times per interlock acquisition:

     1) For Interlock acquisitions using method 1 use:
        CAL_VMAIPTEI (total IPTE Interlock acquisitions
                      using method 1)

        VMAIIWTM (accumulated time waiting for the
                  interlock using method 1 or 2)

        VMAIIWTSSQ (accumulated sum of squares of time
                    waiting for the interlock
                    using method 1 or 2)

     2) For interlock acquisitions using method 2 use:
        VMAIIA (total IPTE interlock acquisitions
                using method 2)

        VMAIIWTM (accumulated time waiting for the
                  interlock using method 1 or 2)

        VMAIIWTSSQ (accumulated sum of squares of time
                   waiting for the interlock using
                   method 1 or 2)

    It is important to note that VMAIIA=0 when method 1
    is in use. When method 2 is used then
    VMAIIA=CAL_VMAIPTEI. Sums of wait times, squares of
    wait times, hold times and squares of hold times are
    accumulated for one method only.

    The remaining metric, VMAIIADD, is incremented
    whenever an interlock acquisition is granted and a
    host share is already held. It may be used with the
    total number of Interlock acquisitions to calculate
    the mean number of additional host shares per
    initial host interlock acquisition where its host
    share is not held already.

    To make this calculation, VMAIIADD and CAL_VMAIPTEI
    (or VMAIIA) are summed across all virtual CPUs.
    See note below about calculating mean and variance
    of hold times.

    Thus:

       delta-VMAIIADD/(delta-VMAIPTEI - delta-VMAIIADD)

    provides the desired mean.

    The second set is a triple relating to Interlock hold time. It comprises:

       CAL_VMAIINHLD, VMAIIHLD and VMAIIHDSSQ.

    These three values are used to calculate the mean and variance of the
    intervals over which the IPTE Interlock was continuously held by the
    host.

    Because an IPTE Interlock continuous-hold interval may begin on one
    logical CPU and terminate on another then the three values should be
    summed over all virtual CPUs of the virtual configuration before
    calculating mean and variance.

    Fields that provide sums of times are expressed in
    TOD units; and those that provide sums of squares of
    times are expressed in TOD-units-squared.

    If we carry out of the high-order bit position when
    calculating any component of the two tuples then the
    entire tuple affected is reset to zero.

    The only time any metric component within a tuple is
    observed not to increase monotonically between
    successive sample records is where the tuple has
    been reset. In all cases the recorded tuple is
    self-consistent.

    A tuple may be used as the base from which to
    calculate a delta from the previous sample provided
    each component value in that tuple is greater than
    or equal to the corresponding component of the
    previous sample's tuple.

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description
     724 2D4  Unsigned      4  USEACT_CAL_VMAIPTEI    Total count of IPTE
                                                      Interlock acquisitions using
                                                      methods 1 and 2.
      728 2D8  Unsigned     4  USEACT_VMAIIA          Count of IPTE Interlock
                                                      acquisitions using method 2.
      732 2DC  Unsigned     4  USEACT_VMAIIADD        Count of times IPTE
                                                      Interlock was acquired as an
                                                      additional host share.
      736 2E0  Character    8  USEACT_VMAIIWTM        Cumulative amount of time
                                                      spent waiting for IPTE
                                                      Interlock acquisition.
      744 2E8  Character   16  USEACT_VMAIIWTSSQ      Sum of squared time
                                                      spent waiting for IPTE
                                                      Interlock acquisition.
      760 2F8  Unsigned     4  USEACT_CAL_VMAIINHLD   Count of intervals
                                                      over which one or more host
                                                      shares of and IPTE Interlock
                                                      were continuously held.
      764 2FC  Character    8  USEACT_VMAIIHLD        Cumulative amount of
                                                      time over which one or more
                                                      of host shares of an IPTE
                                                      Interlock were continuously
                                                      held.
      772 304  Character   16  USEACT_VMAIIHDSSQ      Sum of squared time
                                                      over which one or more of the
                                                      host shares of an IPTE
                                                      Interlock were continuously
                                                      held.

    The following fields are statistics gathered by the dispatcher about how
    long a VMDBK has been dispatched and how long the VMDBK had to wait to be
    dispatched once it was ready to consume CPU time. The deltas of these
    fields between monitor intervals can be used to determine average
    dispatch time and average wait times, and using the sum of squares, the
    standard deviations of those time samples.

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description
     788 314  Unsigned      4  USEACT_CALDWTCT        Count of the number of
                                                      times this VMDBK became ready
                                                      to be dispatched (unsigned
                                                      fullword). This is calculated
                                                      using VMUDWTCT.
     792 318  Character     8  USEACT_VMUDWTETM       Accumulated elapsed time
                                                      between when this VMDBK
                                                      became ready to be dispatched
                                                      and when it was dispatched
                                                      (unsigned doubleword in
                                                      microseconds)
     800 320  Character    16  USEACT_VMUDWTTSQ       Sum of the squares of the
                                                      individual elapsed time
                                                      samples which comprise
                                                      USEACT_VMUDWTETM (unsigned
                                                      quadword in squared
                                                      microseconds) Note: Use
                                                      deltas of USEACT_CALDWTCT,
                                                      USEACT_VMUDWTETM, and this
                                                      field to calculate the
                                                      average amount of elapsed
                                                      time this VMDBK waited to be
                                                      dispatched once it became
                                                      ready, and the standard
                                                      deviation of those time
                                                      samples.
     816 330  Unsigned      4  USEACT_CALDSPCT        Count of the number of
                                                      times this VMDBK was
                                                      dispatched (unsigned
                                                      fullword). This is calculated
                                                      using VMUDSPCT. Note: This
                                                      count can be used with both
                                                      the dispatched times and the
                                                      USEACT_VMDTTIME values as
                                                      those are all calculated at
                                                      the same moment.
     820 334  Character     8  USEACT_VMUDSPETM       Accumulated elapsed time
                                                      during which this VMDBK was
                                                      dispatched (unsigned
                                                      doubleword in microseconds)
     828 33C  Character    16  USEACT_VMUDSPTSQ       Sum of the squares of the
                                                      individual elapsed time
                                                      samples which comprise
                                                      USEACT_VMUDSPETM (unsigned
                                                      quadword in squared
                                                      microseconds) Note: Use
                                                      deltas of USEACT_CALDSPCT,
                                                      USEACT_VMUDSPETM, and this
                                                      field to calculate the
                                                      average amount of elapsed
                                                      time this VMDBK was
                                                      dispatched, and the standard
                                                      deviation of those time
                                                      samples.
     844 34C  Character    16  USEACT_VMUTTIMSQ       Sum of the squares of the
                                                      individual CPU timer samples
                                                      added to VMDTTIME at
                                                      undispatch (unsigned quadword
                                                      in squared TOD clock units)
                                                      Note: Use deltas of
                                                      USEACT_CALDSPCT,
                                                      USEACT_VMDTTIME and this
                                                      field to calculate the
                                                      average amount of CPU time
                                                      this VMDBK consumed while it
                                                      was dispatched, and the
                                                      standard deviation of those
                                                      time samples.
     860 35C  Unsigned      4  USEACT_VMDCPUCH        Count of SIE entries
                                                      with SIEIHCPU <> x'FFFF' and
                                                      this is a different logical
                                                      CPU than the one on which
                                                      this VMDBK was last run
                                                      (i.e. CPU CHanged)
     864 360  Unsigned      2  USEACT_OFFDIAG          Offset to table of diagnose
                                                      counts for this virtual
                                                      processor (USEACT_VMADIAG)
     866 362  Unsigned      2  USEACT_LENDIAG          Length of table of diagnose
                                                      counts for this virtual
                                                      processor (USEACT_VMADIAG)
     868 364  Unsigned      2  USEACT_OFFSIMCT        Offset to table of simulated
                                                      instruction counts for this
                                                      virtual processor
                                                      (USEACT_VMASIMCT)
     870 366  Unsigned      2  USEACT_LENSIMCT        Length of table of simulated
                                                      instruction counts for this
                                                      virtual processor
                                                      (USEACT_VMASIMCT)
     872 368  Unsigned      2  USEACT_OFFINSOT        Offset to table of counts for
                                                      other instruction simulation
                                                      related events for this
                                                      virtual processor
                                                      (USEACT_VMAINSOT)
     874 36A  Unsigned      2  USEACT_LENINSOT        Length of table of counts for
                                                      other instruction simulation
                                                      related events for this
                                                      virtual processor
                                                      (USEACT_VMAINSOT)
     876 36C  Bitstring     1  USEACT_VMDSHELD        CPPROTECT setting
              1... ....        USEACT_VMDSHLOV        1= setting is an override
              .1.. ....        USEACT_VMDSHLON        0= MODE2 OFF
                                                      1= MODE2 ON
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     877 36D  Character     3  *                      Reserved for IBM use
     880 370  Unsigned      4  USEACT_VMDRUNCP        Count of SIE instructions
                                                      run for this VMDBK in the
                                                      HCPRUN long path

                                                      Guest Control Program Identification

                                                      Control Program Name Codes for
                                                      USEACT_VMACPNC:

                                                      X'00'       No CPNC specified.
                                                      X'01'       PR/SM
                                                      X'02'       z/VM
                                                      X'04'       Linux (including KVM)
                                                      X'06'       z/OS
                                                      X'07'       z/TPF
                                                      X'08'       z/VSE
                                                      X'20'-X'23' Supplemental codes for z/VM
                                                      X'24'-X'27' Supplemental codes for
                                                                  Linux/KVM
                                                      X'28'-X'2B' Supplemental codes for z/OS
                                                      X'2C'-X'2F' Supplemental codes for z/TPF
                                                      X'30'-X'33' Supplemental codes for z/VSE
     884 374  Unsigned      1  USEACT_VMACPNC         Control Program name code.
     885 375  Character     7  USEACT_VMACPVC         Control Program version code.
     892 37C  Structure    20  USEACT_VMA370AC        Counters of 370ACCOM
                                                      operations
     892 37C  Unsigned      4  USEACT_VMA370CK        Cumulative count of PSW
                                                      manipulations for 370ACCOM
                                                      in HCPPSWCK
     896 380  Unsigned      4  USEACT_VMA370ME        Cumulative count of PSW
                                                      manipulations for 370ACCOM
                                                      in HCPPSWME
     900 384  Unsigned      4  USEACT_VMA370EM        Cumulative count of PSW
                                                      manipulations for 370ACCOM
                                                      in HCPPSWEM
     904 388  Unsigned      4  USEACT_VMA370NM        Cumulative count of PSW
                                                      manipulations for 370ACCOM
                                                      in HCPPSWNM
     908 38C  Unsigned      4  USEACT_VMA370TMR       Cumulative count of
                                                      interval timer related
                                                      370ACCOM events
     912 390  Character     0  *                      Additional fields may be
                                                      inserted before here. Use
                                                      offsets to locate any fields
                                                      after this point.
       0   0  Unsigned      4  USEACT_VMUPLTL(0:MAXTOPO)  Array of counters of
                                                      maximum rebalance topology
                                                      distance placement. One of
                                                      these counts is incremented
                                                      each time a workload rebalance
                                                      operation assigns VMDBKs in
                                                      this guest to two or more
                                                      different DSVBKs.  None of these
                                                      counts are incremented if the
                                                      rebalance operation placed the
                                                      entire guest in one DSVBK.
                                                      These are all cumulative counts.
                                                      (Valid only in the base VMDBK.)
                                                      Entry 0:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of more
                                                             than one DSVBK that are
                                                             all in an equivalent
                                                             nesting level 1 (NL1)
                                                             topology location.
                                                      Entry 1:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of
                                                             DSVBKs in different
                                                             nesting level 1 (NL1)
                                                             topology locations but
                                                             the same NL2 location.
                                                      Entry 2:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of
                                                             DSVBKs in different
                                                             nesting level 2 (NL2)
                                                             topology locations but
                                                             the same NL3 location.
                                                      Entry 3:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of
                                                             DSVBKs in different
                                                             nesting level 3 (NL3)
                                                             topology locations but
                                                             the same NL4 location.
                                                      Entry 4:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of
                                                             DSVBKs in different
                                                             nesting level 4 (NL4)
                                                             topology locations but
                                                             the same NL5 location.
                                                      Entry 5:Count of times rebalance
                                                             placed VMDBKs of this
                                                             guest at a maximum
                                                             scatter distance of
                                                             DSVBKs in different
                                                             nesting level 5 (NL5)
                                                             topology locations.
                                                      USEACT_MAXTOPO+1 should
                                                      be used to determine the
                                                      number of elements of
                                                      this array.

                                                      Only the first USEACT_CALMNEST
                                                      entries contain valid data.
       0   0  Unsigned      4  USEACT_VMUVMTL(0:MAXTOPO)  Array of counters of
                                                      how far the VMDBK was moved
                                                      topologically during work load
                                                      rebalancing. None of these counts
                                                      are incremented if the VMDBK is
                                                      assigned to its previous home.
                                                      These are all cumulative counts.
                                                      (Valid in all VMDBKs.)
                                                      Entry 0:Count of moves between
                                                             two DSVBKs that are
                                                             both in an equivalent
                                                             nesting level 1 (NL1)
                                                             topology location
                                                      Entry 1:Count of moves between
                                                             DSVBKs in two different
                                                             nesting level 1 (NL1)
                                                             topology locations but
                                                             the same NL2 location.
                                                      Entry 2:Count of moves between
                                                             DSVBKs in two different
                                                             nesting level 2 (NL2)
                                                             topology locations but
                                                             the same NL3 location.
                                                      Entry 3:Count of moves between
                                                             DSVBKs in two different
                                                             nesting level 3 (NL3)
                                                             topology locations but
                                                             the same NL4 location.
                                                      Entry 4:Count of moves between
                                                             DSVBKs in two different
                                                             nesting level 4 (NL4)
                                                             topology locations but
                                                             the same NL5 location.
                                                      Entry 5:Count of moves between
                                                             DSVBKs in two different
                                                             nesting level 5 (NL5)
                                                             topology locations.
                                                      The USEACT_MAXTOPO+1 value
                                                      should be used to determine
                                                      the number of elements
                                                      of this array.

                                                      Only the first USEACT_CALMNEST
                                                      entries contain valid data.
       0   0  Unsigned      4  USEACT_VMUSTLTL(0:MAXTOPO)  Array of counters
                                                      indicating how many times this
                                                      VMDBK was stolen across different
                                                      topology levels.
                                                      (Valid in all VMDBKs.)
                                                      Entry 0:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK that is in an
                                                             equivalent nesting
                                                             level 1 (NL1)
                                                             topology location.
                                                      Entry 1:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK in a different
                                                             nesting level 1 (NL1)
                                                             topology location but
                                                             the same NL2 location.
                                                      Entry 2:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK in a different
                                                             nesting level 2 (NL2)
                                                             topology location but
                                                             the same NL3 location.
                                                      Entry 3:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK in a different
                                                             nesting level 3 (NL3)
                                                             topology location but
                                                             the same NL4 location.
                                                      Entry 4:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK in a different
                                                             nesting level 4 (NL4)
                                                             topology location but
                                                             the same NL5 location.
                                                      Entry 5:Count of times a CPU
                                                             stole a VMDBK from a
                                                             DSVBK in a different
                                                             nesting level 5 (NL5)
                                                             topology location.
                                                      The USEACT_MAXTOPO value
                                                      plus one should be used
                                                      to determine the number
                                                      of elements of this array.

                                                      Only the first USEACT_CALMNEST
                                                      entries contain valid data.
       0   0  Unsigned     16  USEACT_VMUTOPDA(VMUTOPNE)  An array of elements
                                                      that contain the DSVBK ID and
                                                      topology descriptor of the last
                                                      DSVBKs to which this VMDBK
                                                      was assigned by the last
                                                      rebalance functions. This is a
                                                      circular array with the
                                                      USEACT_VMUTOPDX field pointing
                                                      to the most recent element. This
                                                      array is contained in all VMDBK
                                                      records, not just the base.
                                                      Within a virtual configuration
                                                      the Nth element of the array for
                                                      each VMDBK represents the
                                                      assignment made during the same
                                                      rebalance operation.
                                                      The USEACT_VMUTOPNS value
                                                      defines the size of
                                                      one array's element.
                                                      The USEACT_VMUTOPNE value
                                                      should be used to determine
                                                      the number of elements
                                                      in this array.
                                                      Each entry is all FFs initially
                                                      until it is used and made valid.
       0   0  Character     2  USEACT_VMUTOPDI        Dispatch vector ID
       2   2  Character     4  USEACT_VMUTOPDS        This topology descriptor
                                                      or identifier consists of
                                                      the container IDs for each
                                                      level of the topology tree
                                                      above the dispatch vector
                                                      specified in USEACT_VMUTOPDI.
                                                      These container IDs are
                                                      positioned left to right with
                                                      the highest nesting level
                                                      listed first.
       6   6  Character     1  *                      Reserved for possible future
                                                      topology level expansion.
       7   7  Bitstring     1  USEACT_VMUTOPFL        Flag byte
              1... ....        USEACT_VMURROBN        Placed via round
                                                      robin algorithm
              .1.. ....        USEACT_VMUMODRB        Placed by a modified
                                                      rebalance.
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
       8   8  Character     4  USEACT_VMUTOPLU        Last CPU usage of this VMDBK
                                                      which was used to do the
                                                      home DSVBK assignment. This is
                                                      a scaled number where x'10000'
                                                      represents 100% of one CPU.
      12   C  Unsigned      4  USEACT_VMUASNORD       DSV assignment order number
                                                      that represents the relative
                                                      position in which this guest
                                                      was visited and assigned a
                                                      home by rebalance.
                                                      Valid in VMUBK for all VMDBKs.

    Provides the number of times a Diagnose was executed for this virtual
    processor.

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description
       0   0  Structure   528  USEACT_VMADIAG         Diagnose counts
       0   0  Unsigned      4  USEACT_VMADGUCT        Count of all USER diagnose
                                                      operations.
                                                      i.e. diag 100-1FC
       4   4  Unsigned      4  USEACT_VMADIAGT        Count of all z/VM defined
                                                      diagnose operations.
       8   8  Structure   516  USEACT_VMADIAG0        Diagnose counts
       8   8  Unsigned      4  USEACT_VMADGX00        Count of DIAG x'00'
      12   C  Unsigned      4  USEACT_VMADGX04        Count of DIAG x'04'
      16  10  Unsigned      4  USEACT_VMADGX08        Count of DIAG x'08'
      20  14  Unsigned      4  USEACT_VMADGX0C        Count of DIAG x'0C'
      24  18  Unsigned      4  USEACT_VMADGX10        Count of DIAG x'10'
      28  1C  Unsigned      4  USEACT_VMADGX14        Count of DIAG x'14'
      32  20  Unsigned      4  USEACT_VMADGX18        Count of DIAG x'18'
      36  24  Unsigned      4  USEACT_VMADGX1C        Count of DIAG x'1C'
      40  28  Unsigned      4  USEACT_VMADGX20        Count of DIAG x'20'
      44  2C  Unsigned      4  USEACT_VMADGX24        Count of DIAG x'24'
      48  30  Unsigned      4  USEACT_VMADGX28        Count of DIAG x'28'
      52  34  Unsigned      4  USEACT_VMADGX2C        Count of DIAG x'2C'
      56  38  Unsigned      4  USEACT_VMADGX30        Count of DIAG x'30'
      60  3C  Unsigned      4  USEACT_VMADGX34        Count of DIAG x'34'
      64  40  Unsigned      4  USEACT_VMADGX38        Count of DIAG x'38'
      68  44  Unsigned      4  USEACT_VMADGX3C        Count of DIAG x'3C'
      72  48  Unsigned      4  USEACT_VMADGX40        Count of DIAG x'40'
      76  4C  Unsigned      4  USEACT_VMADGX44        Count of DIAG x'44'
      80  50  Unsigned      4  USEACT_VMADGX48        Count of DIAG x'48'
      84  54  Unsigned      4  USEACT_VMADGX4C        Count of DIAG x'4C'
      88  58  Unsigned      4  USEACT_VMADGX50        Count of DIAG x'50'
      92  5C  Unsigned      4  USEACT_VMADGX54        Count of DIAG x'54'
      96  60  Unsigned      4  USEACT_VMADGX58        Count of DIAG x'58'
     100  64  Unsigned      4  USEACT_VMADGX5C        Count of DIAG x'5C'
     104  68  Unsigned      4  USEACT_VMADGX60        Count of DIAG x'60'
     108  6C  Unsigned      4  USEACT_VMADGX64        Count of DIAG x'64'
     112  70  Unsigned      4  USEACT_VMADGX68        Count of DIAG x'68'
     116  74  Unsigned      4  USEACT_VMADGX6C        Count of DIAG x'6C'
     120  78  Unsigned      4  USEACT_VMADGX70        Count of DIAG x'70'
     124  7C  Unsigned      4  USEACT_VMADGX74        Count of DIAG x'74'
     128  80  Unsigned      4  USEACT_VMADGX78        Count of DIAG x'78'
     132  84  Unsigned      4  USEACT_VMADGX7C        Count of DIAG x'7C'
     136  88  Unsigned      4  USEACT_VMADGX80        Count of DIAG x'80'
     140  8C  Unsigned      4  USEACT_VMADGX84        Count of DIAG x'84'
     144  90  Unsigned      4  USEACT_VMADGX88        Count of DIAG x'88'
     148  94  Unsigned      4  USEACT_VMADGX8C        Count of DIAG x'8C'
     152  98  Unsigned      4  USEACT_VMADGX90        Count of DIAG x'90'
     156  9C  Unsigned      4  USEACT_VMADGX94        Count of DIAG x'94'
     160  A0  Unsigned      4  USEACT_VMADGX98        Count of DIAG x'98'
     164  A4  Unsigned      4  USEACT_VMADGX9C        Count of DIAG x'9C'
     168  A8  Unsigned      4  USEACT_VMADGXA0        Count of DIAG x'A0'
     172  AC  Unsigned      4  USEACT_VMADGXA4        Count of DIAG x'A4'
     176  B0  Unsigned      4  USEACT_VMADGXA8        Count of DIAG x'A8'
     180  B4  Unsigned      4  USEACT_VMADGXAC        Count of DIAG x'AC'
     184  B8  Unsigned      4  USEACT_VMADGXB0        Count of DIAG x'B0'
     188  BC  Unsigned      4  USEACT_VMADGXB4        Count of DIAG x'B4'
     192  C0  Unsigned      4  USEACT_VMADGXB8        Count of DIAG x'B8'
     196  C4  Unsigned      4  USEACT_VMADGXBC        Count of DIAG x'BC'
     200  C8  Unsigned      4  USEACT_VMADGXC0        Count of DIAG x'C0'
     204  CC  Unsigned      4  USEACT_VMADGXC4        Count of DIAG x'C4'
     208  D0  Unsigned      4  USEACT_VMADGXC8        Count of DIAG x'C8'
     212  D4  Unsigned      4  USEACT_VMADGXCC        Count of DIAG x'CC'
     216  D8  Unsigned      4  USEACT_VMADGXD0        Count of DIAG x'D0'
     220  DC  Unsigned      4  USEACT_VMADGXD4        Count of DIAG x'D4'
     224  E0  Unsigned      4  USEACT_VMADGXD8        Count of DIAG x'D8'
     228  E4  Unsigned      4  USEACT_VMADGXDC        Count of DIAG x'DC'
     232  E8  Unsigned      4  USEACT_VMADGXE0        Count of DIAG x'E0'
     236  EC  Unsigned      4  USEACT_VMADGXE4        Count of DIAG x'E4'
     240  F0  Unsigned      4  USEACT_VMADGXE8        Count of DIAG x'E8'
     244  F4  Unsigned      4  USEACT_VMADGXEC        Count of DIAG x'EC'
     248  F8  Unsigned      4  USEACT_VMADGXF0        Count of DIAG x'F0'
     252  FC  Unsigned      4  USEACT_VMADGXF4        Count of DIAG x'F4'
     256 100  Unsigned      4  USEACT_VMADGXF8        Count of DIAG x'F8'
     260 104  Unsigned      4  USEACT_VMADGXFC        Count of DIAG x'FC'

     264 108  Structure    64  USEACT_VMADIAG2        Diagnose counts
     264 108  Unsigned      4  USEACT_VMADG200        Count of DIAG x'200'
     268 10C  Unsigned      4  USEACT_VMADG204        Count of DIAG x'204'
     272 110  Unsigned      4  USEACT_VMADG208        Count of DIAG x'208'
     276 114  Unsigned      4  USEACT_VMADG20C        Count of DIAG x'20C'
     280 118  Unsigned      4  USEACT_VMADG210        Count of DIAG x'210'
     284 11C  Unsigned      4  USEACT_VMADG214        Count of DIAG x'214'
     288 120  Unsigned      4  USEACT_VMADG218        Count of DIAG x'218'
     292 124  Unsigned      4  USEACT_VMADG21C        Count of DIAG x'21C'
     296 128  Unsigned      4  USEACT_VMADG220        Count of DIAG x'220'
     300 12C  Unsigned      4  USEACT_VMADG224        Count of DIAG x'224'
     304 130  Unsigned      4  USEACT_VMADG228        Count of DIAG x'228'
     308 134  Unsigned      4  USEACT_VMADG22C        Count of DIAG x'22C'
     312 138  Unsigned      4  USEACT_VMADG230        Count of DIAG x'230'
     316 13C  Unsigned      4  USEACT_VMADG234        Count of DIAG x'234'
     320 140  Unsigned      4  USEACT_VMADG238        Count of DIAG x'238'
     324 144  Unsigned      4  USEACT_VMADG23C        Count of DIAG x'23C'
     328 148  Unsigned      4  USEACT_VMADG240        Count of DIAG x'240'
     332 14C  Unsigned      4  USEACT_VMADG244        Count of DIAG x'244'
     336 150  Unsigned      4  USEACT_VMADG248        Count of DIAG x'248'
     340 154  Unsigned      4  USEACT_VMADG24C        Count of DIAG x'24C'
     344 158  Unsigned      4  USEACT_VMADG250        Count of DIAG x'250'
     348 15C  Unsigned      4  USEACT_VMADG254        Count of DIAG x'254'
     352 160  Unsigned      4  USEACT_VMADG258        Count of DIAG x'258'
     356 164  Unsigned      4  USEACT_VMADG25C        Count of DIAG x'25C'
     360 168  Unsigned      4  USEACT_VMADG260        Count of DIAG x'260'
     364 16C  Unsigned      4  USEACT_VMADG264        Count of DIAG x'264'
     368 170  Unsigned      4  USEACT_VMADG268        Count of DIAG x'268'
     372 174  Unsigned      4  USEACT_VMADG26C        Count of DIAG x'26C'
     376 178  Unsigned      4  USEACT_VMADG270        Count of DIAG x'270'
     380 17C  Unsigned      4  USEACT_VMADG274        Count of DIAG x'274'
     384 180  Unsigned      4  USEACT_VMADG278        Count of DIAG x'278'
     388 184  Unsigned      4  USEACT_VMADG27C        Count of DIAG x'27C'
     392 188  Unsigned      4  USEACT_VMADG280        Count of DIAG x'280'
     396 18C  Unsigned      4  USEACT_VMADG284        Count of DIAG x'284'
     400 190  Unsigned      4  USEACT_VMADG288        Count of DIAG x'288'
     404 194  Unsigned      4  USEACT_VMADG28C        Count of DIAG x'28C'
     408 198  Unsigned      4  USEACT_VMADG290        Count of DIAG x'290'
     412 19C  Unsigned      4  USEACT_VMADG294        Count of DIAG x'294'
     416 1A0  Unsigned      4  USEACT_VMADG298        Count of DIAG x'298'
     420 1A4  Unsigned      4  USEACT_VMADG29C        Count of DIAG x'29C'
     424 1A8  Unsigned      4  USEACT_VMADG2A0        Count of DIAG x'2A0'
     428 1AC  Unsigned      4  USEACT_VMADG2A4        Count of DIAG x'2A4'
     432 1B0  Unsigned      4  USEACT_VMADG2A8        Count of DIAG x'2A8'
     436 1B4  Unsigned      4  USEACT_VMADG2AC        Count of DIAG x'2AC'
     440 1B8  Unsigned      4  USEACT_VMADG2B0        Count of DIAG x'2B0'
     444 1BC  Unsigned      4  USEACT_VMADG2B4        Count of DIAG x'2B4'
     448 1C0  Unsigned      4  USEACT_VMADG2B8        Count of DIAG x'2B8'
     452 1C4  Unsigned      4  USEACT_VMADG2BC        Count of DIAG x'2BC'
     456 1C8  Unsigned      4  USEACT_VMADG2C0        Count of DIAG x'2C0'
     460 1CC  Unsigned      4  USEACT_VMADG2C4        Count of DIAG x'2C4'
     464 1D0  Unsigned      4  USEACT_VMADG2C8        Count of DIAG x'2C8'
     468 1D4  Unsigned      4  USEACT_VMADG2CC        Count of DIAG x'2CC'
     472 1D8  Unsigned      4  USEACT_VMADG2D0        Count of DIAG x'2D0'
     476 1DC  Unsigned      4  USEACT_VMADG2D4        Count of DIAG x'2D4'
     480 1E0  Unsigned      4  USEACT_VMADG2D8        Count of DIAG x'2D8'
     484 1E4  Unsigned      4  USEACT_VMADG2DC        Count of DIAG x'2DC'
     488 1E8  Unsigned      4  USEACT_VMADG2E0        Count of DIAG x'2E0'
     492 1EC  Unsigned      4  USEACT_VMADG2E4        Count of DIAG x'2E4'
     496 1F0  Unsigned      4  USEACT_VMADG2E8        Count of DIAG x'2E8'
     500 1F4  Unsigned      4  USEACT_VMADG2EC        Count of DIAG x'2EC'
     504 1F8  Unsigned      4  USEACT_VMADG2F0        Count of DIAG x'2F0'
     508 1FC  Unsigned      4  USEACT_VMADG2F4        Count of DIAG x'2F4'
     512 200  Unsigned      4  USEACT_VMADG2F8        Count of DIAG x'2F8'
     516 204  Unsigned      4  USEACT_VMADG2FC        Count of DIAG x'2FC'

     520 208  Structure     8  USEACT_VMADIAG3        Diagnose counts
     520 208  Unsigned      4  USEACT_VMADG308        Count of DIAG x'308'
     524 20C  Unsigned      4  USEACT_VMADG318        Count of DIAG x'318'

    Counts of instructions simulated for this virtual processor. Actually they are
    counts of the number of times the various instructions were intercepted.
    There are occasions when an instruction is intercepted and CP takes
    an action other than simulating the instruction.

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description
       0   0  Structure   496  USEACT_VMASIMCT        Table of Counters
       0   0  Unsigned      4  USEACT_VMA_PR          PR    (0101)
       4   4  Unsigned      4  USEACT_VMAPTFF         PTFF  (0104)
       8   8  Unsigned      4  USEACT_VMA_0105              (0105)
      12   C  Unsigned      4  USEACT_VMA_0106              (0106)
      16  10  Unsigned      4  USEACT_VMASCKPF        SCKPF (0107)
      20  14  Unsigned      4  USEACT_VMA_0108              (0108)
      24  18  Unsigned      4  USEACT_VMA_0109              (0109)
      28  1C  Unsigned      4  USEACT_VMAKEYSK        SSK   (08)
      32  20  Unsigned      4  USEACT_VMAKEYIK        ISK   (09)
      36  24  Unsigned      4  USEACT_VMAPRVSV        SVC   (0A)
      40  28  Unsigned      4  USEACT_VMAPRVMS        SSM   (80)
      44  2C  Unsigned      4  USEACT_VMAPRVLP        LPSW  (82)
      48  30  Unsigned      4  USEACT_VMASIOCT        SIO   (9C)
                                                      Also SIOF and RIO
      52  34  Unsigned      4  USEACT_VMA_TIO         TIO   (9D)
                                                      Also CLRIO
      56  38  Unsigned      4  USEACT_VMA_HIO         HIO   (9E)
                                                      Also HDV
      60  3C  Unsigned      4  USEACT_VMA_TCH         TCH   (9F)
                                                      Also CLRCH
      64  40  Unsigned      4  USEACT_VMAPRVMN        STNSM (AC)
      68  44  Unsigned      4  USEACT_VMAPRVMO        STOSM (AD)
      72  48  Unsigned      4  USEACT_VMAPRVGP        SIGP  (AE)
      76  4C  Unsigned      4  USEACT_VMABISCP        STIDP (B202)
      80  50  Unsigned      4  USEACT_VMA_STIDC       STIDC (B203)
      84  54  Unsigned      4  USEACT_VMABISTE        SCK   (B204)
      88  58  Unsigned      4  USEACT_VMABISPB        PTLB  (B20D)
      92  5C  Unsigned      4  USEACT_VMABISXE        SPX   (B210)
      96  60  Unsigned      4  USEACT_VMABISXS        STPX  (B211)
     100  64  Unsigned      4  USEACT_VMABISAS        STAP  (B212)
     104  68  Unsigned      4  USEACT_VMAKEYRR        RRB   (B213)
     108  6C  Unsigned      4  USEACT_VMABISSI        SIE   (B214)
     112  70  Unsigned      4  USEACT_VMA_PC          PC    (B218)
     116  74  Unsigned      4  USEACT_VMAPCVSC        SERVC (B220)
     120  78  Unsigned      4  USEACT_VMAVPTNV        IPTE  (B221)
     124  7C  Unsigned      4  USEACT_VMA_PT          PT    (B228)
     128  80  Unsigned      4  USEACT_VMAKEYIE        ISKE  (B229)
     132  84  Unsigned      4  USEACT_VMAKEYRE        RRBE  (B22A)
     136  88  Unsigned      4  USEACT_VMAKEYSE        SSKE  (B22B)
     140  8C  Unsigned      4  USEACT_VMABISBT        TB    (B22C)
     144  90  Unsigned      4  USEACT_VMAXPGIN        PGIN  (B22E)
     148  94  Unsigned      4  USEACT_VMAXPGOU        PGOUT (B22F)
     152  98  Unsigned      4  USEACT_VMA_CSCH        CSCH  (B230)
     156  9C  Unsigned      4  USEACT_VMA_HSCH        HSCH  (B231)
     160  A0  Unsigned      4  USEACT_VMA_MSCH        MSCH  (B232)
     164  A4  Unsigned      4  USEACT_VMA_SSCH        SSCH  (B233)
     168  A8  Unsigned      4  USEACT_VMA_STSCH       STSCH (B234)
     172  AC  Unsigned      4  USEACT_VMA_TSCH        TSCH  (B235)
     176  B0  Unsigned      4  USEACT_VMA_TPI         TPI   (B236)
     180  B4  Unsigned      4  USEACT_VMA_SAL         SAL   (B237)
     184  B8  Unsigned      4  USEACT_VMA_RSCH        RSCH  (B238)
     188  BC  Unsigned      4  USEACT_VMA_STCRW       STCRW (B239)
     192  C0  Unsigned      4  USEACT_VMA_STCPS       STCPS (B23A)
     196  C4  Unsigned      4  USEACT_VMA_RCHP        RCHP  (B23B)
     200  C8  Unsigned      4  USEACT_VMA_SCHM        SCHM  (B23C)
     204  CC  Unsigned      4  USEACT_VMA_PALB        PALB  (B248)
     208  D0  Unsigned      4  USEACT_VMA_TAR         TAR   (B24C)
     212  D4  Unsigned      4  USEACT_VMAVCSP         CSP   (B250)
     216  D8  Unsigned      4  USEACT_VMASTHYI        STHYI (B256)
     220  DC  Unsigned      4  USEACT_VMA_BSG         BSG   (B258)
     224  E0  Unsigned      4  USEACT_VMAVIESB        IESBE (B259)
     228  E4  Unsigned      4  USEACT_VMAXPG5A        BSA   (B25A)
     232  E8  Unsigned      4  USEACT_VMA_B25F              (B25F)
     236  EC  Unsigned      4  USEACT_VMA_B260              (B260)
     240  F0  Unsigned      4  USEACT_VMA_B261              (B261)
     244  F4  Unsigned      4  USEACT_VMA_B264              (B264)
     248  F8  Unsigned      4  USEACT_VMA_B265              (B265)
     252  FC  Unsigned      4  USEACT_VMA_B266              (B266)
     256 100  Unsigned      4  USEACT_VMA_B267              (B267)
     260 104  Unsigned      4  USEACT_VMA_B268              (B268)
     264 108  Unsigned      4  USEACT_VMA_B272              (B272)
     268 10C  Unsigned      4  USEACT_VMA_B274              (B274)
     272 110  Unsigned      4  USEACT_VMA_XSCH        XSCH  (B276)
     276 114  Unsigned      4  USEACT_VMA_B27A              (B27A)
     280 118  Unsigned      4  USEACT_VMABISST        STSI  (B27D)
     284 11C  Unsigned      4  USEACT_VMA_B27E              (B27E)
     288 120  Unsigned      4  USEACT_VMA_B27F              (B27F)
     292 124  Unsigned      4  USEACT_VMA_B2A4              (B2A4)
     296 128  Unsigned      4  USEACT_VMA_B2AD              (B2AD)
     300 12C  Unsigned      4  USEACT_VMA_B2AE              (B2AE)
     304 130  Unsigned      4  USEACT_VMA_B2AF              (B2AF)
     308 134  Unsigned      4  USEACT_VMASTFLE        STFLE (B2B0)
     312 138  Unsigned      4  USEACT_VMA0STFL        STFL  (B2B1)
     316 13C  Unsigned      4  USEACT_VMALPSWE        LPSWE (B2B2)
     320 140  Unsigned      4  USEACT_VMABISIU        IUCV  (B2F0)
     324 144  Unsigned      4  USEACT_VMAPRVTC        STCTL (B6)
     328 148  Unsigned      4  USEACT_VMAPRVLC        LCTL  (B7)
     332 14C  Unsigned      4  USEACT_VMA_KMAC        KMAC  (B91E)
     336 150  Unsigned      4  USEACT_VMA_PCKMO       PCKMO (B928)
     340 154  Unsigned      4  USEACT_VMA_KMA         KMA   (B929)
     344 158  Unsigned      4  USEACT_VMA_KMF         KMF   (B92A)
     348 15C  Unsigned      4  USEACT_VMA_KMO         KMO   (B92B)
     352 160  Unsigned      4  USEACT_VMA_PCC         PCC   (B92C)
     356 164  Unsigned      4  USEACT_VMA_KMCTR       KMCTR (B92D)
     360 168  Unsigned      4  USEACT_VMA_KM          KM    (B92E)
     364 16C  Unsigned      4  USEACT_VMA_KMC         KMC   (B92F)
     368 170  Unsigned      4  USEACT_VMA_PPNO        PPNO  (B93C)
     372 174  Unsigned      4  USEACT_VMA_KIMD        KIMD  (B93E)
     376 178  Unsigned      4  USEACT_VMA_KLMD        KLMD  (B93F)
     380 17C  Unsigned      4  USEACT_VMAVCSPG        CSPG  (B98A)
     384 180  Unsigned      4  USEACT_VMA0EPSW        EPSW  (B98D)
     388 184  Unsigned      4  USEACT_VMAVIDTE        IDTE  (B98E)
     392 188  Unsigned      4  USEACT_VMA_B99C              (B99C)
     396 18C  Unsigned      4  USEACT_VMA0ESEA        ESEA  (B99D)
     400 190  Unsigned      4  USEACT_VMA_PTI         PTI   (B99E)
     404 194  Unsigned      4  USEACT_VMA_B9A0              (B9A0)
     408 198  Unsigned      4  USEACT_VMAESSA         ESSA  (B9AB)
     412 19C  Unsigned      4  USEACT_VMABPFMF        PFMF  (B9AF)
     416 1A0  Unsigned      4  USEACT_VMA_B9D0              (B9D0)
     420 1A4  Unsigned      4  USEACT_VMA_B9D2              (B9D2)
     424 1A8  Unsigned      4  USEACT_VMA_B9D3              (B9D3)
     428 1AC  Unsigned      4  USEACT_VMA_E328              (E328)
     432 1B0  Unsigned      4  USEACT_VMA_E3D0              (E3D0)
     436 1B4  Unsigned      4  USEACT_VMA_E3D1              (E3D1)
     440 1B8  Unsigned      4  USEACT_VMA_E3D4              (E3D4)
     444 1BC  Unsigned      4  USEACT_VMA_LASP        LASP  (E500)
     448 1C0  Unsigned      4  USEACT_VMAPRVTP        TPROT (E501)
     452 1C4  Unsigned      4  USEACT_VMAPRVSG        STCTG (EB25)
     456 1C8  Unsigned      4  USEACT_VMAPRVLG        LCTLG (EB2F)
     460 1CC  Unsigned      4  USEACT_VMA_EB8A              (EB8A)
     464 1D0  Unsigned      4  USEACT_VMA_EBD0              (EBD0)
     468 1D4  Unsigned      4  USEACT_VMA_EBD1              (EBD1)
     472 1D8  Unsigned      4  USEACT_VMA_PLO         PLO   (EE)
     476 1DC  Unsigned      4  USEACT_VMA_SORTL       SORTL (B938)
     480 1E0  Unsigned      4  USEACT_VMA_DFLTC      DFLTCC (B939)
     484 1E4  Unsigned      4  USEACT_VMA_KDSA        KDSA  (B93A)
     488 1E8  Unsigned      4  USEACT_VMALPSWY       LPSWEY (EB71)
     492 1EC  Unsigned      4  USEACT_VMARDP          RDP   (B98B)

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description
       0   0  Structure    24  USEACT_VMAINSOT        Other instruction
                                                      simulation related counters.
       0   0  Unsigned      4  USEACT_VMAPRVVN        Guest SVC 76's reflected
                                                      to the guest
       4   4  Unsigned      4  USEACT_VMAPRVSC        Count of SVC interrupts
                                                      reflected to the guest
       8   8  Unsigned      4  USEACT_VMAFST44        Count of fast path diagnose
                                                      44s
      12   C  Unsigned      4  USEACT_VMAFSTPX        Count of fast path
                                                      processing of partial
                                                      execution intercepts
      16  10  Unsigned      4  USEACT_VMAFSTSG        Count of fast path
                                                      simulations of SIGP
                                                      external calls
      20  14  Unsigned      4  USEACT_VMAFSTXC        Count of fast path
                                                      reflections of guest
                                                      external call interruptions
       *   *  Character     0  USEACT_END

#### MRUSEACT Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    USEACT                     0    912+
    USEACT_ASCDEFSZ          128      8
    USEACT_CAL_VMAIINHLD     2F8      4
    USEACT_CAL_VMAIPTEI      2D4      4
    USEACT_CALBASE            22           80
    USEACT_CALCPFNR          250      4
    USEACT_CALCPFRY          24C      4
    USEACT_CALCPINT          238      4
    USEACT_CALCPINV          240      4
    USEACT_CALCPPFA          248      4
    USEACT_CALCPPFI          244      4
    USEACT_CALCPPGR           74      4
    USEACT_CALCPPGW           78      4
    USEACT_CALCPPST           9C      4
    USEACT_CALCPREL          23C      4
    USEACT_CALCTAGLA2G       22C      4
    USEACT_CALCTAGLB2G       228      4
    USEACT_CALCTIBRA2G       224      4
    USEACT_CALCTIBRB2G       220      4
    USEACT_CALCTINS          21C      4
    USEACT_CALCTPGS           68      4
    USEACT_CALCTRABISA2G     234      4
    USEACT_CALCTRABISB2G     230      4
    USEACT_CALDEFHI          128      4
    USEACT_CALDEFLO          12C      4
    USEACT_CALDIAL            22           20
    USEACT_CALDSPCT          330      4
    USEACT_CALDWTCT          314      4
    USEACT_CALFLAG1           22      1
    USEACT_CALIUCVR           BC      4
    USEACT_CALIUCVS           B8      4
    USEACT_CALIUCVY           C0      4
    USEACT_CALMESA            1F           40
    USEACT_CALMESAM           1F           04
    USEACT_CALMNEST          139      1
    USEACT_CALMODE            1F      1
    USEACT_CALMXA             1F           20
    USEACT_CALMXC             1F           08
    USEACT_CALMZONL           1F           01
    USEACT_CALM370            1F           10
    USEACT_CALSHARF           DA      1
    USEACT_CALSNA             22           10
    USEACT_CALTODON          10C      8
    USEACT_CALVARCH           1F           02
    USEACT_CALVMCF            C4      4
    USEACT_END                 *      *
    USEACT_IPQABSRG          134           40
    USEACT_IPQDSKIP          13C      4
    USEACT_IPQEFHI           138      1
    USEACT_IPQEFLO           137      1
    USEACT_IPQF0             134      1
    USEACT_IPQGSSC           134           20
    USEACT_IPQRELRG          134           80
    USEACT_IPQRQHI           136      1
    USEACT_IPQRQLO           135      1
    USEACT_IUCMXCN           122      2
    USEACT_IUCTOTCN          120      2
    USEACT_LCLFLAGS           DB      1
    USEACT_LENDIAG           362      2
    USEACT_LENINSOT          36A      2
    USEACT_LENSIMCT          366      2
    USEACT_LIMPOOL           612      8
    USEACT_MAXTOPO           203      1
    USEACT_MRHDR               0      0
    USEACT_OFFDIAG           360      2
    USEACT_OFFINSOT          368      2
    USEACT_OFFPLTL           204      2
    USEACT_OFFSIMCT          364      2
    USEACT_OFFSTLTL          208      2
    USEACT_OFFTOPDA          20A      2
    USEACT_OFFVMTL           206      2
    USEACT_PROBITS           2D0      1
    USEACT_RDMMMASK          1F8      4
    USEACT_RDMNAME           1F0      8
    USEACT_RELO1              DB           80
    USEACT_VEBALERT          140      4
    USEACT_VEBHDWAI          154      4
    USEACT_VEBSVSCT          148      4
    USEACT_VEBTPIAI          14C      4
    USEACT_VEBTVSCT          144      4
    USEACT_VEBVIRAI          150      4
    USEACT_VMA_0105            8      4
    USEACT_VMA_0106            C      4
    USEACT_VMA_0108           14      4
    USEACT_VMA_0109           18      4
    USEACT_VMA_BSG            DC      4
    USEACT_VMA_B25F           E8      4
    USEACT_VMA_B260           EC      4
    USEACT_VMA_B261           F0      4
    USEACT_VMA_B264           F4      4
    USEACT_VMA_B265           F8      4
    USEACT_VMA_B266           FC      4
    USEACT_VMA_B267          100      4
    USEACT_VMA_B268          104      4
    USEACT_VMA_B272          108      4
    USEACT_VMA_B274          10C      4
    USEACT_VMA_B27A          114      4
    USEACT_VMA_B27E          11C      4
    USEACT_VMA_B27F          120      4
    USEACT_VMA_B2A4          124      4
    USEACT_VMA_B2AD          128      4
    USEACT_VMA_B2AE          12C      4
    USEACT_VMA_B2AF          130      4
    USEACT_VMA_B99C          188      4
    USEACT_VMA_B9A0          194      4
    USEACT_VMA_B9D0          1B0      4
    USEACT_VMA_B9D2          1B4      4
    USEACT_VMA_B9D3          1B8      4
    USEACT_VMA_CSCH           98      4
    USEACT_VMA_DFLTC         1E0      4
    USEACT_VMA_E328          1BC      4
    USEACT_VMA_E3D0          1C0      4
    USEACT_VMA_E3D1          1C4      4
    USEACT_VMA_E3D4          1C8      4
    USEACT_VMA_EB8A          1CC      4
    USEACT_VMA_EBD0          1D0      4
    USEACT_VMA_EBD1          1D4      4
    USEACT_VMA_HIO            38      4
    USEACT_VMA_HSCH           9C      4
    USEACT_VMA_KDSA          1E4      4
    USEACT_VMA_KIMD          174      4
    USEACT_VMA_KLMD          178      4
    USEACT_VMA_KM            168      4
    USEACT_VMA_KMA           154      4
    USEACT_VMA_KMAC          14C      4
    USEACT_VMA_KMC           16C      4
    USEACT_VMA_KMCTR         164      4
    USEACT_VMA_KMF           158      4
    USEACT_VMA_KMO           15C      4
    USEACT_VMA_LASP          1CC      4
    USEACT_VMA_MSCH           A0      4
    USEACT_VMA_PALB           CC      4
    USEACT_VMA_PC             70      4
    USEACT_VMA_PCC           160      4
    USEACT_VMA_PCKMO         150      4
    USEACT_VMA_PLO           1D8      4
    USEACT_VMA_PPNO          170      4
    USEACT_VMA_PR              0      4
    USEACT_VMA_PT             7C      4
    USEACT_VMA_PTI           190      4
    USEACT_VMA_RCHP           C4      4
    USEACT_VMA_RSCH           B8      4
    USEACT_VMA_SAL            B4      4
    USEACT_VMA_SCHM           C8      4
    USEACT_VMA_SORTL         1DC      4
    USEACT_VMA_SSCH           A4      4
    USEACT_VMA_STCPS          C0      4
    USEACT_VMA_STCRW          BC      4
    USEACT_VMA_STIDC          50      4
    USEACT_VMA_STSCH          A8      4
    USEACT_VMA_TAR            D0      4
    USEACT_VMA_TCH            3C      4
    USEACT_VMA_TIO            34      4
    USEACT_VMA_TPI            B0      4
    USEACT_VMA_TSCH           AC      4
    USEACT_VMA_XSCH          110      4
    USEACT_VMA0EPSW          180      4
    USEACT_VMA0ESEA          18C      4
    USEACT_VMA0STFL          138      4
    USEACT_VMA370AC          37C     20
    USEACT_VMA370CK          37C      4
    USEACT_VMA370EM          384      4
    USEACT_VMA370ME          380      4
    USEACT_VMA370NM          388      4
    USEACT_VMA370TMR         38C      4
    USEACT_VMABISAS           64      4
    USEACT_VMABISBT           8C      4
    USEACT_VMABISCP           4C      4
    USEACT_VMABISIU          140      4
    USEACT_VMABISPB           58      4
    USEACT_VMABISSI           6C      4
    USEACT_VMABISST          118      4
    USEACT_VMABISTE           54      4
    USEACT_VMABISXE           5C      4
    USEACT_VMABISXS           60      4
    USEACT_VMABPFMF          19C      4
    USEACT_VMACPNC           374      1
    USEACT_VMACPVC           375      7
    USEACT_VMADGUCT            0      0
    USEACT_VMADGX00            8      4
    USEACT_VMADGX04            C      4
    USEACT_VMADGX08           10      4
    USEACT_VMADGX0C           14      4
    USEACT_VMADGX10           18      4
    USEACT_VMADGX14           1C      4
    USEACT_VMADGX18           20      4
    USEACT_VMADGX1C           24      4
    USEACT_VMADGX20           28      4
    USEACT_VMADGX24           2C      4
    USEACT_VMADGX28           30      4
    USEACT_VMADGX2C           34      4
    USEACT_VMADGX30           38      4
    USEACT_VMADGX34           3C      4
    USEACT_VMADGX38           40      4
    USEACT_VMADGX3C           44      4
    USEACT_VMADGX40           48      4
    USEACT_VMADGX44           4C      4
    USEACT_VMADGX48           50      4
    USEACT_VMADGX4C           54      4
    USEACT_VMADGX50           58      4
    USEACT_VMADGX54           5C      4
    USEACT_VMADGX58           60      4
    USEACT_VMADGX5C           64      4
    USEACT_VMADGX60           68      4
    USEACT_VMADGX64           6C      4
    USEACT_VMADGX68           70      4
    USEACT_VMADGX6C           74      4
    USEACT_VMADGX70           78      4
    USEACT_VMADGX74           7C      4
    USEACT_VMADGX78           80      4
    USEACT_VMADGX7C           84      4
    USEACT_VMADGX80           88      4
    USEACT_VMADGX84           8C      4
    USEACT_VMADGX88           90      4
    USEACT_VMADGX8C           94      4
    USEACT_VMADGX90           98      4
    USEACT_VMADGX94           9C      4
    USEACT_VMADGX98           A0      4
    USEACT_VMADGX9C           A4      4
    USEACT_VMADGXA0           A8      4
    USEACT_VMADGXA4           AC      4
    USEACT_VMADGXA8           B0      4
    USEACT_VMADGXAC           B4      4
    USEACT_VMADGXB0           B8      4
    USEACT_VMADGXB4           BC      4
    USEACT_VMADGXB8           C0      4
    USEACT_VMADGXBC           C4      4
    USEACT_VMADGXC0           C8      4
    USEACT_VMADGXC4           CC      4
    USEACT_VMADGXC8           D0      4
    USEACT_VMADGXCC           D4      4
    USEACT_VMADGXD0           D8      4
    USEACT_VMADGXD4           DC      4
    USEACT_VMADGXD8           E0      4
    USEACT_VMADGXDC           E4      4
    USEACT_VMADGXE0           E8      4
    USEACT_VMADGXE4           EC      4
    USEACT_VMADGXE8           F0      4
    USEACT_VMADGXEC           F4      4
    USEACT_VMADGXF0           F8      4
    USEACT_VMADGXF4           FC      4
    USEACT_VMADGXF8          100      4
    USEACT_VMADGXFC          104      4
    USEACT_VMADG200          108      4
    USEACT_VMADG204          10C      4
    USEACT_VMADG208          110      4
    USEACT_VMADG20C          114      4
    USEACT_VMADG210          118      4
    USEACT_VMADG214          11C      4
    USEACT_VMADG218          120      4
    USEACT_VMADG21C          124      4
    USEACT_VMADG220          128      4
    USEACT_VMADG224          12C      4
    USEACT_VMADG228          130      4
    USEACT_VMADG22C          134      4
    USEACT_VMADG230          138      4
    USEACT_VMADG234          13C      4
    USEACT_VMADG238          140      4
    USEACT_VMADG23C          144      4
    USEACT_VMADG240          148      4
    USEACT_VMADG244          14C      4
    USEACT_VMADG248          150      4
    USEACT_VMADG24C          154      4
    USEACT_VMADG250          158      4
    USEACT_VMADG254          15C      4
    USEACT_VMADG258          160      4
    USEACT_VMADG25C          164      4
    USEACT_VMADG260          168      4
    USEACT_VMADG264          16C      4
    USEACT_VMADG268          170      4
    USEACT_VMADG26C          174      4
    USEACT_VMADG270          178      4
    USEACT_VMADG274          17C      4
    USEACT_VMADG278          180      4
    USEACT_VMADG27C          184      4
    USEACT_VMADG280          188      4
    USEACT_VMADG284          18C      4
    USEACT_VMADG288          190      4
    USEACT_VMADG28C          194      4
    USEACT_VMADG290          198      4
    USEACT_VMADG294          19C      4
    USEACT_VMADG298          1A0      4
    USEACT_VMADG29C          1A4      4
    USEACT_VMADG2A0          1A8      4
    USEACT_VMADG2A4          1AC      4
    USEACT_VMADG2A8          1B0      4
    USEACT_VMADG2AC          1B4      4
    USEACT_VMADG2B0          1B8      4
    USEACT_VMADG2B4          1BC      4
    USEACT_VMADG2B8          1C0      4
    USEACT_VMADG2BC          1C4      4
    USEACT_VMADG2C0          1C8      4
    USEACT_VMADG2C4          1CC      4
    USEACT_VMADG2C8          1D0      4
    USEACT_VMADG2CC          1D4      4
    USEACT_VMADG2D0          1D8      4
    USEACT_VMADG2D4          1DC      4
    USEACT_VMADG2D8          1E0      4
    USEACT_VMADG2DC          1E4      4
    USEACT_VMADG2E0          1E8      4
    USEACT_VMADG2E4          1EC      4
    USEACT_VMADG2E8          1F0      4
    USEACT_VMADG2EC          1F4      4
    USEACT_VMADG2F0          1F8      4
    USEACT_VMADG2F4          1FC      4
    USEACT_VMADG2F8          200      4
    USEACT_VMADG2FC          204      4
    USEACT_VMADG308          208      4
    USEACT_VMADG318          20C      4
    USEACT_VMADIAG             0    528
    USEACT_VMADIAGT            4      4
    USEACT_VMADIAG0            8      8
    USEACT_VMADIAG2          108     64
    USEACT_VMADIAG3          208      8
    USEACT_VMAESSA           198      4
    USEACT_VMAFST44            8      4
    USEACT_VMAFSTPX            C      4
    USEACT_VMAFSTSG           10      4
    USEACT_VMAFSTXC           14      4
    USEACT_VMAIIA            2D8      4
    USEACT_VMAIIADD          2DC      4
    USEACT_VMAIIHDSSQ        304     16
    USEACT_VMAIIHLD          2FC      8
    USEACT_VMAIIWTM          2E0      8
    USEACT_VMAIIWTSSQ        2E8     16
    USEACT_VMAINSOT            0     24
    USEACT_VMAKEYIE           80      4
    USEACT_VMAKEYIK           20      4
    USEACT_VMAKEYRE           84      4
    USEACT_VMAKEYRR           68      4
    USEACT_VMAKEYSE           88      4
    USEACT_VMAKEYSK           1C      4
    USEACT_VMALPSWE          13C      4
    USEACT_VMALPSWY          1E8      4
    USEACT_VMAPCVSC           74      4
    USEACT_VMAPRCAL          2D0           80
    USEACT_VMAPRVGP           48      4
    USEACT_VMAPRVLC          148      4
    USEACT_VMAPRVLG          1C8      4
    USEACT_VMAPRVLP           2C      4
    USEACT_VMAPRVMN           40      4
    USEACT_VMAPRVMO           44      4
    USEACT_VMAPRVMS           28      4
    USEACT_VMAPRVSC            4      4
    USEACT_VMAPRVSG          1C4      4
    USEACT_VMAPRVSV           24      4
    USEACT_VMAPRVTC          144      4
    USEACT_VMAPRVTP          1C0      4
    USEACT_VMAPRVVN            0      4
    USEACT_VMAPTFF             4      4
    USEACT_VMARDP            1EC      4
    USEACT_VMASCKPF           10      4
    USEACT_VMASIMCT            0    496
    USEACT_VMASIOCT           30      4
    USEACT_VMASTFLE          134      4
    USEACT_VMASTHYI           D8      4
    USEACT_VMATTIME_PRO      29C      8
    USEACT_VMATTMP_PRO       2B4      8
    USEACT_VMATTMS_PRO       2C4      8
    USEACT_VMAVCSP            D4      4
    USEACT_VMAVCSPG          17C      4
    USEACT_VMAVIDTE          184      4
    USEACT_VMAVIESB           E0      4
    USEACT_VMAVPTNV           78      4
    USEACT_VMAVTIME_PRO      2A4      8
    USEACT_VMAVTMP_PRO       2AC      8
    USEACT_VMAVTMS_PRO       2BC      8
    USEACT_VMAXPG5A           E4      4
    USEACT_VMAXPGIN           90      4
    USEACT_VMAXPGOU           94      4
    USEACT_VMDABSSH           F0      4
    USEACT_VMDACTNO           FC      8
    USEACT_VMDAFSUP          18A           80
    USEACT_VMDASMCT           D8      2
    USEACT_VMDBLKCT           DC      4
    USEACT_VMDCACHN          1AC      4
    USEACT_VMDCFGEM          189      1
    USEACT_VMDCPUAD           1C      2
    USEACT_VMDCPUAF          189           40
    USEACT_VMDCPUCH          35C      4
    USEACT_VMDCTFLT           58      4
    USEACT_VMDCTISO           E8      4
    USEACT_VMDCTPVG          124      4
    USEACT_VMDCTPVL           48      4
    USEACT_VMDCTPVLA         158      8
    USEACT_VMDCTPVR           44      4
    USEACT_VMDCTPWT           70      4
    USEACT_VMDCTSHL          160      4
    USEACT_VMDCTSHLA         164      8
    USEACT_VMDCTSPR           7C      4
    USEACT_VMDCTSPW           80      4
    USEACT_VMDCTSTA          1B0      4
    USEACT_VMDCTSTO          1B4      4
    USEACT_VMDCUPGM          184      4
    USEACT_VMDDSRSV          252      4
    USEACT_VMDDTPLX          1CC      4
    USEACT_VMDDTTOD          1D0      8
    USEACT_VMDDTTOT          1C8      4
    USEACT_VMDELIST           21      1
    USEACT_VMDGRPN           104      8
    USEACT_VMDISEVM           A0      4
    USEACT_VMDISTVM           A4      4
    USEACT_VMDISUVM           A8      4
    USEACT_VMDLIMTH           DA           02
    USEACT_VMDLKPLX          1BC      4
    USEACT_VMDLKTOD          1C0      8
    USEACT_VMDLKTOT          1B8      4
    USEACT_VMDMAACT           22           01
    USEACT_VMDMASST           22           02
    USEACT_VMDMDCIA           E0      4
    USEACT_VMDMODE            1E      1
    USEACT_VMDMVB2G          130      4
    USEACT_VMDMXRVP           F8      4
    USEACT_VMDMXSHA           DA           80
    USEACT_VMDMXSHR          118      4
    USEACT_VMDNOFSL           22           04
    USEACT_VMDNOINS           22           08
    USEACT_VMDPBKCT          17C      4
    USEACT_VMDPGSPL           84      4
    USEACT_VMDPUST           18A      1
    USEACT_VMDPUTYP          188      1
    USEACT_VMDQDSPU           22           40
    USEACT_VMDRELSH           EC      4
    USEACT_VMDREOFL           DB           40
    USEACT_VMDRLLST          1E8      8
    USEACT_VMDRUNCP          370      4
    USEACT_VMDSHELD          36C      1
    USEACT_VMDSHLON          36C           40
    USEACT_VMDSHLOV          36C           80
    USEACT_VMDSLIST           20      1
    USEACT_VMDSSIZE           F4      4
    USEACT_VMDSTFHW          212      2
    USEACT_VMDSTLFC          210      2
    USEACT_VMDSTOP            DA           40
    USEACT_VMDSTOPD           DA           20
    USEACT_VMDSTYPE           23      1
    USEACT_VMDTHRCT          11C      4
    USEACT_VMDTTIME           24      8
    USEACT_VMDTTIME_MT1      26C      8
    USEACT_VMDTTMP           194      8
    USEACT_VMDTTMP_MT1       284      8
    USEACT_VMDTTMS           1A4      8
    USEACT_VMDTTMS_MT1       294      8
    USEACT_VMDUFACTC         214      4
    USEACT_VMDUFIBRC         218      4
    USEACT_VMDUFOLKCT        16C      4
    USEACT_VMDUFOLKTM        170      8
    USEACT_VMDUSER            14      8
    USEACT_VMDVCSCT           88      4
    USEACT_VMDVDISK          114      4
    USEACT_VMDVDSCT           8C      4
    USEACT_VMDVOSCT           98      4
    USEACT_VMDVSEVM           AC      4
    USEACT_VMDVSTVM           B0      4
    USEACT_VMDVSUVM           B4      4
    USEACT_VMDVTIME           2C      8
    USEACT_VMDVTIME_MT1      274      8
    USEACT_VMDVTMP           18C      8
    USEACT_VMDVTMP_MT1       27C      8
    USEACT_VMDVTMS           19C      8
    USEACT_VMDVTMS_MT1       28C      8
    USEACT_VMDVTSCT           94      4
    USEACT_VMDVUSCT           90      4
    USEACT_VMDVVEXT           DB           20
    USEACT_VMDWASTE          25C      4
    USEACT_VMDWKPLX          1DC      4
    USEACT_VMDWKTOD          1E0      8
    USEACT_VMDWKTOT          1D8      4
    USEACT_VMDWSSPR           4C      4
    USEACT_VMDX98CT           C8      4
    USEACT_VMUASNORD           C      4
    USEACT_VMUDSPETM         334      8
    USEACT_VMUDSPTSQ         33C     16
    USEACT_VMUDWTETM         318      8
    USEACT_VMUDWTTSQ         320     16
    USEACT_VMUMODRB            6           40
    USEACT_VMUNRBAL          1FC      4
    USEACT_VMUPLTL             0      4
    USEACT_VMUREBAL          20C      4
    USEACT_VMURROBN            6           80
    USEACT_VMUSTLTL            0      4
    USEACT_VMUTOPDA            0     16
    USEACT_VMUTOPDI            0      2
    USEACT_VMUTOPDS            2      4
    USEACT_VMUTOPDX          202      1
    USEACT_VMUTOPFL            7      1
    USEACT_VMUTOPLU            8      4
    USEACT_VMUTOPNE          200      1
    USEACT_VMUTOPNS          201      1
    USEACT_VMUTTIMSQ         34C     16
    USEACT_VMUVMTL             0      4

    This information is
    based on z/VM V7R2.0.

    Last updated on 21 April 2022 at 15:23:00.

    Copyright IBM Corporation, 1990, 2022