PFXPG | Back to Index page

| Prolog Control Block Contents PFXPG DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

PFXPG Prolog | Top of page

     NAME       : HCPPFXPG
     DESCRIPTION: PREFIX PAGE FOR ALL HOST CPU'S
     DSECT      : PFXPG
     FUNCTION   : HCPPFXPG IS PAGE ZERO FOR EACH HOST PROCESSOR.  IT CONTAINS
                  PROCESSOR-RELATED INFORMATION DEFINED BY BOTH HARDWARE AND
                  SOFTWARE.
     LOCATED BY : HOST REAL PREFIX REGISTER
                  HCPPFX    MODULE CONTAINS THE PFXPG FOR IPL'D PROCESSOR
                  SYSPRFIX  FIELD OF HCPSYSCM (PFXPG FOR IPL'D PROCESSOR)
                  PFXPRFIX  FIELD OF HCPPFXPG (PREFIX VALUE FOR THIS CPU)
                  PFXNXTPF  FIELD OF HCPPFXPG (CYCLIC POINTER TO NEXT PFXPG)
                  DFIPFX    FIELD OF HCPDFIR  (PFXPG OF DUMPED SYSTEM)
                  TRQCCPFX  FIELD OF HCPTRQBK (PFXPG where TRQBVAL set
                  in clock comparator)
     CREATED BY : HCPLOD    DURING SYSTEM INITIALIZATION (IPL'D PROCESSOR)
                  (LOADS HCPPFX MODULE AS IPL'D PROCESSOR PFXPG)
                  HCPMPS    DURING SYSTEM INITIALIZATION AND VARY ON PROCESSOR
                  (ALTERNATE PROCESSOR)
     DELETED BY : HCPMPS    DURING VARY OFF OF AN ALTERNATE PROCESSOR
                  (IPL'D PROCESSOR'S PFXPG NEVER DELETED, BUT ZEROED
                  OUT IF THE PROCESSOR IS VARIED OFF)
     RELOCATION CONSIDERATIONS : None
     NOTES      : 1. Even though the term "Prefix Page" is used here,
                  in z/Architecture, the prefix area is an 8K block.
                  The second page is contiguous with the first and
                  is defined by DSECT PF2PG.
                  2. Some ESA/390 fields remain defined in this block
                  because they are still valid during the brief time
                  when CP is in ESA/390 mode.

PFXPG Control Block Content | Top of page

     PFXPG DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      PFXPG          PREFIX PAGE FOR ALL HOST CPU'S
    0000    0 Dbl-Word     8 PFXMACHN (64)  MACHINE USAGE
    0200  512 Dbl-Word     8 PFXMACCM (24)  Machine communication area
    02C0  704 Dbl-Word     8 PFXTIMES (8)   CPU Timer Region
    0300  768 Dbl-Word     8 PFXSAVES (192) Static Save Areas
    0900 2304 Dbl-Word     8 PFXADCON (32)  ADDRESS CONSTANT
    0A00 2560 Dbl-Word     8 PFXCONST (32)  COMMON CONSTANTS
    0B00 2816 Dbl-Word     8 PFXCNTRL (112) CPU Control Region
    0E80 3712 Dbl-Word     8 PFXCPCRS (16)  CP images of host control
                                            registers
    0F00 3840 Bitstring  256 PFXPATCH       FE Patch Area, 32D = 64F = 128H
                 MACHINE USAGE - COVERED BY LOW ADDRESS PROTECT
    0000    0 Dbl-Word     8 PFXILPSW       IPL START PSW, RESTART NEW PSW
    0008    8 Dbl-Word     8 PFXRSTOP (0)   RESTART OLD PSW
    0008    8 Dbl-Word     8 PFXICCW1       IPL CCW, RESTART OLD PSW
    0010   16 Dbl-Word     8 PFXICCW2       IPL CCW
    0018   24 Dbl-Word     8 PFXEXTOP       EXTERNAL OLD PSW
    0020   32 Dbl-Word     8 PFXSVCOP       SVC OLD PSW
    0028   40 Dbl-Word     8 PFXPRGOP       PROGRAM OLD PSW
    0030   48 Dbl-Word     8 PFXMCHOP       MACHINE CHECK OLD PSW
    0038   56 Dbl-Word     8 PFXIOOP        INPUT/OUTPUT OLD PSW
    0040   64 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    0044   68 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    0048   72 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    004C   76 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    0050   80 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    0054   84 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    0058   88 Dbl-Word     8 PFXEXTNP       EXTERNAL NEW PSW
    0060   96 Dbl-Word     8 PFXSVCNP       SVC NEW PSW
    0068  104 Dbl-Word     8 PFXPRGNP       PROGRAM NEW PSW
    0070  112 Dbl-Word     8 PFXMCHNP       MACHINE CHECK NEW PSW
    0078  120 Dbl-Word     8 PFXIONP        INPUT/OUTPUT NEW PSW
    0080  128 Dbl-Word     8 PFXCPULG (0)   CPU AND STORAGE LOGOUT AREA
    0080  128 Signed       4 PFXEXTPM (0)   External interruption parameter
              .... ....      EXTIMIEA       X'80000000' EXTIMIEA Invalid
                                            entry address
              .... ....      EXTIMISE       X'40000000' EXTIMISE Incorrect
                                            SDBT entry
              .... ....      EXTIMPRA       X'20000000' EXTIMPRA Program
                                            request alert
              PFXEXTPM       EXTIMSAC       X'00800000' EXTIMSAC Sampling
                                            authorization change
              PFXEXTPM       EXTIMLSD       X'00400000' EXTIMLSD Loss of
                                            sample data
              PFXEXTPM       EXTITSC        X'00020000' EXTITSC Timing-status
                                            change
              PFXEXTPM       EXTILAC        X'00010000' EXTILAC
                                            Link-availability change
              PFXEXTPM       EXTITPC        X'00008000' EXTITPC
                                            Time-control-parameter change
              PFXEXTPM       EXTIMLMT       X'00008000' EXTIMLMT
                                            Loss-of-MT-counter-data
              1... ....      EXTIMCAC       X'00000080' EXTIMCAC Counter
                                            authorization change
              .1.. ....      EXTIMLCD       X'00000040' EXTIMLCD Loss of
                                            counter data
    0080  128 Signed       4 PFXEXTDB       PROCESSOR CONTROLLER DATA BLOCK
                                            ADDRESS FOR SERVICE SIGNAL
                                            INTERRUPT
    0084  132 Signed       4 PFXEXTCF (0)   EXTERNAL INTERRUPT CODE FIELDS
    0084  132 Signed       2 PFXEXTCP       EXTERNAL INTERRUPT CPU ADDR
    0086  134 Signed       2 PFXEXTIN (0)   EXTERNAL INTERRUPT CODE
    0086  134 Bitstring    1 PFXEXTCL       EXTERNAL INTERRUPT CLASS CODE
              00000000       EXTICL00       00 EXTICL00 CLASS 00 EXTERNAL
                                            INTERRUPTS (INTERRUPT KEY,
                                            INTERVAL TIMER)
              00000010       EXTICL10       16 EXTICL10 CLASS 10 EXTERNAL
                                            INTERRUPTS (TIMER, COMPARATOR,
                                            TOD SYNCH)
              00000012       EXTICL12       18 EXTICL12 CLASS 12 EXTERNAL
                                            INTERRUPTS (MULTI-CPU SIGNALS)
              00000014       EXTICL14       20 EXTICL14 CLASS 14 EXTERNAL
                                            INTERRUPTS (ETR INTERRUPTS)
              00000020       EXTICL20       32 EXTICL20 Class 20 external
                                            interrupts (Time zone transition)
              00000024       EXTICL24       36 EXTICL24 CLASS 24 EXTERNAL
                                            INTERRUPTS (SERVICE SIGNALS)
              00000026       EXTICL26       38 EXTICL26 CLASS 26 EXTERNAL
                                            INTERRUPTS (ESA/XC INTERRUPTS)
              00000040       EXTICL40       64 EXTICL40 CLASS 40 EXTERNAL
                                            INTERRUPTS (VMCF AND IUCV
                                            COMMUNICATION)
    0087  135 Bitstring    1 PFXEXTCD       EXTERNAL INTERRUPT TYPE CODE
              00000040       EXTIKEY        64 EXTIKEY CODE X'0040' INTERRUPT
                                            KEY
              00000080       EXTITMR        128 EXTITMR CODE X'0080' 370
                                            INTERVAL TIMER
              00000004       EXTICKC        04 EXTICKC CODE X'1004' CLOCK
                                            COMPARATOR
              00000005       EXTICPU        05 EXTICPU CODE X'1005' CPU TIMER
              00000000       EXTIMALF       00 EXTIMALF CODE X'1200'
                                            MALFUNCTION ALERT
              00000001       EXTIEMGS       01 EXTIEMGS CODE X'1201'
                                            EMERGENCY SIGNAL
              00000002       EXTICALL       02 EXTICALL CODE X'1202' EXTERNAL
                                            CALL
              00000006       EXTIETR        06 EXTIETR CODE X'1406' ETR
                                            INTERRUPT
              00000007       EXTIMEAS       07 EXTIMEAS Code X'1407'
                                            Measurement Alert
              00000004       EXTITZCH       04 EXTITZCH CODE X'2004' Time
                                            Zone Change
              00000001       EXTISVSG       01 EXTISVSG CODE X'2401' SERVICE
                                            SIGNAL
              00000002       EXTIPVM        02 EXTIPVM CODE X'2402' PVM
                                            LOGICAL DEVICE
              00000003       EXTIXC         03 EXTIXC CODE X'2603' ESA/XC and
                                            other VM external interrupts
              00000000       EXTIIUCV       00 EXTIIUCV CODE X'4000' IUCV
                                            INTERRUPTION
              00000001       EXTIVMCF       01 EXTIVMCF CODE X'4001' VMCF
                                            INTERRUPTION
    0088  136 Signed       4 PFXSVCIF (0)   SVC INTERRUPT CODE FIELDS
    0088  136 Signed       2 PFXSVCIL       SVC INSTRUCTION LENGTH CODE
    008A  138 Signed       2 PFXSVCNT (0)   SVC Interrupt Code (halfword)
    008A  138 Bitstring    1 *              SVC Interrupt Code (1st byte)
    008B  139 Bitstring    1 PFXSVCIC       SVC Interrupt Code (2nd byte)
              00000000       SVCABEND       00 SVCABEND SVC 00 = HOST CP
                                            SYSTEM ABEND
              00000004       SVCSABND       04 SVCSABND SVC 04 = HOST CP
                                            SYSTEM SOFT ABEND
              0000001C       SVCTRAP        28 SVCTRAP SVC 28 = PROCESS DATA
                                            TYPE TRACE (TRACE SERVICE TOOL)
              00000020       SVCTRET        32 SVCTRET SVC 32 = RETURN FROM
                                            DATA TYPE TRACE (TRACE SERVICE
                                            TOOL) PROCESSING
              00000024       SVCSDABN       36 SVCSDABN SVC 36 = Host CP
                                            Snapdump ABEND
              00000028       SVCEXIT        40 SVCEXIT SVC 40 = Dynamic CP
                                            Exit
              0000004C       SVC76ERP       76 SVC76ERP SVC 76 = ERROR
                                            RECORDING MODULE CALL
    008C  140 Signed       4 PFXPRGCF (0)   PROGRAM INTERRUPT CODE FIELDS
    008C  140 Signed       2 PFXPRGIL       PROGRAM INTERRUPT INSTRUCTION
                                            LENGTH CODE
              00000002       TXHAILC        2 TXHAILC Default ILC used when
                                            propagating an interruption to
                                            the guest arising from a host
                                            interruption during a guest
                                            transaction.
    008E  142 Signed       2 PFXPRGIN (0)   PROGRAM INTERRUPT CODE, HALFWORD
    008E  142 Bitstring    1 PFXPRGEE       Exception extension code
    008F  143 Bitstring    1 PFXPRGIC       PROGRAM INTERRUPT CODE
              00000136       PRGIADCP       X'0136' PRGIADCP Addressing
                                            capability
              00000400       PRGITXHA       X'0400' PRGITXHA Host
                                            interrupting guest TX
              00000200       PRGITRXA       X'0200' PRGITRXA Transaction
                                            aborted by PRG intrpt
              00000600       PRGITXMD       PRGITXHA+PRGITRXA PRGITXMD TX
                                            modifiers combined
              00000680       PRGIHMOD       PRGITXHA+PRGITRXA+PRGIPER
                                            PRGIHMOD Prg intrpt modifiers
                                            used in host interruption
                                            handling
              0000F97F       PRGICHMD       X'FFFF'-PRGIHMOD PRGICHMD Mask
                                            used for clearing host
                                            interruption modifiers
    0090  144 Signed       4 PFXTRXAD (0)   Translation-Exception Ident. ESA
                                            (Fault address/related info) ESA
                                            - see PFXGTRAD for z/Arch ESA
    0090  144 Bitstring    3 *              ESA
    0093  147 Bitstring    1 PFXTRXA3       FLAGS FOR TRANSLATION SPACE ID
                                            ESA
              .... ....      PRGXPRIM       X'00' PRGXPRIM Primary space
              .... ...1      PRGXAR         X'01' PRGXAR
                                            Access-register-specified space
              .... ..1.      PRGXSEC        X'02' PRGXSEC Secondary space
              .... ..11      PRGXHOME       X'03' PRGXHOME Home space zArch
                                            Translation-Exception
                                            Identification byte 7 bit
                                            definitions for protection codes
                                            for ESOP-2
              1... 11..      PRGESOP2M      X'8C' PRGESOP2M ESOP-2 Protection
                                            Code Mask
              .... .1..      PRGESOP2D      X'04' PRGESOP2D ESOP-2 Protection
                                            Code DATP
              .... 1...      PRGESOP2K      X'08' PRGESOP2K ESOP-2 Protection
                                            Code KCP
              .... 11..      PRGESOP2A      X'0C' PRGESOP2A ESOP-2 Protection
                                            Code ALCP
              1... ....      PRGESOP2L      X'80' PRGESOP2L ESOP-2 Protection
                                            Code LAP
              1... .1..      PRGESOP2I      X'84' PRGESOP2I ESOP-2 Protection
                                            Code IEP Other bits defined in
                                            low byte of TEID:
              .... .1..      PRGXMVPG       X'04' PRGXMVPG Exception occurred
                                            on MVPG instructn Data exception
                                            codes
              1111 111.      PRGDXCVR       X'FE' PRGDXCVR Vector-register
                                            data exception
              .... ..1.      PRGDXBFP       X'02' PRGDXBFP BFP-instruction
                                            data exception
              .... ...1      PRGDXAFP       X'01' PRGDXAFP AFP-register data
                                            exception
    0090  144 Signed       4 PFXFPARM (0)   Data exception information
    0090  144 Bitstring    3 *
    0093  147 Bitstring    1 PFXDXCOD       Data exception code
    0090  144 Signed       4 PFXVPARM (0)   Vector exception information
    0090  144 Bitstring    3 *
    0093  147 Bitstring    1 PFXVXCOD       Vector exception code
    0094  148 Signed       2 PFXMNCLS       MONITOR CLASS
    0096  150 Signed       2 PFXPERCD       PROGRAM EVENT RECORDER (PER) CODE
    0098  152 Signed       4 PFXPERAD       PER Address ESA - see PFXGPERA
                                            for z/Arch ESA
    009C  156 Signed       4 PFXMNCOD       Monitor interrupt code ESA - see
                                            PFXGMNCD for z/Arch ESA
    0098  152 Dbl-Word     8 PFXGPERA (0)   PER Address for z/Architecture
                                            mode
    0098  152 Signed       4 PFXGPERL       Left Half PER address
    009C  156 Signed       4 PFXGPERR       Right Half PER address
    00A0  160 Bitstring    1 PFXXCPAR       EXCEPTION ACCESS IDENTIFICATION
              ..1. ....      PRGXCPRI       X'20' PRGXCPRI Primary-tran
                                            problem (not Access Register
                                            related)
              ...1 ....      PRGXCSEC       X'10' PRGXCSEC Secondary-tran
                                            problem (not Access Register
                                            related)
              .... 1111      PRGXCREG       X'0F' PRGXCREG Access-register
                                            number
    00A1  161 Bitstring    1 PFXPERAR       PER ACCESS IDENTIFICATION
    00A2  162 Bitstring    1 PFXOPRID       Operand access identification
    00A3  163 Bitstring    1 PFXARCHM       Architectural Mode ID
              .... ...1      PFXAINME       X'01' PFXAINME Bit 7 on indicates
                                            CP is currently executing in
                                            z/Architecture mode. When off CP
                                            is currently in ESA/390 mode.
    00A4  164 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    00A8  168 Dbl-Word     8 PFXGTRAD       Translation-Exception Ident.
                                            z/Arch - see PFXTRXAD for ESA/390
    00B0  176 Dbl-Word     8 PFXGMNCD (0)   Monitor interrupt code
    00B0  176 Signed       4 PFXGMNCL       Monitor interrupt code left
    00B4  180 Signed       4 PFXGMNCR       Monitor interrupt code right -
                                            see PFXMNCOD for ESA/390
    00B4  180 Bitstring    2 *              Zero
    00B6  182 Bitstring    1 PFXGMNAC       Actual class
    00B7  183 Bitstring    1 PFXGMNAR       Actual record
    00A8  168 Signed       4 *              RESERVED FOR FUTURE HW USE ESA
    00AC  172 Signed       4 *              RESERVED FOR FUTURE HW USE ESA
    00B0  176 Signed       4 *              RESERVED FOR FUTURE HW USE ESA
    00B4  180 Signed       4 *              RESERVED FOR FUTURE HW USE ESA
    00B8  184 Signed       4 PFXIOSID (0)   SUBCHANNEL IDENTIFICATION
    00B8  184 Signed       2 PFXIOINT       I/O INTERRUPT CONSTANT 0001
    00BA  186 Signed       2 PFXIORNM       I/O INTERRUPT SUBCHANNEL NUMBER
    00B8  184 Signed       4 PFXIOICA (0)   I/O Int Code Word 0 - I/O
                                            Adapters
    00B8  184 Bitstring    1 PFXAISM        Adapter-Interruption Source
                                            Mask-AISM
              1... ....      PFXQDIOA       X'80' PFXQDIOA QDIO Adapter
                                            Interrupt
              .1.. ....      PFXPCIA        X'40' PFXPCIA PCI Function
                                            Interrupt
    00B9  185 Bitstring    1 *              Reserved for IBM future use
    00BA  186 Bitstring    1 *              Reserved for IBM future use
    00BB  187 Bitstring    1 PFXADPFG       Adapter Flags
              .... ..1.      PFXEBIT        X'02' PFXEBIT Host Error
                                            Condition
              .... ...1      PFXHBIT        X'01' PFXHBIT Host Forwarding
                                            Request
    00BC  188 Signed       4 PFXINPRM       I/O INTERRUPT PARAMETER
    00C0  192 Signed       4 PFXINTID (0)   INTERRUPTION ID WORD:
    00C0  192 Bitstring    1 PFXINISC       FIRST BYTE - THE ISC
              00000080       PFXIOADP       X'80' PFXIOADP Adapter Interrupt
              000000B0       PFXINIFI       X'30'+PFXIOADP PFXINIFI Use
                                            Alternate I/O FLIH
    00C1  193 Bitstring    1 *              Reserved for IBM future use
    00C2  194 Bitstring    1 PFXSCHTP       Subchannel type
              00000000       PFXSCHT0       X'00' PFXSCHT0 Type 0 subchannel
              00000070       PFXSCHTM       X'70' PFXSCHTM Mask for location
                                            of subchannel type bits within
                                            this byte.
    00C3  195 Bitstring    1 *              Reserved for IBM future use
    00C4  196 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    00C8  200 Signed       4 PFXSTFL (0)    STFL facilities list
    00C8  200 Bitstring    1 PFXSTFL0       Byte 0, Bits 0-7
              1... ....      STFL0N3A       X'80' STFL0N3A "N3" instructions
                                            available
              .1.. ....      STFL0MEA       X'40' STFL0MEA zArch available
              ..1. ....      STFL0MEE       X'20' STFL0MEE zArch enabled
              ...1 ....      STFL0IDT       X'10' STFL0IDT IDTE is installed
              .... 1...      STFL0ICS       X'08' STFL0ICS IDTE performs the
                                            Invalidation-and- Clearing
                                            operation selectively when STE(s)
                                            are invalidated. IDTE also
                                            performs the Clearing-by-ASCE
                                            function selectively. In both
                                            cases, "selectively" means the
                                            TLB purging is limited to those
                                            specific entries required by
                                            architecture. If this bit is off,
                                            IDTE simply purges all TLBs. If
                                            this bit is on, STFL0IDT is also
                                            on.
              .... .1..      STFL0ICR       X'04' STFL0ICR IDTE performs the
                                            Invalidation-and- Clearing
                                            operation selectively when RTE(s)
                                            are invalidated. "Selectively"
                                            means the TLB purging is limited
                                            to those specific entries
                                            required by architecture. If this
                                            bit is off, IDTE
                                            Invalidation-and-Clearing of
                                            RTE(s) simply purges all TLBs. If
                                            this bit is on, STFL0IDT and
                                            STFL0ICS are also on.
              .... ..1.      STFL0ALR       X'02' STFL0ALR ASN-and-LX-reuse
                                            facility installed
              .... ...1      STFL0FLE       X'01' STFL0FLE STFLE facility
                                            installed Absolute bit position
                                            definitiions for byte 0 for use
                                            with HCPARDSF
    00C9  201 Bitstring    1 PFXSTFL1       Byte 1, bits 8-15
              1... ....      STFLEDAT       X'80' STFLEDAT Enhanced-DAT
                                            facility (z/Arch)
              .1.. ....      STFLSRS        X'40' STFLSRS
                                            Sense-running-status facility
              ..1. ....      STFLSSKE       X'20' STFLSSKE Conditional-SSKE
                                            (z/Arch)
              ...1 ....      STFLCTOP       X'10' STFLCTOP
                                            Configuration-Topology (z/Arch)
              .... 1...      STFLIBM4       X'08' STFLIBM4 Assigned to IBM
                                            Internal Use
              .... .1..      STFLIPTR       X'04' STFLIPTR IPTE-Range
                                            (z/Arch)
              .... ..1.      STFLNQKS       X'02' STFLNQKS
                                            Non-Quiescing-Key-Setting
                                            (z/Arch)
              .... ...1      STFLIBM1       X'01' STFLIBM1 Assigned to IBM
                                            Internal Use. Absolute bit
                                            position definitiions for byte 1
                                            for use with HCPARDSF
    00CA  202 Bitstring    1 PFXSTFL2       Byte 2, bits 16-23
              1... ....      STFLETF2       X'80' STFLETF2 Extended
                                            Translation Facility 2
              .1.. ....      STFLCCA        X'40' STFLCCA CPU Crypto Assist
                                            installed
              ..1. ....      STFLLDF        X'20' STFLLDF Long Displacement
                                            Facility available
              ...1 ....      STFLHPO        X'10' STFLHPO LDF High
                                            Performance Option installed
              .... 1...      STFLHFPM       X'08' STFLHFPM
                                            HFP-Mult-Add/Subtract facility
              .... .1..      STFLEXTI       X'04' STFLEXTI Extended-Immediate
                                            facility installed
              .... ..1.      STFLETF3       X'02' STFLETF3 Extended-Trans
                                            Facility 3 installed
              .... ...1      STFLHFPU       X'01' STFLHFPU
                                            HFP-Unnormalized-extension
                                            facility Absolute bit position
                                            definitiions for byte 2 for use
                                            with HCPARDSF
    00CB  203 Bitstring    1 PFXSTFL3       Byte 3, bits 24-31
              1... ....      STFLE2EN       X'80' STFLE2EN ETF2-Enhancement
                                            Facility installed
              .1.. ....      STFLSTCF       X'40' STFLSTCF Store-Clock-Fast
                                            Facility
              ..1. ....      STFLPARS       X'20' STFLPARS
                                            Parsing-enhancement Facility
                                            installed
              ...1 ....      STFLMVCS       X'10' STFLMVCS
                                            Move-with-optional-specifications
              .... 1...      STFLPTFF       X'08' STFLPTFF TOD-clock steering
                                            facility installed
              .... ..1.      STFLE3EN       X'02' STFLE3EN ETF3-Enhancement
                                            Facility installed
              .... ...1      STFLECTG       X'01' STFLECTG Extract-CPU-Time
                                            Facility installed Absolute bit
                                            position definitiions for byte 3
                                            for use with HCPARDSF
    00CC  204 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    00D0  208 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    00D4  212 Signed       4 PFXFPXSA       Extended-Save-Area Address ESA
    00D4  212 Signed       4 *              Reserved for IBM hardware use
    00D8  216 Dbl-Word     8 PFXMCPUT       Machine check CPU Timer logout
                                            ESA - see PF2CPTLG for z/Arch ESA
    00E0  224 Dbl-Word     8 PFXMCKCP       Machine check TOD Comp. logout
                                            ESA - see PF2CKCLG for z/Arch ESA
    00E8  232 Dbl-Word     8 PFXMCHIN       MACHINE CHECK INTERRUPT CODE
    00F0  240 Signed       4 *              RESERVED FOR FUTURE HARDWARE USE
    00F4  244 Signed       4 PFXMCHDC       MACHINE CHECK EXTERNAL-DAMAGE
                                            CODE
    00F8  248 Signed       4 PFXMCFSA       Machine check failing storage ESA
                                            address ESA - see PFXGMCFS for
                                            z/Arch ESA
    00FC  252 Signed       4 PFXMCHRD       Machine-dependent region code ESA
                                            - no equivalent for z/Arch ESA
    00F8  248 Dbl-Word     8 PFXGMCFS       Machine check failing storage
                                            address
    0100  256 Bitstring   16 PFXFXLOG       MACHINE DEPENDENT FIXED LOGOUT
                                            AREA
              ...1 ....      PFXFXLEN       L'PFXFXLOG PFXFXLEN LENGTH OF
                                            FIXED LOGOUT AREA.
    0110  272 Dbl-Word     8 PFXBEAR        Breaking-Event Address EASME
    0118  280 Bitstring    8 *              RESERVED FOR FUTURE HARDWARE USE
    0120  288 Signed       4 PFXARLG (16)   Access Register Logout Area ESA
    0160  352 Dbl-Word     8 PFXFPRLG (4)   FLOATING POINT REG LOGOUT AREA
                                            ESA
    0180  384 Signed       4 PFXGPRLG (16)  GENERAL REGISTER LOGOUT AREA ESA
    01C0  448 Signed       4 PFXCRLG (16)   CONTROL REGISTER LOGOUT AREA ESA
              00000040       PFXCRLGL       (L'PFXCRLG*16) LENGTH OF CR
                                            LOGOUT AREA ESA
    0120  288 Bitstring   16 PFXGRSTO       Restart Old PSW
    0130  304 Bitstring   16 PFXGEXTO       External Old PSW
    0140  320 Bitstring   16 PFXGSVCO       Supervisor-Call Old PSW
    0150  336 Bitstring   16 PFXGPRGO       Program Old PSW
    0160  352 Bitstring   16 PFXGMCHO       Machine-Check Old PSW
    0170  368 Bitstring   16 PFXGIOO        Input/Output Old PSW
    0180  384 Dbl-Word     8 * (4)          Reserved for hardware use
    01A0  416 Bitstring   16 PFXGRSTN       Restart New PSW
    01B0  432 Bitstring   16 PFXGEXTN       External New PSW
    01C0  448 Bitstring   16 PFXGSVCN       Supervisor-Call New PSW
    01D0  464 Bitstring   16 PFXGPRGN       Program New PSW
    01E0  480 Bitstring   16 PFXGMCHN       Machine-Check New PSW
    01F0  496 Bitstring   16 PFXGION        Input/Output New PSW
              00000200       PFXLAPND       * END OF AREA COVERED BY LOW
                                            ADDRESS PROTECTION
    0000    0 Bitstring    1 PFXILPO0       ILP PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0001    1 Bitstring    1 PFXILPO1       ILP PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0002    2 Bitstring    1 PFXILPO2       ILP PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0003    3 Bitstring    1 PFXILPO3       ILP PSW BYTE 3
    0004    4 Signed       4 PFXILPOI (0)   ILP PSW INSTRUCTION COUNTER
    0004    4 Bitstring    1 PFXILPO4       ILP PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0005    5 Bitstring    1 * (3)          ILP PSW BYTES 5-7
    0010   16 Bitstring    1 PFXSGPND       SIGP RESTART FUNCTION COMPLETION
                                            FLAG
              000000FF       PFXSGPGD       255 PFXSGPGD SUCCESSFUL
                                            COMPLETION
              000000EE       PFXSGPNG       238 PFXSGPNG NOT SUCCESSFUL
                                            COMPLETION
    0011   17 Bitstring    7 PFXCC2B1 (0)   BYTES 1-7 OF PFXICCW2
    0011   17 Bitstring    1 * (5)          RESERVED FOR FUTURE USE
    0016   22 Bitstring    2 PFXSGPCP       SIGP RESTART FUNCTION WORK AREA
    0018   24 Bitstring    1 PFXEXTO0       EXT OLD PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0019   25 Bitstring    1 PFXEXTO1       EXT OLD PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    001A   26 Bitstring    1 PFXEXTO2       EXT OLD PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    001B   27 Bitstring    1 PFXEXTO3       EXT OLD PSW BYTE 3
    001C   28 Signed       4 PFXEXTOI (0)   EXT OLD PSW INSTRUCTION COUNTER
    001C   28 Bitstring    1 PFXEXTO4       EXT OLD PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    001D   29 Bitstring    1 * (3)          EXT OLD PSW BYTES 5-7
    0020   32 Bitstring    1 PFXSVCO0       SVC OLD PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0021   33 Bitstring    1 PFXSVCO1       SVC OLD PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0022   34 Bitstring    1 PFXSVCO2       SVC OLD PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0023   35 Bitstring    1 PFXSVCO3       SVC OLD PSW BYTE 3
    0024   36 Signed       4 PFXSVCOI (0)   SVC OLD PSW INSTRUCTION COUNTER
    0024   36 Bitstring    1 PFXSVCO4       SVC OLD PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0025   37 Bitstring    1 * (3)          SVC OLD PSW BYTES 5-7
    0028   40 Bitstring    1 PFXPRGO0       PRG OLD PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0029   41 Bitstring    1 PFXPRGO1       PRG OLD PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    002A   42 Bitstring    1 PFXPRGO2       PRG OLD PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    002B   43 Bitstring    1 PFXPRGO3       PRG OLD PSW BYTE 3
    002C   44 Signed       4 PFXPRGOI (0)   PRG OLD PSW INSTRUCTION COUNTER
    002C   44 Bitstring    1 PFXPRGO4       PRG OLD PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    002D   45 Bitstring    1 * (3)          PRG OLD PSW BYTES 5-7
    0030   48 Bitstring    1 PFXMCHO0       MCH OLD PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0031   49 Bitstring    1 PFXMCHO1       MCH OLD PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0032   50 Bitstring    1 PFXMCHO2       MCH OLD PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0033   51 Bitstring    1 PFXMCHO3       MCH OLD PSW BYTE 3
    0034   52 Signed       4 PFXMCHOI (0)   MCH OLD PSW INSTRUCTION COUNTER
    0034   52 Bitstring    1 PFXMCHO4       MCH OLD PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0035   53 Bitstring    1 * (3)          MCH OLD PSW BYTES 5-7
    0038   56 Bitstring    1 PFXIOPO0       I/O OLD PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0039   57 Bitstring    1 PFXIOPO1       I/O OLD PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    003A   58 Bitstring    1 PFXIOPO2       I/O OLD PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    003B   59 Bitstring    1 PFXIOPO3       I/O OLD PSW BYTE 3
    003C   60 Signed       4 PFXIOPOI (0)   I/O OLD PSW INSTRUCTION COUNTER
    003C   60 Bitstring    1 PFXIOPO4       I/O OLD PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    003D   61 Bitstring    1 * (3)          I/O OLD PSW BYTES 5-7
    0058   88 Bitstring    1 PFXEXTN0       EXT NEW PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0059   89 Bitstring    1 PFXEXTN1       EXT NEW PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    005A   90 Bitstring    1 PFXEXTN2       EXT NEW PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    005B   91 Bitstring    1 PFXEXTN3       EXT NEW PSW BYTE 3
    005C   92 Signed       4 PFXEXTNI (0)   EXT NEW PSW INSTRUCTION COUNTER
    005C   92 Bitstring    1 PFXEXTN4       EXT NEW PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    005D   93 Bitstring    1 * (3)          EXT NEW PSW BYTES 5-7
    0060   96 Bitstring    1 PFXSVCN0       SVC NEW PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0061   97 Bitstring    1 PFXSVCN1       SVC NEW PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0062   98 Bitstring    1 PFXSVCN2       SVC NEW PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0063   99 Bitstring    1 PFXSVCN3       SVC NEW PSW BYTE 3
    0064  100 Signed       4 PFXSVCNI (0)   SVC NEW PSW INSTRUCTION COUNTER
    0064  100 Bitstring    1 PFXSVCN4       SVC NEW PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0065  101 Bitstring    1 * (3)          SVC NEW PSW BYTES 5-7
    0068  104 Bitstring    1 PFXPRGN0       PRG NEW PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0069  105 Bitstring    1 PFXPRGN1       PRG NEW PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    006A  106 Bitstring    1 PFXPRGN2       PRG NEW PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    006B  107 Bitstring    1 PFXPRGN3       PRG NEW PSW BYTE 3
    006C  108 Signed       4 PFXPRGNI (0)   PRG NEW PSW INSTRUCTION COUNTER
    006C  108 Bitstring    1 PFXPRGN4       PRG NEW PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    006D  109 Bitstring    1 * (3)          PRG NEW PSW BYTES 5-7
    0070  112 Bitstring    1 PFXMCHN0       MCH NEW PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0071  113 Bitstring    1 PFXMCHN1       MCH NEW PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    0072  114 Bitstring    1 PFXMCHN2       MCH NEW PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    0073  115 Bitstring    1 PFXMCHN3       MCH NEW PSW BYTE 3
    0074  116 Signed       4 PFXMCHNI (0)   MCH NEW PSW INSTRUCTION COUNTER
    0074  116 Bitstring    1 PFXMCHN4       MCH NEW PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    0075  117 Bitstring    1 * (3)          MCH NEW PSW BYTES 5-7
    0078  120 Bitstring    1 PFXIOPN0       I/O NEW PSW BYTE 0
              .1.. ....      PSWPERA        X'40' PSWPERA PROGRAM EVENT
                                            RECORDING ACTIVE
              .... .1..      PSWTRAN        X'04' PSWTRAN ADDRESS TRANSLATE
                                            MODE ACTIVE
              .... ..1.      PSWIOSM        X'02' PSWIOSM I/O INTERRUPTION
                                            SUMMARY MASK
              .... ...1      PSWEXSM        X'01' PSWEXSM EXTERNAL INTERRUPT
                                            SUMMARY MASK
    0079  121 Bitstring    1 PFXIOPN1       I/O NEW PSW BYTE 1
              1111 ....      PSWKEY         X'F0' PSWKEY PSW ACCESS KEY
                                            EXTRACTION MASK
              .... 1...      PSWECMD        X'08' PSWECMD EXTENDED CONTROL
                                            MODE ACTIVE
              .... .1..      PSWMCHK        X'04' PSWMCHK MACHINE CHECK
                                            SUMMARY MASK
              .... ..1.      PSWWAIT        X'02' PSWWAIT PROGRAM WAIT STATE
              .... ...1      PSWPROB        X'01' PSWPROB PROGRAM PROBLEM
                                            STATE
              .... ...1      PSWMAPPD       X'01' PSWMAPPD For BC-mode PSWs
                                            created by the 370 Accommodation
                                            facility, this bit being set
                                            indicates that the PSW is really
                                            a "mapped" PSW. See HCPPSW.
    007A  122 Bitstring    1 PFXIOPN2       I/O NEW PSW BYTE 2
              11.. ....      PSWASMSK       X'C0' PSWASMSK ADDRESS SPACE
                                            CONTROL MASK
              11.. ....      PSWHMODE       X'C0' PSWHMODE HOME-SPACE MODE
              1... ....      PSWSMODE       X'80' PSWSMODE SECONDARY MODE
              .1.. ....      PSWAMODE       X'40' PSWAMODE ACCESS-REGISTER
                                            MODE
              ..11 ....      PSWCOND        X'30' PSWCOND PSW CONDITION CODE
              ..1. ....      PSWCOND2       X'20' PSWCOND2 PSW CONDITION CODE
                                            BIT FOR CC=2,3
              ...1 ....      PSWCOND1       X'10' PSWCOND1 PSW CONDITION CODE
                                            BIT FOR CC=1,3
              .... 1111      PSWPMSK        X'0F' PSWPMSK FIXO+DECO+EXUN+SIGN
                                            PROGRAM MASK
              .... 1...      PSWFIXO        X'08' PSWFIXO FIXED-PT OVERFLOW
                                            INTRPT MASK
              .... .1..      PSWDECO        X'04' PSWDECO DECIMAL OVERFLOW
                                            INTRPT MASK
              .... ..1.      PSWEXUN        X'02' PSWEXUN EXPONENT UNDERFLOW
                                            INTRPT MASK
              .... ...1      PSWSIGN        X'01' PSWSIGN SIGNIFICANCE
                                            INTERRUPT MASK
              .... ....      PSWPMODE       X'00' PSWPMODE PRIMARY-SPACE MODE
    007B  123 Bitstring    1 PFXIOPN3       I/O NEW PSW BYTE 3
    007C  124 Signed       4 PFXIOPNI (0)   I/O NEW PSW INSTRUCTION COUNTER
    007C  124 Bitstring    1 PFXIOPN4       I/O NEW PSW BYTE 4
              1... ....      PSW31BT        X'80' PSW31BT 31-BIT LOGICAL
                                            ADDRESSING MODE
              1... ....      PSWBA          PSW31BT PSWBA Basic Addressing
                                            Mode
              .111 1111      PSWHIADR       X'7F' PSWHIADR INSTRUCTION
                                            COUNTER BITS 1-7 - MUST BE ZERO
                                            IN 24-BIT MODE.
              .... ....      PSW31AMF       X'80000000' PSW31AMF ADDRESS MODE
                                            FULLWORD MASK - CORRESPONDS TO
                                            PSW31BT
    007D  125 Bitstring    1 * (3)          I/O NEW PSW BYTES 5-7
    00E8  232 Bitstring    1 PFXMCHI0       MACHINE CHECK INTERRUPT CODE BYTE
                                            0
              1111 1111      MCIPRIM0       X'FF' MCIPRIM0 PRIMARY MACHINE
                                            CHECK BITS - BYTE 0
              1... ....      MCICSD         X'80' MCICSD SYSTEM DAMAGE BIT.
              .1.. ....      MCICPD         X'40' MCICPD PROCESSING DAMAGE
                                            BIT.
              ..1. ....      MCICSR         X'20' MCICSR SYSTEM RECOVERY BIT.
              ...1 ....      MCICITD        X'10' MCICITD INTERVAL TIMER
                                            DAMAGE. (370 GUESTS)
              .... 1...      MCICCD         X'08' MCICCD TIMING (CLOCK)
                                            FACILITY DAMAGE.
              .... .1..      MCICED         X'04' MCICED EXTERNAL DAMAGE.
              .... ...1      MCICDG         X'01' MCICDG DEGRADATION BIT.
    00E9  233 Bitstring    1 PFXMCHI1       MACHINE CHECK INTERRUPT CODE BYTE
                                            1
              1111 ....      MCIPRIM1       X'F0' MCIPRIM1 PRIMARY MACHINE
                                            CHECK BITS - BYTE 1
              1... ....      MCICW          X'80' MCICW WARNING BIT.
              .1.. ....      MCICCRW        X'40' MCICCRW PENDING-CRW REPORT.
              ..1. ....      MCICSP         X'20' MCICSP SERVICE PROCESSOR
                                            DAMAGE.
              ...1 ....      MCICCSD        X'10' MCICCSD CHANNEL-SUBSYSTEM
                                            DAMAGE.
              .... ..1.      MCICBU         X'02' MCICBU 'BACKED UP' BIT.
              .... ...1      MCICDL         X'01' MCICDL 'DELAYED' BIT. (370
                                            GUESTS)
    00EA  234 Bitstring    1 PFXMCHI2       MACHINE CHECK INTERRUPT CODE BYTE
                                            2
              1... ....      MCICSE         X'80' MCICSE STORAGE ERROR
                                            UNCORRECTED.
              .1.. ....      MCICSC         X'40' MCICSC STORAGE ERROR
                                            CORRECTED.
              ..1. ....      MCICKE         X'20' MCICKE STORAGE-KEY ERROR
                                            UNCORRECTED.
              ...1 ....      MCICSDG        X'10' MCICSDG STORAGE
                                            DEGRADATION. MODIFIES STORAGE
                                            ERROR CORRECTED.
              .... 1...      MCICVWP        X'08' MCICVWP BITS 12-15 OF MC
                                            OLD PSW VALID.
              .... .1..      MCICVMS        X'04' MCICVMS SYSTEM MASK & KEY
                                            OF MC OLD PSW VALID.
              .... ..1.      MCICVPM        X'02' MCICVPM PROGRAM MASK & CC
                                            OF MC OLD PSW VALID.
              .... ...1      MCICVIA        X'01' MCICVIA INSTR ADDR OF MC
                                            OLD PSW IS VALID.
    00EB  235 Bitstring    1 PFXMCHI3       MACHINE CHECK INTERRUPT CODE BYTE
                                            3
              1... ....      MCICVFA        X'80' MCICVFA FAILING STORAGE
                                            ADDRESS IS VALID.
              .1.. ....      MCICVVR        X'40' MCICVVR Vector Registers
                                            stored are valid
              ..1. ....      MCICVED        X'20' MCICVED EXTERNAL-DAMAGE
                                            CODE IS VALID.
              ...1 ....      MCICVFP        X'10' MCICVFP FP REGISTERS STORED
                                            ARE VALID.
              .... 1...      MCICVGR        X'08' MCICVGR GP REGISTERS STORED
                                            ARE VALID.
              .... .1..      MCICVCR        X'04' MCICVCR CONTROL REGISTERS
                                            STORED VALID.
              .... ..1.      MCIC30         X'02' MCIC30 MCIC.30
              .... ...1      MCICVST        X'01' MCICVST INST. MODIFIED
                                            STORAGE IS VALID.
    00EC  236 Bitstring    1 PFXMCHI4       MACHINE CHECK INTERRUPT CODE BYTE
                                            4
              1... ....      MCICIE         X'80' MCICIE INDIRECT STORAGE
                                            ERROR
              .1.. ....      MCICVAR        X'40' MCICVAR ACCESS REGISTERS
                                            STORED ARE VALID
              ..1. ....      MCICDA         X'20' MCICDA DELAYED ACCESS
                                            EXCEPTION BIT
              .... 1...      MCICVGS        X'08' MCICVGS Guarded Storage
                                            regs stored are valid
    00ED  237 Bitstring    1 PFXMCHI5       MACHINE CHECK INTERRUPT CODE BYTE
                                            5
              ..1. ....      MCICVTPR       X'20' MCICVTPR TOD programmable
                                            register validity
              ...1 ....      MCICVXFP       X'10' MCICVXFP Additional FP
                                            Registers Validity (ESA390) FP
                                            Control Register Validity (zArch)
              .... 1...      MCICAR         X'08' MCICAR Ancillary Report Bit
              .... ..1.      MCICVCT        X'02' MCICVCT CPU TIMER STORED IS
                                            VALID.
              .... ...1      MCICVCC        X'01' MCICVCC CLOCK COMPARATOR
                                            STORED IS VALID.
    00EE  238 Bitstring    2 PFXMCHI6       MACHINE CHECK INTERRUPT CODE BYTE
                                            6-7
    00F4  244 Bitstring    1 PFXDCBY0       Byte 0 of the external damage
                                            code
              .... ....      MCEXTD0        X'00' MCEXTD0 No bits defined
    00F5  245 Bitstring    1 PFXDCBY1       Byte 1 of the external damage
                                            code
              .... ....      MCEXTD1        X'00' MCEXTD1 No bits defined
    00F6  246 Bitstring    1 PFXDCBY2       Byte 2 of the external damage
                                            code
              ...1 ....      MCEXTDSC       X'10' MCEXTDSC Bit 19 - ETR Sync
                                            check
    00F7  247 Bitstring    1 PFXDCBY3       Byte 3 of the external damage
                                            code
              1... ....      MCEXTDSS       X'80' MCEXTDSS Bit 24 - STP Sync
                                            Check
              .1.. ....      MCEXTDIC       X'40' MCEXTDIC Bit 25 - Island
                                            Condition
              ..1. ....      MCEXTDCC       X'20' MCEXTDCC Bit 26 - CTN
                                            Configuration Change
              ...1 ....      MCEXTDCS       X'10' MCEXTDCS Bit 27 - STP Clock
                                            Source Error
    0100  256 Dbl-Word     8 PFXSTPSW       STORE STATUS PSW LOGOUT AREA
    0108  264 Signed       4 PFXSTPFX       STORE STATUS PREFIX LOGOUT AREA
    010C  268 Signed       4 PFXSTMDL       STORE STATUS MODEL DEPENDENT DATA
    0160  352 Dbl-Word     8 PFXFPRY0       Floating Point Register 0
    0168  360 Dbl-Word     8 PFXFPRY2       Floating Point Register 2
    0170  368 Dbl-Word     8 PFXFPRY4       Floating Point Register 4
    0178  376 Dbl-Word     8 PFXFPRY6       Floating Point Register 6
         ** Start of section zeroed during alternate
         ** processor init.  Updates to this section
         ** should also hit ncPFXFMPB in module HCPMPS.
              00000200       PFXZALT        * Start of zeroed section.
             The following fields are used by the Paging fast path.
    0200  512 Signed       4 PFXCLPLCnt     Count of frames on the cleared
                                            local available list plus the
                                            count of frames on the firmware
                                            processed list. Serialized
                                            exclusively by CS.
                                            Incremented/Decremented by the
                                            local CPU when items are
                                            added/removed from PFXCLAL.
                                            Decremented by any CPU upon
                                            completion of reaping and
                                            processing the PFXfwPROCL.
    0204  516 Address      4 *              Reserved for IBM use
          The following fields are architected for use by both
          firmware and software.  Their displacements must not be
          changed.
    0208  520 Address      8 PFXfwPROCL     Processed list anchor See HCPHTT
                                            for comments.
    0210  528 Address      8 PFXCLALPtr     Cleared Local Available List. See
                                            HCPHTT for comments.
    0218  536 Address      8 PFXAFOBL       Available-FOB list origin.
    0220  544 Signed       4 PFXAFOBC       Available-FOB list count.
    0224  548 Signed       4 *              Reserved for IBM use
    0228  552 Dbl-Word     8 PFXDPPCAO      Origin pointer to the class 1
                                            Delta-pinned-page-count array.
                                            The class 1 DPPCA resides in
                                            RSMBK (RSMDPPB/RSMDPPA)
    0230  560 Dbl-Word     8 * (2)          Reserved for IBM use
          End of architected fields section
    0240  576 Signed       2 *              Reserved for IBM use (was
                                            PFXLAVFU)
    0242  578 Signed       2 *              Reserved for IBM use (was
                                            PFXLAVDF)
    0244  580 Signed       2 *              Reserved for IBM use (was
                                            PFXLAVU)
    0246  582 Bitstring    1 PFXGPFLG       General purpose flag
              1... ....      PFX2GU         X'80' PFX2GU Usable storage
                                            exists for the >= 2G available
                                            list
    0247  583 Bitstring    1 *              Reserved for IBM use
    0248  584 Signed       8 *              Reserved for IBM use (was
                                            PFXLAVAU)
              00000050       PFXZALTL       *-PFXZALT Length of block
         ** End of section zeroed during alternate processor init
          Frame Table management area.
    0250  592 Address      8 PFXFTBLG       Origin of Frame Table This is a
                                            host logical address >2G.
    0258  600 Address      8 PFX2GFTE       Address of FRMTE for the frame
                                            with address 2G. If there is no
                                            frame with address 2G, this is
                                            where the FRMTE would be. This is
                                            a host logical address >2G.
    0260  608 Signed       8 PFXFTLEN       Length of frame table
          SXS Page Management Table attributes.
    0268  616 Address      8 PFXSTBLG       Origin of SXS Page Mgt Table.
                                            This is a host logical address.
    0270  624 Signed       8 PFXSTLEN       Length of SXS Page Mgt Table
          Software Last-Translated Address Lookaside Buffer area.
          NOTES      : For 5.1.0, the use of this buffer changes
                from: Fast Translation to HOST REAL    ADDRESS
                to:   Fast Translation to HOST LOGICAL ADDRESS
                As a result, PFXGLFRA is being renamed to PFXGLSXP.
          If it is decided to use this buffer for Fast Translations
          to HOST LOGICAL ADDRESS AND HOST ABSOLUTE ADDRESS, then
          a 64-bit PFXGLFRA field will need to be added for the
          HOST ABSOLUTE translations.
          PFXGLFRA DS    0F        Last translated frame address
          Notes      :  Buffer path reads and translation updates are done
                 in opposite order so there is no safe order for
                 reach across clearing of the SLTALB.  If reach
                 across clearing of the SLTALB is to be done, it
                 must be done using CDSG logic to guarentee that
                 the clearing will not leave PFXGLPAG in the
                 cleared state without PGXGLPAS also being cleared.
    0278  632 Dbl-Word     8 PFXSLTLB (3)   Software Last-Translated
                                            LookAside Buffer
    0278  632 Signed       4 *              Reserved for future IBM use
    027C  636 Signed       4 PFXGLSXP       Last translated SXS Page Address
                                            The next two fields must be
                                            together on a quadword coundary
    0280  640 Dbl-Word     8 PFXGLPAG       Last translated guest page
    0280  640 Signed       4 PFXGLPW0       Word 0 of last translated guest
                                            page
    0284  644 Signed       4 PFXGLPW1       Word 1 of last translated guest
                                            page
    0288  648 Dbl-Word     8 PFXGLPAS       Last translated primary ASCE
    0288  648 Signed       4 PFXGLAW0       Word 0 of last translated primary
                                            ASCE
    028C  652 Signed       4 PFXGLAW1       Word 1 of last translated primary
                                            ASCE
          Address Space Control Elements (ASCEs) and Access List
          Entry Tokens (ALETs) for frequently used System owned
          permanent spaces.  Note that we don't save an ASCE for the
          Real Space, since it's just a doubleword of zeros with the
          R bit set. We don't have an ALET for the System Execution
          Space (SXS) because it will be the primary space when in
          AR-mode, so use ALETPRIM to load the access registers.
    0290  656 Address      8 PFXSXASC       System Execution Space ASCE
                                            (Address Space Control Element)
    0290  656 Signed       4 PFXXASW0       Word 0 of System Execution Space
                                            ASCE
    0294  660 Signed       4 PFXXASW1       Word 1 of System Execution Space
                                            ASCE
    0298  664 Address      8 PFXNASCE       ASCE for "null" address space
    0298  664 Signed       4 PFXNASW0       Word 0 of "null" space ASCE
    029C  668 Signed       4 PFXNASW1 (0)   Word 1 of "null" space ASCE
                                  private space bit and 8K length.
    029C  668 Address      4 *              Pointer to HCPSYSNS
    02A0  672 Signed       4 *              Reserved for IBM use
    02A4  676 Signed       4 PFXRSAL        Real Space ALET
    02A8  680 Dbl-Word     8 * (3)          Reserved for future IBM use
          PFXSAVES - savearea region
    0300  768 Bitstring  256 PFXTMPSG (0)   Temporary Save Area (Large)
    0300  768 Bitstring  128 PFXTMPSV       TEMPORARY SAVE AREA
    0380  896 Bitstring  128 *
    0400 1024 Bitstring  256 PFXWRKSG (0)   Special Work Save Area (Large)
    0400 1024 Bitstring  128 PFXWRKSV       SPECIAL WORK SAVE AREA
    0480 1152 Bitstring  128 *
    0500 1280 Bitstring  256 PFXBALSG (0)   BALR Linkage Save Area (Large)
    0500 1280 Bitstring  128 PFXBALSV       BALR LINKAGE SAVE AREA
    0580 1408 Bitstring  128 *
    0600 1536 Bitstring  256 PFXPTRSG (0)   BALR Linkage Save Area (Large)
    0600 1536 Bitstring  128 PFXPTRSV       PAGE TRANSLATION SAVE AREA
    0680 1664 Bitstring  128 *
    0700 1792 Bitstring  256 PFXFRESG (0)   HCPFRE Save Area (Large)
    0700 1792 Bitstring  128 PFXFRESV       HCPFRE SAVE AREA
    0780 1920 Bitstring  128 *
    0800 2048 Bitstring   32 PFXIRPSG (0)   R12-R15 Save Area for FLIHs
                                            (Large)
    0800 2048 Bitstring   16 PFXIRPSV       R12-R15 SAVE AREA FOR FLIHS
    0810 2064 Bitstring   16 *
    0820 2080 Bitstring   32 PFXLNKSG (0)   Call/Return Linkage Save Area
                                            (Large)
    0820 2080 Bitstring   16 PFXLNKSV       CP CALL/RETURN LINKAGE SAVEAREA
    0830 2096 Bitstring   16 *
    0840 2112 Bitstring  128 PFXSVCSG (0)   SVC R0-R15 Save Area (Large)
    0840 2112 Bitstring   64 PFXSVCSV       SVC R0-R15 savearea
    0880 2176 Bitstring   64 *
    08C0 2240 Address      4 PFXSVC         HCPSVC address
    08C4 2244 Address      4 PFXLRQND       A(last freed SAVBK) only if
                                            &HCPDBG
    08C8 2248 Signed       4 PFXLRC         Local SAVBK return queue count
    08CC 2252 Address      4 PFXLRQ         Local SAVBK return queue PFXLRC
                                            and PFXLRQ should be in the same
                                            d-word for fastest access.
    08D0 2256 Address      4 PFXCPRQA       Cross processor return queue
                                            addr. Bit 0 of this word may be
                                            used as a flag. Be careful when
                                            using this field when in Amode64.
    08D4 2260 Address      4 PFXCPRQP       Cross processor return queue
                                            addr. Bit 0 of this word may be
                                            used as a flag. Be careful when
                                            using this field when in Amode64.
    08D8 2264 Address      4 PFXSSABK       Static savearea pointer
    08DC 2268 Address      4 PFX2WAY        A(current STATIC savearea)
    08E0 2272 Address      4 PFXSVU         HCPSVU address
    08E4 2276 Address      4 PFXSVF         HCPSVF address
    08E8 2280 Address      8 PFXSVR13       Temporary R13 save for SSABK
                                            usage
    08F0 2288 Signed       2 *              Reserved for IBM use
    08F2 2290 Bitstring    1 PFXIACR        Caller IAC for linkage PFXIACR
                                            should remain at byte 2 within
                                            its word in storage so that
                                            HCPCALL can use L PFXIACR-2 to
                                            get the field into byte 6 of the
                                            register for subsequent SACF
                                            0(Rx).
    08F3 2291 Bitstring    1 PFXIACE        Callee IAC for linkage
    08F4 2292 Signed       4 *              Reserved for IBM use
    08F8 2296 Dbl-Word     8 PFXDBGRX       1-register save for debug things
          THIS AREA HAS THE SAME FORMAT AS A SAVEAREA IN HCPSAVBK
    0300  768 Signed       4 PFXTMPFP
    0304  772 Signed       4 PFXTMPBP
    0308  776 Signed       4 *
    030C  780 Signed       4 *
    0310  784 Bitstring    1 PFXTMPSC
    0311  785 Bitstring    1 PFXTMPCL
    0312  786 Bitstring    1 *
    0313  787 Bitstring    1 *
    0314  788 Signed       4 *
    0318  792 Bitstring  232 PFXTMPAREA (0) Register and working storage
    0318  792 Bitstring   64 PFXTMPRG (0)   Caller's registers
    0318  792 Signed       4 PFXTMPR0 (0)   Caller's saved register 0
    0318  792 Bitstring    1 PFXTMPR0B0     byte 0
    0319  793 Bitstring    1 PFXTMPR0B1     byte 1
    031A  794 Bitstring    1 PFXTMPR0B2     byte 2
    031B  795 Bitstring    1 PFXTMPR0B3     byte 3
    031C  796 Signed       4 PFXTMPR1 (0)   Caller's saved register 1
    031C  796 Bitstring    1 PFXTMPR1B0     byte 0
    031D  797 Bitstring    1 PFXTMPR1B1     byte 1
    031E  798 Bitstring    1 PFXTMPR1B2     byte 2
    031F  799 Bitstring    1 PFXTMPR1B3     byte 3
    0320  800 Signed       4 PFXTMPR2 (0)   Caller's saved register 2 THE
                                            FOLLOWING BYTE DEFINITIONS OF
                                            SAVER2 ARE FOR TESTING PARAMETERS
                                            PASSED BETWEEN MODULES.
    0320  800 Bitstring    1 PFXTMPR2B0     byte 0
    0321  801 Bitstring    1 PFXTMPR2B1     byte 1
    0322  802 Bitstring    1 PFXTMPR2B2     byte 2
    0323  803 Bitstring    1 PFXTMPR2B3     byte 3
    0324  804 Signed       4 PFXTMPR3       Caller's saved register 3
    0328  808 Signed       4 PFXTMPR4       Caller's saved register 4
    032C  812 Signed       4 PFXTMPR5       Caller's saved register 5
    0330  816 Signed       4 PFXTMPR6       Caller's saved register 6
    0334  820 Signed       4 PFXTMPR7       Caller's saved register 7
    0338  824 Signed       4 PFXTMPR8       Caller's saved register 8
    033C  828 Signed       4 PFXTMPR9       Caller's saved register 9
    0340  832 Signed       4 PFXTMPRA       Caller's saved register 10
    0344  836 Signed       4 PFXTMPRB       Caller's saved register 11; ALSO
                                            VMDBK ADDRESS OF USER ON WHICH
                                            SAVBK IS SCHEDULED
    0348  840 Bitstring   16 PFXTMPRCF (0)  Caller's saved register 12-15
    0348  840 Signed       4 PFXTMPRC       Caller's saved register 12
    034C  844 Signed       4 PFXTMPRD       Caller's saved register 13; ALSO
                                            PREVIOUS SAVBK ADDRESS ON CALL
    0350  848 Signed       4 PFXTMPRE       Caller's saved register 14; ALSO
                                            RETURN ADDRESS ON CALL OR STACKED
                                            SAVBK RETURN
    0354  852 Signed       4 PFXTMPRF       Caller's saved register 15; ALSO
                                            GOTO ADDRESS ON SCHEDULED SAVBK
                                            EXECUTION; ALSO REGISTER 15
                                            RETURN CODE ON HCPEXIT OR STACKED
                                            SAVBK RETURN
    0358  856 Bitstring   40 PFXTMPWK (0)   Workarea for callee
    0358  856 Signed       4 PFXTMPW0
    035C  860 Signed       4 PFXTMPW1
    0360  864 Signed       4 PFXTMPW2
    0364  868 Signed       4 PFXTMPW3
    0368  872 Signed       4 PFXTMPW4
    036C  876 Signed       4 PFXTMPW5
    0370  880 Signed       4 PFXTMPW6
    0374  884 Signed       4 PFXTMPW7
    0378  888 Signed       4 PFXTMPW8
    037C  892 Signed       4 PFXTMPW9
    0380  896 Bitstring    1 PFXTMPW$ (0)
          SAVBK extension:  Saveareas in the
          SAVBK format *may* have the high halves of
          registers stored in the tail end.  Bit SAVERG64 in the
          savearea header indicates that these fields are valid.
    0380  896 Signed       4 * (4)          Reserved for future use
    0390  912 Signed       4 * (4)          Reserved for future use
          The SAVBK SAVEAARP and the SVGBK SVGAARP fields must be
          at the same offset into each control block.  The only
          available area in both that satisfies this requirement
          is, unfortunately, here in the middle of the control
          block.
    03A0  928 Address      4 PFXTMPOPNR     A(who set SVHOPEN)
    03A4  932 Signed       4 *              Reserved for IBM use
    03A8  936 Address      4 PFXTMPAARP     A(AR sidecar) for PFX saveareas
    03AC  940 Bitstring    1 PFXTMPIACA     Caller actual IAC
    03AD  941 Bitstring    1 PFXTMPAMDE     Amode of callee at entry.
    03AE  942 Bitstring    1 PFXTMPIACR     Caller "should be" IAC
    03AF  943 Bitstring    1 PFXTMPIACE     Callee "should be" IAC
    03B0  944 Signed       4 * (4)          Reserved for future use
    03C0  960 Bitstring   64 PFXTMPHIRG (0)
    03C0  960 Signed       4 PFXTMPH0       High word of zArch general reg 0
    03C4  964 Signed       4 PFXTMPH1       High word of zArch general reg 1
    03C8  968 Signed       4 PFXTMPH2       High word of zArch general reg 2
    03CC  972 Signed       4 PFXTMPH3       High word of zArch general reg 3
    03D0  976 Signed       4 PFXTMPH4       High word of zArch general reg 4
    03D4  980 Signed       4 PFXTMPH5       High word of zArch general reg 5
    03D8  984 Signed       4 PFXTMPH6       High word of zArch general reg 6
    03DC  988 Signed       4 PFXTMPH7       High word of zArch general reg 7
    03E0  992 Signed       4 PFXTMPH8       High word of zArch general reg 8
    03E4  996 Signed       4 PFXTMPH9       High word of zArch general reg 9
    03E8 1000 Signed       4 PFXTMPH10      High word of zArch general reg 10
    03EC 1004 Signed       4 PFXTMPH11      High word of zArch general reg 11
    03F0 1008 Signed       4 PFXTMPH12      High word of zArch general reg 12
    03F4 1012 Signed       4 PFXTMPH13      High word of zArch general reg 13
    03F8 1016 Signed       4 PFXTMPH14      High word of zArch general reg 14
    03FC 1020 Signed       4 PFXTMPH15      High word of zArch general reg 15
    03A8  936 Bitstring    4 *              A(AR SIDECAR) FOR PFX SAVEAREA
          THIS AREA HAS THE SAME FORMAT AS A SAVEAREA IN HCPSAVBK
    0400 1024 Signed       4 PFXWRKFP
    0404 1028 Signed       4 PFXWRKBP
    0408 1032 Signed       4 *
    040C 1036 Signed       4 *
    0410 1040 Bitstring    1 PFXWRKSC
    0411 1041 Bitstring    1 PFXWRKCL
    0412 1042 Bitstring    1 *
    0413 1043 Bitstring    1 *
    0414 1044 Signed       4 *
    0418 1048 Bitstring  232 PFXWRKAREA (0) Register and working storage
    0418 1048 Bitstring   64 PFXWRKRG (0)   Caller's registers
    0418 1048 Signed       4 PFXWRKR0 (0)   Caller's saved register 0
    0418 1048 Bitstring    1 PFXWRKR0B0     byte 0
    0419 1049 Bitstring    1 PFXWRKR0B1     byte 1
    041A 1050 Bitstring    1 PFXWRKR0B2     byte 2
    041B 1051 Bitstring    1 PFXWRKR0B3     byte 3
    041C 1052 Signed       4 PFXWRKR1 (0)   Caller's saved register 1
    041C 1052 Bitstring    1 PFXWRKR1B0     byte 0
    041D 1053 Bitstring    1 PFXWRKR1B1     byte 1
    041E 1054 Bitstring    1 PFXWRKR1B2     byte 2
    041F 1055 Bitstring    1 PFXWRKR1B3     byte 3
    0420 1056 Signed       4 PFXWRKR2 (0)   Caller's saved register 2 THE
                                            FOLLOWING BYTE DEFINITIONS OF
                                            SAVER2 ARE FOR TESTING PARAMETERS
                                            PASSED BETWEEN MODULES.
    0420 1056 Bitstring    1 PFXWRKR2B0     byte 0
    0421 1057 Bitstring    1 PFXWRKR2B1     byte 1
    0422 1058 Bitstring    1 PFXWRKR2B2     byte 2
    0423 1059 Bitstring    1 PFXWRKR2B3     byte 3
    0424 1060 Signed       4 PFXWRKR3       Caller's saved register 3
    0428 1064 Signed       4 PFXWRKR4       Caller's saved register 4
    042C 1068 Signed       4 PFXWRKR5       Caller's saved register 5
    0430 1072 Signed       4 PFXWRKR6       Caller's saved register 6
    0434 1076 Signed       4 PFXWRKR7       Caller's saved register 7
    0438 1080 Signed       4 PFXWRKR8       Caller's saved register 8
    043C 1084 Signed       4 PFXWRKR9       Caller's saved register 9
    0440 1088 Signed       4 PFXWRKRA       Caller's saved register 10
    0444 1092 Signed       4 PFXWRKRB       Caller's saved register 11; ALSO
                                            VMDBK ADDRESS OF USER ON WHICH
                                            SAVBK IS SCHEDULED
    0448 1096 Bitstring   16 PFXWRKRCF (0)  Caller's saved register 12-15
    0448 1096 Signed       4 PFXWRKRC       Caller's saved register 12
    044C 1100 Signed       4 PFXWRKRD       Caller's saved register 13; ALSO
                                            PREVIOUS SAVBK ADDRESS ON CALL
    0450 1104 Signed       4 PFXWRKRE       Caller's saved register 14; ALSO
                                            RETURN ADDRESS ON CALL OR STACKED
                                            SAVBK RETURN
    0454 1108 Signed       4 PFXWRKRF       Caller's saved register 15; ALSO
                                            GOTO ADDRESS ON SCHEDULED SAVBK
                                            EXECUTION; ALSO REGISTER 15
                                            RETURN CODE ON HCPEXIT OR STACKED
                                            SAVBK RETURN
    0458 1112 Bitstring   40 PFXWRKWK (0)   Workarea for callee
    0458 1112 Signed       4 PFXWRKW0
    045C 1116 Signed       4 PFXWRKW1
    0460 1120 Signed       4 PFXWRKW2
    0464 1124 Signed       4 PFXWRKW3
    0468 1128 Signed       4 PFXWRKW4
    046C 1132 Signed       4 PFXWRKW5
    0470 1136 Signed       4 PFXWRKW6
    0474 1140 Signed       4 PFXWRKW7
    0478 1144 Signed       4 PFXWRKW8
    047C 1148 Signed       4 PFXWRKW9
    0480 1152 Bitstring    1 PFXWRKW$ (0)
          SAVBK extension:  Saveareas in the
          SAVBK format *may* have the high halves of
          registers stored in the tail end.  Bit SAVERG64 in the
          savearea header indicates that these fields are valid.
    0480 1152 Signed       4 * (4)          Reserved for future use
    0490 1168 Signed       4 * (4)          Reserved for future use
          The SAVBK SAVEAARP and the SVGBK SVGAARP fields must be
          at the same offset into each control block.  The only
          available area in both that satisfies this requirement
          is, unfortunately, here in the middle of the control
          block.
    04A0 1184 Address      4 PFXWRKOPNR     A(who set SVHOPEN)
    04A4 1188 Signed       4 *              Reserved for IBM use
    04A8 1192 Address      4 PFXWRKAARP     A(AR sidecar) for PFX saveareas
    04AC 1196 Bitstring    1 PFXWRKIACA     Caller actual IAC
    04AD 1197 Bitstring    1 PFXWRKAMDE     Amode of callee at entry.
    04AE 1198 Bitstring    1 PFXWRKIACR     Caller "should be" IAC
    04AF 1199 Bitstring    1 PFXWRKIACE     Callee "should be" IAC
    04B0 1200 Signed       4 * (4)          Reserved for future use
    04C0 1216 Bitstring   64 PFXWRKHIRG (0)
    04C0 1216 Signed       4 PFXWRKH0       High word of zArch general reg 0
    04C4 1220 Signed       4 PFXWRKH1       High word of zArch general reg 1
    04C8 1224 Signed       4 PFXWRKH2       High word of zArch general reg 2
    04CC 1228 Signed       4 PFXWRKH3       High word of zArch general reg 3
    04D0 1232 Signed       4 PFXWRKH4       High word of zArch general reg 4
    04D4 1236 Signed       4 PFXWRKH5       High word of zArch general reg 5
    04D8 1240 Signed       4 PFXWRKH6       High word of zArch general reg 6
    04DC 1244 Signed       4 PFXWRKH7       High word of zArch general reg 7
    04E0 1248 Signed       4 PFXWRKH8       High word of zArch general reg 8
    04E4 1252 Signed       4 PFXWRKH9       High word of zArch general reg 9
    04E8 1256 Signed       4 PFXWRKH10      High word of zArch general reg 10
    04EC 1260 Signed       4 PFXWRKH11      High word of zArch general reg 11
    04F0 1264 Signed       4 PFXWRKH12      High word of zArch general reg 12
    04F4 1268 Signed       4 PFXWRKH13      High word of zArch general reg 13
    04F8 1272 Signed       4 PFXWRKH14      High word of zArch general reg 14
    04FC 1276 Signed       4 PFXWRKH15      High word of zArch general reg 15
    04A8 1192 Bitstring    4 *              A(AR SIDECAR) FOR PFX SAVEAREA
          THIS AREA HAS THE SAME FORMAT AS A SAVEAREA IN HCPSAVBK
    0500 1280 Signed       4 PFXBALFP
    0504 1284 Signed       4 PFXBALBP
    0508 1288 Signed       4 *
    050C 1292 Signed       4 *
    0510 1296 Bitstring    1 PFXBALSC
    0511 1297 Bitstring    1 PFXBALCL
    0512 1298 Bitstring    1 *
    0513 1299 Bitstring    1 *
    0514 1300 Signed       4 *
    0518 1304 Bitstring  232 PFXBALAREA (0) Register and working storage
    0518 1304 Bitstring   64 PFXBALRG (0)   Caller's registers
    0518 1304 Signed       4 PFXBALR0 (0)   Caller's saved register 0
    0518 1304 Bitstring    1 PFXBALR0B0     byte 0
    0519 1305 Bitstring    1 PFXBALR0B1     byte 1
    051A 1306 Bitstring    1 PFXBALR0B2     byte 2
    051B 1307 Bitstring    1 PFXBALR0B3     BYTE 3
    051C 1308 Signed       4 PFXBALR1 (0)   Caller's saved register 1
    051C 1308 Bitstring    1 PFXBALR1B0     byte 0
    051D 1309 Bitstring    1 PFXBALR1B1     byte 1
    051E 1310 Bitstring    1 PFXBALR1B2     byte 2
    051F 1311 Bitstring    1 PFXBALR1B3     byte 3
    0520 1312 Signed       4 PFXBALR2 (0)   Caller's saved register 2 THE
                                            FOLLOWING BYTE DEFINITIONS OF
                                            SAVER2 ARE FOR TESTING PARAMETERS
                                            PASSED BETWEEN MODULES.
    0520 1312 Bitstring    1 PFXBALR2B0     byte 0
    0521 1313 Bitstring    1 PFXBALR2B1     byte 1
    0522 1314 Bitstring    1 PFXBALR2B2     byte 2
    0523 1315 Bitstring    1 PFXBALR2B3     byte 3
    0524 1316 Signed       4 PFXBALR3       Caller's saved register 3
    0528 1320 Signed       4 PFXBALR4       Caller's saved register 4
    052C 1324 Signed       4 PFXBALR5       Caller's saved register 5
    0530 1328 Signed       4 PFXBALR6       Caller's saved register 6
    0534 1332 Signed       4 PFXBALR7       Caller's saved register 7
    0538 1336 Signed       4 PFXBALR8       Caller's saved register 8
    053C 1340 Signed       4 PFXBALR9       Caller's saved register 9
    0540 1344 Signed       4 PFXBALRA       Caller's saved register 10
    0544 1348 Signed       4 PFXBALRB       Caller's saved register 11; ALSO
                                            VMDBK ADDRESS OF USER ON WHICH
                                            SAVBK IS SCHEDULED
    0548 1352 Bitstring   16 PFXBALRCF (0)  Caller's saved register 12-15
    0548 1352 Signed       4 PFXBALRC       Caller's saved register 12
    054C 1356 Signed       4 PFXBALRD       Caller's saved register 13; ALSO
                                            PREVIOUS SAVBK ADDRESS ON CALL
    0550 1360 Signed       4 PFXBALRE       Caller's saved register 14; ALSO
                                            RETURN ADDRESS ON CALL OR STACKED
                                            SAVBK RETURN
    0554 1364 Signed       4 PFXBALRF       Caller's saved register 15; ALSO
                                            GOTO ADDRESS ON SCHEDULED SAVBK
                                            EXECUTION; ALSO REGISTER 15
                                            RETURN CODE ON HCPEXIT OR STACKED
                                            SAVBK RETURN
    0558 1368 Bitstring   40 PFXBALWK (0)   Workarea for callee
    0558 1368 Signed       4 PFXBALW0
    055C 1372 Signed       4 PFXBALW1
    0560 1376 Signed       4 PFXBALW2
    0564 1380 Signed       4 PFXBALW3
    0568 1384 Signed       4 PFXBALW4
    056C 1388 Signed       4 PFXBALW5
    0570 1392 Signed       4 PFXBALW6
    0574 1396 Signed       4 PFXBALW7
    0578 1400 Signed       4 PFXBALW8
    057C 1404 Signed       4 PFXBALW9
    0580 1408 Bitstring    1 PFXBALW$ (0)
          SAVBK extension:  Saveareas in the
          SAVBK format *may* have the high halves of
          registers stored in the tail end.  Bit SAVERG64 in the
          savearea header indicates that these fields are valid.
    0580 1408 Signed       4 * (4)          Reserved for future use
    0590 1424 Signed       4 * (4)          Reserved for future use
          The SAVBK SAVEAARP and the SVGBK SVGAARP fields must be
          at the same offset into each control block.  The only
          available area in both that satisfies this requirement
          is, unfortunately, here in the middle of the control
          block.
    05A0 1440 Address      4 PFXBALOPNR     A(who set SVHOPEN)
    05A4 1444 Signed       4 *              Reserved for IBM use
    05A8 1448 Address      4 PFXBALAARP     A(AR sidecar) for PFX saveareas
    05AC 1452 Bitstring    1 PFXBALIACA     Caller actual IAC
    05AD 1453 Bitstring    1 PFXBALAMDE     AMODE OF CALLEE AT ENTRY.
    05AE 1454 Bitstring    1 PFXBALIACR     Caller "should be" IAC
    05AF 1455 Bitstring    1 PFXBALIACE     Callee "should be" IAC
    05B0 1456 Signed       4 * (4)          Reserved for future use
    05C0 1472 Bitstring   64 PFXBALHIRG (0)
    05C0 1472 Signed       4 PFXBALH0       High word of zArch general reg 0
    05C4 1476 Signed       4 PFXBALH1       High word of zArch general reg 1
    05C8 1480 Signed       4 PFXBALH2       High word of zArch general reg 2
    05CC 1484 Signed       4 PFXBALH3       High word of zArch general reg 3
    05D0 1488 Signed       4 PFXBALH4       High word of zArch general reg 4
    05D4 1492 Signed       4 PFXBALH5       High word of zArch general reg 5
    05D8 1496 Signed       4 PFXBALH6       High word of zArch general reg 6
    05DC 1500 Signed       4 PFXBALH7       High word of zArch general reg 7
    05E0 1504 Signed       4 PFXBALH8       High word of zArch general reg 8
    05E4 1508 Signed       4 PFXBALH9       High word of zArch general reg 9
    05E8 1512 Signed       4 PFXBALH10      High word of zArch general reg 10
    05EC 1516 Signed       4 PFXBALH11      High word of zArch general reg 11
    05F0 1520 Signed       4 PFXBALH12      High word of zArch general reg 12
    05F4 1524 Signed       4 PFXBALH13      High word of zArch general reg 13
    05F8 1528 Signed       4 PFXBALH14      High word of zArch general reg 14
    05FC 1532 Signed       4 PFXBALH15      High word of zArch general reg 15
    05A8 1448 Bitstring    4 *              A(AR SIDECAR) FOR PFX SAVEAREA
          THIS AREA HAS THE SAME FORMAT AS A SAVEAREA IN HCPSAVBK
    0600 1536 Signed       4 PFXPTRFP
    0604 1540 Signed       4 PFXPTRBP
    0608 1544 Signed       4 *
    060C 1548 Signed       4 *
    0610 1552 Bitstring    1 PFXPTRSC
    0611 1553 Bitstring    1 PFXPTRCL
    0612 1554 Bitstring    1 *
    0613 1555 Bitstring    1 *
    0614 1556 Signed       4 *
    0618 1560 Bitstring  232 PFXPTRAREA (0) Register and working storage
    0618 1560 Bitstring   64 PFXPTRRG (0)   Caller's registers
    0618 1560 Signed       4 PFXPTRR0 (0)   Caller's saved register 0
    0618 1560 Bitstring    1 PFXPTRR0B0     byte 0
    0619 1561 Bitstring    1 PFXPTRR0B1     BYTE 1
    061A 1562 Bitstring    1 PFXPTRR0B2     byte 2
    061B 1563 Bitstring    1 PFXPTRR0B3     byte 3
    061C 1564 Signed       4 PFXPTRR1 (0)   Caller's saved register 1
    061C 1564 Bitstring    1 PFXPTRR1B0     byte 0
    061D 1565 Bitstring    1 PFXPTRR1B1     byte 1
    061E 1566 Bitstring    1 PFXPTRR1B2     byte 2
    061F 1567 Bitstring    1 PFXPTRR1B3     byte 3
    0620 1568 Signed       4 PFXPTRR2 (0)   Caller's saved register 2 THE
                                            FOLLOWING BYTE DEFINITIONS OF
                                            SAVER2 ARE FOR TESTING PARAMETERS
                                            PASSED BETWEEN MODULES.
    0620 1568 Bitstring    1 PFXPTRR2B0     byte 0
    0621 1569 Bitstring    1 PFXPTRR2B1     byte 1
    0622 1570 Bitstring    1 PFXPTRR2B2     byte 2
    0623 1571 Bitstring    1 PFXPTRR2B3     byte 3
    0624 1572 Signed       4 PFXPTRR3       Caller's saved register 3
    0628 1576 Signed       4 PFXPTRR4       Caller's saved register 4
    062C 1580 Signed       4 PFXPTRR5       Caller's saved register 5
    0630 1584 Signed       4 PFXPTRR6       Caller's saved register 6
    0634 1588 Signed       4 PFXPTRR7       Caller's saved register 7
    0638 1592 Signed       4 PFXPTRR8       Caller's saved register 8
    063C 1596 Signed       4 PFXPTRR9       Caller's saved register 9
    0640 1600 Signed       4 PFXPTRRA       Caller's saved register 10
    0644 1604 Signed       4 PFXPTRRB       Caller's saved register 11; ALSO
                                            VMDBK ADDRESS OF USER ON WHICH
                                            SAVBK IS SCHEDULED
    0648 1608 Bitstring   16 PFXPTRRCF (0)  Caller's saved register 12-15
    0648 1608 Signed       4 PFXPTRRC       Caller's saved register 12
    064C 1612 Signed       4 PFXPTRRD       Caller's saved register 13; ALSO
                                            PREVIOUS SAVBK ADDRESS ON CALL
    0650 1616 Signed       4 PFXPTRRE       Caller's saved register 14; ALSO
                                            RETURN ADDRESS ON CALL OR STACKED
                                            SAVBK RETURN
    0654 1620 Signed       4 PFXPTRRF       Caller's saved register 15; ALSO
                                            GOTO ADDRESS ON SCHEDULED SAVBK
                                            EXECUTION; ALSO REGISTER 15
                                            RETURN CODE ON HCPEXIT OR STACKED
                                            SAVBK RETURN
    0658 1624 Bitstring   40 PFXPTRWK (0)   Workarea for callee
    0658 1624 Signed       4 PFXPTRW0
    065C 1628 Signed       4 PFXPTRW1
    0660 1632 Signed       4 PFXPTRW2
    0664 1636 Signed       4 PFXPTRW3
    0668 1640 Signed       4 PFXPTRW4
    066C 1644 Signed       4 PFXPTRW5
    0670 1648 Signed       4 PFXPTRW6
    0674 1652 Signed       4 PFXPTRW7
    0678 1656 Signed       4 PFXPTRW8
    067C 1660 Signed       4 PFXPTRW9
    0680 1664 Bitstring    1 PFXPTRW$ (0)
          SAVBK extension:  Saveareas in the
          SAVBK format *may* have the high halves of
          registers stored in the tail end.  Bit SAVERG64 in the
          savearea header indicates that these fields are valid.
    0680 1664 Signed       4 * (4)          Reserved for future use
    0690 1680 Signed       4 * (4)          Reserved for future use
          The SAVBK SAVEAARP and the SVGBK SVGAARP fields must be
          at the same offset into each control block.  The only
          available area in both that satisfies this requirement
          is, unfortunately, here in the middle of the control
          block.
    06A0 1696 Address      4 PFXPTROPNR     A(who set SVHOPEN)
    06A4 1700 Signed       4 *              Reserved for IBM use
    06A8 1704 Address      4 PFXPTRAARP     A(AR sidecar) for PFX saveareas
    06AC 1708 Bitstring    1 PFXPTRIACA     Caller actual IAC
    06AD 1709 Bitstring    1 PFXPTRAMDE     Amode of callee at entry.
    06AE 1710 Bitstring    1 PFXPTRIACR     Caller "should be" IAC
    06AF 1711 Bitstring    1 PFXPTRIACE     Callee "should be" IAC
    06B0 1712 Signed       4 * (4)          Reserved for future use
    06C0 1728 Bitstring   64 PFXPTRHIRG (0)
    06C0 1728 Signed       4 PFXPTRH0       High word of zArch general reg 0
    06C4 1732 Signed       4 PFXPTRH1       High word of zArch general reg 1
    06C8 1736 Signed       4 PFXPTRH2       High word of zArch general reg 2
    06CC 1740 Signed       4 PFXPTRH3       High word of zArch general reg 3
    06D0 1744 Signed       4 PFXPTRH4       High word of zArch general reg 4
    06D4 1748 Signed       4 PFXPTRH5       High word of zArch general reg 5
    06D8 1752 Signed       4 PFXPTRH6       High word of zArch general reg 6
    06DC 1756 Signed       4 PFXPTRH7       High word of zArch general reg 7
    06E0 1760 Signed       4 PFXPTRH8       High word of zArch general reg 8
    06E4 1764 Signed       4 PFXPTRH9       High word of zArch general reg 9
    06E8 1768 Signed       4 PFXPTRH10      High word of zArch general reg 10
    06EC 1772 Signed       4 PFXPTRH11      High word of zArch general reg 11
    06F0 1776 Signed       4 PFXPTRH12      High word of zArch general reg 12
    06F4 1780 Signed       4 PFXPTRH13      High word of zArch general reg 13
    06F8 1784 Signed       4 PFXPTRH14      High word of zArch general reg 14
    06FC 1788 Signed       4 PFXPTRH15      High word of zArch general reg 15
    06A8 1704 Bitstring    4 *              A(AR SIDECAR) FOR PFX SAVEAREA
          THIS AREA HAS THE SAME FORMAT AS A SAVEAREA IN HCPSAVBK
    0700 1792 Signed       4 PFXFREFP
    0704 1796 Signed       4 PFXFREBP
    0708 1800 Signed       4 *
    070C 1804 Signed       4 *
    0710 1808 Bitstring    1 PFXFRESC
    0711 1809 Bitstring    1 PFXFRECL
    0712 1810 Bitstring    1 *
    0713 1811 Bitstring    1 *
    0714 1812 Signed       4 *
    0718 1816 Bitstring  232 PFXFREAREA (0) Register and working storage
    0718 1816 Bitstring   64 PFXFRERG (0)   Caller's registers
    0718 1816 Signed       4 PFXFRER0 (0)   Caller's saved register 0
    0718 1816 Bitstring    1 PFXFRER0B0     byte 0
    0719 1817 Bitstring    1 PFXFRER0B1     byte 1
    071A 1818 Bitstring    1 PFXFRER0B2     byte 2
    071B 1819 Bitstring    1 PFXFRER0B3     byte 3
    071C 1820 Signed       4 PFXFRER1 (0)   Caller's saved register 1
    071C 1820 Bitstring    1 PFXFRER1B0     byte 0
    071D 1821 Bitstring    1 PFXFRER1B1     byte 1
    071E 1822 Bitstring    1 PFXFRER1B2     byte 2
    071F 1823 Bitstring    1 PFXFRER1B3     byte 3
    0720 1824 Signed       4 PFXFRER2 (0)   Caller's saved register 2 THE
                                            FOLLOWING BYTE DEFINITIONS OF
                                            SAVER2 ARE FOR TESTING PARAMETERS
                                            PASSED BETWEEN MODULES.
    0720 1824 Bitstring    1 PFXFRER2B0     byte 0
    0721 1825 Bitstring    1 PFXFRER2B1     byte 1
    0722 1826 Bitstring    1 PFXFRER2B2     byte 2
    0723 1827 Bitstring    1 PFXFRER2B3     byte 3
    0724 1828 Signed       4 PFXFRER3       Caller's saved register 3
    0728 1832 Signed       4 PFXFRER4       Caller's saved register 4
    072C 1836 Signed       4 PFXFRER5       Caller's saved register 5
    0730 1840 Signed       4 PFXFRER6       Caller's saved register 6
    0734 1844 Signed       4 PFXFRER7       Caller's saved register 7
    0738 1848 Signed       4 PFXFRER8       Caller's saved register 8
    073C 1852 Signed       4 PFXFRER9       Caller's saved register 9
    0740 1856 Signed       4 PFXFRERA       Caller's saved register 10
    0744 1860 Signed       4 PFXFRERB       Caller's saved register 11; ALSO
                                            VMDBK ADDRESS OF USER ON WHICH
                                            SAVBK IS SCHEDULED
    0748 1864 Bitstring   16 PFXFRERCF (0)  Caller's saved register 12-15
    0748 1864 Signed       4 PFXFRERC       Caller's saved register 12
    074C 1868 Signed       4 PFXFRERD       Caller's saved register 13; ALSO
                                            PREVIOUS SAVBK ADDRESS ON CALL
    0750 1872 Signed       4 PFXFRERE       Caller's saved register 14; ALSO
                                            RETURN ADDRESS ON CALL OR STACKED
                                            SAVBK RETURN
    0754 1876 Signed       4 PFXFRERF       Caller's saved register 15; ALSO
                                            GOTO ADDRESS ON SCHEDULED SAVBK
                                            EXECUTION; ALSO REGISTER 15
                                            RETURN CODE ON HCPEXIT OR STACKED
                                            SAVBK RETURN
    0758 1880 Bitstring   40 PFXFREWK (0)   Workarea for callee
    0758 1880 Signed       4 PFXFREW0
    075C 1884 Signed       4 PFXFREW1
    0760 1888 Signed       4 PFXFREW2
    0764 1892 Signed       4 PFXFREW3
    0768 1896 Signed       4 PFXFREW4
    076C 1900 Signed       4 PFXFREW5
    0770 1904 Signed       4 PFXFREW6
    0774 1908 Signed       4 PFXFREW7
    0778 1912 Signed       4 PFXFREW8
    077C 1916 Signed       4 PFXFREW9
    0780 1920 Bitstring    1 PFXFREW$ (0)
          SAVBK extension:  Saveareas in the
          SAVBK format *may* have the high halves of
          registers stored in the tail end.  Bit SAVERG64 in the
          savearea header indicates that these fields are valid.
    0780 1920 Signed       4 * (4)          Reserved for future use
    0790 1936 Signed       4 * (4)          Reserved for future use
          The SAVBK SAVEAARP and the SVGBK SVGAARP fields must be
          at the same offset into each control block.  The only
          available area in both that satisfies this requirement
          is, unfortunately, here in the middle of the control
          block.
    07A0 1952 Address      4 PFXFREOPNR     A(who set SVHOPEN)
    07A4 1956 Signed       4 *              Reserved for IBM use
    07A8 1960 Address      4 PFXFREAARP     A(AR sidecar) for PFX saveareas
    07AC 1964 Bitstring    1 PFXFREIACA     CALLER ACTUAL IAC
    07AD 1965 Bitstring    1 PFXFREAMDE     Amode of callee at entry.
    07AE 1966 Bitstring    1 PFXFREIACR     Caller "should be" IAC
    07AF 1967 Bitstring    1 PFXFREIACE     Callee "should be" IAC
    07B0 1968 Signed       4 * (4)          Reserved for future use
    07C0 1984 Bitstring   64 PFXFREHIRG (0)
    07C0 1984 Signed       4 PFXFREH0       High word of zArch general reg 0
    07C4 1988 Signed       4 PFXFREH1       High word of zArch general reg 1
    07C8 1992 Signed       4 PFXFREH2       High word of zArch general reg 2
    07CC 1996 Signed       4 PFXFREH3       High word of zArch general reg 3
    07D0 2000 Signed       4 PFXFREH4       High word of zArch general reg 4
    07D4 2004 Signed       4 PFXFREH5       High word of zArch general reg 5
    07D8 2008 Signed       4 PFXFREH6       High word of zArch general reg 6
    07DC 2012 Signed       4 PFXFREH7       High word of zArch general reg 7
    07E0 2016 Signed       4 PFXFREH8       High word of zArch general reg 8
    07E4 2020 Signed       4 PFXFREH9       High word of zArch general reg 9
    07E8 2024 Signed       4 PFXFREH10      High word of zArch general reg 10
    07EC 2028 Signed       4 PFXFREH11      High word of zArch general reg 11
    07F0 2032 Signed       4 PFXFREH12      High word of zArch general reg 12
    07F4 2036 Signed       4 PFXFREH13      High word of zArch general reg 13
    07F8 2040 Signed       4 PFXFREH14      High word of zArch general reg 14
    07FC 2044 Signed       4 PFXFREH15      High word of zArch general reg 15
    07A8 1960 Bitstring    4 *              A(AR SIDECAR) FOR PFX SAVEAREA
          RE-DEFINITION OF PFXIRPSV FOR INDIVIDUAL REGISTERS
    0800 2048 Signed       4 PFXIRP12       R12 SAVE AREA
    0804 2052 Signed       4 PFXIRP13       R13 SAVE AREA
    0808 2056 Signed       4 PFXIRP14       R14 SAVE AREA
    080C 2060 Signed       4 PFXIRP15       R15 SAVE AREA
          RE-DEFINITION OF PFXLNKSG FOR 64-BIT REGISTERS
    0820 2080 Dbl-Word     8 PFXLNKGC       R12 SAVE AREA
    0828 2088 Dbl-Word     8 PFXLNKGD       R13 SAVE AREA
    0830 2096 Dbl-Word     8 PFXLNKGE       R14 SAVE AREA
    0838 2104 Dbl-Word     8 PFXLNKGF       R15 SAVE AREA
          RE-DEFINITION OF PFXLNKSV FOR INDIVIDUAL REGISTERS
    0820 2080 Signed       4 PFXLNK12       R12 SAVE AREA
    0824 2084 Signed       4 PFXLNK13       R13 SAVE AREA
    0828 2088 Signed       4 PFXLNK14       R14 SAVE AREA
    082C 2092 Signed       4 PFXLNK15       R15 SAVE AREA
                 TIMER WORK REGION
    02C0  704 Signed       4 PFXTODHO (0)   High half of TOD clock
    02C0  704 Signed       8 PFXCVTDA       Work area for HCPCVTxx. Some code
                                            also relies on finding a recent
                                            TOD value left behind here. (Such
                                            a value might be from STCK or
                                            STCKF, or a substring from
                                            STCKE.)
    02C8  712 Signed       8 PFXPTLBT       TOD clock at (actually, before)
                                            last TLB (and ALB) purge (whether
                                            by PTLB & PALB or CSP / CSPG
                                            purging both ALBs and TLBs
                                            globally) on this CPU
    02D0  720 Signed       8 PFXTMRUN       CPU TIMER AT USER RUN
    02D8  728 Signed       8 PFXTMURN       CPU TIMER AT USER UN-RUN
    02E0  736 Signed       8 PFXTMDSP       CPU TIMER AT USER DISPATCH
    02E8  744 Signed       8 PFXTMUDS       CPU TIMER AT USER UN-DISPATCH
    02F0  752 Signed       8 PFXVTDSP       VALUE OF VMSVTIME AT USER
                                            DISPATCH
    02F8  760 Signed       8 PFXPTLBL       TOD Clock at last PTLB on this
                                            CPU (never zeroed, unlike
                                            PFXPTLBT)
                 Host Control Register Savearea
                 Although z/Architecture CRs are 8 bytes, in most
                 cases, CP only uses the rightmost word or 4 bytes,
                 with zeros in the leftmost word of the CR.  CR1,
                 CR7, and CR13 contain ASCEs, and are exceptions:
                 ASCEs designate upper level DAT tables (Region
                 First, Region Second, Region Third, or Segment
                 Tables) which can reside above 2G and thus may have
                 non-zero values in the leftmost word.
                 For CR0, CP never sets the two bits defined in the
                          leftmost word (CR0.0 and CR0.1).
                 For CR1,7,13 the ASCEs loaded always point to CP
                          allocated control blocks that may be above
                          or below the 2G line.  LCTLG and STCTLG
                          must be used for these CRs.
                 For CR10,11 CP never sets host PER addresses.
                 For CR12 the CP trace table is always allocated
                          in pages below the 2G line.
                 For CR15 CP never uses the Linkage-Stack facility.
    0E80 3712 Bitstring  128 PFXCPCR (0)    Host Control Registers
          CR0  Control bits and masks
    0E80 3712 Signed       8 PFXCPCR0G (0)  Control and External Masks
    0E80 3712 Signed       4 PFXCPCR0H (0)  CR0 high word
    0E80 3712 Bitstring    1 *              Reserved for IBM use
    0E81 3713 Bitstring    1 PFXCR0HB1
    0E82 3714 Bitstring    2 *              Reserved for IBM use
    0E84 3716 Signed       4 PFXCPCR0 (0)   Control and External Masks
    0E84 3716 Bitstring    1 PFXCR0B0
    0E85 3717 Bitstring    1 PFXCR0B1
    0E86 3718 Bitstring    1 PFXCR0B2
    0E87 3719 Bitstring    1 PFXCR0B3
          CR1  Primary Address-Space-Control Element (ASCE)
    0E88 3720 Signed       8 PFXCPCR1G (0)  Primary ASCE
    0E88 3720 Signed       4 PFXCPCR1H      CR1 high half (Primary ASCE)
    0E8C 3724 Signed       4 PFXCPCR1 (0)   Primary ASCE
    0E8C 3724 Bitstring    1 PFXCR1B0       NO BITS DEFINED FOR PFXCR1B1
              1... ....      CR1SSXA        X'80' CR1SSXA 370/XA SPACE SWITCH
                                            EVENT MASK
    0E8D 3725 Bitstring    1 PFXCR1B1       NO BITS DEFINED FOR PFXCR1B2
    0E8E 3726 Bitstring    1 PFXCR1B2       NO BITS DEFINED FOR PFXCR1B3
    0E8F 3727 Bitstring    1 PFXCR1B3
          CR2  Dispatchable-Unit-Control-Table Origin
    0E90 3728 Signed       8 PFXCPCR2G (0)  DUCTO
    0E90 3728 Signed       4 PFXCPCR2H      CR2 high half (DUCTO) @
    0E94 3732 Signed       4 PFXCPCR2 (0)   NO BITS DEFINED FOR PFXCR2B0
    0E94 3732 Bitstring    1 PFXCR2B0       NO BITS DEFINED FOR PFXCR2B1 BY
                                            HCPEQUAT
    0E95 3733 Bitstring    1 PFXCR2B1       NO BITS DEFINED FOR PFXCR2B2 BY
                                            HCPEQUAT
    0E96 3734 Bitstring    1 PFXCR2B2       NO BITS DEFINED FOR PFXCR2B3 BY
                                            HCPEQUAT
    0E97 3735 Bitstring    1 PFXCR2B3
          CR3  PSW-Key Mask, Secondary Address-Space-Number (ASN)
    0E98 3736 Signed       8 PFXCPCR3G (0)  CR3
    0E98 3736 Signed       4 PFXCPCR3H      CR3 high half (reserved)
    0E9C 3740 Signed       4 PFXCPCR3 (0)   NO BITS DEFINED FOR PFXCR3B0 BY
                                            HCPEQUAT
    0E9C 3740 Bitstring    1 PFXCR3B0       NO BITS DEFINED FOR PFXCR3B1 BY
                                            HCPEQUAT
    0E9D 3741 Bitstring    1 PFXCR3B1       NO BITS DEFINED FOR PFXCR3B2 BY
                                            HCPEQUAT
    0E9E 3742 Bitstring    1 PFXCR3B2       NO BITS DEFINED FOR PFXCR3B3 BY
                                            HCPEQUAT
    0E9F 3743 Bitstring    1 PFXCR3B3
          CR4  Authorization Index, Primary Address-Space-Number
    0EA0 3744 Signed       8 PFXCPCR4G (0)  CR4
    0EA0 3744 Signed       4 PFXCPCR4H      CR4 high half (reserved)
    0EA4 3748 Signed       4 PFXCPCR4 (0)   NO BITS DEFINED FOR PFXCR4B0 BY
                                            HCPEQUAT
    0EA4 3748 Bitstring    1 PFXCR4B0       NO BITS DEFINED FOR PFXCR4B1 BY
                                            HCPEQUAT
    0EA5 3749 Bitstring    1 PFXCR4B1       NO BITS DEFINED FOR PFXCR4B2 BY
                                            HCPEQUAT
    0EA6 3750 Bitstring    1 PFXCR4B2       NO BITS DEFINED FOR PFXCR4B3 BY
                                            HCPEQUAT
    0EA7 3751 Bitstring    1 PFXCR4B3
          CR5  Primary-ASTE origin
    0EA8 3752 Signed       8 PFXCPCR5G (0)  CR5
    0EA8 3752 Signed       4 PFXCPCR5H      CR5 high half (reserved)
    0EAC 3756 Signed       4 PFXCPCR5 (0)   NO BITS DEFINED FOR PFXCR5B0 BY
                                            HCPEQUAT
    0EAC 3756 Bitstring    1 PFXCR5B0       NO BITS DEFINED FOR PFXCR5B1 BY
                                            HCPEQUAT
    0EAD 3757 Bitstring    1 PFXCR5B1       NO BITS DEFINED FOR PFXCR5B2 BY
                                            HCPEQUAT
    0EAE 3758 Bitstring    1 PFXCR5B2       NO BITS DEFINED FOR PFXCR5B3 BY
                                            HCPEQUAT
    0EAF 3759 Bitstring    1 PFXCR5B3
          CR6  I/O-Interruption Subclass Mask
    0EB0 3760 Signed       8 PFXCPCR6G (0)  CR6
    0EB0 3760 Signed       4 PFXCPCR6H      CR6 high half (reserved)
    0EB4 3764 Signed       4 PFXCPCR6 (0)   I/0 INTERRUPTION SUBCLASS MASKS
    0EB4 3764 Bitstring    1 PFXCR6B0
              1... ....      PFXCPIOI       X'80' PFXCPIOI I/O INTERRUPT
                                            SUBCLASS 00 FOR CP-INITIATED I/O
              1... ....      PFXIOCL0       X'80' PFXIOCL0 FLOATING CHANNEL
                                            INTERRUPT CLASS 0
              .1.. ....      PFXIOCL1       X'40' PFXIOCL1 FLOATING CHANNEL
                                            INTERRUPT CLASS 1
              ..1. ....      PFXIOCL2       X'20' PFXIOCL2 FLOATING CHANNEL
                                            INTERRUPT CLASS 2
              ...1 ....      PFXIOCL3       X'10' PFXIOCL3 FLOATING CHANNEL
                                            INTERRUPT CLASS 3
              .... 1...      PFXIOCL4       X'08' PFXIOCL4 FLOATING CHANNEL
                                            INTERRUPT CLASS 4
              .... .1..      PFXIOCL5       X'04' PFXIOCL5 FLOATING CHANNEL
                                            INTERRUPT CLASS 5
              .... ..1.      PFXIOCL6       X'02' PFXIOCL6 FLOATING CHANNEL
                                            INTERRUPT CLASS 6
              .... ...1      PFXIOCL7       X'01' PFXIOCL7 FLOATING CHANNEL
                                            INTERRUPT CLASS 7
              ...1 11.1      PFXDRFPT       X'1D' PFXDRFPT INTERRUPTION
                                            SUBCLASSES DEDICATED FOR LEVEL 2
                                            I/O PASS THRU'S USE.(3,4,5,7) NO
                                            BITS DEFINED FOR PFXCR6B1 BY
                                            HCPEQUAT
    0EB5 3765 Bitstring    1 PFXCR6B1       NO BITS DEFINED FOR PFXCR6B2 BY
                                            HCPEQUAT
    0EB6 3766 Bitstring    1 PFXCR6B2       NO BITS DEFINED FOR PFXCR6B3 BY
                                            HCPEQUAT
    0EB7 3767 Bitstring    1 PFXCR6B3
          CR7  Secondary Address-Space-Control Element (ASCE)
    0EB8 3768 Signed       8 PFXCPCR7G (0)  CR7
    0EB8 3768 Signed       4 PFXCPCR7H      CR7 high half (Secondary ASCE)
    0EBC 3772 Signed       4 PFXCPCR7 (0)   NO BITS DEFINED FOR PFXCR7B0 BY
                                            HCPEQUAT
    0EBC 3772 Bitstring    1 PFXCR7B0       NO BITS DEFINED FOR PFXCR7B1 BY
                                            HCPEQUAT
    0EBD 3773 Bitstring    1 PFXCR7B1       NO BITS DEFINED FOR PFXCR7B2 BY
                                            HCPEQUAT
    0EBE 3774 Bitstring    1 PFXCR7B2       NO BITS DEFINED FOR PFXCR7B3 BY
                                            HCPEQUAT
    0EBF 3775 Bitstring    1 PFXCR7B3
          CR8  Extended Authorization Index, Monitor Masks
    0EC0 3776 Signed       8 PFXCPCR8G (0)  CR8
    0EC0 3776 Signed       4 PFXCPCR8H      CR8 high half (reserved)
    0EC4 3780 Signed       4 PFXCPCR8 (0)   MONITOR CALL ENABLE MASKS
              NO BITS DEFINED FOR PFXCR8B0 BY HCPEQUAT
    0EC4 3780 Bitstring    1 PFXCR8B0       NO BITS DEFINED FOR PFXCR8B1 BY
                                            HCPEQUAT
    0EC5 3781 Bitstring    1 PFXCR8B1       NO BITS DEFINED FOR PFXCR8B2 BY
                                            HCPEQUAT
    0EC6 3782 Bitstring    1 PFXCR8B2       NO BITS DEFINED FOR PFXCR8B3 BY
                                            HCPEQUAT
    0EC7 3783 Bitstring    1 PFXCR8B3
          CR9  PER Control
    0EC8 3784 Signed       8 PFXCPCR9G (0)  CR9
    0EC8 3784 Signed       4 PFXCPCR9H      CR9 high half (reserved)
    0ECC 3788 Signed       4 PFXCPCR9 (0)   PER CONTROL
    0ECC 3788 Bitstring    1 PFXCR9B0       NO BITS DEFINED FOR PFXCR9B1 BY
                                            HCPEQUAT
    0ECD 3789 Bitstring    1 PFXCR9B1
    0ECE 3790 Bitstring    1 PFXCR9B2
    0ECF 3791 Bitstring    1 PFXCR9B3
          CR10 PER Address Range - Starting Address
    0ED0 3792 Signed       8 PFXCPCRAG (0)  CR10
    0ED0 3792 Signed       4 PFXCPCRAH      CR10 high half (PER range)
    0ED4 3796 Signed       4 PFXCPCRA       PER ADDRESS RANGE
          CR11 PER Address Range - Ending Address
    0ED8 3800 Signed       8 PFXCPCRBG (0)  CR11
    0ED8 3800 Signed       4 PFXCPCRBH      CR11 high half (PER range)
    0EDC 3804 Signed       4 PFXCPCRB       PER ADDRESS RANGE
          CR12 Trace Controls
    0EE0 3808 Signed       8 PFXCPCRCG (0)  CR12
    0EE0 3808 Signed       4 PFXCPCRCH      CR12 high half (Trace controls)
    0EE4 3812 Signed       4 PFXCPCRC (0)
    0EE4 3812 Bitstring    1 PFXCRCB0       NO BITS DEFINED FOR PFXCRCB1 BY
                                            HCPEQUAT
              1... ....      CRCBRCTL       X'80' CRCBRCTL BRANCH TRACE
                                            CONTROL BIT. WHEN ON, BALR, BASR,
                                            BASSM, BAKR AND BSG INST MAY BE
                                            TRACED BY THE HARDWARE. Note that
                                            for zArch, this bit is moved to
                                            GCRC0.0 of a 64-bit CRC with a
                                            label of CRCBTCTL.
    0EE5 3813 Bitstring    1 PFXCRCB1       NO BITS DEFINED FOR PFXCRCB2 BY
                                            HCPEQUAT
    0EE6 3814 Bitstring    1 PFXCRCB2
    0EE7 3815 Bitstring    1 PFXCRCB3
          CR13 Home Address-Space-Control Element
    0EE8 3816 Signed       8 PFXCPCRDG (0)  CR13
    0EE8 3816 Signed       4 PFXCPCRDH      CR13 high half (Home ASCE)
    0EEC 3820 Signed       4 PFXCPCRD (0)   NO BITS DEFINED FOR PFXCRDB0 BY
                                            HCPEQUAT CRDB0
    0EEC 3820 Bitstring    1 PFXCRDB0       NO BITS DEFINED FOR PFXCRDB1 BY
                                            HCPEQUAT CRDB1
    0EED 3821 Bitstring    1 PFXCRDB1       NO BITS DEFINED FOR PFXCRDB2 BY
                                            HCPEQUAT CRDB2
    0EEE 3822 Bitstring    1 PFXCRDB2       NO BITS DEFINED FOR PFXCRDB3 BY
                                            HCPEQUAT CRDB3
    0EEF 3823 Bitstring    1 PFXCRDB3
          CR14 Machine Check Masks, TOD clock control,
               ASN Translation Control
    0EF0 3824 Signed       8 PFXCPCREG (0)  CR14
    0EF0 3824 Signed       4 PFXCPCREH      CR14 high half (reserved)
    0EF4 3828 Signed       4 PFXCPCRE (0)   MACHINE CHECK CONTROL MASK
    0EF4 3828 Bitstring    1 PFXCREB0
    0EF5 3829 Bitstring    1 PFXCREB1       NO BITS DEFINED FOR PFXCREB2 BY
                                            HCPEQUAT
    0EF6 3830 Bitstring    1 PFXCREB2       NO BITS DEFINED FOR PFXCREB3 BY
                                            HCPEQUAT
    0EF7 3831 Bitstring    1 PFXCREB3
          CR15 Linkage-Stack-Entry Address
    0EF8 3832 Signed       8 PFXCPCRFG (0)  CR15
    0EF8 3832 Signed       4 PFXCPCRFH      CR15 high half (Linkage Stack)
    0EFC 3836 Signed       4 PFXCPCRF (0)   NO BITS DEFINED FOR PFXCRFB0 BY
                                            HCPEQUAT
    0EFC 3836 Bitstring    1 PFXCRFB0       NO BITS DEFINED FOR PFXCRFB1 BY
                                            HCPEQUAT
    0EFD 3837 Bitstring    1 PFXCRFB1       NO BITS DEFINED FOR PFXCRFB2 BY
                                            HCPEQUAT
    0EFE 3838 Bitstring    1 PFXCRFB2       NO BITS DEFINED FOR PFXCRFB3 BY
                                            HCPEQUAT
    0EFF 3839 Bitstring    1 PFXCRFB3
                 THE FOLLOWING INITIAL VALUES FOR THE CONTROL REGS
                 ARE FOR USE BY SYSTEM INITIALIZATION PRIOR TO
                 SETTING THE ACTUAL RUNNING VALUE.
                       PFXCPCR6,PFXCPCR7,PFXCPCR8,PFXCPCR9,PFXCPCRA,PFXCPCRB,
                       PFXCPCRC,PFXCPCRD,PFXCPCRE,PFXCPCRF
    0E80 3712 Address      4 * (0)          R5,PFXCPCR6,PFXCPCR7,PFXCPCR8,PFX
                                            CPCR9,PFXCPCRA,PFXCPCRB
                                            ,PFXCPCRC,PFXCPCRD,PFXCPCRE,PFXCP
                                            CRF) Force a cross reference
                                            PFXCPCR5H,PFXCPCR6H,PFXCPCR7H,PFX
                                            CPCR8H,PFXCPCR9H,
                                            PFXCPCRAH,PFXCPCRBH,PFXCPCRCH,PFX
                                            CPCRDH,PFXCPCREH, PFXCPCRFH
    0E80 3712 Address      4 * (0)          FXCPCR5H,PFXCPCR6H,PFXCPCR7H,PFXC
                                            PCR8H,PFXCPCR9H,PFXCPCR
                                            AH,PFXCPCRBH,PFXCPCRCH,PFXCPCRDH,
                                            PFXCPCREH,PFXCPCRFH) Force a
                                            cross reference
                                            PFXCPCR5G,PFXCPCR6G,PFXCPCR7G,PFX
                                            CPCR8G,PFXCPCR9G,
                                            PFXCPCRAG,PFXCPCRBG,PFXCPCRCG,PFX
                                            CPCRDG,PFXCPCREG, PFXCPCRFG
    0E80 3712 Address      4 * (0)          FXCPCR5G,PFXCPCR6G,PFXCPCR7G,PFXC
                                            PCR8G,PFXCPCR9G,PFXCPCR
                                            AG,PFXCPCRBG,PFXCPCRCG,PFXCPCRDG,
                                            PFXCPCREG,PFXCPCRFG) Force a
                                            cross reference
    0E80 3712 Address      4 * (0)          Force a cross reference
    0E80 3712 Signed       4 *              CR0 High half
    0E84 3716 Bitstring    4 *              CR0 Control, external masks
    0E88 3720 Signed       4 *              CR1 Primary-space ASCE
    0E90 3728 Signed       4 *              CR2 DUCT Origin
    0E98 3736 Signed       4 *              CR3 PSW-Key Mask, SASN
    0EA0 3744 Signed       4 *              CR4 Auth. Index, PASN
    0EA8 3752 Signed       4 *              CR5 Primary ASTE origin
    0EB0 3760 Signed       4 *              CR6 I/O Int. Subclass Masks
    0EB8 3768 Signed       4 *              CR7 Secondary-space ASCE
    0EC0 3776 Signed       4 *              CR8 Monitor Call Masks
    0EC8 3784 Signed       4 *              CR9 PER Control
    0ED0 3792 Signed       4 *              CR10 PER Address Range - start
    0ED8 3800 Signed       4 *              CR11 PER Address Range - end
    0EE0 3808 Signed       4 *              CR12 Trace Controls
    0EE8 3816 Signed       4 *              CR13 Home-space ASCE
    0EF0 3824 Signed       4 *              CR14 Machine check subclasses
    0EF8 3832 Signed       4 *              CR15 Linkage-Stack-Entry Address
                 SYSTEM MAINTENANCE SERVICE CODE IDENTIFIER
    0900 2304 Character   16 PFXFEIBM       5741-A09 '
    0910 2320 Signed       4 * (9)          Reserved for future IBM use.
                 FREQUENTLY REFERENCED ADDRESS CONSTANTS
                 Notes      : The address constants below that refer to
                       module entry points may contain addressing
                       mode bits and thus should not be used in
                       situations in which the presence of these
                       bits would not be appropriate, such as to set
                       interrupt return addresses in control blocks.
    0934 2356 Address      4 PFXSVR         Pointer to HCPSVR
    0938 2360 Address      4 PFXCFMRD       Pointer to HCPCFMRD
    093C 2364 Address      4 PFXCVTBH       Pointer to HCPCVTBH
    0940 2368 Address      4 PFXCVTDT       Pointer to HCPCVTDT
    0944 2372 Address      4 PFXCVTOD       Pointer to HCPCVTOD
    0948 2376 Address      4 PFXDSPCH       Pointer to HCPDSPCH
    094C 2380 Address      4 PFXERMES       Pointer to HCPERMES
    0950 2384 Address      4 PFXFREE        Pointer to HCPFREE
    0954 2388 Address      4 PFXFRET        Pointer to HCPFRET
    0958 2392 Address      4 PFXGSVC0       Pointer to HCPGSVC0
    095C 2396 Address      4 PFXGSVC1       Pointer to HCPGSVC1
    0960 2400 Address      4 PFXGSVC2       Pointer to HCPGSVC2
    0964 2404 Address      4 PFXGSVC3       Pointer to HCPGSVC3
    0968 2408 Address      4 PFXTTATB       Pointer to HCPTTATB
    096C 2412 Address      4 PFXIOSRQ       Pointer to HCPIOSRQ
    0970 2416 Address      4 PFXHTRAN       Pointer to HCPHTR2N
    0974 2420 Address      4 PFXLALLK       Pointer to HCPLALLK
    0978 2424 Address      4 PFXLALLU       Pointer to HCPLALLU
    097C 2428 Address      4 PFXHTRAB       Pointer to HCPHTR2B
    0980 2432 Address      4 PFXCFRWT       Pointer to HCPCFRWT
    0984 2436 Address      4 PFXRUNXT       Pointer to HCPRUNXT
    0988 2440 Address      4 PFXSTKCP       Pointer to HCPSTKCP
    098C 2444 Address      4 PFXSTKGT       Pointer to HCPSTKGT
    0990 2448 Address      4 PFXSTKIO       Pointer to HCPSTKIO
    0994 2452 Address      4 PFXSCCFD       Pointer to HCPSCCFD
    0998 2456 Address      4 PFXSYS         SYSTEM COMMON AREA
    099C 2460 Address      4 PFXSXLEN       Shared-exclusive spinlock SXLEN
                                            array origin address. Updates
                                            serialized by HCPRCCVA (Vary
                                            Proc).
    09A0 2464 Address      4 PFXSYSVM       SYSTEM VMDBLOCK
    09A4 2468 Address      4 PFXSYSMP       Address of SYSTEMMP VMDBK
    09A8 2472 Address      4 PFXRUNU        Pointer to HCPRUNU
    09AC 2476 Address      4 PFXENDOP       Pointer to HCPENDOP
                                               Called by BASR from
                                               deep within MASTER or
                                               HCPCALL macros.
    09B0 2480 Address      4 PFXSVUSW       Pointer to HCPSVUSW
    09B4 2484 Signed       4 *              Reserved for IBM use
    09B8 2488 Address      4 PFXSVUGS       Pointer to HCPSVUGS
    09BC 2492 Address      4 PFXPAGCP       End of the CP Nucleus (and
                                            RAMDISK if present.)
    09C0 2496 Address      4 PFXSVURS       Pointer to HCPSVURS
    09C4 2500 Address      4 PFXLUSER       PRIOR RUNNING USER
    09C8 2504 Address      4 PFXPRFIX       PREFIX VALUE FOR THIS CPU
    09CC 2508 Address      4 PFXNXTPF       CYCLIC POINTER TO NEXT PREFIX
                                            AREA If there is only one
                                            processor (in other words no
                                            other prefix areas) then it
                                            points to its own prefix area.
    09D0 2512 Signed       4 PFXABEND (0)   CP ABNORMAL TERMINATION CODE
    09D0 2512 Signed       4 PFXTRMCD (0)   Machine check termination code
    09D0 2512 Bitstring    3 PFXABENM       CP ABEND MODULE ID
    09D3 2515 Bitstring    1 PFXABENN       CP ABEND DETAIL CODE
    09D4 2516 Address      4 PFXSXAST       Host real address of ASTE for...
                                            system-execution address space.
    09D8 2520 Address      4 PFXSTDBK       SYSTEM TERMINATION DUMP BLOCK
                                            ADDRESS
    09DC 2524 Address      4 PFXMCHA        MACHINE CHECK WORK AREA
    09E0 2528 Address      4 PFXMCVBK       THIS CPU'S PERMANENT MCVBK. IF
                                            BLOCK IS NON-0, A DAMAGE INCIDENT
                                            IS IN PROGRESS.
    09E4 2532 Signed       4 PFXINST1       RESERVED FOR INSTALLATION USE
    09E8 2536 Signed       4 PFXINST2       RESERVED FOR INSTALLATION USE
    09EC 2540 Signed       4 PFXINST3       RESERVED FOR INSTALLATION USE
    09F0 2544 Signed       4 PFXINST4       RESERVED FOR INSTALLATION USE
                 COMMONLY USED CONSTANTS
                 WARNING: THIS AREA IS OVERLAID BELOW TO PROVIDE
                 HALFWORD AND BYTE CONSTANTS.  CHANGES TO THIS
                 AREA MUST TAKE THE HALFWORDS AND BYTES INTO
                 CONSIDERATION.
    0A00 2560 Dbl-Word     8 PFXZEROS (8)   64 bytes of binary zeroes
    0A40 2624 Bitstring    8 PFXBLANK
    0A48 2632 Bitstring    8 PFXFFS
              00PFXFFS       PFX0           00004 PFXZEROS,4
    0A50 2640 Signed       4 PFX1
    0A54 2644 Signed       4 PFX2
    0A58 2648 Signed       4 PFX3
    0A5C 2652 Signed       4 PFX4
    0A60 2656 Signed       4 PFX5
    0A64 2660 Signed       4 PFX6
    0A68 2664 Signed       4 PFX7
    0A6C 2668 Signed       4 PFX8
    0A70 2672 Signed       4 PFX9
    0A74 2676 Signed       4 PFX10
    0A78 2680 Signed       4 PFX15          ALSO = X'0000000F'
    0A7C 2684 Signed       4 PFX16
    0A80 2688 Signed       4 PFX17
    0A84 2692 Signed       4 PFX20
    0A88 2696 Signed       4 PFX24
    0A8C 2700 Signed       4 PFX60          ALSO = X'0000003C'
    0A90 2704 Signed       4 PFX240         ALSO = X'000000F0' = C'0'
    0A94 2708 Signed       4 PFX255         ALSO = X'000000FF'
    0A98 2712 Signed       4 PFX256         ALSO = X'00000100'
    0A9C 2716 Signed       4 PFX512         ALSO = X'00000200'
    0AA0 2720 Signed       4 PFX2047        ALSO = X'000007FF'
    0AA4 2724 Signed       4 PFX2048        ALSO = X'00000800'
    0AA8 2728 Signed       4 PFX4095        ALSO = X'00000FFF'
    0AAC 2732 Signed       4 PFX4096        ALSO = X'00001000'
              0PFX4096       PFXPG2AD       PFX4096 PFXPG2AD Address of the
                                            2nd page of the PSA The above is
                                            a temporary proposal for how to
                                            address page 2 of the prefix
                                            area. Directly loading PFX4096
                                            seems wrong.
    0AB0 2736 Bitstring    8 PFX24MSK (0)   24-bit address mask
    0AB0 2736 Bitstring    4 PFX24HSK       . . . 1st half of big mask
    0AB4 2740 Bitstring    4 PFX00FFS       . . . 2nd half (also small mask)
    0AB8 2744 Bitstring    8 PFX2GM1 (0)    2G-1 as unsigned Fixed 64
    0AB8 2744 Bitstring    8 PFX31MSK (0)   31-bit address mask
    0AB8 2744 Bitstring    4 PFX31HSK       . . . 1st half of big mask
    0ABC 2748 Bitstring    4 PFX7FFFS       . . . 2nd half (also small mask)
                                            . . . also x'7FFFFFFF' in 4 bytes
    0AC0 2752 Bitstring    4 PFXHALF        ALSO = F'65535' (64K-1)
    0AC4 2756 Bitstring    4 PFXPGNUM
              PFXPGNUM       PFX7F000       PFXPGNUM PFX7F000 XL4'7FFFF000'
              PFXPGNUM       PFX2GM4K       PFXPGNUM PFX2GM4K XL4'2G-4K'
    0AC8 2760 Bitstring    4 PFXHLFPG
    0ACC 2764 Bitstring    4 PFXSTEMK       MASK TO ISOLATE SEGTABLE ENTRY
    0AD0 2768 Bitstring    8 PFX2G (0)      2G as unsigned Fixed 64
    0AD0 2768 Bitstring    4 PFX2GHI        1st half of 64 bit value
    0AD4 2772 Bitstring    4 PFX8000S       2nd half (also 32 bit value)
    0AD8 2776 Signed       4 *              Reserved for IBM use
    0ADC 2780 Bitstring    4 PFXNOADD
    0AE0 2784 Signed       4 PFX8192        ALSO = X'00002000'
              0PFX8192       PFX8K          PFX8192 PFX8K
    0AE4 2788 Bitstring    4 PFX7FFE0       Mask to isolate 8K-aligned
                                            address
    0AE8 2792 Dbl-Word     8 * (0)
    0AE8 2792 Bitstring    8 PFXRXMSK       Isolate Region Index
    0AF0 2800 Bitstring    8 PFXGPFRA       Isolate Frame address
              PFXGPFRA       PFXGSTOM       PFXGPFRA PFXGSTOM Isolate STO
              PFXGPFRA       PFXGRTOM       PFXGPFRA PFXGRTOM Isolate Region
                                            Origin
    0AF8 2808 Signed       8 * (0)
    0AF8 2808 Character    8 PFXFREYE       Free Storage trail
                                            pseudo-constant (first word may
                                            be overlaid with FSCBK address
                                            for free storage limit detection,
                                            but is later restored)
                 COMMONLY USED HALF WORD CONSTANTS
                 THIS AREA OVERLAYS THE FULL-WORD CONSTANTS
                 WITH OFFSET +2 FROM THE FULL-WORD FORM.
    0A00 2560 Dbl-Word     8 * (8)
    0A40 2624 Bitstring    8 *
    0A48 2632 Bitstring    8 *
    0A50 2640 Signed       2 PFXH0
    0A52 2642 Signed       2 PFXH1
    0A54 2644 Signed       2 *
    0A56 2646 Signed       2 PFXH2
    0A58 2648 Signed       2 *
    0A5A 2650 Signed       2 PFXH3
    0A5C 2652 Signed       2 *
    0A5E 2654 Signed       2 PFXH4
    0A60 2656 Signed       2 *
    0A62 2658 Signed       2 PFXH5
    0A64 2660 Signed       2 *
    0A66 2662 Signed       2 PFXH6
    0A68 2664 Signed       2 *
    0A6A 2666 Signed       2 PFXH7
    0A6C 2668 Signed       2 *
    0A6E 2670 Signed       2 PFXH8
    0A70 2672 Signed       2 *
    0A72 2674 Signed       2 PFXH9
    0A74 2676 Signed       2 *
    0A76 2678 Signed       2 PFXH10
    0A78 2680 Signed       2 *
    0A7A 2682 Signed       2 PFXH15
    0A7C 2684 Signed       2 *
    0A7E 2686 Signed       2 PFXH16
    0A80 2688 Signed       2 *
    0A82 2690 Signed       2 PFXH17
    0A84 2692 Signed       2 *
    0A86 2694 Signed       2 PFXH20
    0A88 2696 Signed       2 *
    0A8A 2698 Signed       2 PFXH24
    0A8C 2700 Signed       2 *
    0A8E 2702 Signed       2 PFXH60
    0A90 2704 Signed       2 *
    0A92 2706 Signed       2 PFXH240
    0A94 2708 Signed       2 *
    0A96 2710 Signed       2 PFXH255
    0A98 2712 Signed       2 *
    0A9A 2714 Signed       2 PFXH256
    0A9C 2716 Signed       2 *
    0A9E 2718 Signed       2 PFXH512
    0AA0 2720 Signed       2 *
    0AA2 2722 Signed       2 PFXH2047
    0AA4 2724 Signed       2 *
    0AA6 2726 Signed       2 PFXH2048
    0AA8 2728 Signed       2 *
    0AAA 2730 Signed       2 PFXH4095
    0AAC 2732 Signed       2 *
    0AAE 2734 Signed       2 PFXH4096
    0AE0 2784 Signed       2 *
    0AE2 2786 Signed       2 PFXH8192
                 COMMONLY USED ONE-BYTE WORD CONSTANTS
                 THIS AREA OVERLAYS THE FULL-WORD CONSTANTS
                 WITH OFFSET +3 FROM THE FULL-WORD FORM.
    0A00 2560 Dbl-Word     8 * (8)
    0A40 2624 Bitstring    8 *
    0A48 2632 Bitstring    8 *
    0A50 2640 Address      1 PFXB0
    0A51 2641 Bitstring    2 *
    0A53 2643 Address      1 PFXB1
    0A54 2644 Bitstring    3 *
    0A57 2647 Address      1 PFXB2
    0A58 2648 Bitstring    3 *
    0A5B 2651 Address      1 PFXB3
    0A5C 2652 Bitstring    3 *
    0A5F 2655 Address      1 PFXB4
    0A60 2656 Bitstring    3 *
    0A63 2659 Address      1 PFXB5
    0A64 2660 Bitstring    3 *
    0A67 2663 Address      1 PFXB6
    0A68 2664 Bitstring    3 *
    0A6B 2667 Address      1 PFXB7
    0A6C 2668 Bitstring    3 *
    0A6F 2671 Address      1 PFXB8
    0A70 2672 Bitstring    3 *
    0A73 2675 Address      1 PFXB9
    0A74 2676 Bitstring    3 *
    0A77 2679 Address      1 PFXB10
    0A78 2680 Bitstring    3 *
    0A7B 2683 Address      1 PFXB15
    0A7C 2684 Bitstring    3 *
    0A7F 2687 Address      1 PFXB16
    0A80 2688 Bitstring    3 *
    0A83 2691 Address      1 PFXB17
    0A84 2692 Bitstring    3 *
    0A87 2695 Address      1 PFXB20
    0A88 2696 Bitstring    3 *
    0A8B 2699 Address      1 PFXB24
    0A8C 2700 Bitstring    3 *
    0A8F 2703 Address      1 PFXB60
    0A90 2704 Bitstring    3 *
    0A93 2707 Address      1 PFXB240 (0)
    0A93 2707 Character    1 PFXCHR0
    0A94 2708 Bitstring    3 *
    0A97 2711 Address      1 PFXB255
    0B00 2816 Bitstring    1 PFXSMPFL       CPUMF Sampler fast path flags
              1... ....      PFXSPART       X'80' PFXSPART LCPU is
                                            participating in sampling
              .1.. ....      PFXSGST        X'40' PFXSGST Sampling during
                                            guest execution indicator
    0B01 2817 Bitstring    1 PFXATTRB       Attributes from ICRBK+ICLBK
    0B02 2818 Bitstring    1 PFXVCNFG       Virtual mode
              1... ....      PFXVVMXA       X'80' PFXVVMXA Running 2nd level
                                            under VM
              .1.. ....      PFXVLPAR       X'40' PFXVLPAR Running in logical
                                            partition
              ..1. ....      PFXVEXFP       X'20' PFXVEXFP Extended Floating
                                            Point installed
              ...1 ....      PFXVVECT       X'10' PFXVVECT Vector Facility
                                            installed. This flag indicates
                                            that host STFLE.129 is on and the
                                            vector register size is 2DW,
                                            which is the only VR size
                                            supported by CP.
              .... .1..      PFXVMVPG       X'04' PFXVMVPG Allow MVPG for all
                                            guests
              .... ..1.      PFXVDG9C       X'02' PFXVDG9C Diagnose x'9C' is
                                            installed
              .... ...1      PFXVNALC       X'01' PFXVNALC
                                            Address-limit-facility not
                                            installed
    0B03 2819 Address      1 PFXPREMT       CPU PREEMPTION FLAG
              000000FF       PFXPRERQ       255 PFXPRERQ CPU PREEMPTION IS
                                            REQUESTED
              00000000       PFXPREMF       000 PFXPREMF CPU PREEMPTION HAS
                                            BEEN SATISFIED
    0B04 2820 Address      4 PFXDSVBK       Address of this CPU's dispatch
                                            vector
    0B08 2824 Dbl-Word     8 PFXCPUID (0)   CPU IDENTIFICATION FIELD
    0B08 2824 Bitstring    1 PFXIDVER       CPU MODEL VERSION CODE
              000000FF       CPUIDVM        X'FF' CPUIDVM VIRTUAL MACHINE
                                            VERSION CODE
    0B09 2825 Bitstring    3 PFXIDSER       CPU SERIAL NUMBER - HEXADECIMAL
    0B0C 2828 Bitstring    2 PFXIDMDL       CPU MODEL NUMBER - HEXADECIMAL
    0B0E 2830 Signed       2 *              RESERVED FOR FUTURE IBM USE.
    0B10 2832 Dbl-Word     8 PFXRNPSW       PSW FOR LAST RUN USER
    0B18 2840 Dbl-Word     8 PFXDSPRI       DISPATCH PRIORITY OF DISPATCHED
                                            VMDBK
    0B20 2848 Signed       4 PFXUDED        VMDBK TO WHICH THIS CPU IS
                                            DEDICATED (ZERO = NOT A DEDICATED
                                            FIELD)
    0B24 2852 Signed       4 PFXIORET       RETURN LINKAGE FOR I/O
    0B28 2856 Signed       8 PFXLPPUV       Doubleword used as the operand of
                                            the LPP instruction by the
                                            dispatcher. The dispatched user's
                                            VMDBK address is in the second
                                            word of this field.
    0B28 2856 Signed       4 *              Zeroes (first half of LPP
                                            operand)
    0B2C 2860 Address      4 PFXRNUSR       LAST RUN USER (2nd half of LPP
                                            operand)
    0B30 2864 Signed       2 PFXZNNUM       HOST ZONE NUMBER
    0B32 2866 Bitstring    1 PFXZNMSK       HOST ZONE MASK
           PFXCPIMG is set very early during system initialization.
           It represents the compiled image of the system.
    0B33 2867 Bitstring    1 PFXCPIMG       Image of CP Executing
              .1.. ....      PFXCPME        X'40' PFXCPME This is the
                                            z/Architecture version
    0B34 2868 Signed       4 PFXAZMWD (0)   Alert Zone Mask word. This
                                            mapping is used for
                                            compare-and-swap operations.
    0B34 2868 Bitstring    1 PFXAZM         Alert Zone Mask. This mask
                                            contains a one for each zone
                                            which must be alerted for by this
                                            processor. Serialized by
                                            compare-and-swap.
    0B35 2869 Bitstring    3 *              Rest of PFXAZMWD
    0B38 2872 Signed       4 PFXFLAGS (0)   STATUS FLAGS
    0B38 2872 Address      1 PFXHSTAT       HOST CP RUNNING STATUS
              1... ....      PFXHWAIT       X'80' PFXHWAIT HOST CP IN WAIT
                                            STATE
              .1.. ....      PFXHRUN        X'40' PFXHRUN DISPATCHED USER HAS
                                            BEEN PUT IN THE SIE, OR EXITED
                                            FROM SIE BUT NOT YET 'UN-RUN'.
                                            THE HOST GPR'S AND FPR'S CONTAIN
                                            GUEST DATA, AND THE CPU TIMER IS
                                            TRACKING EMULATION-MODE TIME.
              ..1. ....      PFXHSYS        X'20' PFXHSYS HOST CP EXECUTING
                                            ON BEHALF OF SYSTEM
              ...1 ....      PFXHUSER       X'10' PFXHUSER HOST CP EXECUTING
                                            ON BEHALF OF USER (PFXHRUN AND/OR
                                            PFXHSYS MAY ALSO BE INDICATED
                                            WITH PFXHUSER)
              .... 1...      PFXHABEN       X'08' PFXHABEN HOST CP ABEND
                                            MACRO HAS BEEN ISSUED
              .... .1..      PFXHSIE        X'04' PFXHSIE SIE IS RUNNING ON
                                            THIS CPU. (FLAG IS SET JUST
                                            BEFORE START, UNSET JUST AFTER
                                            EXIT.)
              .... ..1.      PFXHRUNX       X'02' PFXHRUNX DISPATCHED USER IS
                                            IN THE 'RUN' STATE, WITH THE
                                            POSSIBLE EXCEPTION OF HOST GPR'S,
                                            WHOSE STATE IS INDICATED SOLELY
                                            BY PFXHRUN.
    0B39 2873 Bitstring    1 PFXTNDLK       SYSTEM SPECIAL STATES FLAGS
              1... ....      PFXPWROF       X'80' PFXPWROF SHUTDOWN POWEROFF
                                            was issued, and now the IPL
                                            should be done WARM
                                            automatically, with no OPERATOR
                                            intervention. This is set during
                                            IPL based on info contained in
                                            HCPCKPBK (Checkpoint)
              .1.. ....      PFXHINIT       X'40' PFXHINIT CONTROL PROGRAM IS
                                            INITIALIZING
              ..1. ....      PFXSFIPL       X'20' PFXSFIPL INITIALIZATION IS
                                            DUE TO SOFTWARE IPL This could be
                                            a bounce or a reIPL of the same
                                            nucleus
              ...1 ....      PFXREIPL       X'10' PFXREIPL Initialization is
                                            due to software IPL
              .... 1...      PFXNOCKP       X'08' PFXNOCKP Checkpoint
                                            cylinders were not initialized
              .... .1..      PFXTINIT       X'04' PFXTINIT TIMER HAS BEEN
                                            INITIALIZED
              .... ..1.      PFXTRPON       X'02' PFXTRPON FREE STORAGE TRAP
                                            IN EFFECT
              .... ...1      PFXNULOD       X'01' PFXNULOD We needed a new
                                            copy of HCPLOD when we bounced
                                            (or SHUTDOWN REIPL same nucleus)
    0B3A 2874 Bitstring    1 PFXRCVFG       CPU RECOVERY CONTROL FLAGS
              1... ....      PFXMALFW       X'80' PFXMALFW SPIN LOCK
                                            MALFUNCTION ALERT WINDOW IS IN
                                            PROGRESS
              .1.. ....      PFXHDLAY       X'40' PFXHDLAY PREFIX PAGE IS
                                            AWAITING DE-ALLOCATION
              ..1. ....      PFXRLPST       X'20' PFXRLPST Releasing
                                            additional Prefix page STorage at
                                            VARY OFF time
    0B3B 2875 Bitstring    1 PFXCPUTY       CPU Type of this CPU
    0B3C 2876 Bitstring    3 PFXDSPWK (0)   Dispatcher work controls
    0B3C 2876 Bitstring    1 PFXRCVWK       CPU RECOVERY TYPE WORK CONTROLS
              .1.. ....      PFXMALFP       X'40' PFXMALFP MALFUNCTION ALERT
                                            WORK IS PENDING
              ..1. ....      PFXEMSWK       X'20' PFXEMSWK EMERGENCY SIGNAL
                                            WORK IS PENDING
              ...1 ....      PFXMCHWK       X'10' PFXMCHWK MACHINE CHECK
                                            RECOVERY WORK PENDING
              .... ...1      PFXPRLWK       X'01' PFXPRLWK Work pending to
                                            process the page- fault
                                            "processed list" (NOTE: code in
                                            HCPDSP depends on value X'01' for
                                            this)
    0B3D 2877 Bitstring    1 PFXTSKST       Task state of current task
              1... ....      PFXDWMCO       X'80' PFXDWMCO Dispatched work
                                            can run on Master CPU only.
    0B3E 2878 Bitstring    1 PFXAVLwk       Various Available List controls.
                                            Serialized by processor local
                                            references only.
              .... .1..      PFXCLALtrm     X'04' CLAL trim requested
              .... ..1.      PFXULALtrm     X'02' ULAL trim requested
              .... ...1      PFXCGALtrm     X'01' CGAL trim requested
    0B3F 2879 Bitstring    1 PFXEMODE       Execution mode flags
              1... ....      PFXDATON       X'80' PFXDATON Run with Dynamic
                                            Address Translation
    0B40 2880 Bitstring    1 PFXSVMSK       Field used to temporarily save
                                            the program mask. Located in a
                                            cache line frequently ref'd by
                                            HCPDSP and HCPRUN
    0B41 2881 Bitstring    1 PFXPNDTK       Pending CPU specific tasks,
                                            serialized by compare-and-swap to
                                            allow reach across scheduling of
                                            these tasks
              1... ....      PFXFOBTR       X'80' PFXFOBTR This CPU has been
                                            requested to trim its FOB list
                                            (PFXAFOBL)
              .1.. ....      PFXNDMRL       X'40' PFXNDMRL This CPU has been
                                            requested to reclaim NDMBKs from
                                            it's local recycle queue.
              ..1. ....      PFXMTCTR       X'20' PFXMTCTR This CPU has been
                                            requested to extract MT CPUMF
                                            counters.
    0B42 2882 Bitstring    1 PFXPKFFL       Used to indicate which required
                                            management task needs to be run
                                            for a parked processor. It is
                                            serialized by the Vary Processor
                                            Lock (HCPRCCVA).
              000000FF       PFXPKINI       X'FF' PFXPKINI Initial value when
                                            a CPU is parked
              00000001       PFXTTIAE       X'01' PFXTTIAE Call HCPTTIAE for
                                            a parked CPU
              00000002       PFXUPCR8       X'02' PFXUPCR8 Update CR8 for
                                            Monitor for a parked CPU
              00000003       PFXCCFET       X'03' PFXCCFET Call HCPCCFET for
                                            a parked CPU
              00000004       PFXCCFED       X'04' PFXCCFED Call HCPCCFED for
                                            a parked CPU
              00000005       PFXCCFCC       X'05' PFXCCFCC Call HCPCCFCC for
                                            a parked CPU
              00000006       PFXMTCCE       X'06' PFXMTCCE Call HCPMTCCE for
                                            a parked CPU
              00000007       PFXPROEN       X'07' PFXPROEN Call HCPMTFPR for
                                            a parked CPU to turn PFXPROEX oN.
              00000008       PFXPROEF       X'08' PFXPROEF Call HCPMTFPR for
                                            a parked CPU to turn PFXPROEX
                                            oFf.
              00000009       PFXRFIP3       X'09' PFXRFIP3 Call HCPRFIP3 for
                                            a parked CPU
              0000000A       PFXSMPLE       X'0A' PFXSMPLE Call HCPSMPLE for
                                            a parked CPU
              0000000A       PFXPKMAX       PFXSMPLE PFXPKMAX Maximum value
                                            for PFXPKFFL. PFXPROFL is used
                                            for the prorated core time
                                            calculation. The prorated core
                                            time is only calculated when
                                            Multithreading is enabled. Also
                                            when there is only one activated
                                            thread in a core, the prorated
                                            core time will be same as the raw
                                            time.
    0B43 2883 Bitstring    1 PFXPROFL       Prorated core time calculation
                                            flag
              .... ....      PFXPRONO       X'00' PFXPRONO Prorated core time
                                            is not calculated
              .... ...1      PFXPROUP       X'01' PFXPROUP Update prorated
                                            core time fields. Set when MT is
                                            enabled. When this bit is off,
                                            the remaining bits in this byte
                                            are also off.
              .... ..1.      PFXPROEX       X'02' PFXPROEX Extract MT
                                            counters for prorated core time
                                            calculation. Set when MT is
                                            enabled and the processor runs on
                                            a multi- threaded core. When this
                                            bit is off, both PFXPREER and
                                            PFXPRMVI are also off.
              .... .1..      PFXPREER       X'04' PFXPREER MT counters
                                            extraction error and prorated
                                            core time = raw time. When this
                                            bit is on, both PFXPROUP and
                                            PFXPROEX are also on.
              .... 1...      PFXPRMVI       X'08' PFXPRMVI MT counters
                                            monotonicity violation and
                                            prorated core time = raw time.
                                            When this bit is on, both
                                            PFXPROUP and PFXPROEX are also
                                            on.
              ...1 ....      PFXPRNSE       X'10' PFXPRNSE No starting
                                            counter values extracted.
                                            Prorated core time = raw time.
                                            When this bit is on, both
                                            PFXPROUP and PFXPROEX are also
                                            on. This bit is set when PFXPROEX
                                            is turned on in case it was done
                                            during a dispatch.
    0B44 2884 Signed       2 PFXCPUAD       'STAP' PROCESSOR ADDRESS Note
                                            that we initialize to FF's so
                                            field will be considered
                                            uninitialized when it is GEN'd
                                            into HCPPFX, since we don't know
                                            which processor will IPL
    0B46 2886 Bitstring    1 PFXABFLG       CP status flag
              1... ....      PFXSNPQU       X'80' PFXSNPQU This CPU is
                                            quiesced/quiesce pending on
                                            behalf of SNAPDUMP processing
              .1.. ....      PFXSVCMR       X'40' PFXSVCMR CP is obtaining a
                                            frame for SAVBKs
    0B47 2887 Bitstring    1 PFXHSFLG       SHARED NAMED SYSTEMS FLAG
              1... ....      PFXSHRLK       X'80' PFXSHRLK PROCESSING SHARED
                                            NAMED SYSTEM PAGE
                 CPU TIME RESOURCE CONSUMPTION MEASUREMENTS
    0B48 2888 Bitstring    8 PFXTMMAX       MAXIMUM TIMER VALUE. CONSTANT TO
                                            BE USED FOR INITIALIZING OTHER
                                            FIELDS AND FOR TIMER ARITHMETIC.
    0B50 2896 Bitstring    8 PFXTOTWT       SYSTEM TOTAL WAIT TIME ON THIS
                                            CPU
    0B58 2904 Bitstring    8 PFXPRBTM       TOTAL EMULATION STATE TIME FOR
                                            ALL USERS ON THIS CPU
    0B60 2912 Bitstring    8 PFXTMSYS       SYSTEM TIMER VALUE ON THIS CPU
    0B68 2920 Bitstring    8 PFXUTIME       TOTAL CPU TIME FOR ALL USERS ON
                                            THIS CPU
    0B70 2928 Bitstring    8 PFXACTTS       SYSTEM ACCOUNTING TIME, VALUE OF
                                            PFXTMSYS AT LAST 'ACNT' COMMAND
    0B78 2936 Bitstring    8 PFXSCITS       A copy of PFXTMSYS the last time
                                            it was inspected by the scheduler
                                            running on this CPU. This field
                                            is protected by Scheduler lock
                                            exclusive or a share of Scheduler
                                            lock and SRMATDLK exclusive.
    0B80 2944 Bitstring    8 PFXSPINT       ELAPSED TIME IN SPIN LOCK ON THIS
                                            CPU STARTING AT ZERO AND COUNTING
                                            UPWARDS
                 THIS POINTER IS USED TO LOCATE THE TRACE TABLE
                 PAGES FOR THIS PROCESSOR.
    0B88 2952 Signed       4 PFXTTPNT       TRACE TABLE PAGES FOR THIS CPU
    0B8C 2956 Signed       4 PFXTTPHL       HLA of current Trace Table Page.
                                            Must be set to the HLA for the
                                            trace frame PFXCPCRC points to.
                 MP-CONTROL AND CPU RECOVERY CONTROL FIELDS
    0B90 2960 Signed       4 PFXSPINC       COUNT OF SPINS ON A SPIN LOCK
    0B94 2964 Signed       4 PFXEMSAN       EMERGENCY SIGNAL EMSBK ANCHOR
    0B98 2968 Address      1 PFXDOWNR       TERMINATION REQUEST FIELD
              000000FF       PFXDOWN        255 PFXDOWN REQUEST FOR
                                            TERMINATION
              00000000       PFXDNRZ        000 PFXDNRZ NO REQUEST FOR
                                            TERMINATION
    0B99 2969 Address      1 PFXDOWNC       TERMINATION COMPLETE FIELD
              00000000       PFXDNCZ        000 PFXDNCZ TERMINATION NOT
                                            COMPLETE
              000000FF       PFXDNEMS       255 PFXDNEMS TERM COMPLETE DUE TO
                                            EMS
              000000EE       PFXDNRES       238 PFXDNRES TERM COMPLETE DUE TO
                                            RESET
              000000DD       PFXDNU         221 PFXDNU CPU TERM STATUS
                                            UNKNOWN
              000000CC       PFXDNSW        204 PFXDNSW Term Complete on
                                            Secondary
    0B9A 2970 Address      1 PFXTYPE        HOST CPU USAGE TYPE IDENTIFIER
              00000000       PFXTYOFL       000 PFXTYOFL CPU IS NOT
                                            OPERATIONAL, SEE PFXSTATE FIELD
                                            FOR DETAILS
              00000014       PFXMASTR       020 PFXMASTR THIS IS A
                                            MASTER-TYPE CPU
              0000001E       PFXTYDED       030 PFXTYDED THIS IS A DEDICATED
                                            CPU
              00000028       PFXTYSLV       040 PFXTYSLV THIS IS A SLAVE-TYPE
                                            CPU
              00000032       PFXPARKD       050 PFXPARKD This is a parked CPU
    0B9B 2971 Address      1 PFXDETUP       FLAG USED DURING DETECTION FOR
                                            UNRESPONSIVE PROCESSORS
              00000000       PFXPRESP       000 PFXPRESP PROCESSOR IS
                                            RESPONSIVE
              000000FF       PFXTESTP       255 PFXTESTP TEST PROCESSOR
                                            RESPONSIVE
              000000CC       PFXPRUNR       204 PFXPRUNR PROCESSOR APPEARS
                                            UNRESPONSIVE
              00000011       PFXTMOUT       017 PFXTMOUT PROCESSOR IS
                                            UNRESPONSIVE AND IS TIMED OUT
    0B9C 2972 Address      1 PFXSTATE       CPU OPERATING STATUS
              00000000       PFXAVAIL       000 PFXAVAIL CPU IS ONLINE AND
                                            AVAILABLE (SEE PFXTYPE FOR
                                            ALLOWED USAGE)
              0000000B       PFXRPARK       011 PFXRPARK Attempting to
                                            quiesce this CPU so it can be
                                            parked
              00000016       PFXRQUIS       022 PFXRQUIS ATTEMPTING TO
                                            QUIESCE THIS CPU SO IT CAN BE
                                            TAKEN OFFLINE
              0000002C       PFXVWAIT       044 PFXVWAIT CPU HAS BEEN
                                            QUIESCED AND IS IN DISABLED WAIT
                                            STATE SO IT CAN BE TAKEN OFFLINE
              00000037       PFXCSTOP       055 PFXCSTOP CPU IS CHECK-STOPPED
                                            AND HCPMCHCS HAS DEALT WITH IT.
                                            OR IT WAS RESET AND HCPMCWRS HAS
                                            DEALT WITH IT.
              00000042       PFXLGOFF       066 PFXLGOFF CPU IS NOW LOGICALLY
                                            OFFLINE
              0000006E       PFXNOCPU       110 PFXNOCPU CPU IS PHYSICALLY
                                            OFFLINE
              000000EE       PFXUNKNO       238 PFXUNKNO CPU IS IN AN UNKNOWN
                                            STATE (SIGP COMMUNICATION
                                            FAILURE)
              00000082       PFXNEWCP       130 PFXNEWCP CPU IS BEING BROUGHT
                                            ONLINE
    0B9D 2973 Bitstring    1 PFXTYPS        PFXTYPE SAVEAREA WHILE CPU IS
                                            QUIESCED. Used by SNAPDUMP and
                                            park/unpark processing.
    0B9E 2974 Bitstring    1 PFXCPUFL       CPU flag used for parking,
                                            unparking, and vary-off
                                            processes. Serialized by by the
                                            Vary Processor Lock (HCPRCCVA).
              .... ...1      PFXPRKNG       X'01' PFXPRKNG CPU is in parking
                                            process
              .... ..1.      PFXUNPRK       X'02' PFXUNPRK CPU is in
                                            unparking process
              .... .1..      PFXPRKOF       X'04' PFXPRKOF Varying off a
                                            parked CPU
              .... 1...      PFXCMDOF       X'08' PFXCMDOF Varying off by
                                            command
              ...1 ....      PFXVONFA       X'10' PFXVONFA Varying off a CPU
                                            with initialization failure
              ..1. ....      PFXPRKFA       X'20' PFXPRKFA Varying off a CPU
                                            with parking failure
              .1.. ....      PFXUPKFA       X'40' PFXUPKFA Varying off a CPU
                                            with unparking failure
              1... ....      PFXVOFTD       X'80' PFXVOFTD Varying off due to
                                            thread deactivation.
    0B9F 2975 Bitstring    1 PFXCPUF2       Extension to PFXCPUFL for Vary On
                                            flags.
              1... ....      PFXVONCM       X'80' PFXVONCM Varying on by
                                            command.
              .1.. ....      PFXVONIN       X'40' PFXVONIN Varying on due to
                                            CP initialization.
              ..1. ....      PFXVONTA       X'20' PFXVONTA Varying on due to
                                            thread activation.
    0BA0 2976 Bitstring    1 PFXMPFLG       MP DEFER FLAGS
              1... ....      PFXCPLOC       X'80' PFXCPLOC CP loss of control
                                            checkpoint
              .1.. ....      PFXLOCTL       X'40' PFXLOCTL Loss of control
                                            checkpoint
    0BA1 2977 Bitstring    1 PFXMPCNT       Flag set if this processor has
                                            been counted in SRMNCPUA.
    0BA2 2978 Bitstring    1 PFXPOLAR       Current CPU polarization and
                                            entitlement. Valid only when
                                            PFXTYPE is not PFXTYOFL.
                                            Serialized by the Vary Processor
                                            Lock (HCPRCCVA).
              00000000       PFXPOLHZ       X'00' PFXPOLHZ - Horizontal
              00000001       PFXPOLVL       X'01' PFXPOLVL - Vertical Low
              00000002       PFXPOLVM       X'02' PFXPOLVM - Vertical Medium
              00000003       PFXPOLVH       X'03' PFXPOLVH - Vertical High
    0BA3 2979 Address      1 PFXSYNTY       Synchronization type
              00000000       PFXSYNCL       0 PFXSYNCL None
              000000E5       PFXSYNWT       C'V' PFXSYNWT HCPSYNWT requested
    0BA4 2980 Address      4 PFXDSPBR       Addr of HCPDSP internal branch to
                                            optimize work selection
                                            Serialization: block- concurrent
                                            and processor-local See HCPDSP
                                            block comments for details.
    0BA8 2984 Signed       4 PFXTSKBK       Address of current Task Control
                                            Block
    0BAC 2988 Signed       4 PFXTRQOF       Address of TRQBK used to delay
                                            storage cleanup at VARY OFF VARY
                                            lock serializes PFXTRQOF.
    0BB0 2992 Signed       4 PFXNOLOC       A count of the number of
                                            assertions outstanding that the
                                            task running on this CPU cannot
                                            lose control. Serialized by
                                            processor local references only.
    0BB4 2996 Address      4 PFXNLADR       For debugging: The address of the
                                            last NOLOC or LASTTRANS BEGIN
                                            assertion.
    0BB8 3000 Signed       8 PFXNLR15       Save area for R15 (used by
                                            HCPASERT NOLOC)
                 The following is a copy of the entry in the
                 SCPINFO CPU description list for this processor.
                 This field initialized to zeros if the SCLP
                 interface is not available.
    0BC0 3008 Bitstring   16 PFXCPDES (0)   CPU description entry
    0BC0 3008 Signed       2 *              Reserved
    0BC2 3010 Bitstring   14 PFXCPFAC (0)   CPU Facility bit map
    0BC2 3010 Bitstring    1 PFXCPF0        CPU Facility bit map byte 0
    0BC3 3011 Bitstring    1 PFXCPF1        CPU FACILITY BIT MAP BYTE 1
    0BC4 3012 Bitstring    1 PFXCPF2        CPU Facility bit map byte 2
    0BC5 3013 Bitstring    1 PFXCPF3        CPU Facility bit map byte 3
    0BC6 3014 Bitstring    1 PFXCPF4        CPU Facility bit map byte 4
    0BC7 3015 Bitstring    1 PFXCPF5        CPU Facility bit map byte 5
    0BC8 3016 Bitstring    1 PFXCPF6        CPU Facility bit map byte 6
    0BC9 3017 Bitstring    1 PFXCPF7        CPU Facility bit map byte 7
    0BCA 3018 Bitstring    1 PFXCPF8        CPU Facility bit map byte 8
    0BCB 3019 Bitstring    1 PFXCPF9        CPU Facility bit map byte 9
    0BCC 3020 Bitstring    1 PFXCPF10       CPU Facility bit map byte 10
    0BCD 3021 Bitstring    1 PFXCPF11       CPU Facility bit map byte 11
    0BCE 3022 Bitstring    1 PFXCPF12       CPU Facility bit map byte 12
    0BCF 3023 Bitstring    1 PFXCPF13       CPU Facility bit map byte 13
    0BD0 3024 Signed       2 * (3)          Reserved for IBM use
    0BD6 3030 Signed       2 PFXCPUAO       Logical CPU Address Origin.. this
                                            origin is a bit index
    0BD8 3032 Dbl-Word     8 PFXLCPUA       Logical CPU Address Note that we
                                            initialize this to 00's so it is
                                            uninitialized in HCPPFX when we
                                            GEN it in. This is because we
                                            don't know on CPU we will be
                                            IPLing.
    0BE0 3040 Address      8 * (0)          Ensure dw boundary
    0BE0 3040 Signed       4 PFXPLSBK       PLSBK address for this processor
    0BE4 3044 Address      4 PFXEVTBK       Trace Services local storage
    0BE8 3048 Dbl-Word     8 PFXSAPSW       Soft Abend PSW for Asynch dump
    0BF0 3056 Signed       4 PFXPGIN        Count of fastpath PGINS.
                                            Serialized by Processing list
                                            lock (PLSProLock) due to PLP
                                            reach across case.
    0BF4 3060 Signed       4 PFXCLEAR       Count of fastpath page fault
                                            resolutions not involving PGINs,
                                            i.e. page clears and copies from
                                            a resident alternate-PTE page.
                                            Serialized by Processing list
                                            lock (PLSProLock) due to PLP
                                            reach across case.
    0BF8 3064 Signed       4 PFXCBF         Chargeback factor. Updated only
                                            by the single HCPMTCPL task in
                                            the system and when processor
                                            DSVBK assignments are changed.
    0BFC 3068 Signed       4 *              Reserved for IBM use.
                 THIS SAVEAREA IS REQUIRED BY HCPPRGIN (PROGRAM
                 INTERRUPT FLIH) TO AVOID DESTROYING THE CONTENTS
                 OF PFXIRPSV IN THE CASE OF HCPEXT GETTING A TRACE
                 PROGRAM INTERRUPT WHILE TRYING TO TRACE AN
                 EXTERNAL INTERRUPT.  THE CONTENTS OF THIS SAVEAREA
                 WILL BE PLACED IN PFXIRPSV IF IT IS DETERMINED
                 THAT THE PROGRAM INTERRUPT WAS NOT A TRACE
                 PROGRAM INTERRUPT.
    0C00 3072 Signed       8 PFXPRGSG (5)   Scratch area HCPPRG: 5 full regs
    0C00 3072 Bitstring   40 PFXPRGSV (0)   FLIH save area for HCPPRG
    0C00 3072 Signed       4 PFXPRGRC       REGISTER 12 ON ENTRY TO HCPPRG
    0C04 3076 Signed       4 PFXPRGRD       REGISTER 13 ON ENTRY TO HCPPRG
    0C08 3080 Signed       4 PFXPRGRE       REGISTER 14 ON ENTRY TO HCPPRG
    0C0C 3084 Signed       4 PFXPRGRF       REGISTER 15 ON ENTRY TO HCPPRG
    0C10 3088 Signed       4 PFXPRGR0       REGISTER 0 ON ENTRY TO HCPPRG
    0C14 3092 Signed       4 PFXPRGR1       REGISTER 1 ON ENTRY TO HCPPRG
    0C18 3096 Signed       4 PFXPRGR2       REGISTER 2 ON ENTRY TO HCPPRG
    0C1C 3100 Signed       4 PFXPRGR3       REGISTER 3 ON ENTRY TO HCPPRG
    0C20 3104 Signed       4 PFXPRGR4       REGISTER 4 ON ENTRY TO HCPPRG
    0C24 3108 Signed       4 PFXPRGR5       REGISTER 5 on entry to HCPPRG
                 THE FOLLOWING SAVEAREA IS USED BY THE MODULES
                 WHICH ISSUE THE TRACE INSTRUCTION TO PRESERVE
                 THE CONTENTS OF THE REGISTERS WHICH ARE USED
                 TO CONTAIN DATA FOR THE TRACE EVENT BY THE
                 TRACE INSTRUCTION.
          Notes      :  This area now has a second use, by the TSGET macro
                 as a temporary save area.
    0C28 3112 Bitstring   48 PFXTRCSV (0)   Trace instruction save area
    0C28 3112 Dbl-Word     8 PFXTRCR0       Save R0 across TRACE instruction
    0C30 3120 Dbl-Word     8 PFXTRCR1       Save R1 across TRACE instruction
    0C38 3128 Dbl-Word     8 PFXTRCR2       Save R2 across TRACE instruction
    0C40 3136 Dbl-Word     8 PFXTRCR3       Save R3 across TRACE instruction
    0C48 3144 Dbl-Word     8 PFXTRCR4       Save R4 across TRACE instruction
    0C50 3152 Dbl-Word     8 PFXTRCR5       Save R5 across TRACE instruction
    0C28 3112 Bitstring   48 PFXTSGSV (0)   TSGET save area
    0C28 3112 Dbl-Word     8 PFXTSTOD       Location for TOD clock
    0C30 3120 Dbl-Word     8 PFXTSREG (4)   Location for saved work regs
    0C50 3152 Signed       4 PFXTSAR (2)    Location for saved ARs
                 THE FOLLOWING AREA IS USED BY MODULE HCPSTP TO
                 CALCULATE THE SMOOTHED TOTAL RUN TIME FOR EACH
                 CPU.  THE RESULT IS STORED IN PFXSTRN FOR USE
                 BY THE INDICATE LOAD COMMAND IN CALCULATING THE
                 CPU UTILIZATION PERCENTAGE.
    0C58 3160 Bitstring   40 PFXRNHST (0)   RUN HISTORY AREA FOR HCPSTP
    0C58 3160 Dbl-Word     8 PFXRNH0 (0)
    0C58 3160 Signed       4 PFXRNH00
    0C5C 3164 Signed       4 PFXRNH04
    0C60 3168 Dbl-Word     8 PFXRNH1        .
    0C68 3176 Dbl-Word     8 PFXRNH2 (0)    .
    0C68 3176 Signed       4 PFXRNH20
    0C6C 3180 Signed       4 PFXRNH24
    0C70 3184 Dbl-Word     8 PFXRNH3        .
    0C78 3192 Dbl-Word     8 PFXRNH4        .
    0C80 3200 Dbl-Word     8 PFXFRTC1       Function Related CR12, before
    0C88 3208 Dbl-Word     8 PFXFRTC2       Function Related CR12, after
    0C90 3216 Dbl-Word     8 *              RESERVED FOR IBM USE
    0C98 3224 Dbl-Word     8 *              RESERVED FOR IBM USE
    0CA0 3232 Dbl-Word     8 *              RESERVED FOR IBM USE
    0CA8 3240 Signed       4 *              RESERVED FOR IBM USE
    0CAC 3244 Signed       4 PFXSTRN        SMOOTHED TOTAL RUN TIME (IN
                                            QUARTER SECONDS)
    0CB0 3248 Signed       4 *              RESERVED FOR IBM USE
    0CB4 3252 Signed       4 PFXINDEX       Index into fullword array (i.e.
                                            multiple of 4) based on cpu
                                            address. Note that we initialize
                                            this value to all FF's so when we
                                            gen HCPPFX it can be considered
                                            uninitialized, since we don't
                                            know which CPU we will IPL on.
    0CB8 3256 Signed       4 * (9)          Unused
    0CDC 3292 Address      4 PFXSVRD        Trace Services R13 save
             The following fields are used by wait-state processing.
    0CE0 3296 Signed       4 PFXWTCR6       Copy of host CR6 preserved while
                                            in wait state. This field is only
                                            significant when the PFXWFCR6
                                            flag bit is set.
    0CE4 3300 Bitstring    1 PFXWTFLG       Flags related to wait-state
                                            processing.
              1... ....      PFXWFCR6       X'80' PFXWFCR6 When set, host CR6
                                            is preserved in PFXWTCR6.
    0CE5 3301 Bitstring    1 PFXSSFLG       Read Storage Status
    0CE6 3302 Bitstring    1 * (2)          Reserved for future IBM use
    0CE8 3304 Bitstring   40 PFXWTWRK       Wait-state processing work area
                                            The portion of PFXWTWRK used for
                                            parked processors (PFXPKCR0 and
                                            PFXPKFRC) is serialized by the
                                            Vary Processor Lock (HCPRCCVA).
    0CE8 3304 Signed       4 PFXIOCOD (3)   Results of test pending zone
                                            interruption
    0CF4 3316 Signed       4 *              Reserved for future IBM use
    0CF8 3320 Dbl-Word     8 PFXPKCR0G (0)  CR0 before a CPU is parked
    0CF8 3320 Signed       4 PFXPKCR0H      CR0 high half (reserved)
    0CFC 3324 Signed       4 PFXPKCR0       CR0 before a CPU is parked
    0D00 3328 Signed       4 PFXPKFRC       Return code from a required task
                                            running on a parked CPU
    0D04 3332 Signed       4 * (3)          Reserved for future IBM use
                 Miscellaneous PFXPG fields
    0D10 3344 Signed       4 PFXFSTPX       Count of fast path processing of
                                            partial execution intercepts
    0D14 3348 Address      4 PFXCACPG       Address of intemediate minidisk
                                            cache buffer (filled in by
                                            HCPMDC).
    0D18 3352 Signed       4 PFXABSAD       Savearea address at abend. For
                                            HCPABEND MACRO code use only.
    0D1C 3356 Signed       4 PFXABRSV       Register saveword. For HCPABEND
                                            MACRO code use only.
                 The following fields are used to store CPU parked
                 timer and track park time.
                 PFXPKTOD and PFXPRKWT are fetched and updated
                 concurrently by CDSG, so no new fields should
                 be inserted between them.
    0D20 3360 Dbl-Word     8 PFXPKTOD       A TOD timestamp. Tells when this
                                            CPU was parked. This field will
                                            be zero if the processor is not
                                            parked currently and be updated
                                            with PFXPRKWT by CDSG.
    0D28 3368 Dbl-Word     8 PFXPRKWT       Accumulated wall clock time for
                                            total parked time. This field
                                            will be updated with PFXPKTOD by
                                            CDSG.
              00000B48       PFXPTMER       PFXTMMAX CPU timer for park wait
                                            time. This field is only used to
                                            have some reasonable value in the
                                            CPU timer when a CPU is parked,
                                            and not to actually track time
                                            which will be done with TOD
                                            clock.
    0D30 3376 Dbl-Word     8 *              Reserved for IBM use
          The following field is used by LPAR to locate the TOD
          clock field in a guest's Accounting Information Area (AIA).
          The address of this field must be on a doubleword boundary
          and specified between locations 512 and 4088 of the prefix
          page.  At initialization time, we'll determine if the
          64-bit diagnose x'20C' is supported on the machine.
          PFXAIAPTG is used for a new-style (64-bit) diag x'20C' and
          PFXAIAPT for an old-style (31-bit) diag x'20C'.
    0D38 3384 Dbl-Word     8 PFXAIAPTG      64-bit pointer to guest's AIA.TOD
    0D38 3384 Address      4 *              64-bit pointer AIA.TOD high half
    0D3C 3388 Address      4 PFXAIAPT       31-bit pointer to guest's AIA.TOD
                 The following word is used by HCPWRP FLIHs as a
                 temporary save area.
    0D40 3392 Signed       4 PFXWRPSV       Temporary save area for HCPWRP
    0D44 3396 Signed       4 PFXCCTRQ       TRQBK committed to the local
                                            clock comparator. Serialized by
                                            use of the TRQBK queue lock.
    0D48 3400 Dbl-Word     8 PFXIASIT       Work area, which may be used by a
                                            task with no savearea, in which
                                            an i-ASIT may be temporarily
                                            stored. This field is primarily
                                            for GOTO entry points. Any other
                                            routine that uses this field must
                                            be careful that all callers and
                                            all called routines do not
                                            destroy the data nor do so in the
                                            future. PFXIASIT should only be
                                            used for calling entry points
                                            that expressly state that they
                                            can accept input data in this
                                            field.
                 The following is a copy of the configuration
                 characteristics field of the Read-SCP-Information
                 response.
    0D50 3408 Bitstring   16 PFXCNFG (0)    Configuration Characteristics
    0D50 3408 Bitstring    1 PFXCNFG0       Configuration byte 0
    0D51 3409 Bitstring    1 PFXCNFG1       Configuration byte 1
    0D52 3410 Bitstring    1 PFXCNFG2       Configuration byte 2
    0D53 3411 Bitstring    1 PFXCNFG3       Configuration byte 3
    0D54 3412 Bitstring    1 PFXCNFG4       Configuration byte 4
    0D55 3413 Bitstring    1 PFXCNFG5       Configuration byte 5
    0D56 3414 Bitstring    5 *              Configuration bytes 6 to 10
    0D5B 3419 Bitstring    1 PFXCNFGB       Configuration byte 11
    0D5C 3420 Bitstring    4 *              Configuration bytes 12 to 15
          The following field contains bits describing whether
          certain architectural facilities are installed.  It
          describes facilities which have no direct indication in
          the PFXCPFAC or PFXCNFG fields.  These facilities are
          generally tested for via special code.
    0D60 3424 Dbl-Word     8 PFXAFAC (0)    Architectural facility
                                            indications
    0D60 3424 Bitstring    1 PFXAFAC0       Byte 0 of facility flags
              1... ....      PFXASPO        X'80' PFXASPO Storage-Protection
                                            Override
              .1.. ....      PFXAASP        X'40' PFXAASP Asynchronous Paging
              ..1. ....      PFXASGF        X'20' PFXASGF Subspace-Group
                                            Facility
              ...1 ....      PFXABSA        X'10' PFXABSA Branch and Set
                                            Authority Facility
              .... 1...      PFXACMM        X'08' PFXACMM
              .... .1..      PFXADELY       X'04' PFXADELY Delay Facility
              .... ..1.      PFXAIIA        X'02' PFXAIIA
              .... ...1      PFXBUSY        X'01' PFXBUSY
    0D61 3425 Bitstring    1 PFXAFAC1       Byte 1 of facility flags
              1... ....      PFXSEMA        X'80' PFXSEMA
              .1.. ....      PFXIOEA        X'40' PFXIOEA
    0D62 3426 Bitstring    1 PFXAFAC2       Byte 2 of facility flags
    0D63 3427 Bitstring    1 PFXAFAC3       Byte 3 of facility flags
    0D64 3428 Bitstring    1 PFXAFAC4       Byte 4 of facility flags
    0D65 3429 Bitstring    1 PFXAFAC5       Byte 5 of facility flags
    0D66 3430 Bitstring    1 PFXAFAC6       Byte 6 of facility flags
    0D67 3431 Bitstring    1 PFXSHELD       Shield state for this CPU
              .1.. ....      PFXSHLON       X'40' PFXSHLON Shield activation
                                            selected
                 Following are some scheduler fields.
    0D68 3432 Dbl-Word     8 *              Reserved for IBM use
    0D70 3440 Dbl-Word     8 PFXATODD       A TOD timestamp. When TOD clock
                                            reaches this value, CPU should do
                                            an ATOD-check-in to update
                                            schedul- er's ATOD clock.
                                            (Sometimes equal to SRMATODD, but
                                            sometimes behind.) Updates
                                            serialized by Scheduler lock
                                            exclusive or a share of Scheduler
                                            lock and SRMATDLK exclusive.
    0D78 3448 Bitstring    1 *              Reserved for IBM use
    0DB8 3512 Bitstring   16 PFXMALFM       Mask of malfunction alerts
                                            received but not yet handled.
                                            Bits correspond to logical CPU
                                            identifiers of failing CPU's.
                                            (PFXMALFP bit on if non-zero)
    0DC8 3528 Signed       4 PFXSLCNT       Spin lock counter for C services
    0DCC 3532 Signed       4 PFXCTPRG       Host logical address of trace
                                            pages' 8 bytes control struct:
                                            'AAAAABBB CCCCCCCC', 'AAAAA000'
                                            is start address, 'BBB' is num of
                                            trace pages, 'CCCCCCCC' is cursor
                                            of trace pages.
    0DD0 3536 Signed       4 PFXCVTWK (0)   Register savearea for HCPCVTDB
    0DD0 3536 Signed       4 PFXCVTW1       GPR1
    0DD4 3540 Signed       4 PFXCVTW2       GPR2
    0DD8 3544 Signed       4 PFXCVTW3       GPR3
    0DDC 3548 Signed       4 PFXCVTW4       GPR4
    0DE0 3552 Dbl-Word     8 PFXCVTWX (2)   Work area for HCPCVT and HCPIOS
                 Adcons for dynamic linkage
    0DF0 3568 Address      4 PFXSVCBJ       Pointer to HCPSVCBJ
    0DF4 3572 Address      4 PFXSVCBK       Pointer to HCPSVCBK
    0DF8 3576 Signed       4 * (8)          Reserved for IBM use
    0E18 3608 Dbl-Word     8 PFXOSIAD (0)   OS Info address. C chokes on VD.
    0E18 3608 Signed       4 *              Do it in pieces for GENH.
    0E1C 3612 Address      4 *              OS Info address. The value is
                                            also set in absolute page 0 for
                                            stand-alone dump accessibility.
                                            The field is used to generate an
                                            offset to use to set the field
                                            while reverse prefixing. Set at
                                            initialization and never changes.
    0E20 3616 Signed       4 * (5)          Reserved for IBM use
                 THE FOLLOWING FIELDS ARE USED BY CP TO KEEP HIGH
                 PRIORITY USAGE DATA.
    0E34 3636 Signed       4 PFXPRGCT       Count times purge was requested
                                            at SIE entry (SIEIHCPU=x'FFFF').
    0E38 3640 Signed       4 PFXDSPCS       COUNT OF FULL SELECT PATHS
                                            THROUGH THE DISPATCHER
    0E3C 3644 Signed       4 PFXDSPCT       COUNT OF ENTRIES TO DISPATCHER
    0E40 3648 Signed       4 PFXDSWCT       COUNT OF ENTRIES TO USER WORK
                                            SELECT
    0E44 3652 Signed       4 PFXSTKCR       COUNT OF TIME-SLICE END REORDERS
    0E48 3656 Signed       4 PFXSTKPQ       COUNT OF DISPATCH LIST ADDS
    0E4C 3660 Signed       4 PFXPTRCT       COUNT OF FAST PATH PAGE
                                            TRANSLATIONS
    0E50 3664 Signed       4 PFXCTID        COUNT OF TIMES THE INTERRUPT
                                            QUEUE LOCK REQUEST IS DEFERRED
    0E54 3668 Signed       4 PFXCTIG        COUNT OF TIMES THE INTERRUPT
                                            QUEUE LOCK REQUEST IS GRANTED
    0E58 3672 Signed       4 PFXCTVD        COUNT OF TIMES THE V DEV LOCK
                                            REQUEST IS DEFERRED
    0E5C 3676 Signed       4 PFXCTVG        COUNT OF TIEMS THE VDEV LOCK
                                            REQUEST IS GRANTED
    0E60 3680 Signed       4 PFXRUNCI       COUNT OF SIE INTERCEPTIONS
    0E64 3684 Signed       4 PFXRUNCP       COUNT OF SIE INSTRUCTION
                                            EXECUTIONS
    0E68 3688 Signed       4 PFXRUNCR       COUNT OF TIMES GUEST'S WORK IS
                                            DISPATCHED
    0E6C 3692 Signed       4 PFXRUNPF       COUNT OF HOST PAGE FAULTS FOR
                                            GUEST PAGES
    0E70 3696 Signed       4 PFXCPUCH       Count SIE entries on diff CPU
                                            with SIEIHCPU <> x'FFFF'
    0E74 3700 Signed       4 PFXFSTSG       Count of fast path simulations of
                                            SIGP External Call instructions.
    0E78 3704 Signed       4 PFXFSTXC       Count of fast path reflections of
                                            guest External Call interrupts.
    0E7C 3708 Signed       4 PFXFST44       Count of fast path simulations of
                                            Diagnose x'44' instructions.
               THIS AREA IS RESERVED FOR FE PATCHING. IF NO FE PATCH
               IS PROVIDED, THE BR 14 WILL EFFECT A RETURN. THE AREA
               AT THE END OF THIS REGION MAY BE USED FOR REGISTER
               SAVING. SUBSEQUENT RELEASES OF VM MAY REQUIRE
               A REDUCTION IN THE SIZE OF THE PATCHING AREA.
               NO PERMANENT USE SHOULD BE ASSIGNED TO THIS AREA.
               In a debug build, the PFXPATCH area is not available.
               PFXPATCH is always defined with the "BR R14", but
               after that, its contents vary.
               - in a non-debug build, the remainder of PFXPATCH
                 is available for patches
               - in a debug build, the remainder of PFXPATCH
                 contains debug code and control pointers
    0F00 3840 Signed       2 PFXPINST (64)  Room for FE patched instructions
    0F80 3968 Signed       4 PFXPSAVE (32)  FE Register save area
              00001000       PFXPGLEN       (*-PFXPG) Size of PFXPG in bytes
                 The following macro invocation ensures the length of
                 the PFXPG is exactly 4096 bytes (one 4K page).
                 This area is page two of the z/Arch prefix area.

PFXPG Storage Layout | Top of page

    *** PFXPG - PREFIX PAGE FOR ALL HOST CPU'S
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       PFXMACHN                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 200 |                                                       |
    *     =                       PFXMACCM                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 2C0 |                                                       |
    *     =                       PFXTIMES                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 300 |                                                       |
    *     =                       PFXSAVES                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 900 |                                                       |
    *     =                       PFXADCON                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * A00 |                                                       |
    *     =                       PFXCONST                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * B00 |                                                       |
    *     =                       PFXCNTRL                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * E80 |                                                       |
    *     =                       PFXCPCRS                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * F00 |                                                       |
    *     =                       PFXPATCH                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *1000
    *
    *** PFXPG - PREFIX PAGE FOR ALL HOST CPU'S

    *** Overlay for PFXMACHN in PFXPG
    *
    *     +-------------------------------------------------------+
    *   0 |                       PFXILPSW                        |
    *     +-------------------------------------------------------+
    *   8 |                       PFXICCW1                        |
    *     +-------------------------------------------------------+
    *  10 |                       PFXICCW2                        |
    *     +-------------------------------------------------------+
    *  18 |                       PFXEXTOP                        |
    *     +-------------------------------------------------------+
    *  20 |                       PFXSVCOP                        |
    *     +-------------------------------------------------------+
    *  28 |                       PFXPRGOP                        |
    *     +-------------------------------------------------------+
    *  30 |                       PFXMCHOP                        |
    *     +-------------------------------------------------------+
    *  38 |                       PFXIOOP                         |
    *     +---------------------------+---------------------------+
    *  40 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  48 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  50 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  58 |                       PFXEXTNP                        |
    *     +-------------------------------------------------------+
    *  60 |                       PFXSVCNP                        |
    *     +-------------------------------------------------------+
    *  68 |                       PFXPRGNP                        |
    *     +-------------------------------------------------------+
    *  70 |                       PFXMCHNP                        |
    *     +-------------------------------------------------------+
    *  78 |                       PFXIONP                         |
    *     +---------------------------+-------------+------+------+
    *  80 |         PFXEXTDB          |  PFXEXTCP   |:EXTCL|:EXTCD|
    *     +-------------+------+------+-------------+------+------+
    *  88 |  PFXSVCIL   |//////|:SVCIC|  PFXPRGIL   |:PRGEE|:PRGIC|
    *     +-------------+------+------+-------------+------+------+
    *  90 |////////////////////|:TRXA3| 94
    *     +--------------------+------+
    *
    *** Overlay for PFXMACHN in PFXPG

    *** Overlay for PFXTRXAD in PFXPG
    *
    *     +--------------------+------+
    *  90 |////////////////////|:DXCOD| 94
    *     +--------------------+------+
    *
    *** Overlay for PFXTRXAD in PFXPG

    *** Overlay for PFXTRXAD in PFXPG
    *
    *     +--------------------+------+-------------+-------------+
    *  90 |////////////////////|:VXCOD|  PFXMNCLS   |  PFXPERCD   |
    *     +--------------------+------+-------------+-------------+
    *  98 |         PFXPERAD          |         PFXMNCOD          |
    *     +---------------------------+---------------------------+
    *  A0
    *
    *** Overlay for PFXTRXAD in PFXPG

    *** Overlay for PFXPERAD in PFXPG
    *
    *     +---------------------------+---------------------------+
    *  98 |         PFXGPERL          |         PFXGPERR          |
    *     +------+------+------+------+---------------------------+
    *  A0 |:XCPAR|:PERAR|:OPRID|:ARCHM|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  A8 |                       PFXGTRAD                        |
    *     +---------------------------+---------------------------+
    *  B0 |         PFXGMNCL          |         PFXGMNCR          |
    *     +---------------------------+---------------------------+
    *  B8
    *
    *** Overlay for PFXPERAD in PFXPG

    *** Overlay for PFXGMNCR in PFXPG
    *
    *                                 +-------------+------+------+
    *  B0 ...                      B4 |/////////////|:GMNAC|:GMNAR|
    *                                 +-------------+------+------+
    *  B8
    *
    *** Overlay for PFXGMNCR in PFXPG

    *** Overlay for PFXGTRAD in PFXPG
    *
    *     +---------------------------+---------------------------+
    *  A8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  B0 |///////////////////////////|///////////////////////////|
    *     +-------------+-------------+---------------------------+
    *  B8 |  PFXIOINT   |  PFXIORNM   | BC
    *     +-------------+-------------+
    *
    *** Overlay for PFXGTRAD in PFXPG

    *** Overlay for PFXIOSID in PFXPG
    *
    *     +------+------+------+------+---------------------------+
    *  B8 |:AISM |//////|//////|:ADPFG|         PFXINPRM          |
    *     +------+------+------+------+---------------------------+
    *  C0 |:INISC|//////|:SCHTP|//////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  C8 |:STFL0|:STFL1|:STFL2|:STFL3|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    *  D0 |///////////////////////////|         PFXFPXSA          |
    *     +---------------------------+---------------------------+
    *  D8
    *
    *** Overlay for PFXIOSID in PFXPG

    *** Overlay for PFXFPXSA in PFXPG
    *
    *                                 +---------------------------+
    *  D0 ...                      D4 |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  D8 |                       PFXMCPUT                        |
    *     +-------------------------------------------------------+
    *  E0 |                       PFXMCKCP                        |
    *     +-------------------------------------------------------+
    *  E8 |                       PFXMCHIN                        |
    *     +---------------------------+---------------------------+
    *  F0 |///////////////////////////|         PFXMCHDC          |
    *     +---------------------------+---------------------------+
    *  F8 |         PFXMCFSA          |         PFXMCHRD          |
    *     +---------------------------+---------------------------+
    * 100
    *
    *** Overlay for PFXFPXSA in PFXPG

    *** Overlay for PFXMCFSA in PFXPG
    *
    *     +-------------------------------------------------------+
    *  F8 |                       PFXGMCFS                        |
    *     +-------------------------------------------------------+
    * 100 |                       PFXFXLOG                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 110 |                       PFXBEAR                         |
    *     +-------------------------------------------------------+
    * 118 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 120 |                                                       |
    *     =                       PFXARLG                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 160 |                                                       |
    *     =                       PFXFPRLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 180 |                                                       |
    *     =                       PFXGPRLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1C0 |                                                       |
    *     =                       PFXCRLG                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 200
    *
    *** Overlay for PFXMCFSA in PFXPG

    *** Overlay for PFXARLG in PFXPG
    *
    *     +-------------------------------------------------------+
    * 120 |                       PFXGRSTO                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 130 |                       PFXGEXTO                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 140 |                       PFXGSVCO                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 150 |                       PFXGPRGO                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 160 |                       PFXGMCHO                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 170 |                       PFXGIOO                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 180 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 1A0 |                       PFXGRSTN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1B0 |                       PFXGEXTN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1C0 |                       PFXGSVCN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1D0 |                       PFXGPRGN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1E0 |                       PFXGMCHN                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 1F0 |                       PFXGION                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 200
    *
    *** Overlay for PFXARLG in PFXPG

    *** Overlay for PFXILPSW in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *   0 |:ILPO0|:ILPO1|:ILPO2|:ILPO3|:ILPO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *   8
    *
    *** Overlay for PFXILPSW in PFXPG

    *** Overlay for PFXICCW2 in PFXPG
    *
    *     +------+----------------------------------+-------------+
    *  10 |:SGPND|//////////////////////////////////|  PFXSGPCP   |
    *     +------+----------------------------------+-------------+
    *  18
    *
    *** Overlay for PFXICCW2 in PFXPG

    *** Overlay for PFXEXTOP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  18 |:EXTO0|:EXTO1|:EXTO2|:EXTO3|:EXTO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  20
    *
    *** Overlay for PFXEXTOP in PFXPG

    *** Overlay for PFXSVCOP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  20 |:SVCO0|:SVCO1|:SVCO2|:SVCO3|:SVCO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  28
    *
    *** Overlay for PFXSVCOP in PFXPG

    *** Overlay for PFXPRGOP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  28 |:PRGO0|:PRGO1|:PRGO2|:PRGO3|:PRGO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  30
    *
    *** Overlay for PFXPRGOP in PFXPG

    *** Overlay for PFXMCHOP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  30 |:MCHO0|:MCHO1|:MCHO2|:MCHO3|:MCHO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  38
    *
    *** Overlay for PFXMCHOP in PFXPG

    *** Overlay for PFXIOOP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  38 |:IOPO0|:IOPO1|:IOPO2|:IOPO3|:IOPO4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  40
    *
    *** Overlay for PFXIOOP in PFXPG

    *** Overlay for PFXEXTNP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  58 |:EXTN0|:EXTN1|:EXTN2|:EXTN3|:EXTN4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  60
    *
    *** Overlay for PFXEXTNP in PFXPG

    *** Overlay for PFXSVCNP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  60 |:SVCN0|:SVCN1|:SVCN2|:SVCN3|:SVCN4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  68
    *
    *** Overlay for PFXSVCNP in PFXPG

    *** Overlay for PFXPRGNP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  68 |:PRGN0|:PRGN1|:PRGN2|:PRGN3|:PRGN4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  70
    *
    *** Overlay for PFXPRGNP in PFXPG

    *** Overlay for PFXMCHNP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  70 |:MCHN0|:MCHN1|:MCHN2|:MCHN3|:MCHN4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  78
    *
    *** Overlay for PFXMCHNP in PFXPG

    *** Overlay for PFXIONP in PFXPG
    *
    *     +------+------+------+------+------+--------------------+
    *  78 |:IOPN0|:IOPN1|:IOPN2|:IOPN3|:IOPN4|////////////////////|
    *     +------+------+------+------+------+--------------------+
    *  80
    *
    *** Overlay for PFXIONP in PFXPG

    *** Overlay for PFXMCHIN in PFXPG
    *
    *     +------+------+------+------+------+------+-------------+
    *  E8 |:MCHI0|:MCHI1|:MCHI2|:MCHI3|:MCHI4|:MCHI5|  PFXMCHI6   |
    *     +------+------+------+------+------+------+-------------+
    *  F0
    *
    *** Overlay for PFXMCHIN in PFXPG

    *** Overlay for PFXMCHDC in PFXPG
    *
    *                                 +------+------+------+------+
    *  F0 ...                      F4 |:DCBY0|:DCBY1|:DCBY2|:DCBY3|
    *                                 +------+------+------+------+
    *  F8
    *
    *** Overlay for PFXMCHDC in PFXPG

    *** Overlay for PFXFXLOG in PFXPG
    *
    *     +-------------------------------------------------------+
    * 100 |                       PFXSTPSW                        |
    *     +---------------------------+---------------------------+
    * 108 |         PFXSTPFX          |         PFXSTMDL          |
    *     +---------------------------+---------------------------+
    * 110
    *
    *** Overlay for PFXFXLOG in PFXPG

    *** Overlay for PFXFPRLG in PFXPG
    *
    *     +-------------------------------------------------------+
    * 160 |                       PFXFPRY0                        |
    *     +-------------------------------------------------------+
    * 168 |                       PFXFPRY2                        |
    *     +-------------------------------------------------------+
    * 170 |                       PFXFPRY4                        |
    *     +-------------------------------------------------------+
    * 178 |                       PFXFPRY6                        |
    *     +-------------------------------------------------------+
    * 180
    *
    *** Overlay for PFXFPRLG in PFXPG

    *** Overlay for PFXMACCM in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 200 |        PFXCLPLCNT         |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 208 |                      PFXFWPROCL                       |
    *     +-------------------------------------------------------+
    * 210 |                      PFXCLALPTR                       |
    *     +-------------------------------------------------------+
    * 218 |                       PFXAFOBL                        |
    *     +---------------------------+---------------------------+
    * 220 |         PFXAFOBC          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 228 |                      PFXDPPCAO                        |
    *     +-------------------------------------------------------+
    * 230 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------+-------------+-------------+------+------+
    * 240 |/////////////|/////////////|/////////////|:GPFLG|//////|
    *     +-------------+-------------+-------------+------+------+
    * 248 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 250 |                       PFXFTBLG                        |
    *     +-------------------------------------------------------+
    * 258 |                       PFX2GFTE                        |
    *     +-------------------------------------------------------+
    * 260 |                       PFXFTLEN                        |
    *     +-------------------------------------------------------+
    * 268 |                       PFXSTBLG                        |
    *     +-------------------------------------------------------+
    * 270 |                       PFXSTLEN                        |
    *     +-------------------------------------------------------+
    * 278 |                                                       |
    *     =                       PFXSLTLB                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 290
    *
    *** Overlay for PFXMACCM in PFXPG

    *** Overlay for PFXSLTLB in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 278 |///////////////////////////|         PFXGLSXP          |
    *     +---------------------------+---------------------------+
    * 280 |                       PFXGLPAG                        |
    *     +-------------------------------------------------------+
    * 288
    *
    *** Overlay for PFXSLTLB in PFXPG

    *** Overlay for PFXGLPAG in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 280 |         PFXGLPW0          |         PFXGLPW1          |
    *     +---------------------------+---------------------------+
    * 288 |                       PFXGLPAS                        |
    *     +-------------------------------------------------------+
    * 290
    *
    *** Overlay for PFXGLPAG in PFXPG

    *** Overlay for PFXGLPAS in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 288 |         PFXGLAW0          |         PFXGLAW1          |
    *     +---------------------------+---------------------------+
    * 290 |                       PFXSXASC                        |
    *     +-------------------------------------------------------+
    * 298
    *
    *** Overlay for PFXGLPAS in PFXPG

    *** Overlay for PFXSXASC in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 290 |         PFXXASW0          |         PFXXASW1          |
    *     +---------------------------+---------------------------+
    * 298 |                       PFXNASCE                        |
    *     +-------------------------------------------------------+
    * 2A0
    *
    *** Overlay for PFXSXASC in PFXPG

    *** Overlay for PFXNASCE in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 298 |         PFXNASW0          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 2A0 |///////////////////////////|         PFXRSAL           |
    *     +---------------------------+---------------------------+
    * 2A8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 2C0
    *
    *** Overlay for PFXNASCE in PFXPG

    *** Overlay for PFXSAVES in PFXPG
    *
    *     +-------------------------------------------------------+
    * 300 |                                                       |
    *     =                       PFXTMPSV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 380 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 400 |                                                       |
    *     =                       PFXWRKSV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 480 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 500 |                                                       |
    *     =                       PFXBALSV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 580 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 600 |                                                       |
    *     =                       PFXPTRSV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 680 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 700 |                                                       |
    *     =                       PFXFRESV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 780 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 800 |                       PFXIRPSV                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 810 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 820 |                       PFXLNKSV                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 830 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 840 |                                                       |
    *     =                       PFXSVCSV                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 880 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 8C0 |          PFXSVC           |         PFXLRQND          |
    *     +---------------------------+---------------------------+
    * 8C8 |          PFXLRC           |          PFXLRQ           |
    *     +---------------------------+---------------------------+
    * 8D0 |         PFXCPRQA          |         PFXCPRQP          |
    *     +---------------------------+---------------------------+
    * 8D8 |         PFXSSABK          |         PFX2WAY           |
    *     +---------------------------+---------------------------+
    * 8E0 |          PFXSVU           |          PFXSVF           |
    *     +---------------------------+---------------------------+
    * 8E8 |                       PFXSVR13                        |
    *     +-------------+------+------+---------------------------+
    * 8F0 |/////////////|:IACR |:IACE |///////////////////////////|
    *     +-------------+------+------+---------------------------+
    * 8F8 |                       PFXDBGRX                        |
    *     +-------------------------------------------------------+
    * 900
    *
    *** Overlay for PFXSAVES in PFXPG

    *** Overlay for PFXTMPSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 300 |         PFXTMPFP          |         PFXTMPBP          |
    *     +---------------------------+---------------------------+
    * 308 |///////////////////////////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 310 |:TMPSC|:TMPCL|//////|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * 318 |(318) |(319) |(31A) |(31B) |(31C) |(31D) |(31E) |(31F) |
    *     +------+------+------+------+------+------+------+------+
    * 320 |(320) |(321) |(322) |(323) |         PFXTMPR3          |
    *     +------+------+------+------+---------------------------+
    * 328 |         PFXTMPR4          |         PFXTMPR5          |
    *     +---------------------------+---------------------------+
    * 330 |         PFXTMPR6          |         PFXTMPR7          |
    *     +---------------------------+---------------------------+
    * 338 |         PFXTMPR8          |         PFXTMPR9          |
    *     +---------------------------+---------------------------+
    * 340 |         PFXTMPRA          |         PFXTMPRB          |
    *     +---------------------------+---------------------------+
    * 348 |         PFXTMPRC          |         PFXTMPRD          |
    *     +---------------------------+---------------------------+
    * 350 |         PFXTMPRE          |         PFXTMPRF          |
    *     +---------------------------+---------------------------+
    * 358 |         PFXTMPW0          |         PFXTMPW1          |
    *     +---------------------------+---------------------------+
    * 360 |         PFXTMPW2          |         PFXTMPW3          |
    *     +---------------------------+---------------------------+
    * 368 |         PFXTMPW4          |         PFXTMPW5          |
    *     +---------------------------+---------------------------+
    * 370 |         PFXTMPW6          |         PFXTMPW7          |
    *     +---------------------------+---------------------------+
    * 378 |         PFXTMPW8          |         PFXTMPW9          |
    *     +---------------------------+---------------------------+
    * 380 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 390 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 3A0 |        PFXTMPOPNR         |///////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 3A8 |        PFXTMPAARP         |(3AC) |(3AD) |(3AE) |(3AF) |
    *     +---------------------------+------+------+------+------+
    * 3B0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 3C0 |         PFXTMPH0          |         PFXTMPH1          |
    *     +---------------------------+---------------------------+
    * 3C8 |         PFXTMPH2          |         PFXTMPH3          |
    *     +---------------------------+---------------------------+
    * 3D0 |         PFXTMPH4          |         PFXTMPH5          |
    *     +---------------------------+---------------------------+
    * 3D8 |         PFXTMPH6          |         PFXTMPH7          |
    *     +---------------------------+---------------------------+
    * 3E0 |         PFXTMPH8          |         PFXTMPH9          |
    *     +---------------------------+---------------------------+
    * 3E8 |        PFXTMPH10          |        PFXTMPH11          |
    *     +---------------------------+---------------------------+
    * 3F0 |        PFXTMPH12          |        PFXTMPH13          |
    *     +---------------------------+---------------------------+
    * 3F8 |        PFXTMPH14          |        PFXTMPH15          |
    *     +---------------------------+---------------------------+
    * 400
    *
    *** Overlay for PFXTMPSV in PFXPG

    *** Overlay for PFXTMPAARP in PFXPG
    *
    *     +---------------------------+
    * 3A8 |///////////////////////////| 3AC
    *     +---------------------------+
    *
    *** Overlay for PFXTMPAARP in PFXPG

    *** Overlay for PFXWRKSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 400 |         PFXWRKFP          |         PFXWRKBP          |
    *     +---------------------------+---------------------------+
    * 408 |///////////////////////////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 410 |:WRKSC|:WRKCL|//////|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * 418 |(418) |(419) |(41A) |(41B) |(41C) |(41D) |(41E) |(41F) |
    *     +------+------+------+------+------+------+------+------+
    * 420 |(420) |(421) |(422) |(423) |         PFXWRKR3          |
    *     +------+------+------+------+---------------------------+
    * 428 |         PFXWRKR4          |         PFXWRKR5          |
    *     +---------------------------+---------------------------+
    * 430 |         PFXWRKR6          |         PFXWRKR7          |
    *     +---------------------------+---------------------------+
    * 438 |         PFXWRKR8          |         PFXWRKR9          |
    *     +---------------------------+---------------------------+
    * 440 |         PFXWRKRA          |         PFXWRKRB          |
    *     +---------------------------+---------------------------+
    * 448 |         PFXWRKRC          |         PFXWRKRD          |
    *     +---------------------------+---------------------------+
    * 450 |         PFXWRKRE          |         PFXWRKRF          |
    *     +---------------------------+---------------------------+
    * 458 |         PFXWRKW0          |         PFXWRKW1          |
    *     +---------------------------+---------------------------+
    * 460 |         PFXWRKW2          |         PFXWRKW3          |
    *     +---------------------------+---------------------------+
    * 468 |         PFXWRKW4          |         PFXWRKW5          |
    *     +---------------------------+---------------------------+
    * 470 |         PFXWRKW6          |         PFXWRKW7          |
    *     +---------------------------+---------------------------+
    * 478 |         PFXWRKW8          |         PFXWRKW9          |
    *     +---------------------------+---------------------------+
    * 480 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 490 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 4A0 |        PFXWRKOPNR         |///////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 4A8 |        PFXWRKAARP         |(4AC) |(4AD) |(4AE) |(4AF) |
    *     +---------------------------+------+------+------+------+
    * 4B0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 4C0 |         PFXWRKH0          |         PFXWRKH1          |
    *     +---------------------------+---------------------------+
    * 4C8 |         PFXWRKH2          |         PFXWRKH3          |
    *     +---------------------------+---------------------------+
    * 4D0 |         PFXWRKH4          |         PFXWRKH5          |
    *     +---------------------------+---------------------------+
    * 4D8 |         PFXWRKH6          |         PFXWRKH7          |
    *     +---------------------------+---------------------------+
    * 4E0 |         PFXWRKH8          |         PFXWRKH9          |
    *     +---------------------------+---------------------------+
    * 4E8 |        PFXWRKH10          |        PFXWRKH11          |
    *     +---------------------------+---------------------------+
    * 4F0 |        PFXWRKH12          |        PFXWRKH13          |
    *     +---------------------------+---------------------------+
    * 4F8 |        PFXWRKH14          |        PFXWRKH15          |
    *     +---------------------------+---------------------------+
    * 500
    *
    *** Overlay for PFXWRKSV in PFXPG

    *** Overlay for PFXWRKAARP in PFXPG
    *
    *     +---------------------------+
    * 4A8 |///////////////////////////| 4AC
    *     +---------------------------+
    *
    *** Overlay for PFXWRKAARP in PFXPG

    *** Overlay for PFXBALSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 500 |         PFXBALFP          |         PFXBALBP          |
    *     +---------------------------+---------------------------+
    * 508 |///////////////////////////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 510 |:BALSC|:BALCL|//////|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * 518 |(518) |(519) |(51A) |(51B) |(51C) |(51D) |(51E) |(51F) |
    *     +------+------+------+------+------+------+------+------+
    * 520 |(520) |(521) |(522) |(523) |         PFXBALR3          |
    *     +------+------+------+------+---------------------------+
    * 528 |         PFXBALR4          |         PFXBALR5          |
    *     +---------------------------+---------------------------+
    * 530 |         PFXBALR6          |         PFXBALR7          |
    *     +---------------------------+---------------------------+
    * 538 |         PFXBALR8          |         PFXBALR9          |
    *     +---------------------------+---------------------------+
    * 540 |         PFXBALRA          |         PFXBALRB          |
    *     +---------------------------+---------------------------+
    * 548 |         PFXBALRC          |         PFXBALRD          |
    *     +---------------------------+---------------------------+
    * 550 |         PFXBALRE          |         PFXBALRF          |
    *     +---------------------------+---------------------------+
    * 558 |         PFXBALW0          |         PFXBALW1          |
    *     +---------------------------+---------------------------+
    * 560 |         PFXBALW2          |         PFXBALW3          |
    *     +---------------------------+---------------------------+
    * 568 |         PFXBALW4          |         PFXBALW5          |
    *     +---------------------------+---------------------------+
    * 570 |         PFXBALW6          |         PFXBALW7          |
    *     +---------------------------+---------------------------+
    * 578 |         PFXBALW8          |         PFXBALW9          |
    *     +---------------------------+---------------------------+
    * 580 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 590 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 5A0 |        PFXBALOPNR         |///////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 5A8 |        PFXBALAARP         |(5AC) |(5AD) |(5AE) |(5AF) |
    *     +---------------------------+------+------+------+------+
    * 5B0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 5C0 |         PFXBALH0          |         PFXBALH1          |
    *     +---------------------------+---------------------------+
    * 5C8 |         PFXBALH2          |         PFXBALH3          |
    *     +---------------------------+---------------------------+
    * 5D0 |         PFXBALH4          |         PFXBALH5          |
    *     +---------------------------+---------------------------+
    * 5D8 |         PFXBALH6          |         PFXBALH7          |
    *     +---------------------------+---------------------------+
    * 5E0 |         PFXBALH8          |         PFXBALH9          |
    *     +---------------------------+---------------------------+
    * 5E8 |        PFXBALH10          |        PFXBALH11          |
    *     +---------------------------+---------------------------+
    * 5F0 |        PFXBALH12          |        PFXBALH13          |
    *     +---------------------------+---------------------------+
    * 5F8 |        PFXBALH14          |        PFXBALH15          |
    *     +---------------------------+---------------------------+
    * 600
    *
    *** Overlay for PFXBALSV in PFXPG

    *** Overlay for PFXBALAARP in PFXPG
    *
    *     +---------------------------+
    * 5A8 |///////////////////////////| 5AC
    *     +---------------------------+
    *
    *** Overlay for PFXBALAARP in PFXPG

    *** Overlay for PFXPTRSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 600 |         PFXPTRFP          |         PFXPTRBP          |
    *     +---------------------------+---------------------------+
    * 608 |///////////////////////////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 610 |:PTRSC|:PTRCL|//////|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * 618 |(618) |(619) |(61A) |(61B) |(61C) |(61D) |(61E) |(61F) |
    *     +------+------+------+------+------+------+------+------+
    * 620 |(620) |(621) |(622) |(623) |         PFXPTRR3          |
    *     +------+------+------+------+---------------------------+
    * 628 |         PFXPTRR4          |         PFXPTRR5          |
    *     +---------------------------+---------------------------+
    * 630 |         PFXPTRR6          |         PFXPTRR7          |
    *     +---------------------------+---------------------------+
    * 638 |         PFXPTRR8          |         PFXPTRR9          |
    *     +---------------------------+---------------------------+
    * 640 |         PFXPTRRA          |         PFXPTRRB          |
    *     +---------------------------+---------------------------+
    * 648 |         PFXPTRRC          |         PFXPTRRD          |
    *     +---------------------------+---------------------------+
    * 650 |         PFXPTRRE          |         PFXPTRRF          |
    *     +---------------------------+---------------------------+
    * 658 |         PFXPTRW0          |         PFXPTRW1          |
    *     +---------------------------+---------------------------+
    * 660 |         PFXPTRW2          |         PFXPTRW3          |
    *     +---------------------------+---------------------------+
    * 668 |         PFXPTRW4          |         PFXPTRW5          |
    *     +---------------------------+---------------------------+
    * 670 |         PFXPTRW6          |         PFXPTRW7          |
    *     +---------------------------+---------------------------+
    * 678 |         PFXPTRW8          |         PFXPTRW9          |
    *     +---------------------------+---------------------------+
    * 680 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 690 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 6A0 |        PFXPTROPNR         |///////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 6A8 |        PFXPTRAARP         |(6AC) |(6AD) |(6AE) |(6AF) |
    *     +---------------------------+------+------+------+------+
    * 6B0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 6C0 |         PFXPTRH0          |         PFXPTRH1          |
    *     +---------------------------+---------------------------+
    * 6C8 |         PFXPTRH2          |         PFXPTRH3          |
    *     +---------------------------+---------------------------+
    * 6D0 |         PFXPTRH4          |         PFXPTRH5          |
    *     +---------------------------+---------------------------+
    * 6D8 |         PFXPTRH6          |         PFXPTRH7          |
    *     +---------------------------+---------------------------+
    * 6E0 |         PFXPTRH8          |         PFXPTRH9          |
    *     +---------------------------+---------------------------+
    * 6E8 |        PFXPTRH10          |        PFXPTRH11          |
    *     +---------------------------+---------------------------+
    * 6F0 |        PFXPTRH12          |        PFXPTRH13          |
    *     +---------------------------+---------------------------+
    * 6F8 |        PFXPTRH14          |        PFXPTRH15          |
    *     +---------------------------+---------------------------+
    * 700
    *
    *** Overlay for PFXPTRSV in PFXPG

    *** Overlay for PFXPTRAARP in PFXPG
    *
    *     +---------------------------+
    * 6A8 |///////////////////////////| 6AC
    *     +---------------------------+
    *
    *** Overlay for PFXPTRAARP in PFXPG

    *** Overlay for PFXFRESV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 700 |         PFXFREFP          |         PFXFREBP          |
    *     +---------------------------+---------------------------+
    * 708 |///////////////////////////|///////////////////////////|
    *     +------+------+------+------+---------------------------+
    * 710 |:FRESC|:FRECL|//////|//////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * 718 |(718) |(719) |(71A) |(71B) |(71C) |(71D) |(71E) |(71F) |
    *     +------+------+------+------+------+------+------+------+
    * 720 |(720) |(721) |(722) |(723) |         PFXFRER3          |
    *     +------+------+------+------+---------------------------+
    * 728 |         PFXFRER4          |         PFXFRER5          |
    *     +---------------------------+---------------------------+
    * 730 |         PFXFRER6          |         PFXFRER7          |
    *     +---------------------------+---------------------------+
    * 738 |         PFXFRER8          |         PFXFRER9          |
    *     +---------------------------+---------------------------+
    * 740 |         PFXFRERA          |         PFXFRERB          |
    *     +---------------------------+---------------------------+
    * 748 |         PFXFRERC          |         PFXFRERD          |
    *     +---------------------------+---------------------------+
    * 750 |         PFXFRERE          |         PFXFRERF          |
    *     +---------------------------+---------------------------+
    * 758 |         PFXFREW0          |         PFXFREW1          |
    *     +---------------------------+---------------------------+
    * 760 |         PFXFREW2          |         PFXFREW3          |
    *     +---------------------------+---------------------------+
    * 768 |         PFXFREW4          |         PFXFREW5          |
    *     +---------------------------+---------------------------+
    * 770 |         PFXFREW6          |         PFXFREW7          |
    *     +---------------------------+---------------------------+
    * 778 |         PFXFREW8          |         PFXFREW9          |
    *     +---------------------------+---------------------------+
    * 780 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 790 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 7A0 |        PFXFREOPNR         |///////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 7A8 |        PFXFREAARP         |(7AC) |(7AD) |(7AE) |(7AF) |
    *     +---------------------------+------+------+------+------+
    * 7B0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 7C0 |         PFXFREH0          |         PFXFREH1          |
    *     +---------------------------+---------------------------+
    * 7C8 |         PFXFREH2          |         PFXFREH3          |
    *     +---------------------------+---------------------------+
    * 7D0 |         PFXFREH4          |         PFXFREH5          |
    *     +---------------------------+---------------------------+
    * 7D8 |         PFXFREH6          |         PFXFREH7          |
    *     +---------------------------+---------------------------+
    * 7E0 |         PFXFREH8          |         PFXFREH9          |
    *     +---------------------------+---------------------------+
    * 7E8 |        PFXFREH10          |        PFXFREH11          |
    *     +---------------------------+---------------------------+
    * 7F0 |        PFXFREH12          |        PFXFREH13          |
    *     +---------------------------+---------------------------+
    * 7F8 |        PFXFREH14          |        PFXFREH15          |
    *     +---------------------------+---------------------------+
    * 800
    *
    *** Overlay for PFXFRESV in PFXPG

    *** Overlay for PFXFREAARP in PFXPG
    *
    *     +---------------------------+
    * 7A8 |///////////////////////////| 7AC
    *     +---------------------------+
    *
    *** Overlay for PFXFREAARP in PFXPG

    *** Overlay for PFXIRPSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 800 |         PFXIRP12          |         PFXIRP13          |
    *     +---------------------------+---------------------------+
    * 808 |         PFXIRP14          |         PFXIRP15          |
    *     +---------------------------+---------------------------+
    * 810
    *
    *** Overlay for PFXIRPSV in PFXPG

    *** Overlay for PFXLNKSG in PFXPG
    *
    *     +-------------------------------------------------------+
    * 820 |                       PFXLNKGC                        |
    *     +-------------------------------------------------------+
    * 828 |                       PFXLNKGD                        |
    *     +-------------------------------------------------------+
    * 830 |                       PFXLNKGE                        |
    *     +-------------------------------------------------------+
    * 838 |                       PFXLNKGF                        |
    *     +-------------------------------------------------------+
    * 840
    *
    *** Overlay for PFXLNKSG in PFXPG

    *** Overlay for PFXLNKSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * 820 |         PFXLNK12          |         PFXLNK13          |
    *     +---------------------------+---------------------------+
    * 828 |         PFXLNK14          |         PFXLNK15          |
    *     +---------------------------+---------------------------+
    * 830
    *
    *** Overlay for PFXLNKSV in PFXPG

    *** Overlay for PFXTIMES in PFXPG
    *
    *     +-------------------------------------------------------+
    * 2C0 |                       PFXCVTDA                        |
    *     +-------------------------------------------------------+
    * 2C8 |                       PFXPTLBT                        |
    *     +-------------------------------------------------------+
    * 2D0 |                       PFXTMRUN                        |
    *     +-------------------------------------------------------+
    * 2D8 |                       PFXTMURN                        |
    *     +-------------------------------------------------------+
    * 2E0 |                       PFXTMDSP                        |
    *     +-------------------------------------------------------+
    * 2E8 |                       PFXTMUDS                        |
    *     +-------------------------------------------------------+
    * 2F0 |                       PFXVTDSP                        |
    *     +-------------------------------------------------------+
    * 2F8 |                       PFXPTLBL                        |
    *     +-------------------------------------------------------+
    * 300
    *
    *** Overlay for PFXTIMES in PFXPG

    *** Overlay for PFXCPCRS in PFXPG
    *
    *     +------+------+-------------+------+------+------+------+
    * E80 |//////|(E81) |/////////////|:CR0B0|:CR0B1|:CR0B2|:CR0B3|
    *     +------+------+-------------+------+------+------+------+
    * E88 |        PFXCPCR1H          |:CR1B0|:CR1B1|:CR1B2|:CR1B3|
    *     +---------------------------+------+------+------+------+
    * E90 |        PFXCPCR2H          |:CR2B0|:CR2B1|:CR2B2|:CR2B3|
    *     +---------------------------+------+------+------+------+
    * E98 |        PFXCPCR3H          |:CR3B0|:CR3B1|:CR3B2|:CR3B3|
    *     +---------------------------+------+------+------+------+
    * EA0 |        PFXCPCR4H          |:CR4B0|:CR4B1|:CR4B2|:CR4B3|
    *     +---------------------------+------+------+------+------+
    * EA8 |        PFXCPCR5H          |:CR5B0|:CR5B1|:CR5B2|:CR5B3|
    *     +---------------------------+------+------+------+------+
    * EB0 |        PFXCPCR6H          |:CR6B0|:CR6B1|:CR6B2|:CR6B3|
    *     +---------------------------+------+------+------+------+
    * EB8 |        PFXCPCR7H          |:CR7B0|:CR7B1|:CR7B2|:CR7B3|
    *     +---------------------------+------+------+------+------+
    * EC0 |        PFXCPCR8H          |:CR8B0|:CR8B1|:CR8B2|:CR8B3|
    *     +---------------------------+------+------+------+------+
    * EC8 |        PFXCPCR9H          |:CR9B0|:CR9B1|:CR9B2|:CR9B3|
    *     +---------------------------+------+------+------+------+
    * ED0 |        PFXCPCRAH          |         PFXCPCRA          |
    *     +---------------------------+---------------------------+
    * ED8 |        PFXCPCRBH          |         PFXCPCRB          |
    *     +---------------------------+------+------+------+------+
    * EE0 |        PFXCPCRCH          |:CRCB0|:CRCB1|:CRCB2|:CRCB3|
    *     +---------------------------+------+------+------+------+
    * EE8 |        PFXCPCRDH          |:CRDB0|:CRDB1|:CRDB2|:CRDB3|
    *     +---------------------------+------+------+------+------+
    * EF0 |        PFXCPCREH          |:CREB0|:CREB1|:CREB2|:CREB3|
    *     +---------------------------+------+------+------+------+
    * EF8 |        PFXCPCRFH          |:CRFB0|:CRFB1|:CRFB2|:CRFB3|
    *     +---------------------------+------+------+------+------+
    * F00
    *
    *** Overlay for PFXCPCRS in PFXPG

    *** Overlay for PFXCPCR in PFXPG
    *
    *     +---------------------------+---------------------------+
    * E80 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * E88 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * E90 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * E98 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EA0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EA8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EB0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EB8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EC0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EC8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * ED0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * ED8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EE0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EE8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EF0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * EF8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * F00
    *
    *** Overlay for PFXCPCR in PFXPG

    *** Overlay for PFXADCON in PFXPG
    *
    *     +-------------------------------------------------------+
    * 900 |                       PFXFEIBM                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 910 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////+---------------------------+
    * 930 |///////////////////////////|          PFXSVR           |
    *     +---------------------------+---------------------------+
    * 938 |         PFXCFMRD          |         PFXCVTBH          |
    *     +---------------------------+---------------------------+
    * 940 |         PFXCVTDT          |         PFXCVTOD          |
    *     +---------------------------+---------------------------+
    * 948 |         PFXDSPCH          |         PFXERMES          |
    *     +---------------------------+---------------------------+
    * 950 |         PFXFREE           |         PFXFRET           |
    *     +---------------------------+---------------------------+
    * 958 |         PFXGSVC0          |         PFXGSVC1          |
    *     +---------------------------+---------------------------+
    * 960 |         PFXGSVC2          |         PFXGSVC3          |
    *     +---------------------------+---------------------------+
    * 968 |         PFXTTATB          |         PFXIOSRQ          |
    *     +---------------------------+---------------------------+
    * 970 |         PFXHTRAN          |         PFXLALLK          |
    *     +---------------------------+---------------------------+
    * 978 |         PFXLALLU          |         PFXHTRAB          |
    *     +---------------------------+---------------------------+
    * 980 |         PFXCFRWT          |         PFXRUNXT          |
    *     +---------------------------+---------------------------+
    * 988 |         PFXSTKCP          |         PFXSTKGT          |
    *     +---------------------------+---------------------------+
    * 990 |         PFXSTKIO          |         PFXSCCFD          |
    *     +---------------------------+---------------------------+
    * 998 |          PFXSYS           |         PFXSXLEN          |
    *     +---------------------------+---------------------------+
    * 9A0 |         PFXSYSVM          |         PFXSYSMP          |
    *     +---------------------------+---------------------------+
    * 9A8 |         PFXRUNU           |         PFXENDOP          |
    *     +---------------------------+---------------------------+
    * 9B0 |         PFXSVUSW          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 9B8 |         PFXSVUGS          |         PFXPAGCP          |
    *     +---------------------------+---------------------------+
    * 9C0 |         PFXSVURS          |         PFXLUSER          |
    *     +---------------------------+---------------------------+
    * 9C8 |         PFXPRFIX          |         PFXNXTPF          |
    *     +--------------------+------+---------------------------+
    * 9D0 |     PFXABENM       |:ABENN|         PFXSXAST          |
    *     +--------------------+------+---------------------------+
    * 9D8 |         PFXSTDBK          |         PFXMCHA           |
    *     +---------------------------+---------------------------+
    * 9E0 |         PFXMCVBK          |         PFXINST1          |
    *     +---------------------------+---------------------------+
    * 9E8 |         PFXINST2          |         PFXINST3          |
    *     +---------------------------+---------------------------+
    * 9F0 |         PFXINST4          | 9F4
    *     +---------------------------+
    *
    *** Overlay for PFXADCON in PFXPG

    *** Overlay for PFXCONST in PFXPG
    *
    *     +-------------------------------------------------------+
    * A00 |                                                       |
    *     =                       PFXZEROS                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * A40 |                       PFXBLANK                        |
    *     +-------------------------------------------------------+
    * A48 |                        PFXFFS                         |
    *     +---------------------------+---------------------------+
    * A50 |           PFX1            |           PFX2            |
    *     +---------------------------+---------------------------+
    * A58 |           PFX3            |           PFX4            |
    *     +---------------------------+---------------------------+
    * A60 |           PFX5            |           PFX6            |
    *     +---------------------------+---------------------------+
    * A68 |           PFX7            |           PFX8            |
    *     +---------------------------+---------------------------+
    * A70 |           PFX9            |          PFX10            |
    *     +---------------------------+---------------------------+
    * A78 |          PFX15            |          PFX16            |
    *     +---------------------------+---------------------------+
    * A80 |          PFX17            |          PFX20            |
    *     +---------------------------+---------------------------+
    * A88 |          PFX24            |          PFX60            |
    *     +---------------------------+---------------------------+
    * A90 |          PFX240           |          PFX255           |
    *     +---------------------------+---------------------------+
    * A98 |          PFX256           |          PFX512           |
    *     +---------------------------+---------------------------+
    * AA0 |         PFX2047           |         PFX2048           |
    *     +---------------------------+---------------------------+
    * AA8 |         PFX4095           |         PFX4096           |
    *     +---------------------------+---------------------------+
    * AB0 |         PFX24HSK          |         PFX00FFS          |
    *     +---------------------------+---------------------------+
    * AB8 |         PFX31HSK          |         PFX7FFFS          |
    *     +---------------------------+---------------------------+
    * AC0 |         PFXHALF           |         PFXPGNUM          |
    *     +---------------------------+---------------------------+
    * AC8 |         PFXHLFPG          |         PFXSTEMK          |
    *     +---------------------------+---------------------------+
    * AD0 |         PFX2GHI           |         PFX8000S          |
    *     +---------------------------+---------------------------+
    * AD8 |///////////////////////////|         PFXNOADD          |
    *     +---------------------------+---------------------------+
    * AE0 |         PFX8192           |         PFX7FFE0          |
    *     +---------------------------+---------------------------+
    * AE8 |                       PFXRXMSK                        |
    *     +-------------------------------------------------------+
    * AF0 |                       PFXGPFRA                        |
    *     +-------------------------------------------------------+
    * AF8 |                       PFXFREYE                        |
    *     +-------------------------------------------------------+
    * B00
    *
    *** Overlay for PFXCONST in PFXPG

    *** Overlay for PFXCONST in PFXPG
    *
    *     +-------------------------------------------------------+
    * A00 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * A40 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * A48 |///////////////////////////////////////////////////////|
    *     +-------------+-------------+-------------+-------------+
    * A50 |   PFXH0     |   PFXH1     |/////////////|   PFXH2     |
    *     +-------------+-------------+-------------+-------------+
    * A58 |/////////////|   PFXH3     |/////////////|   PFXH4     |
    *     +-------------+-------------+-------------+-------------+
    * A60 |/////////////|   PFXH5     |/////////////|   PFXH6     |
    *     +-------------+-------------+-------------+-------------+
    * A68 |/////////////|   PFXH7     |/////////////|   PFXH8     |
    *     +-------------+-------------+-------------+-------------+
    * A70 |/////////////|   PFXH9     |/////////////|   PFXH10    |
    *     +-------------+-------------+-------------+-------------+
    * A78 |/////////////|   PFXH15    |/////////////|   PFXH16    |
    *     +-------------+-------------+-------------+-------------+
    * A80 |/////////////|   PFXH17    |/////////////|   PFXH20    |
    *     +-------------+-------------+-------------+-------------+
    * A88 |/////////////|   PFXH24    |/////////////|   PFXH60    |
    *     +-------------+-------------+-------------+-------------+
    * A90 |/////////////|  PFXH240    |/////////////|  PFXH255    |
    *     +-------------+-------------+-------------+-------------+
    * A98 |/////////////|  PFXH256    |/////////////|  PFXH512    |
    *     +-------------+-------------+-------------+-------------+
    * AA0 |/////////////|  PFXH2047   |/////////////|  PFXH2048   |
    *     +-------------+-------------+-------------+-------------+
    * AA8 |/////////////|  PFXH4095   |/////////////|  PFXH4096   |
    *     +-------------+-------------+-------------+-------------+
    * AB0
    *
    *** Overlay for PFXCONST in PFXPG

    *** Overlay for PFX8192 in PFXPG
    *
    *     +-------------+-------------+
    * AE0 |/////////////|  PFXH8192   | AE4
    *     +-------------+-------------+
    *
    *** Overlay for PFX8192 in PFXPG

    *** Overlay for PFXCONST in PFXPG
    *
    *     +-------------------------------------------------------+
    * A00 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * A40 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * A48 |///////////////////////////////////////////////////////|
    *     +------+-------------+------+--------------------+------+
    * A50 |PFXB0 |/////////////|PFXB1 |////////////////////|PFXB2 |
    *     +------+-------------+------+--------------------+------+
    * A58 |////////////////////|PFXB3 |////////////////////|PFXB4 |
    *     +--------------------+------+--------------------+------+
    * A60 |////////////////////|PFXB5 |////////////////////|PFXB6 |
    *     +--------------------+------+--------------------+------+
    * A68 |////////////////////|PFXB7 |////////////////////|PFXB8 |
    *     +--------------------+------+--------------------+------+
    * A70 |////////////////////|PFXB9 |////////////////////|PFXB10|
    *     +--------------------+------+--------------------+------+
    * A78 |////////////////////|PFXB15|////////////////////|PFXB16|
    *     +--------------------+------+--------------------+------+
    * A80 |////////////////////|PFXB17|////////////////////|PFXB20|
    *     +--------------------+------+--------------------+------+
    * A88 |////////////////////|PFXB24|////////////////////|PFXB60|
    *     +--------------------+------+--------------------+------+
    * A90 |////////////////////|:CHR0 |////////////////////|:B255 |
    *     +--------------------+------+--------------------+------+
    * A98
    *
    *** Overlay for PFXCONST in PFXPG

    *** Overlay for PFXCNTRL in PFXPG
    *
    *     +------+------+------+------+---------------------------+
    * B00 |:SMPFL|:ATTRB|:VCNFG|:PREMT|         PFXDSVBK          |
    *     +------+------+------+------+-------------+-------------+
    * B08 |:IDVER|     PFXIDSER       |  PFXIDMDL   |/////////////|
    *     +------+--------------------+-------------+-------------+
    * B10 |                       PFXRNPSW                        |
    *     +-------------------------------------------------------+
    * B18 |                       PFXDSPRI                        |
    *     +---------------------------+---------------------------+
    * B20 |         PFXUDED           |         PFXIORET          |
    *     +---------------------------+---------------------------+
    * B28 |                       PFXLPPUV                        |
    *     +-------------------------------------------------------+
    * B30
    *
    *** Overlay for PFXCNTRL in PFXPG

    *** Overlay for PFXLPPUV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * B28 |///////////////////////////|         PFXRNUSR          |
    *     +-------------+------+------+------+--------------------+
    * B30 |  PFXZNNUM   |:ZNMSK|:CPIMG|PFXAZM|////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * B38 |:HSTAT|:TNDLK|:RCVFG|:CPUTY|:RCVWK|:TSKST|:AVLWK|:EMODE|
    *     +------+------+------+------+------+------+------+------+
    * B40 |:SVMSK|:PNDTK|:PKFFL|:PROFL|  PFXCPUAD   |:ABFLG|:HSFLG|
    *     +------+------+------+------+-------------+------+------+
    * B48 |                       PFXTMMAX                        |
    *     +-------------------------------------------------------+
    * B50 |                       PFXTOTWT                        |
    *     +-------------------------------------------------------+
    * B58 |                       PFXPRBTM                        |
    *     +-------------------------------------------------------+
    * B60 |                       PFXTMSYS                        |
    *     +-------------------------------------------------------+
    * B68 |                       PFXUTIME                        |
    *     +-------------------------------------------------------+
    * B70 |                       PFXACTTS                        |
    *     +-------------------------------------------------------+
    * B78 |                       PFXSCITS                        |
    *     +-------------------------------------------------------+
    * B80 |                       PFXSPINT                        |
    *     +---------------------------+---------------------------+
    * B88 |         PFXTTPNT          |         PFXTTPHL          |
    *     +---------------------------+---------------------------+
    * B90 |         PFXSPINC          |         PFXEMSAN          |
    *     +------+------+------+------+------+------+------+------+
    * B98 |:DOWNR|:DOWNC|:TYPE |:DETUP|:STATE|:TYPS |:CPUFL|:CPUF2|
    *     +------+------+------+------+------+------+------+------+
    * BA0 |:MPFLG|:MPCNT|:POLAR|:SYNTY|         PFXDSPBR          |
    *     +------+------+------+------+---------------------------+
    * BA8 |         PFXTSKBK          |         PFXTRQOF          |
    *     +---------------------------+---------------------------+
    * BB0 |         PFXNOLOC          |         PFXNLADR          |
    *     +---------------------------+---------------------------+
    * BB8 |                       PFXNLR15                        |
    *     +-------------+------+------+------+------+------+------+
    * BC0 |/////////////|:CPF0 |:CPF1 |:CPF2 |:CPF3 |:CPF4 |:CPF5 |
    *     +------+------+------+------+------+------+------+------+
    * BC8 |:CPF6 |:CPF7 |:CPF8 |:CPF9 |:CPF10|:CPF11|:CPF12|:CPF13|
    *     +------+------+------+------+------+------+------+------+
    * BD0 |/////////////////////////////////////////|  PFXCPUAO   |
    *     +-----------------------------------------+-------------+
    * BD8 |                       PFXLCPUA                        |
    *     +---------------------------+---------------------------+
    * BE0 |         PFXPLSBK          |         PFXEVTBK          |
    *     +---------------------------+---------------------------+
    * BE8 |                       PFXSAPSW                        |
    *     +---------------------------+---------------------------+
    * BF0 |         PFXPGIN           |         PFXCLEAR          |
    *     +---------------------------+---------------------------+
    * BF8 |          PFXCBF           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * C00 |                                                       |
    *     =                       PFXPRGSG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * C28
    *
    *** Overlay for PFXLPPUV in PFXPG

    *** Overlay for PFXPRGSG in PFXPG
    *
    *     +---------------------------+---------------------------+
    * C00 |         PFXPRGRC          |         PFXPRGRD          |
    *     +---------------------------+---------------------------+
    * C08 |         PFXPRGRE          |         PFXPRGRF          |
    *     +---------------------------+---------------------------+
    * C10 |         PFXPRGR0          |         PFXPRGR1          |
    *     +---------------------------+---------------------------+
    * C18 |         PFXPRGR2          |         PFXPRGR3          |
    *     +---------------------------+---------------------------+
    * C20 |         PFXPRGR4          |         PFXPRGR5          |
    *     +---------------------------+---------------------------+
    * C28 |                       PFXTRCR0                        |
    *     +-------------------------------------------------------+
    * C30 |                       PFXTRCR1                        |
    *     +-------------------------------------------------------+
    * C38 |                       PFXTRCR2                        |
    *     +-------------------------------------------------------+
    * C40 |                       PFXTRCR3                        |
    *     +-------------------------------------------------------+
    * C48 |                       PFXTRCR4                        |
    *     +-------------------------------------------------------+
    * C50 |                       PFXTRCR5                        |
    *     +-------------------------------------------------------+
    * C58
    *
    *** Overlay for PFXPRGSG in PFXPG

    *** Overlay for PFXTRCSV in PFXPG
    *
    *     +-------------------------------------------------------+
    * C28 |                       PFXTSTOD                        |
    *     +-------------------------------------------------------+
    * C30 |                                                       |
    *     =                       PFXTSREG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * C50 |                       PFXTSAR                         |
    *     +-------------------------------------------------------+
    * C58
    *
    *** Overlay for PFXTRCSV in PFXPG

    *** Overlay for PFXTRCSV+L'PFXTRCSV in PFXPG
    *
    *     +---------------------------+---------------------------+
    * C58 |         PFXRNH00          |         PFXRNH04          |
    *     +---------------------------+---------------------------+
    * C60 |                       PFXRNH1                         |
    *     +---------------------------+---------------------------+
    * C68 |         PFXRNH20          |         PFXRNH24          |
    *     +---------------------------+---------------------------+
    * C70 |                       PFXRNH3                         |
    *     +-------------------------------------------------------+
    * C78 |                       PFXRNH4                         |
    *     +-------------------------------------------------------+
    * C80 |                       PFXFRTC1                        |
    *     +-------------------------------------------------------+
    * C88 |                       PFXFRTC2                        |
    *     +-------------------------------------------------------+
    * C90 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * C98 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * CA0 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * CA8 |///////////////////////////|         PFXSTRN           |
    *     +---------------------------+---------------------------+
    * CB0 |///////////////////////////|         PFXINDEX          |
    *     +---------------------------+---------------------------+
    * CB8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////+---------------------------+
    * CD8 |///////////////////////////|         PFXSVRD           |
    *     +---------------------------+------+------+-------------+
    * CE0 |         PFXWTCR6          |:WTFLG|:SSFLG|/////////////|
    *     +---------------------------+------+------+-------------+
    * CE8 |                                                       |
    *     =                       PFXWTWRK                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * D10
    *
    *** Overlay for PFXTRCSV+L'PFXTRCSV in PFXPG

    *** Overlay for PFXWTWRK in PFXPG
    *
    *     +-------------------------------------------------------+
    * CE8 |                       PFXIOCOD                        |
    *     |                           +---------------------------+
    * CF0 |                           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * CF8 |        PFXPKCR0H          |         PFXPKCR0          |
    *     +---------------------------+---------------------------+
    * D00 |         PFXPKFRC          |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * D10 |         PFXFSTPX          |         PFXCACPG          |
    *     +---------------------------+---------------------------+
    * D18 |         PFXABSAD          |         PFXABRSV          |
    *     +---------------------------+---------------------------+
    * D20 |                       PFXPKTOD                        |
    *     +-------------------------------------------------------+
    * D28 |                       PFXPRKWT                        |
    *     +-------------------------------------------------------+
    * D30 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * D38 |                      PFXAIAPTG                        |
    *     +-------------------------------------------------------+
    * D40
    *
    *** Overlay for PFXWTWRK in PFXPG

    *** Overlay for PFXAIAPTG in PFXPG
    *
    *     +---------------------------+---------------------------+
    * D38 |///////////////////////////|         PFXAIAPT          |
    *     +---------------------------+---------------------------+
    * D40 |         PFXWRPSV          |         PFXCCTRQ          |
    *     +---------------------------+---------------------------+
    * D48 |                       PFXIASIT                        |
    *     +------+------+------+------+------+------+-------------+
    * D50 |:CNFG0|:CNFG1|:CNFG2|:CNFG3|:CNFG4|:CNFG5|/////////////|
    *     +------+------+------+------+------+------+-------------+
    * D58 |////////////////////|:CNFGB|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    * D60 |:AFAC0|:AFAC1|:AFAC2|:AFAC3|:AFAC4|:AFAC5|:AFAC6|:SHELD|
    *     +------+------+------+------+------+------+------+------+
    * D68 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * D70 |                       PFXATODD                        |
    *     +------+------------------------------------------------+
    * D78 |//////|////////////////////////////////////////////////|
    *     +------+////////////////////////////////////////////////|
    * D80 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * DB8 |                       PFXMALFM                        |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * DC8 |         PFXSLCNT          |         PFXCTPRG          |
    *     +---------------------------+---------------------------+
    * DD0 |         PFXCVTW1          |         PFXCVTW2          |
    *     +---------------------------+---------------------------+
    * DD8 |         PFXCVTW3          |         PFXCVTW4          |
    *     +---------------------------+---------------------------+
    * DE0 |                       PFXCVTWX                        |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * DF0 |         PFXSVCBJ          |         PFXSVCBK          |
    *     +---------------------------+---------------------------+
    * DF8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * E18 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * E20 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////+---------------------------+
    * E30 |///////////////////////////|         PFXPRGCT          |
    *     +---------------------------+---------------------------+
    * E38 |         PFXDSPCS          |         PFXDSPCT          |
    *     +---------------------------+---------------------------+
    * E40 |         PFXDSWCT          |         PFXSTKCR          |
    *     +---------------------------+---------------------------+
    * E48 |         PFXSTKPQ          |         PFXPTRCT          |
    *     +---------------------------+---------------------------+
    * E50 |         PFXCTID           |         PFXCTIG           |
    *     +---------------------------+---------------------------+
    * E58 |         PFXCTVD           |         PFXCTVG           |
    *     +---------------------------+---------------------------+
    * E60 |         PFXRUNCI          |         PFXRUNCP          |
    *     +---------------------------+---------------------------+
    * E68 |         PFXRUNCR          |         PFXRUNPF          |
    *     +---------------------------+---------------------------+
    * E70 |         PFXCPUCH          |         PFXFSTSG          |
    *     +---------------------------+---------------------------+
    * E78 |         PFXFSTXC          |         PFXFST44          |
    *     +---------------------------+---------------------------+
    * E80
    *
    *** Overlay for PFXAIAPTG in PFXPG

    *** Overlay for PFXPATCH in PFXPG
    *
    *     +-------------------------------------------------------+
    * F00 |                                                       |
    *     =                       PFXPINST                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * F80 |                                                       |
    *     =                       PFXPSAVE                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *1000
    *
    *** Overlay for PFXPATCH in PFXPG

PFXPG Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    CPUIDVM        0B08 000000FF
    CRCBRCTL       0EE4 80
    CR1SSXA        0E8C 80
    EXTICALL       0087 00000002
    EXTICKC        0087 00000004
    EXTICL00       0086 00000000
    EXTICL10       0086 00000010
    EXTICL12       0086 00000012
    EXTICL14       0086 00000014
    EXTICL20       0086 00000020
    EXTICL24       0086 00000024
    EXTICL26       0086 00000026
    EXTICL40       0086 00000040
    EXTICPU        0087 00000005
    EXTIEMGS       0087 00000001
    EXTIETR        0087 00000006
    EXTIIUCV       0087 00000000
    EXTIKEY        0087 00000040
    EXTILAC        0080 PFXEXTPM
    EXTIMALF       0087 00000000
    EXTIMCAC       0080 80
    EXTIMEAS       0087 00000007
    EXTIMIEA       0080 00
    EXTIMISE       0080 00
    EXTIMLCD       0080 40
    EXTIMLMT       0080 PFXEXTPM
    EXTIMLSD       0080 PFXEXTPM
    EXTIMPRA       0080 00
    EXTIMSAC       0080 PFXEXTPM
    EXTIPVM        0087 00000002
    EXTISVSG       0087 00000001
    EXTITMR        0087 00000080
    EXTITPC        0080 PFXEXTPM
    EXTITSC        0080 PFXEXTPM
    EXTITZCH       0087 00000004
    EXTIVMCF       0087 00000001
    EXTIXC         0087 00000003
    MCEXTDCC       00F7 20
    MCEXTDCS       00F7 10
    MCEXTDIC       00F7 40
    MCEXTDSC       00F6 10
    MCEXTDSS       00F7 80
    MCEXTD0        00F4 00
    MCEXTD1        00F5 00
    MCICAR         00ED 08
    MCICBU         00E9 02
    MCICCD         00E8 08
    MCICCRW        00E9 40
    MCICCSD        00E9 10
    MCICDA         00EC 20
    MCICDG         00E8 01
    MCICDL         00E9 01
    MCICED         00E8 04
    MCICIE         00EC 80
    MCICITD        00E8 10
    MCICKE         00EA 20
    MCICPD         00E8 40
    MCICSC         00EA 40
    MCICSD         00E8 80
    MCICSDG        00EA 10
    MCICSE         00EA 80
    MCICSP         00E9 20
    MCICSR         00E8 20
    MCICVAR        00EC 40
    MCICVCC        00ED 01
    MCICVCR        00EB 04
    MCICVCT        00ED 02
    MCICVED        00EB 20
    MCICVFA        00EB 80
    MCICVFP        00EB 10
    MCICVGR        00EB 08
    MCICVGS        00EC 08
    MCICVIA        00EA 01
    MCICVMS        00EA 04
    MCICVPM        00EA 02
    MCICVST        00EB 01
    MCICVTPR       00ED 20
    MCICVVR        00EB 40
    MCICVWP        00EA 08
    MCICVXFP       00ED 10
    MCICW          00E9 80
    MCIC30         00EB 02
    MCIPRIM0       00E8 FF
    MCIPRIM1       00E9 F0
    PFXfwPROCL     0208
    PFXAASP        0D60 40
    PFXABEND       09D0
    PFXABENM       09D0
    PFXABENN       09D3
    PFXABFLG       0B46
    PFXABRSV       0D1C
    PFXABSA        0D60 10
    PFXABSAD       0D18
    PFXACMM        0D60 08
    PFXACTTS       0B70
    PFXADCON       0900
    PFXADELY       0D60 04
    PFXADPFG       00BB
    PFXAFAC        0D60
    PFXAFAC0       0D60
    PFXAFAC1       0D61
    PFXAFAC2       0D62
    PFXAFAC3       0D63
    PFXAFAC4       0D64
    PFXAFAC5       0D65
    PFXAFAC6       0D66
    PFXAFOBC       0220
    PFXAFOBL       0218
    PFXAIAPT       0D3C
    PFXAIAPTG      0D38
    PFXAIIA        0D60 02
    PFXAINME       00A3 01
    PFXAISM        00B8
    PFXARCHM       00A3
    PFXARLG        0120
    PFXASGF        0D60 20
    PFXASPO        0D60 80
    PFXATODD       0D70
    PFXATTRB       0B01
    PFXAVAIL       0B9C 00000000
    PFXAVLwk       0B3E
    PFXAZM         0B34
    PFXAZMWD       0B34
    PFXBALAARP     05A8
    PFXBALAMDE     05AD
    PFXBALAREA     0518
    PFXBALBP       0504
    PFXBALCL       0511
    PFXBALFP       0500
    PFXBALHIRG     05C0
    PFXBALH0       05C0
    PFXBALH1       05C4
    PFXBALH10      05E8
    PFXBALH11      05EC
    PFXBALH12      05F0
    PFXBALH13      05F4
    PFXBALH14      05F8
    PFXBALH15      05FC
    PFXBALH2       05C8
    PFXBALH3       05CC
    PFXBALH4       05D0
    PFXBALH5       05D4
    PFXBALH6       05D8
    PFXBALH7       05DC
    PFXBALH8       05E0
    PFXBALH9       05E4
    PFXBALIACA     05AC
    PFXBALIACE     05AF
    PFXBALIACR     05AE
    PFXBALOPNR     05A0
    PFXBALRA       0540
    PFXBALRB       0544
    PFXBALRC       0548
    PFXBALRCF      0548
    PFXBALRD       054C
    PFXBALRE       0550
    PFXBALRF       0554
    PFXBALRG       0518
    PFXBALR0       0518
    PFXBALR0B0     0518
    PFXBALR0B1     0519
    PFXBALR0B2     051A
    PFXBALR0B3     051B
    PFXBALR1       051C
    PFXBALR1B0     051C
    PFXBALR1B1     051D
    PFXBALR1B2     051E
    PFXBALR1B3     051F
    PFXBALR2       0520
    PFXBALR2B0     0520
    PFXBALR2B1     0521
    PFXBALR2B2     0522
    PFXBALR2B3     0523
    PFXBALR3       0524
    PFXBALR4       0528
    PFXBALR5       052C
    PFXBALR6       0530
    PFXBALR7       0534
    PFXBALR8       0538
    PFXBALR9       053C
    PFXBALSC       0510
    PFXBALSG       0500
    PFXBALSV       0500
    PFXBALW$       0580
    PFXBALWK       0558
    PFXBALW0       0558
    PFXBALW1       055C
    PFXBALW2       0560
    PFXBALW3       0564
    PFXBALW4       0568
    PFXBALW5       056C
    PFXBALW6       0570
    PFXBALW7       0574
    PFXBALW8       0578
    PFXBALW9       057C
    PFXBEAR        0110
    PFXBLANK       0A40
    PFXBUSY        0D60 01
    PFXB0          0A50
    PFXB1          0A53
    PFXB10         0A77
    PFXB15         0A7B
    PFXB16         0A7F
    PFXB17         0A83
    PFXB2          0A57
    PFXB20         0A87
    PFXB24         0A8B
    PFXB240        0A93
    PFXB255        0A97
    PFXB3          0A5B
    PFXB4          0A5F
    PFXB5          0A63
    PFXB6          0A67
    PFXB60         0A8F
    PFXB7          0A6B
    PFXB8          0A6F
    PFXB9          0A73
    PFXCACPG       0D14
    PFXCBF         0BF8
    PFXCCFCC       0B42 00000005
    PFXCCFED       0B42 00000004
    PFXCCFET       0B42 00000003
    PFXCCTRQ       0D44
    PFXCC2B1       0011
    PFXCFMRD       0938
    PFXCFRWT       0980
    PFXCGALtrm     0B3E 01
    PFXCHR0        0A93
    PFXCLALtrm     0B3E 04
    PFXCLALPtr     0210
    PFXCLEAR       0BF4
    PFXCLPLCnt     0200
    PFXCMDOF       0B9E 08
    PFXCNFG        0D50
    PFXCNFGB       0D5B
    PFXCNFG0       0D50
    PFXCNFG1       0D51
    PFXCNFG2       0D52
    PFXCNFG3       0D53
    PFXCNFG4       0D54
    PFXCNFG5       0D55
    PFXCNTRL       0B00
    PFXCONST       0A00
    PFXCPCR        0E80
    PFXCPCRA       0ED4
    PFXCPCRAG      0ED0
    PFXCPCRAH      0ED0
    PFXCPCRB       0EDC
    PFXCPCRBG      0ED8
    PFXCPCRBH      0ED8
    PFXCPCRC       0EE4
    PFXCPCRCG      0EE0
    PFXCPCRCH      0EE0
    PFXCPCRD       0EEC
    PFXCPCRDG      0EE8
    PFXCPCRDH      0EE8
    PFXCPCRE       0EF4
    PFXCPCREG      0EF0
    PFXCPCREH      0EF0
    PFXCPCRF       0EFC
    PFXCPCRFG      0EF8
    PFXCPCRFH      0EF8
    PFXCPCRS       0E80
    PFXCPCR0       0E84
    PFXCPCR0G      0E80
    PFXCPCR0H      0E80
    PFXCPCR1       0E8C
    PFXCPCR1G      0E88
    PFXCPCR1H      0E88
    PFXCPCR2       0E94
    PFXCPCR2G      0E90
    PFXCPCR2H      0E90
    PFXCPCR3       0E9C
    PFXCPCR3G      0E98
    PFXCPCR3H      0E98
    PFXCPCR4       0EA4
    PFXCPCR4G      0EA0
    PFXCPCR4H      0EA0
    PFXCPCR5       0EAC
    PFXCPCR5G      0EA8
    PFXCPCR5H      0EA8
    PFXCPCR6       0EB4
    PFXCPCR6G      0EB0
    PFXCPCR6H      0EB0
    PFXCPCR7       0EBC
    PFXCPCR7G      0EB8
    PFXCPCR7H      0EB8
    PFXCPCR8       0EC4
    PFXCPCR8G      0EC0
    PFXCPCR8H      0EC0
    PFXCPCR9       0ECC
    PFXCPCR9G      0EC8
    PFXCPCR9H      0EC8
    PFXCPDES       0BC0
    PFXCPFAC       0BC2
    PFXCPF0        0BC2
    PFXCPF1        0BC3
    PFXCPF10       0BCC
    PFXCPF11       0BCD
    PFXCPF12       0BCE
    PFXCPF13       0BCF
    PFXCPF2        0BC4
    PFXCPF3        0BC5
    PFXCPF4        0BC6
    PFXCPF5        0BC7
    PFXCPF6        0BC8
    PFXCPF7        0BC9
    PFXCPF8        0BCA
    PFXCPF9        0BCB
    PFXCPIMG       0B33
    PFXCPIOI       0EB4 80
    PFXCPLOC       0BA0 80
    PFXCPME        0B33 40
    PFXCPRQA       08D0
    PFXCPRQP       08D4
    PFXCPUAD       0B44
    PFXCPUAO       0BD6
    PFXCPUCH       0E70
    PFXCPUFL       0B9E
    PFXCPUF2       0B9F
    PFXCPUID       0B08
    PFXCPULG       0080
    PFXCPUTY       0B3B
    PFXCRCB0       0EE4
    PFXCRCB1       0EE5
    PFXCRCB2       0EE6
    PFXCRCB3       0EE7
    PFXCRDB0       0EEC
    PFXCRDB1       0EED
    PFXCRDB2       0EEE
    PFXCRDB3       0EEF
    PFXCREB0       0EF4
    PFXCREB1       0EF5
    PFXCREB2       0EF6
    PFXCREB3       0EF7
    PFXCRFB0       0EFC
    PFXCRFB1       0EFD
    PFXCRFB2       0EFE
    PFXCRFB3       0EFF
    PFXCRLG        01C0
    PFXCRLGL       01C0 00000040
    PFXCR0B0       0E84
    PFXCR0B1       0E85
    PFXCR0B2       0E86
    PFXCR0B3       0E87
    PFXCR0HB1      0E81
    PFXCR1B0       0E8C
    PFXCR1B1       0E8D
    PFXCR1B2       0E8E
    PFXCR1B3       0E8F
    PFXCR2B0       0E94
    PFXCR2B1       0E95
    PFXCR2B2       0E96
    PFXCR2B3       0E97
    PFXCR3B0       0E9C
    PFXCR3B1       0E9D
    PFXCR3B2       0E9E
    PFXCR3B3       0E9F
    PFXCR4B0       0EA4
    PFXCR4B1       0EA5
    PFXCR4B2       0EA6
    PFXCR4B3       0EA7
    PFXCR5B0       0EAC
    PFXCR5B1       0EAD
    PFXCR5B2       0EAE
    PFXCR5B3       0EAF
    PFXCR6B0       0EB4
    PFXCR6B1       0EB5
    PFXCR6B2       0EB6
    PFXCR6B3       0EB7
    PFXCR7B0       0EBC
    PFXCR7B1       0EBD
    PFXCR7B2       0EBE
    PFXCR7B3       0EBF
    PFXCR8B0       0EC4
    PFXCR8B1       0EC5
    PFXCR8B2       0EC6
    PFXCR8B3       0EC7
    PFXCR9B0       0ECC
    PFXCR9B1       0ECD
    PFXCR9B2       0ECE
    PFXCR9B3       0ECF
    PFXCSTOP       0B9C 00000037
    PFXCTID        0E50
    PFXCTIG        0E54
    PFXCTPRG       0DCC
    PFXCTVD        0E58
    PFXCTVG        0E5C
    PFXCVTBH       093C
    PFXCVTDA       02C0
    PFXCVTDT       0940
    PFXCVTOD       0944
    PFXCVTWK       0DD0
    PFXCVTWX       0DE0
    PFXCVTW1       0DD0
    PFXCVTW2       0DD4
    PFXCVTW3       0DD8
    PFXCVTW4       0DDC
    PFXDATON       0B3F 80
    PFXDBGRX       08F8
    PFXDCBY0       00F4
    PFXDCBY1       00F5
    PFXDCBY2       00F6
    PFXDCBY3       00F7
    PFXDETUP       0B9B
    PFXDNCZ        0B99 00000000
    PFXDNEMS       0B99 000000FF
    PFXDNRES       0B99 000000EE
    PFXDNRZ        0B98 00000000
    PFXDNSW        0B99 000000CC
    PFXDNU         0B99 000000DD
    PFXDOWN        0B98 000000FF
    PFXDOWNC       0B99
    PFXDOWNR       0B98
    PFXDPPCAO      0228
    PFXDRFPT       0EB4 1D
    PFXDSPBR       0BA4
    PFXDSPCH       0948
    PFXDSPCS       0E38
    PFXDSPCT       0E3C
    PFXDSPRI       0B18
    PFXDSPWK       0B3C
    PFXDSVBK       0B04
    PFXDSWCT       0E40
    PFXDWMCO       0B3D 80
    PFXDXCOD       0093
    PFXEBIT        00BB 02
    PFXEMODE       0B3F
    PFXEMSAN       0B94
    PFXEMSWK       0B3C 20
    PFXENDOP       09AC
    PFXERMES       094C
    PFXEVTBK       0BE4
    PFXEXTCD       0087
    PFXEXTCF       0084
    PFXEXTCL       0086
    PFXEXTCP       0084
    PFXEXTDB       0080
    PFXEXTIN       0086
    PFXEXTNI       005C
    PFXEXTNP       0058
    PFXEXTN0       0058
    PFXEXTN1       0059
    PFXEXTN2       005A
    PFXEXTN3       005B
    PFXEXTN4       005C
    PFXEXTOI       001C
    PFXEXTOP       0018
    PFXEXTO0       0018
    PFXEXTO1       0019
    PFXEXTO2       001A
    PFXEXTO3       001B
    PFXEXTO4       001C
    PFXEXTPM       0080
    PFXFEIBM       0900
    PFXFFS         0A48
    PFXFLAGS       0B38
    PFXFOBTR       0B41 80
    PFXFPARM       0090
    PFXFPRLG       0160
    PFXFPRY0       0160
    PFXFPRY2       0168
    PFXFPRY4       0170
    PFXFPRY6       0178
    PFXFPXSA       00D4
    PFXFREAARP     07A8
    PFXFREAMDE     07AD
    PFXFREAREA     0718
    PFXFREBP       0704
    PFXFRECL       0711
    PFXFREE        0950
    PFXFREFP       0700
    PFXFREHIRG     07C0
    PFXFREH0       07C0
    PFXFREH1       07C4
    PFXFREH10      07E8
    PFXFREH11      07EC
    PFXFREH12      07F0
    PFXFREH13      07F4
    PFXFREH14      07F8
    PFXFREH15      07FC
    PFXFREH2       07C8
    PFXFREH3       07CC
    PFXFREH4       07D0
    PFXFREH5       07D4
    PFXFREH6       07D8
    PFXFREH7       07DC
    PFXFREH8       07E0
    PFXFREH9       07E4
    PFXFREIACA     07AC
    PFXFREIACE     07AF
    PFXFREIACR     07AE
    PFXFREOPNR     07A0
    PFXFRERA       0740
    PFXFRERB       0744
    PFXFRERC       0748
    PFXFRERCF      0748
    PFXFRERD       074C
    PFXFRERE       0750
    PFXFRERF       0754
    PFXFRERG       0718
    PFXFRER0       0718
    PFXFRER0B0     0718
    PFXFRER0B1     0719
    PFXFRER0B2     071A
    PFXFRER0B3     071B
    PFXFRER1       071C
    PFXFRER1B0     071C
    PFXFRER1B1     071D
    PFXFRER1B2     071E
    PFXFRER1B3     071F
    PFXFRER2       0720
    PFXFRER2B0     0720
    PFXFRER2B1     0721
    PFXFRER2B2     0722
    PFXFRER2B3     0723
    PFXFRER3       0724
    PFXFRER4       0728
    PFXFRER5       072C
    PFXFRER6       0730
    PFXFRER7       0734
    PFXFRER8       0738
    PFXFRER9       073C
    PFXFRESC       0710
    PFXFRESG       0700
    PFXFRESV       0700
    PFXFRET        0954
    PFXFREW$       0780
    PFXFREWK       0758
    PFXFREW0       0758
    PFXFREW1       075C
    PFXFREW2       0760
    PFXFREW3       0764
    PFXFREW4       0768
    PFXFREW5       076C
    PFXFREW6       0770
    PFXFREW7       0774
    PFXFREW8       0778
    PFXFREW9       077C
    PFXFREYE       0AF8
    PFXFRTC1       0C80
    PFXFRTC2       0C88
    PFXFSTPX       0D10
    PFXFSTSG       0E74
    PFXFSTXC       0E78
    PFXFST44       0E7C
    PFXFTBLG       0250
    PFXFTLEN       0260
    PFXFXLEN       0100 10
    PFXFXLOG       0100
    PFXGEXTN       01B0
    PFXGEXTO       0130
    PFXGION        01F0
    PFXGIOO        0170
    PFXGLAW0       0288
    PFXGLAW1       028C
    PFXGLPAG       0280
    PFXGLPAS       0288
    PFXGLPW0       0280
    PFXGLPW1       0284
    PFXGLSXP       027C
    PFXGMCFS       00F8
    PFXGMCHN       01E0
    PFXGMCHO       0160
    PFXGMNAC       00B6
    PFXGMNAR       00B7
    PFXGMNCD       00B0
    PFXGMNCL       00B0
    PFXGMNCR       00B4
    PFXGPERA       0098
    PFXGPERL       0098
    PFXGPERR       009C
    PFXGPFLG       0246
    PFXGPFRA       0AF0
    PFXGPRGN       01D0
    PFXGPRGO       0150
    PFXGPRLG       0180
    PFXGRSTN       01A0
    PFXGRSTO       0120
    PFXGRTOM       0AF0 PFXGPFRA
    PFXGSTOM       0AF0 PFXGPFRA
    PFXGSVCN       01C0
    PFXGSVCO       0140
    PFXGSVC0       0958
    PFXGSVC1       095C
    PFXGSVC2       0960
    PFXGSVC3       0964
    PFXGTRAD       00A8
    PFXHABEN       0B38 08
    PFXHALF        0AC0
    PFXHBIT        00BB 01
    PFXHDLAY       0B3A 40
    PFXHINIT       0B39 40
    PFXHLFPG       0AC8
    PFXHRUN        0B38 40
    PFXHRUNX       0B38 02
    PFXHSFLG       0B47
    PFXHSIE        0B38 04
    PFXHSTAT       0B38
    PFXHSYS        0B38 20
    PFXHTRAB       097C
    PFXHTRAN       0970
    PFXHUSER       0B38 10
    PFXHWAIT       0B38 80
    PFXH0          0A50
    PFXH1          0A52
    PFXH10         0A76
    PFXH15         0A7A
    PFXH16         0A7E
    PFXH17         0A82
    PFXH2          0A56
    PFXH20         0A86
    PFXH2047       0AA2
    PFXH2048       0AA6
    PFXH24         0A8A
    PFXH240        0A92
    PFXH255        0A96
    PFXH256        0A9A
    PFXH3          0A5A
    PFXH4          0A5E
    PFXH4095       0AAA
    PFXH4096       0AAE
    PFXH5          0A62
    PFXH512        0A9E
    PFXH6          0A66
    PFXH60         0A8E
    PFXH7          0A6A
    PFXH8          0A6E
    PFXH8192       0AE2
    PFXH9          0A72
    PFXIACE        08F3
    PFXIACR        08F2
    PFXIASIT       0D48
    PFXICCW1       0008
    PFXICCW2       0010
    PFXIDMDL       0B0C
    PFXIDSER       0B09
    PFXIDVER       0B08
    PFXILPOI       0004
    PFXILPO0       0000
    PFXILPO1       0001
    PFXILPO2       0002
    PFXILPO3       0003
    PFXILPO4       0004
    PFXILPSW       0000
    PFXINDEX       0CB4
    PFXINIFI       00C0 000000B0
    PFXINISC       00C0
    PFXINPRM       00BC
    PFXINST1       09E4
    PFXINST2       09E8
    PFXINST3       09EC
    PFXINST4       09F0
    PFXINTID       00C0
    PFXIOADP       00C0 00000080
    PFXIOCL0       0EB4 80
    PFXIOCL1       0EB4 40
    PFXIOCL2       0EB4 20
    PFXIOCL3       0EB4 10
    PFXIOCL4       0EB4 08
    PFXIOCL5       0EB4 04
    PFXIOCL6       0EB4 02
    PFXIOCL7       0EB4 01
    PFXIOCOD       0CE8
    PFXIOEA        0D61 40
    PFXIOICA       00B8
    PFXIOINT       00B8
    PFXIONP        0078
    PFXIOOP        0038
    PFXIOPNI       007C
    PFXIOPN0       0078
    PFXIOPN1       0079
    PFXIOPN2       007A
    PFXIOPN3       007B
    PFXIOPN4       007C
    PFXIOPOI       003C
    PFXIOPO0       0038
    PFXIOPO1       0039
    PFXIOPO2       003A
    PFXIOPO3       003B
    PFXIOPO4       003C
    PFXIORET       0B24
    PFXIORNM       00BA
    PFXIOSID       00B8
    PFXIOSRQ       096C
    PFXIRPSG       0800
    PFXIRPSV       0800
    PFXIRP12       0800
    PFXIRP13       0804
    PFXIRP14       0808
    PFXIRP15       080C
    PFXLALLK       0974
    PFXLALLU       0978
    PFXLAPND       01F0 00000200
    PFXLCPUA       0BD8
    PFXLGOFF       0B9C 00000042
    PFXLNKGC       0820
    PFXLNKGD       0828
    PFXLNKGE       0830
    PFXLNKGF       0838
    PFXLNKSG       0820
    PFXLNKSV       0820
    PFXLNK12       0820
    PFXLNK13       0824
    PFXLNK14       0828
    PFXLNK15       082C
    PFXLOCTL       0BA0 40
    PFXLPPUV       0B28
    PFXLRC         08C8
    PFXLRQ         08CC
    PFXLRQND       08C4
    PFXLUSER       09C4
    PFXMACCM       0200
    PFXMACHN       0000
    PFXMALFM       0DB8
    PFXMALFP       0B3C 40
    PFXMALFW       0B3A 80
    PFXMASTR       0B9A 00000014
    PFXMCFSA       00F8
    PFXMCHA        09DC
    PFXMCHDC       00F4
    PFXMCHIN       00E8
    PFXMCHI0       00E8
    PFXMCHI1       00E9
    PFXMCHI2       00EA
    PFXMCHI3       00EB
    PFXMCHI4       00EC
    PFXMCHI5       00ED
    PFXMCHI6       00EE
    PFXMCHNI       0074
    PFXMCHNP       0070
    PFXMCHN0       0070
    PFXMCHN1       0071
    PFXMCHN2       0072
    PFXMCHN3       0073
    PFXMCHN4       0074
    PFXMCHOI       0034
    PFXMCHOP       0030
    PFXMCHO0       0030
    PFXMCHO1       0031
    PFXMCHO2       0032
    PFXMCHO3       0033
    PFXMCHO4       0034
    PFXMCHRD       00FC
    PFXMCHWK       0B3C 10
    PFXMCKCP       00E0
    PFXMCPUT       00D8
    PFXMCVBK       09E0
    PFXMNCLS       0094
    PFXMNCOD       009C
    PFXMPCNT       0BA1
    PFXMPFLG       0BA0
    PFXMTCCE       0B42 00000006
    PFXMTCTR       0B41 20
    PFXNASCE       0298
    PFXNASW0       0298
    PFXNASW1       029C
    PFXNDMRL       0B41 40
    PFXNEWCP       0B9C 00000082
    PFXNLADR       0BB4
    PFXNLR15       0BB8
    PFXNOADD       0ADC
    PFXNOCKP       0B39 08
    PFXNOCPU       0B9C 0000006E
    PFXNOLOC       0BB0
    PFXNULOD       0B39 01
    PFXNXTPF       09CC
    PFXOPRID       00A2
    PFXOSIAD       0E18
    PFXPAGCP       09BC
    PFXPARKD       0B9A 00000032
    PFXPATCH       0F00
    PFXPCIA        00B8 40
    PFXPERAD       0098
    PFXPERAR       00A1
    PFXPERCD       0096
    PFXPGIN        0BF0
    PFXPGLEN       0F80 00001000
    PFXPGNUM       0AC4
    PFXPG2AD       0AAC 0PFX4096
    PFXPINST       0F00
    PFXPKCR0       0CFC
    PFXPKCR0G      0CF8
    PFXPKCR0H      0CF8
    PFXPKFFL       0B42
    PFXPKFRC       0D00
    PFXPKINI       0B42 000000FF
    PFXPKMAX       0B42 0000000A
    PFXPKTOD       0D20
    PFXPLSBK       0BE0
    PFXPNDTK       0B41
    PFXPOLAR       0BA2
    PFXPOLHZ       0BA2 00000000
    PFXPOLVH       0BA2 00000003
    PFXPOLVL       0BA2 00000001
    PFXPOLVM       0BA2 00000002
    PFXPRBTM       0B58
    PFXPREER       0B43 04
    PFXPREMF       0B03 00000000
    PFXPREMT       0B03
    PFXPRERQ       0B03 000000FF
    PFXPRESP       0B9B 00000000
    PFXPRFIX       09C8
    PFXPRGCF       008C
    PFXPRGCT       0E34
    PFXPRGEE       008E
    PFXPRGIC       008F
    PFXPRGIL       008C
    PFXPRGIN       008E
    PFXPRGNI       006C
    PFXPRGNP       0068
    PFXPRGN0       0068
    PFXPRGN1       0069
    PFXPRGN2       006A
    PFXPRGN3       006B
    PFXPRGN4       006C
    PFXPRGOI       002C
    PFXPRGOP       0028
    PFXPRGO0       0028
    PFXPRGO1       0029
    PFXPRGO2       002A
    PFXPRGO3       002B
    PFXPRGO4       002C
    PFXPRGRC       0C00
    PFXPRGRD       0C04
    PFXPRGRE       0C08
    PFXPRGRF       0C0C
    PFXPRGR0       0C10
    PFXPRGR1       0C14
    PFXPRGR2       0C18
    PFXPRGR3       0C1C
    PFXPRGR4       0C20
    PFXPRGR5       0C24
    PFXPRGSG       0C00
    PFXPRGSV       0C00
    PFXPRKFA       0B9E 20
    PFXPRKNG       0B9E 01
    PFXPRKOF       0B9E 04
    PFXPRKWT       0D28
    PFXPRLWK       0B3C 01
    PFXPRMVI       0B43 08
    PFXPRNSE       0B43 10
    PFXPROEF       0B42 00000008
    PFXPROEN       0B42 00000007
    PFXPROEX       0B43 02
    PFXPROFL       0B43
    PFXPRONO       0B43 00
    PFXPROUP       0B43 01
    PFXPRUNR       0B9B 000000CC
    PFXPSAVE       0F80
    PFXPTLBL       02F8
    PFXPTLBT       02C8
    PFXPTMER       0D28 00000B48
    PFXPTRAARP     06A8
    PFXPTRAMDE     06AD
    PFXPTRAREA     0618
    PFXPTRBP       0604
    PFXPTRCL       0611
    PFXPTRCT       0E4C
    PFXPTRFP       0600
    PFXPTRHIRG     06C0
    PFXPTRH0       06C0
    PFXPTRH1       06C4
    PFXPTRH10      06E8
    PFXPTRH11      06EC
    PFXPTRH12      06F0
    PFXPTRH13      06F4
    PFXPTRH14      06F8
    PFXPTRH15      06FC
    PFXPTRH2       06C8
    PFXPTRH3       06CC
    PFXPTRH4       06D0
    PFXPTRH5       06D4
    PFXPTRH6       06D8
    PFXPTRH7       06DC
    PFXPTRH8       06E0
    PFXPTRH9       06E4
    PFXPTRIACA     06AC
    PFXPTRIACE     06AF
    PFXPTRIACR     06AE
    PFXPTROPNR     06A0
    PFXPTRRA       0640
    PFXPTRRB       0644
    PFXPTRRC       0648
    PFXPTRRCF      0648
    PFXPTRRD       064C
    PFXPTRRE       0650
    PFXPTRRF       0654
    PFXPTRRG       0618
    PFXPTRR0       0618
    PFXPTRR0B0     0618
    PFXPTRR0B1     0619
    PFXPTRR0B2     061A
    PFXPTRR0B3     061B
    PFXPTRR1       061C
    PFXPTRR1B0     061C
    PFXPTRR1B1     061D
    PFXPTRR1B2     061E
    PFXPTRR1B3     061F
    PFXPTRR2       0620
    PFXPTRR2B0     0620
    PFXPTRR2B1     0621
    PFXPTRR2B2     0622
    PFXPTRR2B3     0623
    PFXPTRR3       0624
    PFXPTRR4       0628
    PFXPTRR5       062C
    PFXPTRR6       0630
    PFXPTRR7       0634
    PFXPTRR8       0638
    PFXPTRR9       063C
    PFXPTRSC       0610
    PFXPTRSG       0600
    PFXPTRSV       0600
    PFXPTRW$       0680
    PFXPTRWK       0658
    PFXPTRW0       0658
    PFXPTRW1       065C
    PFXPTRW2       0660
    PFXPTRW3       0664
    PFXPTRW4       0668
    PFXPTRW5       066C
    PFXPTRW6       0670
    PFXPTRW7       0674
    PFXPTRW8       0678
    PFXPTRW9       067C
    PFXPWROF       0B39 80
    PFXQDIOA       00B8 80
    PFXRCVFG       0B3A
    PFXRCVWK       0B3C
    PFXREIPL       0B39 10
    PFXRFIP3       0B42 00000009
    PFXRLPST       0B3A 20
    PFXRNHST       0C58
    PFXRNH0        0C58
    PFXRNH00       0C58
    PFXRNH04       0C5C
    PFXRNH1        0C60
    PFXRNH2        0C68
    PFXRNH20       0C68
    PFXRNH24       0C6C
    PFXRNH3        0C70
    PFXRNH4        0C78
    PFXRNPSW       0B10
    PFXRNUSR       0B2C
    PFXRPARK       0B9C 0000000B
    PFXRQUIS       0B9C 00000016
    PFXRSAL        02A4
    PFXRSTOP       0008
    PFXRUNCI       0E60
    PFXRUNCP       0E64
    PFXRUNCR       0E68
    PFXRUNPF       0E6C
    PFXRUNU        09A8
    PFXRUNXT       0984
    PFXRXMSK       0AE8
    PFXSAPSW       0BE8
    PFXSAVES       0300
    PFXSCCFD       0994
    PFXSCHTM       00C2 00000070
    PFXSCHTP       00C2
    PFXSCHT0       00C2 00000000
    PFXSCITS       0B78
    PFXSEMA        0D61 80
    PFXSFIPL       0B39 20
    PFXSGPCP       0016
    PFXSGPGD       0010 000000FF
    PFXSGPND       0010
    PFXSGPNG       0010 000000EE
    PFXSGST        0B00 40
    PFXSHELD       0D67
    PFXSHLON       0D67 40
    PFXSHRLK       0B47 80
    PFXSLCNT       0DC8
    PFXSLTLB       0278
    PFXSMPFL       0B00
    PFXSMPLE       0B42 0000000A
    PFXSNPQU       0B46 80
    PFXSPART       0B00 80
    PFXSPINC       0B90
    PFXSPINT       0B80
    PFXSSABK       08D8
    PFXSSFLG       0CE5
    PFXSTATE       0B9C
    PFXSTBLG       0268
    PFXSTDBK       09D8
    PFXSTEMK       0ACC
    PFXSTFL        00C8
    PFXSTFL0       00C8
    PFXSTFL1       00C9
    PFXSTFL2       00CA
    PFXSTFL3       00CB
    PFXSTKCP       0988
    PFXSTKCR       0E44
    PFXSTKGT       098C
    PFXSTKIO       0990
    PFXSTKPQ       0E48
    PFXSTLEN       0270
    PFXSTMDL       010C
    PFXSTPFX       0108
    PFXSTPSW       0100
    PFXSTRN        0CAC
    PFXSVC         08C0
    PFXSVCBJ       0DF0
    PFXSVCBK       0DF4
    PFXSVCIC       008B
    PFXSVCIF       0088
    PFXSVCIL       0088
    PFXSVCMR       0B46 40
    PFXSVCNI       0064
    PFXSVCNP       0060
    PFXSVCNT       008A
    PFXSVCN0       0060
    PFXSVCN1       0061
    PFXSVCN2       0062
    PFXSVCN3       0063
    PFXSVCN4       0064
    PFXSVCOI       0024
    PFXSVCOP       0020
    PFXSVCO0       0020
    PFXSVCO1       0021
    PFXSVCO2       0022
    PFXSVCO3       0023
    PFXSVCO4       0024
    PFXSVCSG       0840
    PFXSVCSV       0840
    PFXSVF         08E4
    PFXSVMSK       0B40
    PFXSVR         0934
    PFXSVRD        0CDC
    PFXSVR13       08E8
    PFXSVU         08E0
    PFXSVUGS       09B8
    PFXSVURS       09C0
    PFXSVUSW       09B0
    PFXSXASC       0290
    PFXSXAST       09D4
    PFXSXLEN       099C
    PFXSYNCL       0BA3 00000000
    PFXSYNTY       0BA3
    PFXSYNWT       0BA3 000000E5
    PFXSYS         0998
    PFXSYSMP       09A4
    PFXSYSVM       09A0
    PFXTESTP       0B9B 000000FF
    PFXTIMES       02C0
    PFXTINIT       0B39 04
    PFXTMDSP       02E0
    PFXTMMAX       0B48
    PFXTMOUT       0B9B 00000011
    PFXTMPAARP     03A8
    PFXTMPAMDE     03AD
    PFXTMPAREA     0318
    PFXTMPBP       0304
    PFXTMPCL       0311
    PFXTMPFP       0300
    PFXTMPHIRG     03C0
    PFXTMPH0       03C0
    PFXTMPH1       03C4
    PFXTMPH10      03E8
    PFXTMPH11      03EC
    PFXTMPH12      03F0
    PFXTMPH13      03F4
    PFXTMPH14      03F8
    PFXTMPH15      03FC
    PFXTMPH2       03C8
    PFXTMPH3       03CC
    PFXTMPH4       03D0
    PFXTMPH5       03D4
    PFXTMPH6       03D8
    PFXTMPH7       03DC
    PFXTMPH8       03E0
    PFXTMPH9       03E4
    PFXTMPIACA     03AC
    PFXTMPIACE     03AF
    PFXTMPIACR     03AE
    PFXTMPOPNR     03A0
    PFXTMPRA       0340
    PFXTMPRB       0344
    PFXTMPRC       0348
    PFXTMPRCF      0348
    PFXTMPRD       034C
    PFXTMPRE       0350
    PFXTMPRF       0354
    PFXTMPRG       0318
    PFXTMPR0       0318
    PFXTMPR0B0     0318
    PFXTMPR0B1     0319
    PFXTMPR0B2     031A
    PFXTMPR0B3     031B
    PFXTMPR1       031C
    PFXTMPR1B0     031C
    PFXTMPR1B1     031D
    PFXTMPR1B2     031E
    PFXTMPR1B3     031F
    PFXTMPR2       0320
    PFXTMPR2B0     0320
    PFXTMPR2B1     0321
    PFXTMPR2B2     0322
    PFXTMPR2B3     0323
    PFXTMPR3       0324
    PFXTMPR4       0328
    PFXTMPR5       032C
    PFXTMPR6       0330
    PFXTMPR7       0334
    PFXTMPR8       0338
    PFXTMPR9       033C
    PFXTMPSC       0310
    PFXTMPSG       0300
    PFXTMPSV       0300
    PFXTMPW$       0380
    PFXTMPWK       0358
    PFXTMPW0       0358
    PFXTMPW1       035C
    PFXTMPW2       0360
    PFXTMPW3       0364
    PFXTMPW4       0368
    PFXTMPW5       036C
    PFXTMPW6       0370
    PFXTMPW7       0374
    PFXTMPW8       0378
    PFXTMPW9       037C
    PFXTMRUN       02D0
    PFXTMSYS       0B60
    PFXTMUDS       02E8
    PFXTMURN       02D8
    PFXTNDLK       0B39
    PFXTODHO       02C0
    PFXTOTWT       0B50
    PFXTRCR0       0C28
    PFXTRCR1       0C30
    PFXTRCR2       0C38
    PFXTRCR3       0C40
    PFXTRCR4       0C48
    PFXTRCR5       0C50
    PFXTRCSV       0C28
    PFXTRMCD       09D0
    PFXTRPON       0B39 02
    PFXTRQOF       0BAC
    PFXTRXAD       0090
    PFXTRXA3       0093
    PFXTSAR        0C50
    PFXTSGSV       0C28
    PFXTSKBK       0BA8
    PFXTSKST       0B3D
    PFXTSREG       0C30
    PFXTSTOD       0C28
    PFXTTATB       0968
    PFXTTIAE       0B42 00000001
    PFXTTPHL       0B8C
    PFXTTPNT       0B88
    PFXTYDED       0B9A 0000001E
    PFXTYOFL       0B9A 00000000
    PFXTYPE        0B9A
    PFXTYPS        0B9D
    PFXTYSLV       0B9A 00000028
    PFXUDED        0B20
    PFXULALtrm     0B3E 02
    PFXUNKNO       0B9C 000000EE
    PFXUNPRK       0B9E 02
    PFXUPCR8       0B42 00000002
    PFXUPKFA       0B9E 40
    PFXUTIME       0B68
    PFXVCNFG       0B02
    PFXVDG9C       0B02 02
    PFXVEXFP       0B02 20
    PFXVLPAR       0B02 40
    PFXVMVPG       0B02 04
    PFXVNALC       0B02 01
    PFXVOFTD       0B9E 80
    PFXVONCM       0B9F 80
    PFXVONFA       0B9E 10
    PFXVONIN       0B9F 40
    PFXVONTA       0B9F 20
    PFXVPARM       0090
    PFXVTDSP       02F0
    PFXVVECT       0B02 10
    PFXVVMXA       0B02 80
    PFXVWAIT       0B9C 0000002C
    PFXVXCOD       0093
    PFXWFCR6       0CE4 80
    PFXWRKAARP     04A8
    PFXWRKAMDE     04AD
    PFXWRKAREA     0418
    PFXWRKBP       0404
    PFXWRKCL       0411
    PFXWRKFP       0400
    PFXWRKHIRG     04C0
    PFXWRKH0       04C0
    PFXWRKH1       04C4
    PFXWRKH10      04E8
    PFXWRKH11      04EC
    PFXWRKH12      04F0
    PFXWRKH13      04F4
    PFXWRKH14      04F8
    PFXWRKH15      04FC
    PFXWRKH2       04C8
    PFXWRKH3       04CC
    PFXWRKH4       04D0
    PFXWRKH5       04D4
    PFXWRKH6       04D8
    PFXWRKH7       04DC
    PFXWRKH8       04E0
    PFXWRKH9       04E4
    PFXWRKIACA     04AC
    PFXWRKIACE     04AF
    PFXWRKIACR     04AE
    PFXWRKOPNR     04A0
    PFXWRKRA       0440
    PFXWRKRB       0444
    PFXWRKRC       0448
    PFXWRKRCF      0448
    PFXWRKRD       044C
    PFXWRKRE       0450
    PFXWRKRF       0454
    PFXWRKRG       0418
    PFXWRKR0       0418
    PFXWRKR0B0     0418
    PFXWRKR0B1     0419
    PFXWRKR0B2     041A
    PFXWRKR0B3     041B
    PFXWRKR1       041C
    PFXWRKR1B0     041C
    PFXWRKR1B1     041D
    PFXWRKR1B2     041E
    PFXWRKR1B3     041F
    PFXWRKR2       0420
    PFXWRKR2B0     0420
    PFXWRKR2B1     0421
    PFXWRKR2B2     0422
    PFXWRKR2B3     0423
    PFXWRKR3       0424
    PFXWRKR4       0428
    PFXWRKR5       042C
    PFXWRKR6       0430
    PFXWRKR7       0434
    PFXWRKR8       0438
    PFXWRKR9       043C
    PFXWRKSC       0410
    PFXWRKSG       0400
    PFXWRKSV       0400
    PFXWRKW$       0480
    PFXWRKWK       0458
    PFXWRKW0       0458
    PFXWRKW1       045C
    PFXWRKW2       0460
    PFXWRKW3       0464
    PFXWRKW4       0468
    PFXWRKW5       046C
    PFXWRKW6       0470
    PFXWRKW7       0474
    PFXWRKW8       0478
    PFXWRKW9       047C
    PFXWRPSV       0D40
    PFXWTCR6       0CE0
    PFXWTFLG       0CE4
    PFXWTWRK       0CE8
    PFXXASW0       0290
    PFXXASW1       0294
    PFXXCPAR       00A0
    PFXZALT        0178 00000200
    PFXZALTL       0248 00000050
    PFXZEROS       0A00
    PFXZNMSK       0B32
    PFXZNNUM       0B30
    PFX0           0A48 00PFXFFS
    PFX00FFS       0AB4
    PFX1           0A50
    PFX10          0A74
    PFX15          0A78
    PFX16          0A7C
    PFX17          0A80
    PFX2           0A54
    PFX2G          0AD0
    PFX2GFTE       0258
    PFX2GHI        0AD0
    PFX2GM1        0AB8
    PFX2GM4K       0AC4 PFXPGNUM
    PFX2GU         0246 80
    PFX2WAY        08DC
    PFX20          0A84
    PFX2047        0AA0
    PFX2048        0AA4
    PFX24          0A88
    PFX24HSK       0AB0
    PFX24MSK       0AB0
    PFX240         0A90
    PFX255         0A94
    PFX256         0A98
    PFX3           0A58
    PFX31HSK       0AB8
    PFX31MSK       0AB8
    PFX4           0A5C
    PFX4095        0AA8
    PFX4096        0AAC
    PFX5           0A60
    PFX512         0A9C
    PFX6           0A64
    PFX60          0A8C
    PFX7           0A68
    PFX7FFE0       0AE4
    PFX7FFFS       0ABC
    PFX7F000       0AC4 PFXPGNUM
    PFX8           0A6C
    PFX8K          0AE0 0PFX8192
    PFX8000S       0AD4
    PFX8192        0AE0
    PFX9           0A70
    PRGDXAFP       0093 01
    PRGDXBFP       0093 02
    PRGDXCVR       0093 FE
    PRGESOP2A      0093 0C
    PRGESOP2D      0093 04
    PRGESOP2I      0093 84
    PRGESOP2K      0093 08
    PRGESOP2L      0093 80
    PRGESOP2M      0093 8C
    PRGIADCP       008F 00000136
    PRGICHMD       008F 0000F97F
    PRGIHMOD       008F 00000680
    PRGITRXA       008F 00000200
    PRGITXHA       008F 00000400
    PRGITXMD       008F 00000600
    PRGXAR         0093 01
    PRGXCPRI       00A0 20
    PRGXCREG       00A0 0F
    PRGXCSEC       00A0 10
    PRGXHOME       0093 03
    PRGXMVPG       0093 04
    PRGXPRIM       0093 00
    PRGXSEC        0093 02
    PSWAMODE       0002 40
    PSWAMODE       001A 40
    PSWAMODE       0022 40
    PSWAMODE       002A 40
    PSWAMODE       0032 40
    PSWAMODE       003A 40
    PSWAMODE       005A 40
    PSWAMODE       0062 40
    PSWAMODE       006A 40
    PSWAMODE       0072 40
    PSWAMODE       007A 40
    PSWASMSK       0002 C0
    PSWASMSK       001A C0
    PSWASMSK       0022 C0
    PSWASMSK       002A C0
    PSWASMSK       0032 C0
    PSWASMSK       003A C0
    PSWASMSK       005A C0
    PSWASMSK       0062 C0
    PSWASMSK       006A C0
    PSWASMSK       0072 C0
    PSWASMSK       007A C0
    PSWBA          0004 80
    PSWBA          001C 80
    PSWBA          0024 80
    PSWBA          002C 80
    PSWBA          0034 80
    PSWBA          003C 80
    PSWBA          005C 80
    PSWBA          0064 80
    PSWBA          006C 80
    PSWBA          0074 80
    PSWBA          007C 80
    PSWCOND        0002 30
    PSWCOND        001A 30
    PSWCOND        0022 30
    PSWCOND        002A 30
    PSWCOND        0032 30
    PSWCOND        003A 30
    PSWCOND        005A 30
    PSWCOND        0062 30
    PSWCOND        006A 30
    PSWCOND        0072 30
    PSWCOND        007A 30
    PSWCOND1       0002 10
    PSWCOND1       001A 10
    PSWCOND1       0022 10
    PSWCOND1       002A 10
    PSWCOND1       0032 10
    PSWCOND1       003A 10
    PSWCOND1       005A 10
    PSWCOND1       0062 10
    PSWCOND1       006A 10
    PSWCOND1       0072 10
    PSWCOND1       007A 10
    PSWCOND2       0002 20
    PSWCOND2       001A 20
    PSWCOND2       0022 20
    PSWCOND2       002A 20
    PSWCOND2       0032 20
    PSWCOND2       003A 20
    PSWCOND2       005A 20
    PSWCOND2       0062 20
    PSWCOND2       006A 20
    PSWCOND2       0072 20
    PSWCOND2       007A 20
    PSWDECO        0002 04
    PSWDECO        001A 04
    PSWDECO        0022 04
    PSWDECO        002A 04
    PSWDECO        0032 04
    PSWDECO        003A 04
    PSWDECO        005A 04
    PSWDECO        0062 04
    PSWDECO        006A 04
    PSWDECO        0072 04
    PSWDECO        007A 04
    PSWECMD        0001 08
    PSWECMD        0019 08
    PSWECMD        0021 08
    PSWECMD        0029 08
    PSWECMD        0031 08
    PSWECMD        0039 08
    PSWECMD        0059 08
    PSWECMD        0061 08
    PSWECMD        0069 08
    PSWECMD        0071 08
    PSWECMD        0079 08
    PSWEXSM        0000 01
    PSWEXSM        0018 01
    PSWEXSM        0020 01
    PSWEXSM        0028 01
    PSWEXSM        0030 01
    PSWEXSM        0038 01
    PSWEXSM        0058 01
    PSWEXSM        0060 01
    PSWEXSM        0068 01
    PSWEXSM        0070 01
    PSWEXSM        0078 01
    PSWEXUN        0002 02
    PSWEXUN        001A 02
    PSWEXUN        0022 02
    PSWEXUN        002A 02
    PSWEXUN        0032 02
    PSWEXUN        003A 02
    PSWEXUN        005A 02
    PSWEXUN        0062 02
    PSWEXUN        006A 02
    PSWEXUN        0072 02
    PSWEXUN        007A 02
    PSWFIXO        0002 08
    PSWFIXO        001A 08
    PSWFIXO        0022 08
    PSWFIXO        002A 08
    PSWFIXO        0032 08
    PSWFIXO        003A 08
    PSWFIXO        005A 08
    PSWFIXO        0062 08
    PSWFIXO        006A 08
    PSWFIXO        0072 08
    PSWFIXO        007A 08
    PSWHIADR       0004 7F
    PSWHIADR       001C 7F
    PSWHIADR       0024 7F
    PSWHIADR       002C 7F
    PSWHIADR       0034 7F
    PSWHIADR       003C 7F
    PSWHIADR       005C 7F
    PSWHIADR       0064 7F
    PSWHIADR       006C 7F
    PSWHIADR       0074 7F
    PSWHIADR       007C 7F
    PSWHMODE       0002 C0
    PSWHMODE       001A C0
    PSWHMODE       0022 C0
    PSWHMODE       002A C0
    PSWHMODE       0032 C0
    PSWHMODE       003A C0
    PSWHMODE       005A C0
    PSWHMODE       0062 C0
    PSWHMODE       006A C0
    PSWHMODE       0072 C0
    PSWHMODE       007A C0
    PSWIOSM        0000 02
    PSWIOSM        0018 02
    PSWIOSM        0020 02
    PSWIOSM        0028 02
    PSWIOSM        0030 02
    PSWIOSM        0038 02
    PSWIOSM        0058 02
    PSWIOSM        0060 02
    PSWIOSM        0068 02
    PSWIOSM        0070 02
    PSWIOSM        0078 02
    PSWKEY         0001 F0
    PSWKEY         0019 F0
    PSWKEY         0021 F0
    PSWKEY         0029 F0
    PSWKEY         0031 F0
    PSWKEY         0039 F0
    PSWKEY         0059 F0
    PSWKEY         0061 F0
    PSWKEY         0069 F0
    PSWKEY         0071 F0
    PSWKEY         0079 F0
    PSWMAPPD       0001 01
    PSWMAPPD       0019 01
    PSWMAPPD       0021 01
    PSWMAPPD       0029 01
    PSWMAPPD       0031 01
    PSWMAPPD       0039 01
    PSWMAPPD       0059 01
    PSWMAPPD       0061 01
    PSWMAPPD       0069 01
    PSWMAPPD       0071 01
    PSWMAPPD       0079 01
    PSWMCHK        0001 04
    PSWMCHK        0019 04
    PSWMCHK        0021 04
    PSWMCHK        0029 04
    PSWMCHK        0031 04
    PSWMCHK        0039 04
    PSWMCHK        0059 04
    PSWMCHK        0061 04
    PSWMCHK        0069 04
    PSWMCHK        0071 04
    PSWMCHK        0079 04
    PSWPERA        0000 40
    PSWPERA        0018 40
    PSWPERA        0020 40
    PSWPERA        0028 40
    PSWPERA        0030 40
    PSWPERA        0038 40
    PSWPERA        0058 40
    PSWPERA        0060 40
    PSWPERA        0068 40
    PSWPERA        0070 40
    PSWPERA        0078 40
    PSWPMODE       0002 00
    PSWPMODE       001A 00
    PSWPMODE       0022 00
    PSWPMODE       002A 00
    PSWPMODE       0032 00
    PSWPMODE       003A 00
    PSWPMODE       005A 00
    PSWPMODE       0062 00
    PSWPMODE       006A 00
    PSWPMODE       0072 00
    PSWPMODE       007A 00
    PSWPMSK        0002 0F
    PSWPMSK        001A 0F
    PSWPMSK        0022 0F
    PSWPMSK        002A 0F
    PSWPMSK        0032 0F
    PSWPMSK        003A 0F
    PSWPMSK        005A 0F
    PSWPMSK        0062 0F
    PSWPMSK        006A 0F
    PSWPMSK        0072 0F
    PSWPMSK        007A 0F
    PSWPROB        0001 01
    PSWPROB        0019 01
    PSWPROB        0021 01
    PSWPROB        0029 01
    PSWPROB        0031 01
    PSWPROB        0039 01
    PSWPROB        0059 01
    PSWPROB        0061 01
    PSWPROB        0069 01
    PSWPROB        0071 01
    PSWPROB        0079 01
    PSWSIGN        0002 01
    PSWSIGN        001A 01
    PSWSIGN        0022 01
    PSWSIGN        002A 01
    PSWSIGN        0032 01
    PSWSIGN        003A 01
    PSWSIGN        005A 01
    PSWSIGN        0062 01
    PSWSIGN        006A 01
    PSWSIGN        0072 01
    PSWSIGN        007A 01
    PSWSMODE       0002 80
    PSWSMODE       001A 80
    PSWSMODE       0022 80
    PSWSMODE       002A 80
    PSWSMODE       0032 80
    PSWSMODE       003A 80
    PSWSMODE       005A 80
    PSWSMODE       0062 80
    PSWSMODE       006A 80
    PSWSMODE       0072 80
    PSWSMODE       007A 80
    PSWTRAN        0000 04
    PSWTRAN        0018 04
    PSWTRAN        0020 04
    PSWTRAN        0028 04
    PSWTRAN        0030 04
    PSWTRAN        0038 04
    PSWTRAN        0058 04
    PSWTRAN        0060 04
    PSWTRAN        0068 04
    PSWTRAN        0070 04
    PSWTRAN        0078 04
    PSWWAIT        0001 02
    PSWWAIT        0019 02
    PSWWAIT        0021 02
    PSWWAIT        0029 02
    PSWWAIT        0031 02
    PSWWAIT        0039 02
    PSWWAIT        0059 02
    PSWWAIT        0061 02
    PSWWAIT        0069 02
    PSWWAIT        0071 02
    PSWWAIT        0079 02
    PSW31AMF       0004 00
    PSW31AMF       001C 00
    PSW31AMF       0024 00
    PSW31AMF       002C 00
    PSW31AMF       0034 00
    PSW31AMF       003C 00
    PSW31AMF       005C 00
    PSW31AMF       0064 00
    PSW31AMF       006C 00
    PSW31AMF       0074 00
    PSW31AMF       007C 00
    PSW31BT        0004 80
    PSW31BT        001C 80
    PSW31BT        0024 80
    PSW31BT        002C 80
    PSW31BT        0034 80
    PSW31BT        003C 80
    PSW31BT        005C 80
    PSW31BT        0064 80
    PSW31BT        006C 80
    PSW31BT        0074 80
    PSW31BT        007C 80
    STFLCCA        00CA 40
    STFLCTOP       00C9 10
    STFLECTG       00CB 01
    STFLEDAT       00C9 80
    STFLETF2       00CA 80
    STFLETF3       00CA 02
    STFLEXTI       00CA 04
    STFLE2EN       00CB 80
    STFLE3EN       00CB 02
    STFLHFPM       00CA 08
    STFLHFPU       00CA 01
    STFLHPO        00CA 10
    STFLIBM1       00C9 01
    STFLIBM4       00C9 08
    STFLIPTR       00C9 04
    STFLLDF        00CA 20
    STFLMVCS       00CB 10
    STFLNQKS       00C9 02
    STFLPARS       00CB 20
    STFLPTFF       00CB 08
    STFLSRS        00C9 40
    STFLSSKE       00C9 20
    STFLSTCF       00CB 40
    STFL0ALR       00C8 02
    STFL0FLE       00C8 01
    STFL0ICR       00C8 04
    STFL0ICS       00C8 08
    STFL0IDT       00C8 10
    STFL0MEA       00C8 40
    STFL0MEE       00C8 20
    STFL0N3A       00C8 80
    SVCABEND       008B 00000000
    SVCEXIT        008B 00000028
    SVCSABND       008B 00000004
    SVCSDABN       008B 00000024
    SVCTRAP        008B 0000001C
    SVCTRET        008B 00000020
    SVC76ERP       008B 0000004C
    TXHAILC        008C 00000002

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:31:57 EDT.
Copyright IBM Corporation, 1990, 2020