Skip to main content

## Library Properties

You can see the following information in the Library Properties dialog page:

Library information

- Vendor - IBM
- Product ID - 3555-TL
- Serial Number - Library serial number
- Base Firmware Revision - Version of the currently installed base library firmware
- Expansion Firmware Revision - Version of the currently installed expansion module firmware. The expansion module firmware is bundled and installed with the library firmware.
- Robotic Hardware Revision - Hardware revision of the robotic assembly currently installed in the library.
- Robotic Firmware Revision - Version of the currently installed robotic assembly firmware. The robotic assembly firmware is bundled and installed with the library firmware.
- Barcode Reader Hardware Revision - Hardware revision of the barcode reader installed on the robotics assembly.
- Barcode Reader Firmware Revision - Version of the currently installed barcode reader firmware. The barcode reader firmware is bundled and installed with the library firmware.
- Host Name - Library hostname
- IP Address - IP address in use by the library. If DHCP is enabled, this address is obtained from the DHCP server. When DHCP is not enabled, the address is configured manually. Depending on the configured protocol, there will be either IPv4, IPv6 or both address types listed.
- WWide Node Name - The World wide unique base number for the library. Based on this number, the assignment for the drive world wide unique numbers is calculated.

Library status

- Library Status - Showing the status of the library like Idle, Moving, Configuring.
- Total Power On Time - Total time that the base module has been powered on since it was manufactured
- Cartridge in Transport - When applicable, displays the barcode label of the cartridge currently in the robotic assembly
- Odometer - Robotic assembly move count
- Robotic Location - The module where the robotic assembly is located. The home location for the robotic assembly is in base module behind the Operator Panel.
- Shipping Lock - The shipping lock is part of the robotic assembly. Under normal operation, the library locks and unlocks the shipping lock as needed when the robotic assembly is in the base module. For instructions on locking or unlocking the shipping lock manually, see the User's Guide.