Skip to main content

## Initial System Setup

For initial configuration go to the Configuration > Initial System Setup screen.

The wizard guides you through setting library network configuration, configuring date and time, and setting the administrator PIN. You can skip items and stop the wizard at any time. When you have configured the network settings, you can initiate the wizard from the Web GUI to complete the remaining configurations.

| NOTE | On the very first power up of the library the user is prompted to walk through the Initial Configuration wizard. It is recommended to walk completely through the wizard and finish the wizard by pressing the Finish Button. Otherwise with every login on the Operator Panel the user will be prompted again to walk through the wizard.

To log in the first time on the Web GUI you should use the default administrator password adm001. To set your own password go to the page Access > Users on the Web GUI.

1. Press Next>, then Enter to start the wizard beginning with the network configuration.
2. In the network configuration part you can configure these items.

- Host Name
- Domain Name
- Protocol
- IPv4 related settings:

- Method
- IPv4 Address
- Netmask
- IPv4 Gateway
- IPv4 DNS1
- IPv4 DNS2

- IPv6 related settings:

- Method
- IPv6 Address
- IPv6 Gateway
- Prefix Length
- IPv6 DNS1
- IPv6 DNS2

1. When finished with the network settings, select Next> and press Enter to switch to date and time.
2. When finished with the date and time settings, select Next> and press Enter to switch where the Operator Panel PIN can be changed.

1. When finished with the PIN change, select Next> and press Enter to switch to the finish screen.
2. To keep the settings select Finish and press Enter. With Cancel, you can skip the configuration and leave the wizard without any changes. With Back, you can correct your changes before they are submitted.