Skip to main content

## Drive Firmware Upgrade

From the Maintenance > Drive Firmware Upgrade pages you can have the possibility to upgrade every drive that is installed in the library.

To update the drive firmware from the Operator Panel, the drive firmware files needs to be available on the USB thumb drive.

1. Use the Up and Down button to select a drive type from the drive list.
2. On the next screen you can select either to upgrade all installed drives of the same type (same Generation, Form Factor and Interface Type) or one specific drive of the previously selected type. Navigate with the Up and Down to one option and confirm the selection with Enter.
3. Press the Down button to navigate to Next.
4. Use the Up and Down buttons to select the firmware image name you can use for the upgrade process and confirm the selection with Enter.
5. Press the Down button togo to Submit.
6. Press Enter to start the upgrade process.