Skip to main content

## Remote Logging (rsyslog)

Use the Settings > Notifications > Remote Logging (rsyslog) page to enable and configure remote logging (rsylog).

This feature allows sending library events to a remote syslog server. The data sent includes only the ticket information generated by library software. No low level logs generated by OS and other applications will be sent to the remote server.

Only non encrypted remote logging is supported.

- Remote Logging Enabled – If selected, the library sends library events to the server listed in the Remote Logging Server field.
- Notification Level – Select the level of severity of events to be sent as SNMP traps. The default is +Warning.

- Inactive – No events are sent.
- Critical – Only Critical events are sent.
- +Warning – Critical and Warning events are sent.
- +Configuration – Critical, Warning, and Configuration events are sent.
- +Informational – All events are sent.

- Server – Hostname or IP address of remote syslog server.
- Server Port – The default port for the selected protocol is selected. You can choose one of the default ports or configure a custom
- Transport Protocol – Can be either TCP or UDP. The default is UDP.