Skip to main content

## Clean Drive

Use this action to start a manual cleaning process on a drive.

1. Select a cleaning cartridge from the Source Elements list. The library uses the barcode label to identify cleaning cartridges. If no cleaning cartridges are available, load one into an I/O slot or magazine slot.
2. Select the tape drive to be cleaned from the Destination Elements list. Tape drives currently loaded with a cartridge are not listed. To clean a tape drive not listed, move the cartridge out of the drive.
3. Click Submit