Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSYTPRP

Prolog
Control Block Contents
Storage Layout
Cross Reference

#### MRSYTPRP Prolog

####

####

     DSECT NAME - SYTPRP
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor control area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSYTPRP
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 0 - System Domain
                        Record 2 - Processor Data (Per Processor)
     DESCRIPTION - Real System or CPU operation exception.
                   A separate record is generated for each online
                   processor.

    MRSYTPRP Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)          Description

      0   0  Structure  104  SYTPRP              Start of monitor record
      0   0  Character    0  SYTPRP_MRHDR        Record header. See MRRECHDR for
                                                 details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN            record length in bytes
      2   2  Unsigned     2  MRHDRZER            field of zeros
      4   4  Unsigned     1  MRHDRDM             domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC             record identifier
      8   8  Character    8  MRHDRTOD            Time at which this record was
                                                 built. In time-of-day (TOD) clock
                                                 format. See IBM System 370 XA
                                                 Principle of Operation for
                                                 explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END           End of header
     20  14  Unsigned     2  SYTPRP_PFXCPUAD     Real processor's CPU address
     22  16  Unsigned     2  SYTPRP_PLSCUHAF     Count of times a VMDBK was
                                                 dispatched with 'hard affinity'
                                                 (i.e., dedicated to this
                                                 processor)
     24  18  Character    8  SYTPRP_PFXPRBTM     Total CPU time spent in
                                                 emulation mode on this processor
                                                 for all users
     32  20  Character    8  SYTPRP_PFXUTIME     Total CPU time spent on this
                                                 processor which was charged to
                                                 users. It does not include any
                                                 time that CP spends on behalf of a
                                                 user doing such things as
                                                 instruction simulation or page
                                                 translation. This is in CPU time,
                                                 not elapsed (or wall clock) time.
     40  28  Character    8  SYTPRP_PFXTMSYS     Total CPU time spent on this
                                                 processor which has been charged
                                                 to the system instead of the user.
                                                 It includes time spent by the
                                                 system on behalf of the user doing
                                                 such things as instruction
                                                 simulation. It also includes time
                                                 doing other types of system work,
                                                 such as making scheduling
                                                 decisions.
     48  30  Character    8  SYTPRP_PLSVFVTM     Amount of CPU time this
                                                 processor has been using the real
                                                 vector facility while in SIE
     56  38  Character    8  SYTPRP_PLSVFOTM     Amount of CPU time that this
                                                 processor has spent on switching
                                                 vector users
     64  40  Unsigned     4  SYTPRP_PLSVFLOD     Cumulative count of the times CP
                                                 loads the vector registers from
                                                 where they were saved on
                                                 guest-owned storage frames.
     68  44  Character    8  SYTPRP_PFXTOTWT     Total system wait time on this
                                                 CPU (includes both active wait and
                                                 enabled CPU wait). It is the time
                                                 this CPU had no work to do,
                                                 measured in CPU time.
     76  4C  Unsigned     4  SYTPRP_PFXRUNCI     Count of interceptions from SIE
                                                 on this processor. It does NOT
                                                 include interceptions from SIE
                                                 instructions issued in order to
                                                 run a 'Vguest', i.e., a guest of a
                                                 guest, during guest SIE
                                                 simulation. It does NOT include
                                                 interceptions handled by the
                                                 fast-path simulation support code.
     80  50  Unsigned     4  SYTPRP_PFXRUNPF     Count of host page faults on
                                                 this processor resulting from
                                                 guest references to storage paged
                                                 out by CP. Does not include faults
                                                 on RCP pages
     84  54  Unsigned     4  SYTPRP_PFXRUNCP     Count of instructions from SIE
                                                 on this processor. It does not
                                                 include instructions issued in
                                                 order to run a 'Vguest', i.e., a
                                                 guest of a guest, during guest SIE
                                                 simulation. It does not include
                                                 instructions issued following a
                                                 successful fast-path simulation
                                                 support code.
     88  58  Unsigned     4  SYTPRP_CALFSTPH     Count of fast-path instruction
                                                 simulations. PFXFSTSG + PFXFSTXC +
                                                 PFXFST44
     92  5C  Character    8  SYTPRP_PFXSPINT     Elapsed time in formal spin
                                                 locks on this real CPU starting at
                                                 zero and counting upwards. This is
                                                 measured in TOD clock units since
                                                 system IPL.
    100  64  Unsigned     4  SYTPRP_PFXSPINC     Count of spin lock requests on
                                                 this real CPU since IPL that were
                                                 not granted immediately. The lock
                                                 was obtained only after spinning.
    104  68  Character    0  SYTPRP_END

    MRSYTPRP Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                   0     20
    MRHDR_END              14      0
    MRHDRDM                 4      1
    MRHDRLEN                0      2
    MRHDRRC                 6      2
    MRHDRTOD                8      8
    MRHDRZER                2      2
    SYTPRP                  0    104
    SYTPRP_CALFSTPH        58      4
    SYTPRP_END             68      0
    SYTPRP_MRHDR            0      0
    SYTPRP_PFXCPUAD        14      2
    SYTPRP_PFXPRBTM        18      8
    SYTPRP_PFXRUNCI        4C      4
    SYTPRP_PFXRUNCP        54      4
    SYTPRP_PFXRUNPF        50      4
    SYTPRP_PFXSPINC        64      4
    SYTPRP_PFXSPINT        5C      8
    SYTPRP_PFXTMSYS        28      8
    SYTPRP_PFXTOTWT        44      8
    SYTPRP_PFXUTIME        20      8
    SYTPRP_PLSCUHAF        16      2
    SYTPRP_PLSVFLOD        40      4
    SYTPRP_PLSVFOTM        38      8
    SYTPRP_PLSVFVTM        30      8

    This information is
    based on z/VM V4R3.0.

    Last updated on 1 May 2002 at 16:20:33.

    Copyright IBM Corporation, 1990, 2002