DFIR - 32-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### DFIR

Prolog

Control Block Contents
DFIR DSECT
DFIZ DSECT
DFIZCPU DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### DFIR Prolog

     NAME       : HCPDFIR
     DESCRIPTION: DUMP FILE INFORMATION RECORD
     DSECT      : DFIR
     FUNCTION   : HCPDFIR contains vital system register and storage
                  location values for a dump of a system.
                  HCPDFIR is the ESA/390 snapshot of this information
                  and HCPDFIZ is the ESAME snapshot of the same
                  information.  The HCPDFIZ DSECT is included in
                  this file.
     LOCATED BY : The DFIR starts at the third record of a system
                  abend dump to tape or DASD, of a standalone dump to
                  tape, or of an VMDUMP SPOOL file.
     CREATED BY : HCPDMP (SYSTEM ABEND DUMP PROCESSOR) DURING A SYSTEM
                  ABEND DUMP
                  HCPEDM (DUMP PROCESSOR) WHEN PROCESSING A SYSTEM ABEND
                  OR STANDALONE DUMP
                  HCPSAD (STANDALONE DUMP PROCESSOR) DURING A STANDALONE
                  DUMP
                  HCPVDU (VIRTUAL MACHINE DUMP PROCESSOR) DURING A VIRTUAL
                  MACHINE DUMP
     DELETED BY : NOT APPLICABLE
     COMMENTS   : The HCPDFIR is used by HCPEDM (DUMPLOAD) to process a
                  dump from tape or dasd.
                  The DFIR is 5 4k bytes in length and can contain
                  information for up to 63 processors.
                  The DFIZ is 9 4k bytes in length and can contain
                  information for up to 63 processors.
                  HCPDMP builds the DFIR in the work pages HCPWRKA1 to
                  HCPWRKA5.  HCPDMP builds the DFIZ in the work pages
                  HCPWRKA1 to HCPWRKA9.
                  HCPVDU builds the DFIR in the work pages HCPWRKA1 to
                  HCPWRKA5.  HCPVDU builds the DFIZ in the work pages
                  HCPWRKA1 to HCPWRKA9.
                  The displacement of DFIDVF cannot change because
                  DFIDVF is used by DVF to determine if the dump
                  release matches the DUMPSCAN release.
                  The offset and content of some fields in the DFIR
                  DSECT must precisely match the offset and content of
                  equivalent fields in the DFIZ DSECT.  These fields
                  are clearly marked.  DUMPLOAD depends on this fact.

#### DFIR Control Block Content

#### DFIR DSECT

####

####

####

####

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DFIR           DUMP FILE INFORMATION RECORD
    0000    0 Bitstring   64 DFIGPRS        16 GENERAL PURPOSE REGISTERS
    0040   64 Bitstring   64 DFICRS         16 CONTROL REGISTERS
    0080  128 Bitstring   32 DFIFPRS        4 FLOATING POINT REGISTERS
    00A0  160 Dbl-Word     8 DFITODCK       TIME OF DAY CLOCK
    00A8  168 Dbl-Word     8 DFICPUTM       CPU TIMER
    00B0  176 Dbl-Word     8 DFICKCOM       CLOCK COMPARATOR
    00B8  184 Bitstring    1 DFIFLAG        FLAG BYTE. This field must match
                                            the offset and contents of
                                            DFIZFLAG.
              1... ....      DFIHALF        X'80' Obsolete. No longer used by
                                            VM/ESA.
              .1.. ....      DFI370         X'40' Obsolete. No longer used by
                                            VM/ESA
              ..1. ....      DFIXA          X'20' Format of dump is 'XA'. All
                                            dumps by VM/ESA are in this
                                            format.
              ...1 ....      DFIMASI        X'10' MAS INSTALLED ON DUMPED
                                            SYSTEM
              .... 1...      DFIMXC         X'08' Virtual machine was in XC
                                            mode. This is set for VMDUMPs
                                            only.
              .... .1..      DFIMESA        X'04' Virtual machine was in ESA
                                            or XA mode. This is set for
                                            VMDUMPs only.
              .... ..1.      DFIM370        X'02' Virtual machine was in 370
                                            mode. This is set for VMDUMPs
                                            only.
    00B9  185 Bitstring    1 DFITYPE        TYPE OF DUMP FLAG. This field
                                            must match the offset and
                                            contents of DFIZTYPE.
              00000000       DFICP          X'00' CP ABEND OR STAND-ALONE
                                            DUMP
              00000001       DFICPSA        X'01' CP SOFT ABEND DUMP
              00000080       DFIVM          X'80' VIRTUAL MACHINE DUMP
    00BA  186 Bitstring    1 DFICOMP        DUMP COMPLETION FLAG. This field
                                            must match the offset and
                                            contents of DFIZCOMP.
              00000000       DFIDONE        X'00' DUMP IS COMPLETE
              00000040       DFINOLOD       X'40' DUMP WAS NOT COMPLETELY
                                            LOADED BY THE DUMPLOAD COMMAND
              00000080       DFIINC         X'80' DUMP WAS NOT COMPLETE WHEN
                                            CREATED
    00BB  187 Bitstring    1 DFIFMT         Format of the DFIR. This field
                                            must match offset and contents of
                                            DFIZFMT
              00000000       DFIF390        X'00' ESA/390 compatible DFIR
                                            format
              00000082       DFIFEME        X'82' ESAME DFIR format
    00BC  188 Signed       4 DFISYSRV       SYSTEM GENERATED STORAGE SIZE
                                            DFISYSRV is not used in VMDUMPs,
                                            ASISYSRV is used instead.
    00C0  192 Bitstring    1 DFILCORE (256) LOCATIONS 0-255 OF REAL MEMORY
    01C0  448 Signed       4 DFIPFX         PREFIX ADDR FOR DUMPED SYSTEM
    01C4  452 Signed       2 DFICPUNO       NUMBER OF ON-LINE ALTERNATE CPUS
    01C6  454 Bitstring    1 DFICONT        CONT MODE FLAGS
              1... ....      DFICNTMD       X'80' DUMP IS IN CONT FORMAT
    01C7  455 Bitstring    1 DFICDX         Crypto Domain Index Register
    01C8  456 Bitstring    1 DFIVCPI        Virtual CPU information Used in
                                            VMDUMPs only.
              1... ....      DFIVCF         X'80' This vCPU has a vCF
                                            defined.
    01C9  457 Bitstring    1 DFIARCH        Architectural Mode Identifier Not
                                            used in VMDUMPs.
              .... ...1      PFXAINME       X'01' Bit 7 is on indicates ESAME
                                            mode
    01CA  458 Signed       2 DFIDOMN        Crypto domain index mask Used in
                                            VMDUMPs only.
    01CC  460 Signed       4 *              Reserved for future IBM use.
    01D0  464 Signed       4 DFISAMBK       ADDRESS OF THE SNAP AREA MAP
                                            BLOCK Used in Soft Abend Dumps
                                            only.
    01D4  468 Signed       4 * (2)          Reserved for future IBM use.
    01DC  476 Signed       4 DFISYSAD       Address of HCPSYS at the time of
                                            dump
    01E0  480 Signed       4 DFIDVF (20)    Reserved for use by the Dump
                                            Viewing Facility. This field must
                                            match offset and contents of
                                            DFIZDVF.
    0230  560 Dbl-Word     8 DFIPSW         PSW, used only for VMDUMPs and
                                            Standalone dumps.
    0238  568 Signed       2 DFIADCPU       CPU ADDRESS
    023A  570 Signed       2 DFIVFSSZ       SECTION SIZE FOR THE VECTOR
                                            FACILITY
    023C  572 Bitstring   64 DFIARS         16 ACCESS REGISTERS
    027C  636 Bitstring    8 DFIASITP       eASIT OF PRIMARY ADDRESS SPACE -
                                            USED IN VMDUMPS ONLY
    0284  644 Bitstring   33 DFISPACP       SPACEID OF PRIMARY ADDRESS
    02A5  677 Bitstring    1 * (131)        RESERVED FOR FUTURE IBM USE
              00000328       DFIFEND        * Address after end of Failing
                                            CPU data
         OTHER ON-LINE CPU HAS THE FOLLOWING INFORMATION
    0328  808 Bitstring  312 DFICPU (0)     OTHER CPU INFORMATION
    0328  808 Signed       2 DFICPUAD       CPU ADDRESS
    032A  810 Signed       2 DFIVFSIZ       SECTION SIZE FOR THE VECTOR
                                            FACILITY Used in VMDUMPs only.
    032C  812 Signed       4 DFIPFXPG       ADDRESS OF PREFIX PAGE FOR CPU
    0330  816 Bitstring    1 DFICDXOP       Crypto Domain Index Register Used
                                            in VMDUMPs only.
    0331  817 Bitstring    1 DFIVCPUI       Virtual CPU information Used in
                                            VMDUMPs only.
              1... ....      DFIVCF         X'80' This vCPU has a vCF
                                            defined.
    0332  818 Signed       2 DFICDOM        Crypto domain index mask Used in
                                            VMDUMPs only.
    0334  820 Signed       4 *              Reserved for future IBM use
    0338  824 Dbl-Word     8 * (0)
    0338  824 Bitstring  296 DFICPUIF       CPU'S REAL STORAGE LOC. 216-511
              00000138       DFICPULN       *-DFICPUAD LENGTH OF OTHER
                                            PROCESSOR INFO
              0000008C       DFISIZE        (*-DFIR+7)/8 SIZE OF DUMP INFO.
                                            RECORD
              00000000       DFIMCPUT       0,8 CPU TIMER LOGOUT
              00000008       DFIMCKCP       DFIMCPUT+L'DFIMCPUT,8 TOD
                                            COMPARATOR LOGOUT
              00000010       DFIMCHIN       DFIMCKCP+L'DFIMCKCP,8 MACHINE
                                            CHECK INTERRUPT CODE
              00000018       DFISPAR1       DFIMCHIN+L'DFIMCHIN,8 RESERVED
                                            FOR FUTURE HARDWARE USE
              00000020       DFIMCFSA       DFISPAR1+L'DFISPAR1,4 MACHINE
                                            CHECK FAILING STORAGE ADDRESS
              00000024       DFIMCHRD       DFIMCFSA+L'DFIMCFSA,4 MACHINE
                                            DEPENDENT REQION CODE
              00000028       DFIFXLOG       DFIMCHRD+L'DFIMCHRD,16 MACHINE
                                            DEPENDENT FIXED LOGOUT AREA
              00000038       DFISPAR2       DFIFXLOG+L'DFIFXLOG,16 RESERVED
                                            FOR FUTURE HARDWARE USE
              00000048       DFIARLG        DFISPAR2+L'DFISPAR2,64 ACCESS
                                            REGISTERS
              00000088       DFIFPRLG       DFIARLG+L'DFIARLG,32 FLOATING
                                            POINT REGS
              000000A8       DFIGPRLG       DFIFPRLG+L'DFIFPRLG,64 GENERAL
                                            REGISTERS
              000000E8       DFICRLG        DFIGPRLG+L'DFIGPRLG,64 CONTROL
                                            REGISTERS
         FUNCTION : DFIZ DSECT is the ESAME version of the DFIR.
         LOCATED BY : Same as DFIR DSECT
         CREATED BY : Same as DFIR DSECT
         DELETED BY : Same as DFIR DSECT
         COMMENTS : Same as DFIR DSECT except:
         - The DFIZ is bigger because lots of fields are bigger. The DFIZ takes
         up 9 pages (8 full pages and 1 partial page).
         - The order of equivalent fields in the DFIR and DFIZ are different.
         Three fields (DFIZFLAG, DFIZFMT and DFIZDVF) are at the same offset as
         their DFIR equivalents.
         - The data for the non-failing CPU's is defined with a separate DSECT
         (DFIZCPU).
         - HCPDMP builds the DFIZ in the work pages HCPWRKA1 through HCPWRKA9.
         - HCPSAD builds the DFIZ in real storage pages 3 through 11.

    DFIZ DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DFIZ           DUMP FILE INFORMATION RECORD
    0000    0 Character    8 DFIZID         Identification string
    0008    8 Dbl-Word     8 *              Reserved for future IBM Use
    0010   16 Bitstring  128 DFIZGRS        16 64 bit General Purpose
                                            Registers
    0090  144 Signed       4 DFIZPFX        Prefix Register
    0094  148 Signed       4 *              Reserved for future IBM Use
    0098  152 Bitstring    1 *              Reserved for future IBM Use
    0099  153 Bitstring    8 DFIZTOD        Time of Day Clock
    00A1  161 Bitstring    3 *              Reserved for future IBM Use
    00A4  164 Signed       4 *              Reserved for future IBM Use
    00A8  168 Bitstring    1 *              Reserved for future IBM Use
    00A9  169 Bitstring    8 DFIZCPUT       CPU Timer logout area
    00B1  177 Bitstring    3 *              Reserved for future IBM Use
    00B4  180 Signed       4 *              Reserved for future IBM Use
    00B8  184 Bitstring    1 DFIZFLAG       FLAG BYTE. This field must match
                                            the offset and contents of
                                            DFIFLAG.
              1... ....      DFIZHALF       X'80' Obsolete. No longer used by
                                            VM/ESA
              .1.. ....      DFIZ370        X'40' Obsolete. No longer used by
                                            VM/ESA
              ..1. ....      DFIZXA         X'20' Format of dump is 'XA'. All
                                            dumps by VM/ESA are in this
                                            format.
              ...1 ....      DFIZMASI       X'10' MAS Installed on dumped
                                            system
              .... 1...      DFIZMXC        X'08' Virtual machine was in XC
                                            mode. This is set for VMDUMPs
                                            only.
              .... .1..      DFIZMESA       X'04' Virtual machine was in ESA
                                            or XA mode. This is set for
                                            VMDUMPs only.
              .... ..1.      DFIZM370       X'02' Virtual machine was in 370
                                            mode. This is set for VMDUMPs
                                            only.
              .... ...1      DFIZMEME       X'01' Virtual CPU was in ESAME
                                            mode. This is set for VMDUMPs
                                            only.
    00B9  185 Bitstring    1 DFIZTYPE       TYPE OF DUMP FLAG. This field
                                            must match the offset and
                                            contents of DFITYPE.
              00000000       DFIZCP         X'00' CP ABEND OR STAND-ALONE
                                            DUMP
              00000001       DFIZCPSA       X'01' CP SOFT ABEND DUMP
              00000080       DFIZVM         X'80' VIRTUAL MACHINE DUMP
    00BA  186 Bitstring    1 DFIZCOMP       DUMP COMPLETION FLAG. This field
                                            must match the offset and
                                            contents of DFICOMP.
              00000000       DFIZDONE       X'00' DUMP IS COMPLETE
              00000040       DFIZNLOD       X'40' DUMP WAS NOT COMPLETELY
                                            LOADED BY THE DUMPLOAD COMMAND
              00000080       DFIZINC        X'80' DUMP WAS NOT COMPLETE WHEN
                                            CREATED
    00BB  187 Bitstring    1 DFIZFMT        Format of the DFIR. This field
                                            must match offset and contents of
                                            DFIFMT.
              00000000       DFIZF390       X'00' ESA/390 compatible DFIR
                                            format
              00000082       DFIZFEME       X'82' ESAME DFIR format
    00BC  188 Bitstring    1 DFIZCONT       CONT MODE FLAGS
              1... ....      DFIZCTMD       X'80' DUMP IS IN CONT FORMAT
    00BD  189 Bitstring    1 DFIZCDX        Crypto Domain Index Register
    00BE  190 Bitstring    1 DFIZVCPI       Virtual CPU information Used in
                                            VMDUMPs only.
              1... ....      DFIZVCF        X'80' This vCPU has a vCF
                                            defined.
    00BF  191 Bitstring    1 DFIZARCH       Architectural Mode Identifier Not
                                            used in VMDUMPs.
              .... ...1      PFXAINME       X'01' Bit 7 is on indicates ESAME
                                            mode
    00C0  192 Signed       4 DFIZGPSW (4)   128 bit PSW, used only for
                                            VMDUMPs and Standalone dumps.
    00D0  208 Bitstring  128 DFIZCRS        16 64 bit Control Registers
    0150  336 Bitstring  128 DFIZFRS        16 64 bit Floating Point
                                            Registers
    01D0  464 Bitstring    1 *              Reserved for future IBM Use
    01D1  465 Bitstring    8 DFIZCKCM       Clock Comparator logout area
    01D9  473 Bitstring    3 *              Reserved for future IBM Use
    01DC  476 Signed       4 DFIZTPR        TOD Clock Programable Register
    01E0  480 Signed       4 DFIZDVF (20)   Reserved for use by the Dump
                                            Viewing Facility. This field must
                                            match offset and contents of
                                            DFIDVF.
    0230  560 Bitstring   64 DFIZARS        16 32 bit Access Registers
    0270  624 Signed       4 DFIZSYSR       Storage Size up to 2G DFIZSYSR is
                                            not used in VMDUMPs, ASISYSRV is
                                            used instead.
    0274  628 Signed       4 *              Reserved for future IBM Use
    0278  632 Signed       4 DFIZSYSA       Address of HCPSYS at the time of
                                            dump
    027C  636 Signed       4 *              Reserved for future IBM Use
    0280  640 Dbl-Word     8 DFIZSTOR       Storage Size DFIZSTOR is not used
                                            in VMDUMPs, ASIxxxxx is used
                                            instead.
    0288  648 Signed       4 DFIZSAMB       ADDRESS OF THE SNAP AREA MAP
                                            BLOCK Used in Soft Abend Dumps
                                            only.
    028C  652 Signed       4 *              Reserved for future IBM Use
    0290  656 Bitstring    1 DFIZLCOR (256) Locations 0-255 of Real Memory
    0390  912 Signed       2 DFIZCPUN       Number of On-Line Alternate CPUS
    0392  914 Signed       2 DFIZACPU       CPU Address
    0394  916 Signed       2 DFIZVFSZ       Section Size for the Vector
                                            Facility
    0396  918 Signed       2 *              Reserved For future IBM Use
    0398  920 Bitstring    8 DFIZASIT       eASIT of Primary Address Space.
                                            Used in VMDUMPS ONLY
    03A0  928 Bitstring   33 DFIZPSID       SPACEID of Primary Address Space.
    03C1  961 Bitstring    1 * (3)          Reserved for future IBM use.
    03C4  964 Signed       2 DFIZDOMN       Crypto domain index mask Used in
                                            VMDUMPs only.
    03C6  966 Signed       2 *              Reserved for future IBM use.
    03C8  968 Signed       4 DFIZFPCR       Floating Point Control Register
    03CC  972 Signed       4 *              Reserved for future IBM use.
    03D0  976 Dbl-Word     8 * (16)         Reserved for future IBM use.
              00000450       DFIZFCLN       *-DFIZ Length of failing CPU data
         The following space holds the processor data for 63 non-failing CPU's.
         The failing CPU data is stored above.
              00000450       DFIZDATA       * Start of non-failing CPU data
              000087D8       DFIZDATL       63*DFIZCPUL Length of non-failing
                                            CPU data
              00008C28       DFIZDZLN       DFIZFCLN+DFIZDATL Total DFIZ
                                            length in bytes
              00000009       DFIZPGCT       (DFIZDZLN+4095)/4096 Total DFIZ
                                            length in pages
         FUNCTION : Map the the data of 1 non-failing CPU.
         LOCATED BY : DFIZDATA contains DFIZCPU entries.

    DFIZCPU DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DFIZCPU        DUMP FILE INFORMATION RECORD
         Section 1 The data in this section is set individually by the dump
         creating program.
    0000    0 Signed       2 DFIZCPUA       CPU Address
    0002    2 Signed       2 DFIZVFS        Section Size for the Vector
                                            Facility Used in VMDUMPs only.
    0004    4 Bitstring    1 DFIZCDXR       Crypto Domain Index Register Used
                                            in VMDUMPs only.
    0005    5 Bitstring    1 DFIZVCPU       Virtual CPU information Used in
                                            VMDUMPs only.
              1... ....      DFIZVCF        X'80' This vCPU has a vCF
                                            defined.
    0006    6 Signed       2 DFIZCDOM       Crypto domain index mask Used in
                                            VMDUMPs only.
    0008    8 Signed       4 *              Reserved for future IBM use
    000C   12 Signed       4 *              Reserved for future IBM use
    0010   16 Bitstring  128 DFIZFRLG       Floating Point Registers
    0090  144 Bitstring  128 DFIZGRLG       General Registers
    0110  272 Dbl-Word     8 DFIZPSWL (2)   PSW or Fixed Logout Area
    0120  288 Signed       4 *              Reserved for hardware use
    0124  292 Signed       4 *              Reserved for hardware use
    0128  296 Signed       4 DFIZPRLG       Prefix Register
    012C  300 Signed       4 DFIZFCLG       Floating Point Control Register
    0130  304 Signed       4 *              Reserved for hardware use
    0134  308 Signed       4 DFIZTPLG       TOD Clock Programmable Register
    0138  312 Dbl-Word     8 DFIZCTLG       CPU Timer logout area
    0140  320 Bitstring    1 *              Reserved for hardware use
    0141  321 Bitstring    7 DFIZCCLG       Clock Comparator logout area
    0148  328 Signed       4 *              Reserved for hardware use
    014C  332 Signed       4 *              Reserved for hardware use
    0150  336 Bitstring   64 DFIZARLG       Access Registers
    0190  400 Bitstring  128 DFIZCRLG       Control Registers
              ...1 ....      DFIZS2         DFIZFRLG,*-DFIZFRLG Section 2
                                            Label With Length Section 3 The
                                            data in this section is moved in
                                            one block from an ESAME
                                            processor's 8K prefix page. The
                                            data is from HCPPFXPG fields
                                            PFXMCHIN through PFXGMCFS. Thus,
                                            the following fields must be
                                            maintained in order and without
                                            changes to field sizes.
    0210  528 Dbl-Word     8 DFIZMCHI       Machine Check Interrupt Code
    0218  536 Signed       4 *              Reserved for future hardware use
    021C  540 Signed       4 DFIZDCOD       External Damage code
    0220  544 Dbl-Word     8 DFIZMCFA       Machine Check Failing Storage
                                            Address
              DFIZMCFA       DFIZS3         DFIZMCHI,*-DFIZMCHI Section 3
                                            Label With Length
              00000228       DFIZCPUL       *-DFIZCPU Length of non-failing
                                            CPU data area

    DFIR Storage Layout

    *** DFIR - DUMP FILE INFORMATION RECORD
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       DFIGPRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                                                       |
    *     =                        DFICRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  80 |                                                       |
    *     =                       DFIFPRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  A0 |                       DFITODCK                        |
    *     +-------------------------------------------------------+
    *  A8 |                       DFICPUTM                        |
    *     +-------------------------------------------------------+
    *  B0 |                       DFICKCOM                        |
    *     +------+------+------+------+---------------------------+
    *  B8 |:FLAG |:TYPE |:COMP |DFIFMT|         DFISYSRV          |
    *     +------+------+------+------+---------------------------+
    *  C0 |                                                       |
    *     =                       DFILCORE                        =
    *     |                                                       |
    *     +---------------------------+-------------+------+------+
    * 1C0 |          DFIPFX           |  DFICPUNO   |:CONT |DFICDX|
    *     +------+------+-------------+-------------+------+------+
    * 1C8 |:VCPI |:ARCH |  DFIDOMN    |///////////////////////////|
    *     +------+------+-------------+---------------------------+
    * 1D0 |         DFISAMBK          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1D8 |///////////////////////////|         DFISYSAD          |
    *     +---------------------------+---------------------------+
    * 1E0 |                                                       |
    *     =                        DFIDVF                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 230 |                        DFIPSW                         |
    *     +-------------+-------------+---------------------------+
    * 238 |  DFIADCPU   |  DFIVFSSZ   |                           |
    *     +-------------+-------------+                           |
    * 240 |                                                       |
    *     =                        DFIARS                         =
    *     |                           +---------------------------+
    *     |                           |        DFIASITP-          |
    *     +---------------------------+---------------------------+
    * 280 |          -(27C)           |                           |
    *     +---------------------------+                           |
    * 288 |                                                       |
    *     =                       DFISPACP                        =
    *     |                                  +--------------------+
    *     |                                  |////////////////////|
    *     +----------------------------------+////////////////////|
    * 2A8 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------+-------------+---------------------------+
    * 328 |  DFICPUAD   |  DFIVFSIZ   |         DFIPFXPG          |
    *     +------+------+-------------+---------------------------+
    * 330 |:CDXOP|:VCPUI|  DFICDOM    |///////////////////////////|
    *     +------+------+-------------+---------------------------+
    * 338 |                                                       |
    *     =                       DFICPUIF                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 460
    *
    *** DFIR - DUMP FILE INFORMATION RECORD

    *** DFIZ - DUMP FILE INFORMATION RECORD
    *
    *     +-------------------------------------------------------+
    *   0 |                        DFIZID                         |
    *     +-------------------------------------------------------+
    *   8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    *  10 |                                                       |
    *     =                       DFIZGRS                         =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    *  90 |         DFIZPFX           |///////////////////////////|
    *     +------+--------------------+---------------------------+
    *  98 |//////|                   DFIZTOD-                     |
    *     +------+--------------------+---------------------------+
    *  A0 |-(099)|////////////////////|///////////////////////////|
    *     +------+--------------------+---------------------------+
    *  A8 |//////|                   DFIZCPUT-                    |
    *     +------+--------------------+---------------------------+
    *  B0 |-(0A9)|////////////////////|///////////////////////////|
    *     +------+------+------+------+------+------+------+------+
    *  B8 |:ZFLAG|:ZTYPE|:ZCOMP|:ZFMT |:ZCONT|:ZCDX |:ZVCPI|:ZARCH|
    *     +------+------+------+------+------+------+------+------+
    *  C0 |                       DFIZGPSW                        |
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  D0 |                                                       |
    *     =                       DFIZCRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 150 |                                                       |
    *     =                       DFIZFRS                         =
    *     |                                                       |
    *     +------+------------------------------------------------+
    * 1D0 |//////|                   DFIZCKCM-                    |
    *     +------+--------------------+---------------------------+
    * 1D8 |-(1D1)|////////////////////|         DFIZTPR           |
    *     +------+--------------------+---------------------------+
    * 1E0 |                                                       |
    *     =                       DFIZDVF                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 230 |                                                       |
    *     =                       DFIZARS                         =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 270 |         DFIZSYSR          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 278 |         DFIZSYSA          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 280 |                       DFIZSTOR                        |
    *     +---------------------------+---------------------------+
    * 288 |         DFIZSAMB          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 290 |                                                       |
    *     =                       DFIZLCOR                        =
    *     |                                                       |
    *     +-------------+-------------+-------------+-------------+
    * 390 |  DFIZCPUN   |  DFIZACPU   |  DFIZVFSZ   |/////////////|
    *     +-------------+-------------+-------------+-------------+
    * 398 |                       DFIZASIT                        |
    *     +-------------------------------------------------------+
    * 3A0 |                                                       |
    *     =                       DFIZPSID                        =
    *     |      +--------------------+-------------+-------------+
    * 3C0 |      |////////////////////|  DFIZDOMN   |/////////////|
    *     +------+--------------------+-------------+-------------+
    * 3C8 |         DFIZFPCR          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 3D0 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 450
    *
    *** DFIZ - DUMP FILE INFORMATION RECORD

    *** DFIZCPU - DUMP FILE INFORMATION RECORD
    *
    *     +-------------+-------------+------+------+-------------+
    *   0 |  DFIZCPUA   |  DFIZVFS    |:ZCDXR|:ZVCPU|  DFIZCDOM   |
    *     +-------------+-------------+------+------+-------------+
    *   8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    *  10 |                                                       |
    *     =                       DFIZFRLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  90 |                                                       |
    *     =                       DFIZGRLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 110 |                       DFIZPSWL                        |
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 120 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 128 |         DFIZPRLG          |         DFIZFCLG          |
    *     +---------------------------+---------------------------+
    * 130 |///////////////////////////|         DFIZTPLG          |
    *     +---------------------------+---------------------------+
    * 138 |                       DFIZCTLG                        |
    *     +------+------------------------------------------------+
    * 140 |//////|                   DFIZCCLG                     |
    *     +------+--------------------+---------------------------+
    * 148 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 150 |                                                       |
    *     =                       DFIZARLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 190 |                                                       |
    *     =                       DFIZCRLG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 210 |                       DFIZMCHI                        |
    *     +---------------------------+---------------------------+
    * 218 |///////////////////////////|         DFIZDCOD          |
    *     +---------------------------+---------------------------+
    * 220 |                       DFIZMCFA                        |
    *     +-------------------------------------------------------+
    * 228
    *
    *** DFIZCPU - DUMP FILE INFORMATION RECORD

    DFIR Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    DFIADCPU       0238
    DFIARCH        01C9
    DFIARLG        0338 00000048
    DFIARS         023C
    DFIASITP       027C
    DFICDOM        0332
    DFICDX         01C7
    DFICDXOP       0330
    DFICKCOM       00B0
    DFICNTMD       01C6 80
    DFICOMP        00BA
    DFICONT        01C6
    DFICP          00B9 00000000
    DFICPSA        00B9 00000001
    DFICPU         0328
    DFICPUAD       0328
    DFICPUIF       0338
    DFICPULN       0338 00000138
    DFICPUNO       01C4
    DFICPUTM       00A8
    DFICRLG        0338 000000E8
    DFICRS         0040
    DFIDOMN        01CA
    DFIDONE        00BA 00000000
    DFIDVF         01E0
    DFIFEME        00BB 00000082
    DFIFEND        02A5 00000328
    DFIFLAG        00B8
    DFIFMT         00BB
    DFIFPRLG       0338 00000088
    DFIFPRS        0080
    DFIFXLOG       0338 00000028
    DFIF390        00BB 00000000
    DFIGPRLG       0338 000000A8
    DFIGPRS        0000
    DFIHALF        00B8 80
    DFIINC         00BA 00000080
    DFILCORE       00C0
    DFIMASI        00B8 10
    DFIMCFSA       0338 00000020
    DFIMCHIN       0338 00000010
    DFIMCHRD       0338 00000024
    DFIMCKCP       0338 00000008
    DFIMCPUT       0338 00000000
    DFIMESA        00B8 04
    DFIMXC         00B8 08
    DFIM370        00B8 02
    DFINOLOD       00BA 00000040
    DFIPFX         01C0
    DFIPFXPG       032C
    DFIPSW         0230
    DFISAMBK       01D0
    DFISIZE        0338 0000008C
    DFISPACP       0284
    DFISPAR1       0338 00000018
    DFISPAR2       0338 00000038
    DFISYSAD       01DC
    DFISYSRV       00BC
    DFITODCK       00A0
    DFITYPE        00B9
    DFIVCF         01C8 80
    DFIVCF         0331 80
    DFIVCPI        01C8
    DFIVCPUI       0331
    DFIVFSIZ       032A
    DFIVFSSZ       023A
    DFIVM          00B9 00000080
    DFIXA          00B8 20
    DFIZACPU       0392
    DFIZARCH       00BF
    DFIZARLG       0150
    DFIZARS        0230
    DFIZASIT       0398
    DFIZCCLG       0141
    DFIZCDOM       0006
    DFIZCDX        00BD
    DFIZCDXR       0004
    DFIZCKCM       01D1
    DFIZCOMP       00BA
    DFIZCONT       00BC
    DFIZCP         00B9 00000000
    DFIZCPSA       00B9 00000001
    DFIZCPUA       0000
    DFIZCPUL       0220 00000228
    DFIZCPUN       0390
    DFIZCPUT       00A9
    DFIZCRLG       0190
    DFIZCRS        00D0
    DFIZCTLG       0138
    DFIZCTMD       00BC 80
    DFIZDATA       03D0 00000450
    DFIZDATL       03D0 000087D8
    DFIZDCOD       021C
    DFIZDOMN       03C4
    DFIZDONE       00BA 00000000
    DFIZDVF        01E0
    DFIZDZLN       03D0 00008C28
    DFIZFCLG       012C
    DFIZFCLN       03D0 00000450
    DFIZFEME       00BB 00000082
    DFIZFLAG       00B8
    DFIZFMT        00BB
    DFIZFPCR       03C8
    DFIZFRLG       0010
    DFIZFRS        0150
    DFIZF390       00BB 00000000
    DFIZGPSW       00C0
    DFIZGRLG       0090
    DFIZGRS        0010
    DFIZHALF       00B8 80
    DFIZID         0000
    DFIZINC        00BA 00000080
    DFIZLCOR       0290
    DFIZMASI       00B8 10
    DFIZMCFA       0220
    DFIZMCHI       0210
    DFIZMEME       00B8 01
    DFIZMESA       00B8 04
    DFIZMXC        00B8 08
    DFIZM370       00B8 02
    DFIZNLOD       00BA 00000040
    DFIZPFX        0090
    DFIZPGCT       03D0 00000009
    DFIZPRLG       0128
    DFIZPSID       03A0
    DFIZPSWL       0110
    DFIZSAMB       0288
    DFIZSTOR       0280
    DFIZSYSA       0278
    DFIZSYSR       0270
    DFIZS2         0190 10
    DFIZS3         0220 DFIZMCFA
    DFIZTOD        0099
    DFIZTPLG       0134
    DFIZTPR        01DC
    DFIZTYPE       00B9
    DFIZVCF        00BE 80
    DFIZVCF        0005 80
    DFIZVCPI       00BE
    DFIZVCPU       0005
    DFIZVFS        0002
    DFIZVFSZ       0394
    DFIZVM         00B9 00000080
    DFIZXA         00B8 20
    DFIZ370        00B8 40
    DFI370         00B8 40
    PFXAINME       01C9 01
    PFXAINME       00BF 01

    This information is
    based on z/VM V4R4.0.
    Last updated on 29 Jul 2003 at 15:26:10 EDT.

    Copyright IBM Corporation, 1990, 2003