SHPQITEM - 64-bit CP - V4R4.0

Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### SHPQITEM

Prolog

Control Block Contents
SHPQITEM DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### SHPQITEM Prolog

     NAME       : CSESHQBK
     DESCRIPTION: VM Cross-System Requests
                  Request Definition Data Area
                  CSESHQBK - VM CROSS-SYSTEM REQUESTS
                  REQUEST DEFINITION DATA AREA
     DSECT      : SHPQITEM
     FUNCTION   : DEFINES THE FORMAT OF THE 'QITEM' THAT IS USED FOR
                  INTER-SYSTEM COMMUNICATION IN A CROSS SYSTEM
                  EXTENSIONS COMPLEX.
     NOTES      : THE COMMON OR FIXED PART OF ALL REQUEST ITEMS SENT
                  BETWEEN ASSOCIATED SYSTEMS.  THE REMAINDER OF THE
                  BLOCK DEPENDS ON THE FUNCTION CODE AND TYPE.

#### SHPQITEM Control Block Content

#### SHPQITEM DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      SHPQITEM       VM Cross-System Requests
    0000    0 Address      4 SHPQPTR        POINTER TO NEXT QUEUE ELEMENT
    0004    4 Signed       4 SHPQTRN        TRANSACTION NUMBER
    0008    8 Signed       2 SHPQLN         SIZE OF THIS ENTRY, DBL WORDS
    000A   10 Bitstring    1 SHPQFC         FUNCTION CODE
              00000001       SHPQFCAD       X'01' SEND A COPY OF ORIGINAL
                                            SPFBK
              00000002       SHPQFCQU       X'02' LOCK A COPY SPFBK REQUEST
              00000003       SHPQFCDQ       X'03' UNLOCK A COPY SPFBK
              00000004       SHPQFCQN       X'04' NOTICE ORIGINAL SPFBK
                                            LOCKED
              00000005       SHPQFCFN       X'05' NOTICE ORIGINAL OUTPUT
                                            SPFBK UNLOCKED
              00000006       SHPQFCDN       X'06' DELETE A COPY FILE
              00000007       SHPQFCQV       X'07' NOTICE AN INPUT SPFBK
                                            EXISTS
              00000008       SHPQFCMD       X'08' CP COMMAND
              00000009       SHPQFCDL       X'09' DELETE AN ORIGINAL FILE
              0000000A       SHPQFCCK       X'0A' CHECKPOINT AN SPFBK
              0000000B       SHPQFCRP       X'0B' RESPONSE ITEM
              0000000C       SHPQFCLG       X'0C' USER HAS LOGGED ON
              0000000D       SHPQFCRS       X'0D' RESET BROADCAST BITS FOR
                                            ORIGINAL SFB
              0000000E       SHPQFCDS       X'0E' DELETE SYNC (NOT USED)
              0000000F       SHPQFC0F       X'0F' ** RESERVED **
              00000010       SHPQFCDR       X'10' DELETE COPY READER REQUEST
              00000011       SHPQFCTS       X'11' TIMER CONTROLLED SYNC
                                            (XSPOOL SYNC)
              00000012       SHPQFCRR       X'12' Notify RDR *SPL
              00000013       SHPQFCSC       X'13' RDR *SPL CONNECTION/SEVER
              00000014       SHPQFCMG       X'14' CSE MESSAGE
              00000015       SHPQFCMR       X'15' MESSAGE WITH RESPONSE
              00000016       SHPQFCQC       X'16' QUERY COMMAND WITH RESPONSE
              00000017       SHPQFCIN       X'17' INDICATE COMMAND WITH
                                            RESPONSE
              00000018       SHPQFC18       X'18' ** RESERVED **
              00000019       SHPQFC19       X'19' ** RESERVED **
              0000001A       SHPQFC1A       X'1A' ** RESERVED **
              0000001B       SHPQFCQL       X'1B' LOGON CROSS CHECK (LQ)
              0000001C       SHPQFC1C       X'1C' ** RESERVED **
              0000001D       SHPQFC1D       X'1D' ** RESERVED **
              0000001E       SHPQFC1E       X'1E' ** RESERVED **
              0000001F       SHPQFCID       X'1F' VM/CSE Release ID
    000B   11 Bitstring    1 SHPQFLG        FLAG 1
              00000002       SHPQFSZ        (*-SHPQITEM+7)/8 FIXED PART SIZE,
                                            DOUBLE WORDS.
    000C   12 Character   60 SHPQFXND       END OF THE FIXED PART. ***
                                            EXTENSION FOR ITEMS THAT INVOLVE
                                            SPFBKS
    000C   12 Signed       2 SHPQSID        SPOOL ID NUMBER
    000E   14 Bitstring    1 SHPQORGX       INDEX OF ORIGINATING SYSTEM
    000F   15 Bitstring    1 SHPQFLG1       USED FOR THE VARIOUS EXTENSIONS
    0010   16 Character    8 SHPQUSER       USERID OF SPOOL FILE OWNER
    0018   24 Signed       4 SHPQCCPD       SFBSTART: DASD ADDRESS OF THE
                                            FIRST SPMBK IN THE FILE
    001C   28 Address      4 SHPQSPFP       ADDRESS OF SPFBK ON THE SYSTEM
                                            THAT CREATED THIS QITEM
    0020   32 Character    1 SHPQHEND (0)   END OF SPOOLING COMMON AREA
    0020   32 Dbl-Word     8 *              USE VARIES ACCORDING TO SHPQFC
    0028   40 Signed       4 SHPQTRCE       ADDRESS OF TRACE ENTRY FOR REQ
              00000006       SHPQSZ         (*-SHPQITEM+7)/8 QUEUE HEADER
                                            SIZE, DWS.
         *** ADD-SPFBK QITEM'S USE OF THE SPOOLING EXTENSION
    000F   15 Bitstring    1 ADCMDSYS       INDEX OF SYSTEM ISSUING COMMAND;
                                            CONTROLS MESSAGES ON THE
                                            RECEIVING SYSTEM
    0020   32 Character    8 ADOLDOWN       PREVIOUS OWNER OF FILE USED BY
                                            SFV.FM ON RECEIVING SYSTEM ***
                                            LOCK SPFBK REQUEST'S USE OF
                                            SPOOLING EXTENSION
    000F   15 Bitstring    1 QUINDEX        INDEX OF REQUESTING SYSTEM
    0020   32 Address      4 QUADR12        RETURN ADDRESS
    0024   36 Address      4 QUADR13        ADDRESS OF CALLER'S SAVEAREA
         *** LOCK NOTICE'S USE OF THE SPOOLING EXTENSION
         *** REDEFINITION -
    000F   15 Bitstring    1 QNINDEX        INDEX OF THE LOCKED SYSTEM
         *** CHECKPOINT SPFBK REQUEST'S USE OF SPOOLING EXTENSION
    0020   32 Signed       4 CKCPEADR       Address of CPEBK to be stacked
                                            when response for this QITEM is
                                            received
    0024   36 Signed       4 *              *** EXTENSION FOR NOTIFY RDR *SPL
         *** REDEFINITION -
    000E   14 Signed       2 SHPQRDRC       User's rdr file count CSEHPPOL
         *** EXTENSION FOR AN BROADCAST SPOOLING COMMAND QITEM
    000C   12 Address      4 SCMADR12       RETURN ADDRESS
    0010   16 Address      4 SCMADR13       ADDRESS OF CALLER'S SAVEAREA
    0014   20 Bitstring    1 SCMCTYPE       VMDCTYPE OF COMMAND ISSUER
    0015   21 Bitstring    1 SCMMLVL        VMDMLVL OF COMMAND ISSUER
    0016   22 Signed       2 SCMLEN         LENGTH OF COMMAND IN BYTES
    0018   24 Character    8 SCMUSER        USERID ISSUING THE COMMAND
    0020   32 Character    8 SCMDIST        VMDDIST OF COMMAND ISSUER
    0028   40 Address      4 SCMTRCE        ADDRESS OF TRACE ENTRY
    002C   44 Bitstring    1 SCMCMDAU       VMDCMDAU - ACI audit
    002D   45 Bitstring    1 SCMCMDPR       VMDCMDPR - ACI protect
    002E   46 Bitstring    1 SCMSECU1       VMDSECU1 - DIAG/'ANY' ACI
    002F   47 Bitstring    1 *              RESERVED
    0030   48 Character    8 SCMGRPN        ISSUER'S GROUP-NAME
    0038   56 Character    8 SCMALTID       ISSUER'S VMDALTID
              00000008       SCMMDSZ        (*-SHPQITEM+7)/8 SIZE OF FIX AREA
                                            IN DWS
    0040   64 Character    1 SCMDATA (0)    START OF VARIABLE LENGTH CMD ***
                                            EXTENSION FOR QITEMS THAT SAVE
                                            REGISTERS
    000C   12 Address      4 SHPADR12       RETURN ADDRESS
    0010   16 Address      4 SHPADR13       ADDRESS OF CALLER'S SAVEAREA
    0014   20 Signed       4 SHPPARMA       WORK AREA ON COMD SIDE
    0018   24 Character    1 SHPREND (0)    END OF REGISTER AREA
         *** EXTENSION FOR A CSE MESSAGE WITH RESPONSE
    0018   24 Address      4 MRMSGADR       ADDRESS OF MESSAGE TO SEND
    001C   28 Signed       4 MRMSGLN        LENGTH OF MESSAGE TO SEND
    0020   32 Signed       4 MRRECIDL       LENGTH OF RECEIVING USER ID
    0024   36 Character    8 MRRECID        USERID(S) TO RECEIVE MSG
    002C   44 Character    8 MRSNDID        USERID SENDING THE MESSAGE
    0034   52 Bitstring    1 MRTYPE         SMSG, MSG, OR WNG
    0035   53 Bitstring    1 MRATTR         MSGNOH ATTRIBUTE
              00000007       MRSZ           (*-SHPQITEM+7)/8 SIZE OF A
                                            MESSAGE WITH RESPONSE ***
                                            Extension for QUERY and INDICATE
                                            command with *** response
         *** Notes : The QITEM extensions for the general *** QUERY/INDICATE and
         the QUERY LINKS commands *** share a common definition area
    0018   24 Character    8 QCDATA (0)     Individual query/indicate command
                                            parameter
         Query Links Data command parameters
    0018   24 Character    6 QCVOLID        VOLUME ID
    001E   30 Bitstring    1 QCDEVTP        DEVICE TYPE FLAGS
    001F   31 Bitstring    1 QCFLAGS        Flags for QUERY LINKS
    0020   32 Character    8 QCSENDID       USERID ISSUING THE COMMAND
    0028   40 Bitstring    1 QCTYPE         TYPE OF QUERY
    0029   41 Character    4 QCDSPFW (0)    DEFINE FOR REL 2 COMPATABILTY
    0029   41 Character    2 QCDSPSV        FIST HALF OF STARTING MD
    002B   43 Character    2 QCDISP         STARTING MDISK CYL (Q LINKS)
    002D   45 Character    4 QCEDSPFW (0)   DEFINE FOR REL 2 COMPATABILTY
    002D   45 Character    2 QCEDSPSV       FIRST HALF OF ENDING MD
    002F   47 Character    2 QCEDISP        ENDING MINIDISK CYL (Q LINKS)
    0031   49 Bitstring    1 QCCTYPE        VMDCTYPE OF COMMAND ISSUER
    0032   50 Bitstring    1 QCQIFS         Flags for the query and indicate
                                            commands
    0033   51 Character    6 QCRSV1         Reserved for expansion
              00000008       QCMDSZ         (*-SHPQITEM+7)/8 SIZE OF QUERY
                                            CMND W RESPONSE *** EXTENSION FOR
                                            A LOGON CROSS CHECK REQUEST
    0018   24 Character    8 QLUSERID       USERID LOGGING ON.
    0020   32 Character    1 QLTYPE         CURRENTLY NOT USED
    0021   33 Bitstring    3 *
              00000005       QLCMDSZ        (*-SHPQITEM+7)/8 SIZE OF LOGON
                                            CROSS CHECK REQUEST.
         *** EXTENSION FOR TIMER CONTROLLED SYNC (XSPOOL SYNC)
    0014   20 Character    1 *              * RESERVED *
    0015   21 Character    8 TSUSERID       USER ID REQUESTING THE SYNC
              00000004       TSAPSZ         (*-SHPQITEM+7)/8 SIZE IN DOUBLE
                                            WORDS *** EXTENSION FOR AN INPUT
                                            FILE (QV) AND LOGON NOTICE
    000C   12 Character    8 SHPLGID        USERID LOGGING ON
    0014   20 Character    8 QVPREVON       PREVIOUS OWNER OF THE READER FILE
                                            (FOR SFV.FM)
              00000004       SHPQLGSZ       (*-SHPQITEM+7)/8 SIZE IN DOUBLE
                                            WORDS *** EXTENSION FOR THE CSE
                                            MESSAGE
    000C   12 Character    8 MSMSGUSR       USER TO RECEIVE MESSAGE
    0014   20 Character    2 MSMSGLN        LENGTH OF MESSAGE IN BYTES
    0016   22 Character    1 MSMSGDAT (0)   START OF THE MESSAGE
              00000003       MSMSGSZ        (*-SHPQITEM+7)/8 SIZE OF MESSAGE
                                            PREFIX
         *** EXTENSION FOR A RESPONSE ITEM
    000C   12 Character    1 RPAPST (0)     START OF RESPONSE APPENDAGE
    000C   12 Bitstring    1 RPRESPTO       CODE OF THE REQUEST
    000D   13 Character    2 RPMISC1        RETURN INFORMATION
    000F   15 Bitstring    1 RPINDEX        INDEX OF THE RESPONDING SYSTEM
    0010   16 Bitstring    4 RPERRCD        ERROR CODE FOR MSG 0057/6600
              00000003       RPSIZE         (*-SHPQITEM+7)/8 SIZE OF A
                                            RESPONSE ITEM
         - DEFINITIONS -
         THERE ARE BRANCH TABLES IN HCPXHE AND HCPXRP THAT DEPEND ON THESE
         FUNCTION CODES.
         FUNCTION CODES NOT USED IN BRANCH TABLES
              1... ....      SHPQFCSN       X'80' SYNCH ITEM
              1... ...1      SHPQFCLS       X'81' LIST ITEM FOR THE UVM
              1... ..1.      SHPQFCNP       X'82' NOP SENT TO THE UVM
         SHPQFLG DEFINITIONS FOR LOCK ITEM
              .... ...1      SERBYTIM       X'01' ITEM ALREADY BEEN SERVICED,
                                            LEFT ON Q2 WAITING FOR RESPONSE
                                            TO COME BACK
         SHPQFLG DEFINITIONS FOR SYSTEM SYNC
              .... ...1      SYNC1          X'01' TYPE 1 SYNC REQUEST
              .... ..1.      SYNC2          X'02' TYPE 2 SYNC END OF SYNC
                                            DATA
              .... .1..      SYNC3          X'04' TYPE 3 SYNC END OF SPFBK
                                            LIST
         SHPQFLG DEFINITIONS FOR ITEMS INVOLVING SPFBKS ARE THE SAME AS SPFQUEUE
              .... 1...      LOGREQF        X'08' LOG-ON PROCESSING
         SHPQFLG DEFINITIONS FOR RESPONSE ITEMS.
              1... ....      POSRESP        X'80' REQUEST HAS BEEN RECEIVED
              .1.. ....      NEGRESP        X'40' REQUEST HAS BEEN R ED
         SHPQFLG DEFINITIONS FOR MESSAGE.
              1... ....      RSQMSG         X'80' DISPLAY MESSAGE, IGNORE
                                            IMSG
              .... ...1      QCUSERID       X'01' QUERY USER USERID
              .... ..1.      QCUSERS        X'02' QUERY USERS
              .... ..11      QCNAMES        X'03' QUERY NAMES
              .... .1..      QCLINKS        X'04' QUERY LINKS
              ...1 ...1      INLOAD         X'11' INDICATE LOAD
              1... ....      FBADEV         X'80' FBA DEVICE CODE
              .1.. ....      CKDDEV         X'40' CKD DEVICE CODE
              1... ....      QCSTABLE       X'80' QUERY LINKS stable option
              1... ....      QCQEXTND       X'80' The query extended option
                                            was requested

#### SHPQITEM Storage Layout

    *** SHPQITEM - VM Cross-System Requests
    *
    *     +---------------------------+---------------------------+
    *   0 |         SHPQPTR           |         SHPQTRN           |
    *     +-------------+------+------+---------------------------+
    *   8 |   SHPQLN    |SHPQFC|:QFLG |                           |
    *     +-------------+------+------+                           |
    *  10 |                                                       |
    *     =                       SHPQFXND                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  48
    *
    *** SHPQITEM - VM Cross-System Requests

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +-------------+------+------+
    *   8 ...                       C |  SHPQSID    |:QORGX|:QFLG1|
    *     +---------------------------+-------------+------+------+
    *  10 |                       SHPQUSER                        |
    *     +---------------------------+---------------------------+
    *  18 |         SHPQCCPD          |         SHPQSPFP          |
    *     +---------------------------+---------------------------+
    *  20 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    *  28 |         SHPQTRCE          | 2C
    *     +---------------------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

    *** Overlay for SHPQFLG1 in SHPQITEM
    *
    *                                                      +------+
    *   8 ...                                            F |:MDSYS|
    *                                                      +------+
    *  10
    *
    *** Overlay for SHPQFLG1 in SHPQITEM

    *** Overlay for SHPQHEND in SHPQITEM
    *
    *     +-------------------------------------------------------+
    *  20 |                       ADOLDOWN                        |
    *     +-------------------------------------------------------+
    *  28
    *
    *** Overlay for SHPQHEND in SHPQITEM

    *** Overlay for SHPQFLG1 in SHPQITEM
    *
    *                                                      +------+
    *   8 ...                                            F |:NDEX |
    *                                                      +------+
    *  10
    *
    *** Overlay for SHPQFLG1 in SHPQITEM

    *** Overlay for SHPQHEND in SHPQITEM
    *
    *     +---------------------------+---------------------------+
    *  20 |         QUADR12           |         QUADR13           |
    *     +---------------------------+---------------------------+
    *  28
    *
    *** Overlay for SHPQHEND in SHPQITEM

    *** Overlay for SHPQFLG1 in SHPQITEM
    *
    *                                                      +------+
    *   8 ...                                            F |:NDEX |
    *                                                      +------+
    *  10
    *
    *** Overlay for SHPQFLG1 in SHPQITEM

    *** Overlay for SHPQHEND in SHPQITEM
    *
    *     +---------------------------+---------------------------+
    *  20 |         CKCPEADR          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  28
    *
    *** Overlay for SHPQHEND in SHPQITEM

    *** Overlay for SHPQORGX in SHPQITEM
    *
    *                                               +-------------+
    *   8 ...                                     E |  SHPQRDRC   |
    *                                               +-------------+
    *  10
    *
    *** Overlay for SHPQORGX in SHPQITEM

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +---------------------------+
    *   8 ...                       C |         SCMADR12          |
    *     +---------------------------+------+------+-------------+
    *  10 |         SCMADR13          |:CTYPE|:MLVL |   SCMLEN    |
    *     +---------------------------+------+------+-------------+
    *  18 |                       SCMUSER                         |
    *     +-------------------------------------------------------+
    *  20 |                       SCMDIST                         |
    *     +---------------------------+------+------+------+------+
    *  28 |         SCMTRCE           |:CMDAU|:CMDPR|:SECU1|//////|
    *     +---------------------------+------+------+------+------+
    *  30 |                       SCMGRPN                         |
    *     +-------------------------------------------------------+
    *  38 |                       SCMALTID                        |
    *     +-------------------------------------------------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +---------------------------+
    *   8 ...                       C |         SHPADR12          |
    *     +---------------------------+---------------------------+
    *  10 |         SHPADR13          |         SHPPARMA          |
    *     +---------------------------+---------------------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

    *** Overlay for SHPREND in SHPQITEM
    *
    *     +---------------------------+---------------------------+
    *  18 |         MRMSGADR          |         MRMSGLN           |
    *     +---------------------------+---------------------------+
    *  20 |         MRRECIDL          |         MRRECID-          |
    *     +---------------------------+---------------------------+
    *  28 |          -(024)           |         MRSNDID-          |
    *     +---------------------------+------+------+-------------+
    *  30 |          -(02C)           |MRTYPE|MRATTR| 36
    *     +---------------------------+------+------+
    *
    *** Overlay for SHPREND in SHPQITEM

    *** Overlay for SHPREND in SHPQITEM
    *
    *     +-----------------------------------------+------+------+
    *  18 |                QCVOLID                  |:EVTP |:LAGS |
    *     +-----------------------------------------+------+------+
    *  20 |                       QCSENDID                        |
    *     +------+-------------+-------------+-------------+------+
    *  28 |QCTYPE|  QCDSPSV    |   QCDISP    |  QCEDSPSV   |:DISP-|
    *     +------+------+------+-------------+-------------+------+
    *  30 |-(02F)|:TYPE |QCQIFS|             QCRSV1-              |
    *     +------+------+------+----------------------------------+
    *  38 |-(033)| 39
    *     +------+
    *
    *** Overlay for SHPREND in SHPQITEM

    *** Overlay for SHPREND in SHPQITEM
    *
    *     +-------------------------------------------------------+
    *  18 |                       QLUSERID                        |
    *     +------+--------------------+---------------------------+
    *  20 |QLTYPE|////////////////////| 24
    *     +------+--------------------+
    *
    *** Overlay for SHPREND in SHPQITEM

    *** Overlay for SHPPARMA in SHPQITEM
    *
    *                                 +------+--------------------+
    *  10 ...                      14 |//////|      (015)-        |
    *     +---------------------------+------+--------------------+
    *  18 |            -TSUSERID             | 1D
    *     +----------------------------------+
    *
    *** Overlay for SHPPARMA in SHPQITEM

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +---------------------------+
    *     ...                       C |         SHPLGID-          |
    *     +---------------------------+---------------------------+
    *  10 |          -(00C)           |        QVPREVON-          |
    *     +---------------------------+---------------------------+
    *  18 |          -(014)           | 1C
    *     +---------------------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +---------------------------+
    *     ...                       C |        MSMSGUSR-          |
    *     +---------------------------+-------------+-------------+
    *  10 |          -(00C)           |  MSMSGLN    |
    *     +---------------------------+-------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

    *** Overlay for SHPQFXND in SHPQITEM
    *
    *                                 +------+-------------+------+
    *   8 ...                       C |:ESPTO|  RPMISC1    |:NDEX |
    *     +---------------------------+------+-------------+------+
    *  10 |         RPERRCD           | 14
    *     +---------------------------+
    *
    *** Overlay for SHPQFXND in SHPQITEM

#### SHPQITEM Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    ADCMDSYS       000F
    ADOLDOWN       0020
    CKCPEADR       0020
    CKDDEV         0010 40
    FBADEV         0010 80
    INLOAD         0010 11
    LOGREQF        0010 08
    MRATTR         0035
    MRMSGADR       0018
    MRMSGLN        001C
    MRRECID        0024
    MRRECIDL       0020
    MRSNDID        002C
    MRSZ           0035 00000007
    MRTYPE         0034
    MSMSGDAT       0016
    MSMSGLN        0014
    MSMSGSZ        0016 00000003
    MSMSGUSR       000C
    NEGRESP        0010 40
    POSRESP        0010 80
    QCCTYPE        0031
    QCDATA         0018
    QCDEVTP        001E
    QCDISP         002B
    QCDSPFW        0029
    QCDSPSV        0029
    QCEDISP        002F
    QCEDSPFW       002D
    QCEDSPSV       002D
    QCFLAGS        001F
    QCLINKS        0010 04
    QCMDSZ         0033 00000008
    QCNAMES        0010 03
    QCQEXTND       0010 80
    QCQIFS         0032
    QCRSV1         0033
    QCSENDID       0020
    QCSTABLE       0010 80
    QCTYPE         0028
    QCUSERID       0010 01
    QCUSERS        0010 02
    QCVOLID        0018
    QLCMDSZ        0021 00000005
    QLTYPE         0020
    QLUSERID       0018
    QNINDEX        000F
    QUADR12        0020
    QUADR13        0024
    QUINDEX        000F
    QVPREVON       0014
    RPAPST         000C
    RPERRCD        0010
    RPINDEX        000F
    RPMISC1        000D
    RPRESPTO       000C
    RPSIZE         0010 00000003
    RSQMSG         0010 80
    SCMADR12       000C
    SCMADR13       0010
    SCMALTID       0038
    SCMCMDAU       002C
    SCMCMDPR       002D
    SCMCTYPE       0014
    SCMDATA        0040
    SCMDIST        0020
    SCMGRPN        0030
    SCMLEN         0016
    SCMMDSZ        0038 00000008
    SCMMLVL        0015
    SCMSECU1       002E
    SCMTRCE        0028
    SCMUSER        0018
    SERBYTIM       0010 01
    SHPADR12       000C
    SHPADR13       0010
    SHPLGID        000C
    SHPPARMA       0014
    SHPQCCPD       0018
    SHPQFC         000A
    SHPQFCAD       000A 00000001
    SHPQFCCK       000A 0000000A
    SHPQFCDL       000A 00000009
    SHPQFCDN       000A 00000006
    SHPQFCDQ       000A 00000003
    SHPQFCDR       000A 00000010
    SHPQFCDS       000A 0000000E
    SHPQFCFN       000A 00000005
    SHPQFCID       000A 0000001F
    SHPQFCIN       000A 00000017
    SHPQFCLG       000A 0000000C
    SHPQFCLS       0010 81
    SHPQFCMD       000A 00000008
    SHPQFCMG       000A 00000014
    SHPQFCMR       000A 00000015
    SHPQFCNP       0010 82
    SHPQFCQC       000A 00000016
    SHPQFCQL       000A 0000001B
    SHPQFCQN       000A 00000004
    SHPQFCQU       000A 00000002
    SHPQFCQV       000A 00000007
    SHPQFCRP       000A 0000000B
    SHPQFCRR       000A 00000012
    SHPQFCRS       000A 0000000D
    SHPQFCSC       000A 00000013
    SHPQFCSN       0010 80
    SHPQFCTS       000A 00000011
    SHPQFC0F       000A 0000000F
    SHPQFC1A       000A 0000001A
    SHPQFC1C       000A 0000001C
    SHPQFC1D       000A 0000001D
    SHPQFC1E       000A 0000001E
    SHPQFC18       000A 00000018
    SHPQFC19       000A 00000019
    SHPQFLG        000B
    SHPQFLG1       000F
    SHPQFSZ        000B 00000002
    SHPQFXND       000C
    SHPQHEND       0020
    SHPQLGSZ       0014 00000004
    SHPQLN         0008
    SHPQORGX       000E
    SHPQPTR        0000
    SHPQRDRC       000E
    SHPQSID        000C
    SHPQSPFP       001C
    SHPQSZ         0028 00000006
    SHPQTRCE       0028
    SHPQTRN        0004
    SHPQUSER       0010
    SHPREND        0018
    SYNC1          0010 01
    SYNC2          0010 02
    SYNC3          0010 04
    TSAPSZ         0015 00000004
    TSUSERID       0015

This information is based on z/VM V4R4.0. Last updated on 30 Jul 2003 at 12:26:49 EDT.
Copyright IBM Corporation, 1990, 2003