Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### DMPINREC

Prolog

Control Block Contents
DMPINREC DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### DMPINREC Prolog

     NAME       : DMPINREC
     DESCRIPTION: VM/370 SYSTEM PRODUCT DUMP INFORMATION RECORD
     DSECT      : DMPINREC
     FUNCTION   : TO MAP OUT THE VM/370 DUMP INFORMATION RECORD
     LOCATED BY : FIRST RECORD IN A 370-FORMAT VIRTUAL MACHINE DUMP
                  (VMDUMP) READER SPOOL FILE
     CREATED BY : HCPVDUMP - WHEN CREATING A 370-FORMAT VIRTUAL MACHINE
                  DUMP USING THE VMDUMP COMMAND
     DELETED BY : NOT DELETED

#### DMPINREC Control Block Content

#### DMPINREC DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      DMPINREC       VM/370 SYSTEM PRODUCT DUMP
                                            INFORMATION RECORD
    0000    0 Bitstring   64 DMPGPRS        16 GENERAL PURPOSE REGISTERS
    0040   64 Bitstring   64 DMPCRS         16 CONTROL REGISTERS
    0080  128 Bitstring   32 DMPFPRS        4 FLOATING POINT REGISTERS
    00A0  160 Dbl-Word     8 DMPTODCK       TIME-OF-DAY CLOCK
    00A8  168 Dbl-Word     8 DMPCPUTM       CPU TIMER
    00B0  176 Dbl-Word     8 DMPCKCOM       TIME-OF-DAY CLOCK COMPARATOR
    00B8  184 Bitstring    1 DMPFLAG        FLAG BYTE
              1... ....      DMPHALF        X'80' ON MEANS LAST RECORD IN
                                            DUMP FILE = 2K
    00B9  185 Bitstring    1 *              RESERVED FOR FUTURE IBM USE
    00BA  186 Signed       2 DMPPROCA       ABENDING PROCESSOR ADDRESS (NOT
                                            USED FOR VMDUMPS)
    00BC  188 Signed       4 DMPSYSRV       SYSTEM GENERATED STORAGE SIZE
    00C0  192 Bitstring    1 DMPLCORE (256) LOCATIONS 0-256 OF REAL MEMORY
                                            (NOT USED FOR VMDUMPS)
    01C0  448 Signed       4 DMPPRFRG       PREFIX REGISTER
    01C4  452 Signed       4 DMPABEND       ABEND CODE FOR FAILING PROCESSOR
    01C8  456 Character  512 DMPPGMAP       PAGE MAP -INDICATES WHICH PAGES
                                            WERE DUMPED. EACH BIT REPRESENTS
                                            ONE 4K PAGE
    03C8  968 Dbl-Word     8 DMPCPUID       CPU IDENTIFICATION FROM REAL CPU
    03D0  976 Dbl-Word     8 DMPVMTYP       ID OF VM MACHINE TYPE, OBTAINED
                                            FROM 'FORMAT' PARAMETER ONLY FOR
                                            VMDUMPS NOT CP DUMPS
    03D8  984 Dbl-Word     8 DMPPSW         PSW OF VIRTUAL MACHINE ONLY FOR
                                            VMDUMPS NOT CP DUMPS
    03E0  992 Signed       4 DMPSYSRM       REAL SIZE OF STORAGE...IT IS THE
                                            HARDWARE SIZE OF THE MACHINE FOR
                                            CP DUMPS AND THE VIRTUAL MACHINE
                                            (INCLUDING DISCONTIGUOUS SAVED
                                            SEGMENTS) FOR VMDUMPS
    03E4  996 Bitstring   80 DMPIPCS (0)    RESERVED FOR USE BY IPCS
    03E4  996 Signed       4 * (4)          RESERVED FOR USE BY IPCS; NOT
                                            USED BY THE VMDUMP COMMAND
    03F4 1012 Character    8 DMPDATE        DATE OF FAILURE IN FORM MM/DD/YY
    03FC 1020 Signed       4 * (4)          RESERVED FOR USE BY IPCS; NOT
                                            USED BY THE VMDUMP COMMAND
    040C 1036 Character    2 DMPSRID        'SR' SYMPTOM RECORD ID
    040E 1038 Character    1 DMPREL         CP RELEASE NUMBER
    040F 1039 Character    2 DMPLEV         CP FEATURE (SERVICE) LEVEL
    0411 1041 Bitstring    3 *              RESERVED FOR USE BY IPCS
    0414 1044 Signed       4 DMPTOD (2)     LOCAL MIDNIGHT IN TOD CLOCK VALUE
    041C 1052 Signed       4 DMPTICON       LOCAL TIME ZONE CONVERSION FACTOR
    0420 1056 Character    4 DMPMODEL       CPU MODEL NUMBER
    0424 1060 Character    6 DMPSERNO       CPU SERIAL NUMBER
    042A 1066 Signed       2 *              RESERVED FOR FUTURE IBM USE
    042C 1068 Signed       4 * (2)          RESERVED FOR USE BY IPCS; NOT
                                            USED BY THE VMDUMP COMMAND
    0434 1076 Character  100 DMPDMPID       DUMP IDENTIFIER SPECIFIED ON THE
                                            VMDUMP COMMAND LINE, PADDED ON
                                            THE RIGHT WITH BLANKS IF
                                            NECESSARY

#### DMPINREC Storage Layout

    *** DMPINREC - VM/370 SYSTEM PRODUCT DUMP INFORMATION RECORD
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       DMPGPRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                                                       |
    *     =                        DMPCRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  80 |                                                       |
    *     =                       DMPFPRS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  A0 |                       DMPTODCK                        |
    *     +-------------------------------------------------------+
    *  A8 |                       DMPCPUTM                        |
    *     +-------------------------------------------------------+
    *  B0 |                       DMPCKCOM                        |
    *     +------+------+-------------+---------------------------+
    *  B8 |:FLAG |//////|  DMPPROCA   |         DMPSYSRV          |
    *     +------+------+-------------+---------------------------+
    *  C0 |                                                       |
    *     =                       DMPLCORE                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 1C0 |         DMPPRFRG          |         DMPABEND          |
    *     +---------------------------+---------------------------+
    * 1C8 |                                                       |
    *     =                       DMPPGMAP                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 3C8 |                       DMPCPUID                        |
    *     +-------------------------------------------------------+
    * 3D0 |                       DMPVMTYP                        |
    *     +-------------------------------------------------------+
    * 3D8 |                        DMPPSW                         |
    *     +---------------------------+---------------------------+
    * 3E0 |         DMPSYSRM          |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     |///////////////////////////+---------------------------+
    *     |///////////////////////////|         DMPDATE-          |
    *     +---------------------------+---------------------------+
    * 3F8 |          -(3F4)           |///////////////////////////|
    *     +---------------------------+///////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     |///////////////////////////+-------------+------+------+
    * 408 |///////////////////////////|  DMPSRID    |DMPREL|:LEV- |
    *     +------+--------------------+-------------+------+------+
    * 410 |-(40F)|////////////////////|         DMPTOD-           |
    *     +------+--------------------+---------------------------+
    * 418 |          -(414)           |         DMPTICON          |
    *     +---------------------------+---------------------------+
    * 420 |         DMPMODEL          |        DMPSERNO-          |
    *     +-------------+-------------+---------------------------+
    * 428 |   -(424)    |/////////////|///////////////////////////|
    *     +-------------+-------------+---------------------------+
    * 430 |///////////////////////////|                           |
    *     +---------------------------+                           |
    * 438 |                                                       |
    *     =                       DMPDMPID                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 498
    *
    *** DMPINREC - VM/370 SYSTEM PRODUCT DUMP INFORMATION RECORD

#### DMPINREC Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    DMPABEND       01C4
    DMPCKCOM       00B0
    DMPCPUID       03C8
    DMPCPUTM       00A8
    DMPCRS         0040
    DMPDATE        03F4
    DMPDMPID       0434
    DMPFLAG        00B8
    DMPFPRS        0080
    DMPGPRS        0000
    DMPHALF        00B8 80
    DMPIPCS        03E4
    DMPLCORE       00C0
    DMPLEV         040F
    DMPMODEL       0420
    DMPPGMAP       01C8
    DMPPRFRG       01C0
    DMPPROCA       00BA
    DMPPSW         03D8
    DMPREL         040E
    DMPSERNO       0424
    DMPSRID        040C
    DMPSYSRM       03E0
    DMPSYSRV       00BC
    DMPTICON       041C
    DMPTOD         0414
    DMPTODCK       00A0
    DMPVMTYP       03D0

This information is based on z/VM V5R2.0. Last updated on 12 Apr 2006 at 16:38:43 EDT.
Copyright IBM Corporation, 1990, 2005