Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSTOASD

Prolog
Control Block Contents
Cross Reference

#### MRSTOASD Prolog

####

####

     DSECT NAME - STOASD
     FUNCTION - This is an event record that is created when an
                address space is deleted.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSTOASD
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 3  - Storage Domain
                        Record 13 - Address Space Deleted
     DESCRIPTION - Generated when an address space is deleted.

    MRSTOASD Control Block Contents

    Offsets
    Dec Hex  Type       Len  Name (Dim)             Description

      0   0  Structure   52  STOASD                 Start of monitor record
      0   0  Character    0  STOASD_MRHDR           Record header. See MRRECHDR
                                                    for details.
      0   0  Character   20  MRHDR
      0   0  Unsigned     2  MRHDRLEN               record length in bytes
      2   2  Unsigned     2  MRHDRZER               field of zeros
      4   4  Unsigned     1  MRHDRDM                domain identifier
      5   5  Unsigned     1  *
      6   6  Unsigned     2  MRHDRRC                record identifier
      8   8  Character    8  MRHDRTOD               Time at which this record was
                                                    built. In time-of-day (TOD)
                                                    clock format. See IBM System
                                                    370 XA Principle of Operation
                                                    for explanation of format.
     16  10  Character    4  *
     20  14  Character    0  MRHDR_END              End of header
     20  14  Character    8  STOASD_ASCUSRID        Owning userid, padded on the
                                                    right with blanks.
     28  1C  Character   24  STOASD_ASCNAME         Address space name, padded on
                                                    the right with blanks.
     52  34  Character    0  STOASD_END

    MRSTOASD Cross Reference

                          Hex           Hex
    Name                 Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    STOASD                     0     52
    STOASD_ASCNAME            1C     24
    STOASD_ASCUSRID           14      8
    STOASD_END                34      0
    STOASD_MRHDR               0      0

    This information is
    based on z/VM V5R2.0.

    Last updated on 11 Dec 2005 at 18:48:12.

    Copyright IBM Corporation, 1990, 2005