Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

#### NCABK

Prolog

Control Block Contents
NCABK DSECT

Storage Layout

Cross Reference (Contains links to field and bit definitions)

#### NCABK Prolog

     Name       : HCPNCABK
     Description: Network Card Accounting Block.
     DSECT      : NCABK
     Function   :
                  This structure contains accounting information for
                  a fully-simulated Network Interface Card (NIC).
     Located by :
                  NICNCABK - Pointer to NCABK (when accounting is enabled)
     CREATED BY :
                  COUPLE processing when the adapter is connected to a
                  VM LAN segment with ACCOUNTING enabled.
                  SET LAN processing when the adapter is connected to a
                  VM LAN segment for which ACCOUNTING is being enabled.
     DELETED BY :
                  UNCOUPLE processing when the adapter is disconnected
                  from a VM LAN segment with ACCOUNTING enabled.
                  SET LAN processing when the adapter is connected to a
                  VM LAN segment for which ACCOUNTING is being disabled.
     REFERENCES : none.
     SERIALIZED :
                  Adapter Counter Lock (NICCTRLK) must be held EXCLUSIVE
                  to update these fields.
                  Adapter Counter Lock (NICCTRLK) must be held SHARED
                  to safely reference these fields.
     NOTES      : None.
     General Note :

#### NCABK Control Block Content

#### NCABK DSECT

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      NCABK          Network Card Accounting Block.
          Linkage to associated structures.
    0000    0 Address      4 NCANICBK       Pointer to NICBK (adapter)
    0004    4 Address      4 NCALANBK       Pointer to LANBK (network)
          TOD Clock Value when first connected to the LAN
    0008    8 Dbl-Word     8 NCACONN        Connection TOD Clock
          Counters reside in this area.
    0010   16 Dbl-Word     8 NCACTRS (0)    Begin counters
          Count Unicast bytes exchanged with a NON-ROUTER.
    0010   16 Dbl-Word     8 NCATXUCN       Bytes Sent to a Non-Router
    0018   24 Dbl-Word     8 NCARXUCN       Bytes Received from a Non-Router
          Count Unicast bytes exchanged with a designated ROUTER.
            Note that the presence of the NETROUTER user directory
            option designates the user as a "ROUTER" for this
            purpose.
    0020   32 Dbl-Word     8 NCATXUCR       Bytes Sent to a Router
    0028   40 Dbl-Word     8 NCARXUCR       Bytes Received from a Router
          Count Multicast bytes exchanged.
    0030   48 Dbl-Word     8 NCATXMC        Bytes Sent via Multicast
    0038   56 Dbl-Word     8 NCARXMC        Bytes Received via Multicast
          Count Broadcast bytes exchanged.
    0040   64 Dbl-Word     8 NCATXBC        Bytes Sent via Broadcast
    0048   72 Dbl-Word     8 NCARXBC        Bytes Received via Broadcast
          Count Unicast Non-Router packets exchanged with the LAN.
    0050   80 Signed       4 NCATXUPK       Unicast Packets Sent
    0054   84 Signed       4 NCARXUPK       Unicast Packets Received
          Count Unicast Router packets exchanged with the LAN.
    0058   88 Signed       4 NCATXRPK       Router Packets Sent
    005C   92 Signed       4 NCARXRPK       Router Packets Received
          Count Multicast packets exchanged with the LAN.
    0060   96 Signed       4 NCATXMPK       Multicast Packets Sent
    0064  100 Signed       4 NCARXMPK       Multicast Packets Received
          Count Broadcast packets exchanged with the LAN.
    0068  104 Signed       4 NCATXBPK       Broadcast Packets Sent
    006C  108 Signed       4 NCARXBPK       Broadcast Packets Received
          End of NCACTRS area.
              00000060       NCACTRLN       *-NCACTRS Length of counter area
          End of Structure.
              00FFFF90       NCABKLN        NCABK-* Length in bytes
              0000000E       NCABKSZ        (*-NCABK+7)/8 Size in double
                                            words

#### NCABK Storage Layout

    *** NCABK - Network Card Accounting Block.
    *
    *     +---------------------------+---------------------------+
    *   0 |         NCANICBK          |         NCALANBK          |
    *     +---------------------------+---------------------------+
    *   8 |                       NCACONN                         |
    *     +-------------------------------------------------------+
    *  10 |                       NCATXUCN                        |
    *     +-------------------------------------------------------+
    *  18 |                       NCARXUCN                        |
    *     +-------------------------------------------------------+
    *  20 |                       NCATXUCR                        |
    *     +-------------------------------------------------------+
    *  28 |                       NCARXUCR                        |
    *     +-------------------------------------------------------+
    *  30 |                       NCATXMC                         |
    *     +-------------------------------------------------------+
    *  38 |                       NCARXMC                         |
    *     +-------------------------------------------------------+
    *  40 |                       NCATXBC                         |
    *     +-------------------------------------------------------+
    *  48 |                       NCARXBC                         |
    *     +---------------------------+---------------------------+
    *  50 |         NCATXUPK          |         NCARXUPK          |
    *     +---------------------------+---------------------------+
    *  58 |         NCATXRPK          |         NCARXRPK          |
    *     +---------------------------+---------------------------+
    *  60 |         NCATXMPK          |         NCARXMPK          |
    *     +---------------------------+---------------------------+
    *  68 |         NCATXBPK          |         NCARXBPK          |
    *     +---------------------------+---------------------------+
    *  70
    *
    *** NCABK - Network Card Accounting Block.

#### NCABK Cross Reference

    Symbol         Dspl Value
    -------------- ---- -----
    NCABKLN        006C 00FFFF90
    NCABKSZ        006C 0000000E
    NCACONN        0008
    NCACTRLN       006C 00000060
    NCACTRS        0010
    NCALANBK       0004
    NCANICBK       0000
    NCARXBC        0048
    NCARXBPK       006C
    NCARXMC        0038
    NCARXMPK       0064
    NCARXRPK       005C
    NCARXUCN       0018
    NCARXUCR       0028
    NCARXUPK       0054
    NCATXBC        0040
    NCATXBPK       0068
    NCATXMC        0030
    NCATXMPK       0060
    NCATXRPK       0058
    NCATXUCN       0010
    NCATXUCR       0020
    NCATXUPK       0050

This information is based on z/VM V6R1.0. Last updated on 18 Feb 2010 at 08:51:58 EDT.
Copyright IBM Corporation, 1990, 2008