Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSTORSP

Prolog
Control Block Contents
Cross Reference

#### MRSTORSP Prolog

     DSECT NAME - STORSP
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSTORSP
     DESCRIPTIVE NAME - Monitor Sample Record
                        Domain 3 - Storage Domain
                        Record 2 - Real Storage Activity (Per Processor)
     DESCRIPTION - Utilization of real memory on a processor basis.
                   This record is needed because free storage requests
                   are not expected to be evenly distributed across all
                   processors in a complex.  A separate record is
                   generated for each online processor.

#### MRSTORSP Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure   760  STORSP                 Start of monitor record
       0   0  Character     0  STORSP_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Unsigned      2  STORSP_PFXCPUAD        Processor address
      22  16  Unsigned      2  *                      Reserved for IBM use
      24  18  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFRECT)
      28  1C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFRET)
      32  20  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSPGXTD)
      36  24  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFSPCT)
      40  28  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSDXFRE)
      44  2C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFVRRQ)
      48  30  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFVRCT)
      52  34  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful. (STORSP_PLSFVRLS)
      56  38  Unsigned      4  STORSP_PLSPREAD        Total number of page
                                                      translations that resulted in
                                                      a page read
      60  3C  Unsigned      4  STORSP_PLSPNEW         Number of first-time
                                                      referenced page translations,
                                                      including fastpath page
                                                      faults
      64  40  Unsigned      4  STORSP_PFXCLEAR        Number of first-time
                                                      referenced fastpath page
                                                      faults
      68  44  Unsigned      4  STORSP_PFXPTRCT        Number of fast path page
                                                      translations
      72  48  Unsigned      4  STORSP_PLSRELES        Total number of times any
                                                      release function was
                                                      performed. Includes releasing
                                                      any range of virtual system
                                                      pages as well as shared pages
      76  4C  Unsigned      4  STORSP_PLSRETFR        Total number of frames that
                                                      are returned to the <2G
                                                      available list. See
                                                      STORSP_PLSRETFG for the >2G
                                                      value.
      80  50  Unsigned      4  STORSP_PLSRELFR        Total number of frames that
                                                      are returned by any release
                                                      function
      84  54  Unsigned      4  STORSP_PLSALNCT        Number of frames obtained
                                                      from the <2G available list.
                                                      See STORSP_PLSALNCG for the
                                                      >2G value.
      88  58  Unsigned      4  STORSP_PLSSTLWT        Count of frame replacement
                                                      writes pending that are
                                                      requested by the available
                                                      list replenishment demand
                                                      scan
      92  5C  Unsigned      4  *                      Reserved for IBM use
      96  60  Character    24  *
      96  60  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSLTD1).
     100  64  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDORM1).
     104  68  Unsigned      4  *                      Reserved for IBM use
     108  6C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSSHAR1).
     112  70  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELIG1).
     116  74  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDISP1).
     120  78  Character    16  *
     120  78  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSLTD2).
     124  7C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDORM2).
     128  80  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELIG2).
     132  84  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDISP2).
     136  88  Character    20  *
     136  88  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSSHARE).
     140  8C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDORME).
     144  90  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELIGE).
     148  94  Unsigned      4  *                      Reserved for IBM use
     152  98  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDISPE).
     156  9C  Character    24  *
     156  9C  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSLTDP1).
     160  A0  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDRMP1).
     164  A4  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSSHRP1).
     168  A8  Unsigned      4  *                      Reserved for IBM use
     172  AC  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDSPP1).
     176  B0  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELGP1).
     180  B4  Character    20  *
     180  B4  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSLTDP2).
     184  B8  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDRMP2).
     188  BC  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSSHRP2).
     192  C0  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDSPP2).
     196  C4  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELGP2).
     200  C8  Character    20  *
     200  C8  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDRMPE).
     204  CC  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaninful (STORSP_PLSSHRPE).
     208  D0  Unsigned      4  *                      Reserved for IBM use
     212  D4  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSDSPPE).
     216  D8  Unsigned      4  *                      Reserved for IBM use.
                                                      Previous field is no longer
                                                      meaningful (STORSP_PLSELGPE).
     220  DC  Unsigned      4  *                      Reserved for IBM use
     224  E0  Unsigned      4  *                      Reserved for IBM use
     228  E4  Unsigned      4  *                      Reserved for IBM use
     232  E8  Unsigned      4  *                      Reserved for IBM use
     236  EC  Unsigned      4  STORSP_PLSPGDRD        Number of page table
                                                      translations that resulted in
                                                      a page read from auxiliary
                                                      storage (DASD)
     240  F0  Unsigned      4  STORSP_PLSPGDWT        Number of page tables paged
                                                      to auxiliary storage (DASD)
     244  F4  Unsigned      4  STORSP_PLSALNCG        Number of frames obtained
                                                      from the >2G available list.
                                                      See See STORSP_PLSALNCT for
                                                      the <2G value.
     248  F8  Unsigned      4  STORSP_PLSRETFG        Total number of frames that
                                                      are returned to the >2G
                                                      available list. See
                                                      STORSP_PLSRETFR for the <2G
                                                      value.
     252  FC  Unsigned      4  STORSP_PLSFSPRB        Total number of free
                                                      storage pages returned backed
                                                      below 2G.
     256 100  Unsigned      4  STORSP_PLSFSPRA        Total number of free
                                                      storage pages returned backed
                                                      above 2G.
     260 104  Unsigned      4  STORSP_PLSFSCTB        Count of free storage
                                                      obtains backed below 2G.
     264 108  Unsigned      4  STORSP_PLSFSCTA        Count of free storage
                                                      obtains backed above 2G.
     268 10C  Unsigned      4  STORSP_PLSFRETB        Count of free storage
                                                      returns backed below 2G.
     272 110  Unsigned      4  STORSP_PLSFRETA        Count of free storage
                                                      returns backed above 2G.
     276 114  Unsigned      4  STORSP_PLSFSSGB        Count of regular free
                                                      storage obtains backed below
                                                      2G.
     280 118  Unsigned      4  STORSP_PLSFSSGA        Count of regular free
                                                      storage obtains backed above
                                                      2G.
     284 11C  Unsigned      4  STORSP_PLSFSPGB        Count of free storage page
                                                      requests backed below 2G.
     288 120  Unsigned      4  STORSP_PLSFSPGA        Count of free storage page
                                                      requests backed any.
     292 124  Unsigned      4  STORSP_PLSBGCNT        Number of times the
                                                      background replenishment of
                                                      the Cleared Global Available
                                                      List has run.
     296 128  Character     8  STORSP_PLSFGCTM        Amount of raw CPU time
                                                      spent performing foreground
                                                      replenishment of the Cleared
                                                      Global Available List.
     304 130  Unsigned      4  STORSP_PLSFGCNT        Number of times foreground
                                                      replenishment of the Cleared
                                                      Global Available List has
                                                      run.
     308 134  Unsigned      4  STORSP_PLSFOBEM        Unsigned count of times the
                                                      FCP Operations Block (FOB)
                                                      list for this processor was
                                                      empty when a FOB was
                                                      requested since the list was
                                                      last trimmed.
     312 138  Unsigned      4  STORSP_PLSFSSRA        Count of regular subpool
                                                      free storage returns backed
                                                      >2G.
     316 13C  Unsigned      4  STORSP_PLSFSSRB        Count of regular subpool
                                                      free storage returns backed
                                                      <2G.
     320 140  Unsigned      4  STORSP_PLSVATCL        Count of guest virtual to
                                                      host logical address
                                                      translations.
     324 144  Unsigned      4  STORSP_PLSUPAGE        Number of Collaborative
                                                      Memory Management unused
                                                      pages whose frames were
                                                      reclaimed.
     328 148  Unsigned      4  STORSP_PLSVPAGE        Number of Collaborative
                                                      Memory Management volatile
                                                      pages whose frames were
                                                      reclaimed.
     332 14C  Unsigned      4  STORSP_PLSPCPAG        Number of Collaborative
                                                      Memory Management
                                                      potentially-volatile changed
                                                      pages converted to stable
                                                      before being made IBR.
     336 150  Unsigned      4  STORSP_PLSPUPAG        Number of Collaborative
                                                      Memory Management
                                                      potentially-volatile
                                                      unchanged pages whose frames
                                                      were reclaimed.
     340 154  Unsigned      4  *                      Reserved for IBM use - was
                                                      STORSP_PLSUPREC
     344 158  Unsigned      4  STORSP_PLSESSA         ESSA instruction count
     348 15C  Unsigned      4  STORSP_PLSLTDPE        Number of long term dormant
                                                      emergency passes.
     352 160  Unsigned      4  STORSP_PLSASFCL        Count of times a single
                                                      frame request <2G took a
                                                      frame from the <2G contiguous
                                                      frame available list.
     356 164  Unsigned      4  STORSP_PLSASFCG        Count of times a single
                                                      frame request >2G took a
                                                      frame from the >2G contiguous
                                                      frame available list.
     360 168  Unsigned      1  STORSP_PFXCPUTY        CPU Type. Valid values:
                                                      X'00' - General Purpose (CP)
                                                      X'02' - zSeries Application
                                                      Assist (zAAP) X'03' -
                                                      Integrated Facility for Linux
                                                      (IFL) X'04' - Internal
                                                      Coupling Facility (ICF) X'05'
                                                      - zSeries Integrated
                                                      Information (zIIP)
     361 169  Character     3  *                      Reserved for IBM use
     364 16C  Character    60  *                      QDIO stats
     364 16C  Unsigned      4  STORSP_PFXAFOBC        Local List (LL) count of
                                                      FOBs
     368 170  Unsigned      4  STORSP_PLSFOBLO        LL low threshold
     372 174  Unsigned      4  STORSP_PLSFOBHI        LL high threshold
     376 178  Character     8  STORSP_PLSFOB1E        count of times LL found
                                                      empty
     384 180  Character     8  STORSP_PLSFOB1T        TOD 1st trim request for LL
     392 188  Character     8  STORSP_PLSFOBTM        TOD most recent trim req
                                                      for LL
     400 190  Character     8  *                      Reserved for IBM
     408 198  Character     8  *                      Reserved for IBM
     416 1A0  Character     8  *                      Reserved for IBM
     424 1A8  Unsigned      4  *                      Reserved for IBM use - was
                                                      STORSP_PLSPPGM1.
     428 1AC  Unsigned      4  *                      Reserved for IBM use - was
                                                      STORSP_PLSPPGM2.
     432 1B0  Unsigned      4  *                      Reserved for IBM use - was
                                                      STORSP_PLSPPGME.
     436 1B4  Unsigned      4  STORSP_PLSSTPAG        Number of IBR pages found
                                                      in the Collaborative Memory
                                                      Management stable and
                                                      logically zero state whose
                                                      old frames were reclaimed.
     440 1B8  Unsigned      4  STORSP_PLSNDMRQ        Count of NDMBKs that have
                                                      been requested from the NDMBK
                                                      recycle queues, whether
                                                      satisfied or not.
     444 1BC  Unsigned      4  STORSP_PLSNDMLO        Count of NDMBKs that have
                                                      been requested from the NDMBK
                                                      recycle queues and were
                                                      supplied from this CPU's
                                                      local NDMBK recycle queue.
     448 1C0  Unsigned      4  STORSP_PLSNDMGL        Count of NDMBKs that have
                                                      been requested from the NDMBK
                                                      recycle queues and were
                                                      supplied from the global
                                                      NDMBK recycle queue.
     452 1C4  Unsigned      4  STORSP_PLSNDMG2L       Count of NDMBKs that have
                                                      been moved from the global
                                                      NDMBK recycle queue to this
                                                      CPU's local NDMBK recycle
                                                      queue.
     456 1C8  Unsigned      4  STORSP_PLSNDMDX        Count of times a task has
                                                      returned a chain of NDMBKs to
                                                      the local NDMBK recycle
                                                      queue.
     460 1CC  Unsigned      4  STORSP_PLSNDMRET       Total count of NDMBKs that
                                                      have been returned to this
                                                      CPU's local NDMBK recycle
                                                      queue.
     464 1D0  Unsigned      4  STORSP_PLSNDML2G       Count of NDMBKs that have
                                                      been moved from this CPU's
                                                      local NDMBK recycle queue to
                                                      the global NDMBK recycle
                                                      queue because the local NDMBK
                                                      recycle queue was above its
                                                      high threshold.
     468 1D4  Unsigned      4  STORSP_PLSNDMREL       Count of NDMBKs that have
                                                      been returned to free storage
                                                      because both this CPU's local
                                                      NDMBK recycle queue and the
                                                      global NDMBK recycle queue
                                                      were above their high
                                                      thresholds.
     472 1D8  Unsigned      4  STORSP_PLSNDMREC       Count of times a local
                                                      reclaim task has been
                                                      initiated on this CPU.
     476 1DC  Unsigned      4  STORSP_PLSNDMRND       Count of NDMBKs that have
                                                      been returned to free storage
                                                      because a local reclaim task
                                                      was initiated on this CPU.
                                                      *****************************
                                                      ****************************
                                                      Cleared Local Available list
                                                      and Fast Path Page Fault
                                                      resolution stats.
                                                      *****************************
                                                      ****************************
     480 1E0  Unsigned      4  STORSP_PFXCLPLCNT      Count of frames on the
                                                      cleared local available list
                                                      plus the count of frames on
                                                      the firmware processed list.
     484 1E4  Unsigned      4  STORSP_PLSCLALLO       Cleared local available
                                                      list low threshold.
     488 1E8  Unsigned      4  STORSP_PLSCLALHI       Cleared local available
                                                      list high threshold.
     492 1EC  Character     8  STORSP_PLSCLALADDED    Number of frames that were
                                                      added to the cleared local
                                                      available list. Decremented
                                                      only when a processor goes
                                                      offline or is parked.
     500 1F4  Character     8  STORSP_PLSCLALFWREMOVED Number of frames that
                                                      were removed from the cleared
                                                      local available list and
                                                      added to the processed list
                                                      by the firmware. These would
                                                      be considered ideal success
                                                      cases of the CLAL.
     508 1FC  Character     8  STORSP_PLSCLALTRIMMED  Number of frames that were
                                                      trimmed from the cleared
                                                      local available list when it
                                                      was found over its high
                                                      threshold.
     516 204  Character     8  STORSP_PLSFPPFENTERED  Number of times fast path
                                                      page fault processing was
                                                      entered for a guest. Does not
                                                      include VSIE guests.
     524 20C  Character     8  STORSP_PLSFPPFSUCCESS  Number of times fast path
                                                      page fault processing was
                                                      successful.
     532 214  Character     8  STORSP_PLSCPPFENTERED  Number of times fast path
                                                      page fault processing was
                                                      entered for CP.
     540 21C  Character     8  STORSP_PLSCPPFSUCCESS  Number of times fast path
                                                      page fault processing was
                                                      successful for CP.
     548 224  Character     8  STORSP_PLSCPPFMDC      Number of times fast path
                                                      page fault processing exited
                                                      to handle a mini-disk cache
                                                      page fault.
     556 22C  Character     8  STORSP_PLSCLALREQUESTS1 Number of times a frame
                                                      was requested from the cleared
                                                      local available list. Since
                                                      frames come off one at a time
                                                      this is also the number of
                                                      frames requested.
     564 234  Character     8  STORSP_PLSCLALUNFILLED1 Number of times a request
                                                      found the cleared local
                                                      available list empty before
                                                      attempting replenishment on
                                                      demand, if so requested.
     572 23C  Character     8  STORSP_PLSCLALREPLENOD Number of times a request
                                                      found the cleared local
                                                      available list empty and
                                                      attempted replenishment on
                                                      demand.
     580 244  Character     8  STORSP_PLSCLALUNFILLED2 Number of times a request
                                                      found the cleared local
                                                      available list empty before
                                                      attempting replenishment on
                                                      demand, if so requested.
     588 24C  Character     8  STORSP_PLSCLALREQUESTS2 Number of times a frame wa
                                                      requested from the cleared
                                                      local available list. Since
                                                      frames come off one at a time
                                                      this is also the number of
                                                      frames requested.
     596 254  Character     8  STORSP_PLSCLALUNFILLED3 Number of times a request
                                                      found the cleared local
                                                      available list empty before
                                                      attempting replenishment on
                                                      demand, if so requested.
     604 25C  Character     8  STORSP_PLSBGCTM        Amount of raw CPU time
                                                      spent performing background
                                                      replenishment of the cleared
                                                      global available list.
     612 264  Character     8  STORSP_PLSCGALREQUESTS Number of times we wanted
                                                      to move frames from the
                                                      cleared global available list
                                                      to the cleared local
                                                      available list.
     620 26C  Character     8  STORSP_PLSCGALFRAMESR  Number of frames we wanted
                                                      to move from the cleared
                                                      global available list to the
                                                      cleared local available list.
                                                      FramesR should equal
                                                      Moved+UnfilledNL+UnfilledW
     628 274  Character     8  STORSP_PLSCGALMOVED    Number of frames we moved
                                                      from the cleared global
                                                      available list to the cleared
                                                      local available list.
     636 27C  Character     8  STORSP_PLSCGALNOLOCK   Number of times we could
                                                      not move frames from the
                                                      cleared global available list
                                                      to the cleared local
                                                      available list because the
                                                      CGAL lock was not immediately
                                                      available. (Already counted
                                                      as a request.)
     644 284  Character     8  STORSP_PLSCGALUNFILLEDNL Number of frames we
                                                      could not move from the
                                                      cleared global available
                                                      list to the cleared local
                                                      available list because the
                                                      CGAL lock was not
                                                      immediately available.
                                                      (Already counted in
                                                      requests.)
     652 28C  Character     8  STORSP_PLSCGALWANTING  Number of times the cleared
                                                      global available list did not
                                                      have enough frames for a
                                                      request. (Already counted as
                                                      request.)
     660 294  Character     8  STORSP_PLSCGALUNFILLEDW Number of frames we could
                                                      not move from the cleared
                                                      global available list to the
                                                      cleared local available list
                                                      because the CGAL lock was not
                                                      immediately available.
                                                      (Already counted in
                                                      requests.)
     668 29C  Unsigned      4  STORSP_PLSULALCNT      Count of frames on the
                                                      uncleared local available
                                                      list.
     672 2A0  Unsigned      4  STORSP_PLSULALLO       Uncleared local available
                                                      list low threshold.
     676 2A4  Unsigned      4  STORSP_PLSULALHI       Uncleared local available
                                                      list high threshold.
     680 2A8  Character     8  STORSP_PLSULALREQUESTS1 Number of times a frame
                                                      was requested from the uncleared
                                                      local available list. Since
                                                      frames come off one at a time
                                                      this is also the number of
                                                      frames requested.
     688 2B0  Character     8  STORSP_PLSULALUNFILLED1 Number of times a request
                                                      found the uncleared local
                                                      available list empty before
                                                      attempting replenishment on
                                                      demand, if so requested.
     696 2B8  Character     8  STORSP_PLSULALREPLENOD Number of times a request
                                                      found the uncleared local
                                                      available list empty and
                                                      attempted replenishment on
                                                      demand.
     704 2C0  Character     8  STORSP_PLSULALUNFILLED2 Number of times a request
                                                      found the uncleared local
                                                      available list empty before
                                                      attempting replenishment on
                                                      demand, if so requested.
     712 2C8  Character     8  STORSP_PLSSWPROCLCNT   Count of frames on the
                                                      software processed list.
     720 2D0  Unsigned      4  STORSP_PLSENCRYPTPAGES Cumulative number of pages
                                                      encrypted by the paging
                                                      subsystem
     724 2D4  Unsigned      4  STORSP_PLSDECRYPTPAGES Cumulative number of pages
                                                      decrypted by the paging
                                                      subsystem
     728 2D8  Character     8  STORSP_PLSENCPTCPUTIME Cumulative raw CPU Time
                                                      spent doing page encryption
                                                      for the paging subsystem in
                                                      TOD clock units
     736 2E0  Character     8  STORSP_PLSDECPTCPUTIME Cumulative raw CPU Time
                                                      spent doing page decryption
                                                      for the paging subsystem in
                                                      TOD clock units
     744 2E8  Unsigned      4  STORSP_PLSLTPINMOVED   Number of times a page was
                                                      moved from reconfigurable to
                                                      permanent storage prior to a
                                                      long-term first pin.
     748 2EC  Unsigned      4  STORSP_PLSLTPINNOTMOVED Number of times a page
                                                      was long-term first pinned in
                                                      reconfigurable storage.
     752 2F0  Unsigned      4  STORSP_PLSPINWHILEVACATE Number of times a page
                                                      was first pinned (long or short)
                                                      in reconfigurable storage being
                                                      vacated.
     756 2F4  Unsigned      4  STORSP_PLSLTPINNOTFIRST Number of times a
                                                      long-term pin was performed for
                                                      a page that was already pinned
                                                      in reconfigurable storage.
     760 2F8  Character     0  STORSP_END

#### MRSTORSP Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    STORSP                     0    760
    STORSP_END               2F8      0
    STORSP_MRHDR               0      0
    STORSP_PFXAFOBC          16C      4
    STORSP_PFXCLEAR           40      4
    STORSP_PFXCLPLCNT        1E0      4
    STORSP_PFXCPUAD           14      2
    STORSP_PFXCPUTY          168      1
    STORSP_PFXPTRCT           44      4
    STORSP_PLSALNCG           F4      4
    STORSP_PLSALNCT           54      4
    STORSP_PLSASFCG          164      4
    STORSP_PLSASFCL          160      4
    STORSP_PLSBGCNT          124      4
    STORSP_PLSBGCTM          25C      8
    STORSP_PLSCGALFRAMESR    26C      8
    STORSP_PLSCGALMOVED      274      8
    STORSP_PLSCGALNOLOCK     27C      8
    STORSP_PLSCGALREQUESTS   264      8
    STORSP_PLSCGALUNFILLEDNL 284      8
    STORSP_PLSCGALUNFILLEDW  294      8
    STORSP_PLSCGALWANTING    28C      8
    STORSP_PLSCLALADDED      1EC      8
    STORSP_PLSCLALFWREMOVED  1F4      8
    STORSP_PLSCLALHI         1E8      4
    STORSP_PLSCLALLO         1E4      4
    STORSP_PLSCLALREPLENOD   23C      8
    STORSP_PLSCLALREQUESTS1  22C      8
    STORSP_PLSCLALREQUESTS2  24C      8
    STORSP_PLSCLALTRIMMED    1FC      8
    STORSP_PLSCLALUNFILLED1  234      8
    STORSP_PLSCLALUNFILLED2  244      8
    STORSP_PLSCLALUNFILLED3  254      8
    STORSP_PLSCPPFENTERED    214      8
    STORSP_PLSCPPFMDC        224      8
    STORSP_PLSCPPFSUCCESS    21C      8
    STORSP_PLSDECPTCPUTIME   2E0      8
    STORSP_PLSDECRYPTPAGES   2D4      4
    STORSP_PLSENCPTCPUTIME   2D8      8
    STORSP_PLSENCRYPTPAGES   2D0      4
    STORSP_PLSESSA           158      4
    STORSP_PLSFGCNT          130      4
    STORSP_PLSFGCTM          128      8
    STORSP_PLSFOBEM          134      4
    STORSP_PLSFOBHI          174      4
    STORSP_PLSFOBLO          170      4
    STORSP_PLSFOBTM          188      8
    STORSP_PLSFOB1E          178      8
    STORSP_PLSFOB1T          180      8
    STORSP_PLSFPPFENTERED    204      8
    STORSP_PLSFPPFSUCCESS    20C      8
    STORSP_PLSFRETA          110      4
    STORSP_PLSFRETB          10C      4
    STORSP_PLSFSCTA          108      4
    STORSP_PLSFSCTB          104      4
    STORSP_PLSFSPGA          120      4
    STORSP_PLSFSPGB          11C      4
    STORSP_PLSFSPRA          100      4
    STORSP_PLSFSPRB           FC      4
    STORSP_PLSFSSGA          118      4
    STORSP_PLSFSSGB          114      4
    STORSP_PLSFSSRA          138      4
    STORSP_PLSFSSRB          13C      4
    STORSP_PLSLTDPE          15C      4
    STORSP_PLSLTPINMOVED     2E8      4
    STORSP_PLSLTPINNOTFIRST  2F4      4
    STORSP_PLSLTPINNOTMOVED  2EC      4
    STORSP_PLSNDMDX          1C8      4
    STORSP_PLSNDMGL          1C0      4
    STORSP_PLSNDMG2L         1C4      4
    STORSP_PLSNDMLO          1BC      4
    STORSP_PLSNDML2G         1D0      4
    STORSP_PLSNDMREC         1D8      4
    STORSP_PLSNDMREL         1D4      4
    STORSP_PLSNDMRET         1CC      4
    STORSP_PLSNDMRND         1DC      4
    STORSP_PLSNDMRQ          1B8      4
    STORSP_PLSPCPAG          14C      4
    STORSP_PLSPGDRD           EC      4
    STORSP_PLSPGDWT           F0      4
    STORSP_PLSPINWHILEVACATE 2F0      4
    STORSP_PLSPNEW            3C      4
    STORSP_PLSPREAD           38      4
    STORSP_PLSPUPAG          150      4
    STORSP_PLSRELES           48      4
    STORSP_PLSRELFR           50      4
    STORSP_PLSRETFG           F8      4
    STORSP_PLSRETFR           4C      4
    STORSP_PLSSTLWT           58      4
    STORSP_PLSSTPAG          1B4      4
    STORSP_PLSSWPROCLCNT     2C8      8
    STORSP_PLSULALCNT        29C      4
    STORSP_PLSULALHI         2A4      4
    STORSP_PLSULALLO         2A0      4
    STORSP_PLSULALREPLENOD   2B8      8
    STORSP_PLSULALREQUESTS1  2A8      8
    STORSP_PLSULALUNFILLED1  2B0      8
    STORSP_PLSULALUNFILLED2  2C0      8
    STORSP_PLSUPAGE          144      4
    STORSP_PLSVATCL          140      4
    STORSP_PLSVPAGE          148      4

    This information is
    based on z/VM V7R2.0.

    Last updated on 03 March 2021 at 13:57:16.

    Copyright IBM Corporation, 1990, 2021