ABWSECT | Back to Index page

| Prolog Control Block Contents ABWSECT DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

ABWSECT Prolog | Top of page

     NAME       : DMSABW
     DESCRIPTION: Abend Recovery Workspace
     DSECT      : ABWSECT
     FUNCTION   : Mapping macro which maps system
                  information when an abnormal termination
                  occurs. ABWSECT describes the fields used for
                  saving registers and other data during abend
                  recovery. V-constants in DMSABE, DMSDBG,
                  DMSITI, DMSITP, and DMSITS point to the ABWSECT
                  block.

ABWSECT Control Block Content | Top of page

     ABWSECT DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      ABWSECT        Abend Recovery Workspace
    0000    0 Signed       4 ABNREGS (16)   REGS AT TIME OF ABEND
    0040   64 Dbl-Word     8 ABNPSW         PSW AT TIME OF ABEND
    0048   72 Signed       4 ABNRR          TEMP SAVE AREA
    004C   76 Signed       4 ABNPAS13 (18)  AREA PASSED TO NUCLEUS ROUTINES
    0094  148 Character   96 ABNCMSG        CONSOLE MESSAGE SAVE AREA FOR
                                            IPCS
    00F4  244 Signed       4 ABNUWRD        ABEND EXIT USER WORD
    00F8  248 Signed       4 ABNCODE        ABEND CODE
          SPACE FOR DMSMSG PLISTS
    004C   76 Bitstring    1 ABNERLST (62)
    008A  138 Signed       2 * (0)
    00FC  252 Signed       4 ABNLENPL       LENGTH OF THE TOKENIZED PLIST
                                            USED BY DMSABE AND DMSINT.
    0100  256 Character    8 ABNSCBN        USED TO SAVE A NUCLEUS EXTENSION
                                            NAME TEMPORARILY.
    0108  264 Dbl-Word     8 ABNVSTAT       VECTOR STATUS REGISTER
    0110  272 Dbl-Word     8 ABNFREGS (4)   FLOATING POINT REGISTER SAVE AREA
    0130  304 Dbl-Word     8 ABNOPSWS (5)   OLD PSW FIELDS ESA/390
    0158  344 Address      1 ABNFLAG1       FLAG BYTE
              1... ....      ABNVSAVE       X'80' ABNVSAVE VECTOR FACILITY
                                            WAS IN USE
              .1.. ....      ABNVSERR       X'40' ABNVSERR ERROR SAVING
                                            VECTOR STATUS REG
              ..1. ....      ABNDUMPA       X'20' ABNDUMPA SET AUTODUMP ALL
              ...1 ....      ABNDUMPC       X'10' ABNDUMPC SET AUTODUMP CMS
              .... 1...      ABNNODMP       X'08' ABNNODMP Tell DMSDIE not to
                                            dump
              .... .1..      ABNNOFLU       X'04' ABNNOFLU Tell DMSDIE not to
                                            flush buffer
              .... ..1.      ABNDUMPE       X'02' ABNDUMPE ENTIREVM option on
                                            SET AUTODUMP
              .... ...1      ABNSTRT        X'01' ABNSTRT Indicate Dump
                                            Started
    0159  345 Bitstring    1 ABNABEND       SYSTEM OR USER OS/MVS SIM ABEND
              ..1. ....      ABNSYST        X'20' ABNSYST SYSTEM ABEND -
                                            MESSAGE 148
              ...1 ....      ABNUSER        X'10' ABNUSER USER ABEND -
                                            MESSAGE 155
    015A  346 Bitstring    1 ABNEXAID       Access register id from low store
    015B  347 Bitstring    1 ABNPILC        Contains the ILC associated with
                                            the XA or XC PSW at the time of
                                            abend. 370 BC PSW has ILC in PSW.
          ABNDPLST is a Dump Address Parameter List used by the
          AUTODUMP command.  It contains the list of addresses which
          are to be included within the VMDUMP.
          The default plist now dumps 3 locations : DMSNUC, Loader
          Tables and the Storage management work area along with the
          Page Allocation Table.  The addresses of the areas are
          established during initialization.
          If the ENTIREVM option is specified on the AUTODUMP command
          ABNDPLST will be set up to dump the entire virtual machine.
          In this case ABNDNUM will be set to 1 and only the first
          address pair is used. ABNNUCST remains zero and ABNNUCND
          is set to VMSIZE-1. Additionally, specifying the ENTIREVM
          option will dump all discontiguous saved segments in use
          by the virtual machine.
          This info is listed under the DIAG X'94' instruction.
    015C  348 Signed       4 ABNDPLST (0)   Dump Address Parameter List
    015C  348 Address      4 *              Ptr to next list
    0160  352 Signed       4 ABNDNUM        Number of entries in the list
              .... ..11      ABNDDEFN       3 ABNDDEFN Default number of
                                            entries
    0164  356 Bitstring    1 *              Flag byte
    0165  357 Bitstring    7 *              Reserved fields Start of address
                                            list
    016C  364 Address      4 ABNNUCST       Start of DMSNUC (location 0)
    0170  368 Address      4 ABNNUCND       End of DMSNUC (or VMSIZE-1)
    0174  372 Address      4 ABNPAT         Start of PAT
    0178  376 Address      4 ABNFRWRK       End of FRWRK
    017C  380 Address      4 ABNLDRST       Start of loader tables
    0180  384 Address      4 ABNLDRND       End of loader tables
          DMSABEDP issues DIAG X'94' using the below parameter list
          with a length of ANBDPLN for the default AUTODUMP and the
          below parameter list with a length of ABNDPLNA when the
          ENTIREVM option is specified.
    0184  388 Character    8 ABNDPCMD       DUMP ' VMDUMP command plist
    018C  396 Address      4 *              Ptr to Dump Address Parameter
                                            List
    0190  400 Character   11 *              CMS DUMP
              00000017       ABNDPLN        *-ABNDPCMD Length of VMDUMP
                                            command plist
    019B  411 Character    4 *              AND ANY ADDRESSABLE DCSSS
              0000001B       ABNDPLNA       *-ABNDPCMD Length of second
                                            command plist
    019F  415 Character   20 ABNDBUFF       Diag x'08' output buff
    01B3  435 Character   12 ABNDNCON       CLOSE' Close spool
    01B5  437 Character   10 ABNDCON        on 'NOCONT CLOSE' plist
           STRUCTUR PLIST area
    01C0  448 Dbl-Word     8 STRPLIST (0)
    01C0  448 Character    8 *
    01C8  456 Character    8 *
    01D0  464 Character   16 *
    01E0  480 Address      4 *
    01E4  484 Address      1 *
    01E5  485 Address      1 *
    01E6  486 Address      1 *
    01E7  487 Address      1 *
    01E8  488 Address      4 *
    01EC  492 Address      4 *
    01F0  496 Address      4 *
    01F4  500 Bitstring    4 *
    01F8  504 Bitstring    8 *
           STRUCTUR data areas
    0200  512 Signed       4 THISEXIS
    0204  516 Signed       4 OLDEXIS
           -------- SPS & DELETE NAMEDEF PLISTS --------
           BOTH PLISTS SHARE THE SAME STORAGE SINCE THEIR STRUCTURE
           IS IDENTICAL.
    0208  520 Signed       4 ABNSPSPL (0)   SPS REQUEST PARAMETER LIST
    0208  520 Address      4 ABNSPSCA       ADDR OF SPSCA
    020C  524 Address      4 ABNWKUTA       ADDR OF 'ALL WORKUNITS' INDICATOR
    0208  520 Signed       4 ABNNDFPL (0)   DELETE NAMEDEF PLIST
    0208  520 Address      4 ABNNDANC       NAMEDEF CHAIN ANCHOR
    020C  524 Address      4 ABNNDTYP       NAMEDEF CHAIN TYPE (DIRID/FN FT)
           -------- PLIST AREA --------
    0210  528 Signed       4 ABNCSLPL (0)   CSL REQUEST PARAMETER LIST
    0210  528 Address      4 ABNFNCPM       FUNCTION NAME POINTER
    0214  532 Address      4 ABNRETPM       RETURN CODE POINTER
    0218  536 Address      4 ABNREAPM       REASON CODE POINTER,
    021C  540 Address      4 ABNPARM1       1ST USER PARM
    0220  544 Address      4 ABNPARM2       2ND USER PARM
    0224  548 Address      4 *              RESERVED FOR FUTURE IBM USE
            -------- PARAMETERS --------
    0228  552 Signed       4 ABNRETCD       RETURN CODE
    022C  556 Signed       4 ABNREASN       REASON CODE
    0230  560 Character    8 ABNFUNCT       FUNCTION NAME
    0238  568 Signed       4 ABNACTN        ACTION
            Access register information:
    023C  572 Signed       4 ABNAREGS (16)  Access registers at time of abend
    027C  636 Signed       4 ABNTXCP        Access reg. ALET from low store.
                                            (See ABNEXAID above also.)
              00000044       ABNXCLEN       *-ABNAREGS Defines the length of
                                            XC-mode virtual machine areas.
    0280  640 Bitstring    1 ABNTM          Contains the translation mode, AR
                                            or primary, at the time of a
                                            DMSABN macro that was a BALR xfer
              .... ..1.      ABNARM         X'02' Bit 22 of ABNTM is AR-mode
                                            bit
    0281  641 Bitstring    1 ABNKEY         Contains the key at the time of
                                            abend. Used by BALR entries to
                                            DMSABE.
    0282  642 Bitstring    2 ABNINT         Interrupt code stored by DMSITP
                                            if SVC caused, contains SVC code
    0284  644 Bitstring    1 ABNFLSDW       Flag used to indicate SDWA relatd
                                            events, used to setup CMS SDWA
              1... ....      ABNMCKAB       X'80' Indicates abend caused by
                                            MCH Chk
              .1.. ....      ABNPCKAB       X'40' Indicates abend caused by
                                            PGM Chk
              ...1 ....      ABNSVCAB       X'10' Indicates abend initiated
                                            via SVC either by DMSABN or ABEND
                                            macro
    0285  645 Bitstring    1 ABNF2SDW       Flag2 used to indicate SDWA
                                            related information to ABNEXIT
                                            rtn.
              1... ....      ABNFSPRL       X'80' Indicates that the failing
                                            storage page within the Data
                                            Space identifd by the ABNASIT
                                            field has been released. This may
                                            be set prior to invoking the
                                            ABNEXIT rtn, indicating CMS has
                                            already done the release. If CMS
                                            couldn't do the rel, the exit
                                            should do it and set the flag.
                                            This is applicable to X'1F4' and
                                            X'1F5' abends.
    0286  646 Bitstring    2 *              Reserved for IBM use
    0288  648 Signed       4 ABNSDERR (0)
    0288  648 Address      4 *              EXTERROR address
    028C  652 Address      4 *              SPSCA address
    0290  656 Address      4 *              SPS return code
    0294  660 Address      4 *              Output reason code
    0298  664 Address      4 *              Address of parameter
    029C  668 Signed       4 * (18)         Savearea
    02E4  740 Signed       4 ABNABNRC       Reason code at time of abend
    02E8  744 Bitstring    8 ABNASIT        Contains identity of data space
                                            that had storage check.
    02F0  752 Signed       4 ABNFSA         For storage chks in a data space,
                                            this field contains the failing
                                            storage address. It can be used
                                            to determine the page address in
                                            which the error occured.
    02F4  756 Address      4 ABNSDWA        Address of CMS SDWA that was
                                            allocated during CMS initializtn
    02F8  760 Signed       4 ABNRELAL       ALET that is used to release Data
                                            Space storage
    02FC  764 Bitstring    1 ABNMCIC (8)    Contains MCIC when abend initiatd
                                            by machine chk
    0308  776 Dbl-Word     8 ABNALSWK (0)
    0320  800 Signed       4 ABNABEDP (0)   Plist for dumping in DMSABEDP
    0320  800 Signed       4 ABNDICT        Dictionary item number
    0324  804 Address      4 ABNDIAGA       Diag X'94' plist addr
    0328  808 Bitstring    2 ABNDIAGL       Diag X'94' plist length
    032A  810 Bitstring    1 ABNFLAG        Flag byte
              1... ....      ABNDATSP       X'80' ABNDATSP Dump data spaces
              .1.. ....      ABNTRAP        X'40' ABNTRAP Dumping for TRAPMSG
              ..1. ....      ABNITPMS       X'20' ABNITPMS When on indicates
                                            DMSITP did not put out abend
                                            message
              ...1 ....      ABNITPSV       X'10' ABNITPSV Save ABNITPMS
                                            while user exit routines are
                                            running
    032B  811 Bitstring    1 *              Reserved for future use
    032C  812 Bitstring    1 ABNERDP (62)
    036A  874 Signed       2 * (0)
    036A  874 Bitstring    2 *              Need for save area overlay
    036C  876 Signed       4 ABNSAV13 (18)  Another save area
           -------- DMSJFX PARMS --------
    03B4  948 Character    1 ABNSELTY       Select type. A=close all
    03B5  949 Character    1 ABNFILTV       Filter value - immaterial
    03B6  950 Character    2 *              Reserved for future use
    03B8  952 Address      4 ABNAWUER       Address of Wuerror (none)
    03BC  956 Signed       4 ABNJFXP (0)    Address of DMSJFX plist
    03BC  956 Address      4 ABNJFXRC       Address of return code
    03C0  960 Address      4 ABNJFXRS       Address of reason code
    03C4  964 Address      4 ABNJFXST       Address of Select Type
    03C8  968 Address      4 ABNJFXFV       Address of Filter Value
    03CC  972 Address      4 ABNJFXAW       Address of Address of Wuerror
    03D0  976 Character    8 ABNCALLE       DMSITP msg 141T name of calling
                                            program
    03D8  984 Address      4 ABNPLCMD       Saved eplist address
    03DC  988 Address      4 ABNPLBEG       Saved addr of start of args
    03E0  992 Address      4 ABNPLEND       Saved addr of end of args
    03E4  996 Character  536 ABNSAVPL       SAVED TOKENIZED PLIST (CMNDLIST)
                                            USED BY DMSABE AND DMSINT.
    0600 1536 Dbl-Word     8 * (0)
    0600 1536 Bitstring   16 ABNPSWG        PSW AT TIME OF ABEND z/Arch
    0610 1552 Bitstring   16 ABNOPSWG (5)   OLD PSW FIELDS z/Arch
    0660 1632 Signed       4 ABNREGSH (16)  High REGS AT TIME OF ABEND z/Arch
    06A0 1696 Signed       4 * (16)         Reserved for IBM use

ABWSECT Storage Layout | Top of page

    *** ABWSECT - Abend Recovery Workspace
    *
    *     +-------------------------------------------------------+
    *   0 |                                                       |
    *     =                       ABNREGS                         =
    *     |                                                       |
    *     +-------------------------------------------------------+
    *  40 |                        ABNPSW                         |
    *     +---------------------------+---------------------------+
    *  48 |          ABNRR            |                           |
    *     +---------------------------+                           |
    *  50 |                                                       |
    *     =                       ABNPAS13                        =
    *     |                           +---------------------------+
    *     |                           |                           |
    *     +---------------------------+                           |
    *  98 |                                                       |
    *     =                       ABNCMSG                         =
    *     |                           +---------------------------+
    *  F0 |                           |         ABNUWRD           |
    *     +---------------------------+---------------------------+
    *  F8 |         ABNCODE           |         ABNLENPL          |
    *     +---------------------------+---------------------------+
    * 100 |                       ABNSCBN                         |
    *     +-------------------------------------------------------+
    * 108 |                       ABNVSTAT                        |
    *     +-------------------------------------------------------+
    * 110 |                                                       |
    *     =                       ABNFREGS                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 130 |                                                       |
    *     =                       ABNOPSWS                        =
    *     |                                                       |
    *     +------+------+------+------+---------------------------+
    * 158 |:FLAG1|:ABEND|:EXAID|:PILC |///////////////////////////|
    *     +------+------+------+------+------+--------------------+
    * 160 |         ABNDNUM           |//////|////////////////////|
    *     +---------------------------+------+--------------------+
    * 168 |///////////////////////////|         ABNNUCST          |
    *     +---------------------------+---------------------------+
    * 170 |         ABNNUCND          |          ABNPAT           |
    *     +---------------------------+---------------------------+
    * 178 |         ABNFRWRK          |         ABNLDRST          |
    *     +---------------------------+---------------------------+
    * 180 |         ABNLDRND          |        ABNDPCMD-          |
    *     +---------------------------+---------------------------+
    * 188 |          -(184)           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 190 |///////////////////////////////////////////////////////|
    *     |////////////////////+---------------------------+------+
    * 198 |////////////////////|///////////////////////////|      |
    *     +--------------------+---------------------------+      |
    * 1A0 |                                                       |
    *     =                       ABNDBUFF                        =
    *     |                    +----------------------------------+
    * 1B0 |                    |            ABNDNCON              |
    *     +--------------------+                           +------+
    * 1B8 |                                                |//////|
    *     +------------------------------------------------+------+
    * 1C0 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 1C8 |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 1D0 |///////////////////////////////////////////////////////|
    *     |///////////////////////////////////////////////////////|
    *     +---------------------------+------+------+------+------+
    * 1E0 |///////////////////////////|//////|//////|//////|//////|
    *     +---------------------------+------+------+------+------+
    * 1E8 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1F0 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 1F8 |///////////////////////////////////////////////////////|
    *     +---------------------------+---------------------------+
    * 200 |         THISEXIS          |         OLDEXIS           |
    *     +---------------------------+---------------------------+
    * 208 |         ABNSPSCA          |         ABNWKUTA          |
    *     +---------------------------+---------------------------+
    * 210 |         ABNFNCPM          |         ABNRETPM          |
    *     +---------------------------+---------------------------+
    * 218 |         ABNREAPM          |         ABNPARM1          |
    *     +---------------------------+---------------------------+
    * 220 |         ABNPARM2          |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 228 |         ABNRETCD          |         ABNREASN          |
    *     +---------------------------+---------------------------+
    * 230 |                       ABNFUNCT                        |
    *     +---------------------------+---------------------------+
    * 238 |         ABNACTN           |                           |
    *     +---------------------------+                           |
    * 240 |                                                       |
    *     =                       ABNAREGS                        =
    *     |                           +---------------------------+
    * 278 |                           |         ABNTXCP           |
    *     +------+------+-------------+------+------+-------------+
    * 280 |ABNTM |ABNKEY|   ABNINT    |:FLSDW|:F2SDW|/////////////|
    *     +------+------+-------------+------+------+-------------+
    * 288 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 290 |///////////////////////////|///////////////////////////|
    *     +---------------------------+---------------------------+
    * 298 |///////////////////////////|///////////////////////////|
    *     +---------------------------+///////////////////////////|
    * 2A0 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////+---------------------------+
    * 2E0 |///////////////////////////|         ABNABNRC          |
    *     +---------------------------+---------------------------+
    * 2E8 |                       ABNASIT                         |
    *     +---------------------------+---------------------------+
    * 2F0 |          ABNFSA           |         ABNSDWA           |
    *     +---------------------------+---------------------------+
    * 2F8 |         ABNRELAL          |         ABNMCIC-          |
    *     +---------------------------+---------------------------+
    * 300 |          -(2FC)           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 308 |                                                       |
    *     =                       ABNALSWK                        =
    *     |                                                       |
    *     +---------------------------+---------------------------+
    * 320 |         ABNDICT           |         ABNDIAGA          |
    *     +-------------+------+------+---------------------------+
    * 328 |  ABNDIAGL   |:FLAG |//////|                           |
    *     +-------------+------+------+                           |
    * 330 |                                                       |
    *     =                       ABNERDP                         =
    *     |             +-------------+---------------------------+
    * 368 |             |/////////////|                           |
    *     +-------------+-------------+                           |
    * 370 |                                                       |
    *     =                       ABNSAV13                        =
    *     |                           +------+------+-------------+
    * 3B0 |                           |:SELTY|:FILTV|/////////////|
    *     +---------------------------+------+------+-------------+
    * 3B8 |         ABNAWUER          |         ABNJFXRC          |
    *     +---------------------------+---------------------------+
    * 3C0 |         ABNJFXRS          |         ABNJFXST          |
    *     +---------------------------+---------------------------+
    * 3C8 |         ABNJFXFV          |         ABNJFXAW          |
    *     +---------------------------+---------------------------+
    * 3D0 |                       ABNCALLE                        |
    *     +---------------------------+---------------------------+
    * 3D8 |         ABNPLCMD          |         ABNPLBEG          |
    *     +---------------------------+---------------------------+
    * 3E0 |         ABNPLEND          |                           |
    *     +---------------------------+                           |
    * 3E8 |                                                       |
    *     =                       ABNSAVPL                        =
    *     |                           +---------------------------+
    * 5F8 |                           |///////////////////////////|
    *     +---------------------------+---------------------------+
    * 600 |                       ABNPSWG                         |
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 610 |                                                       |
    *     =                       ABNOPSWG                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 660 |                                                       |
    *     =                       ABNREGSH                        =
    *     |                                                       |
    *     +-------------------------------------------------------+
    * 6A0 |///////////////////////////////////////////////////////|
    *     =///////////////////////////////////////////////////////=
    *     |///////////////////////////////////////////////////////|
    *     +-------------------------------------------------------+
    * 6E0
    *
    *** ABWSECT - Abend Recovery Workspace

    *** Overlay for ABNPAS13 in ABWSECT
    *
    *                                 +---------------------------+
    *     ...                      4C |                           |
    *     +---------------------------+                           |
    *  50 |                                                       |
    *     =                       ABNERLST                        =
    *     |             +-----------------------------------------+
    *     |             | 8A
    *     +-------------+
    *
    *** Overlay for ABNPAS13 in ABWSECT

    *** Overlay for ABNDNCON+2 in ABWSECT
    *
    *                                        +--------------------+
    * 1B0 ...                            1B5 |      ABNDCON       |
    *     +----------------------------------+             +------+
    *     |                                                | 1BF
    *     +------------------------------------------------+
    *
    *** Overlay for ABNDNCON+2 in ABWSECT

    *** Overlay for ABNSPSPL in ABWSECT
    *
    *     +---------------------------+---------------------------+
    * 208 |         ABNNDANC          |         ABNNDTYP          |
    *     +---------------------------+---------------------------+
    * 210
    *
    *** Overlay for ABNSPSPL in ABWSECT

ABWSECT Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    ABNABEDP       0320
    ABNABEND       0159
    ABNABNRC       02E4
    ABNACTN        0238
    ABNALSWK       0308
    ABNAREGS       023C
    ABNARM         0280 02
    ABNASIT        02E8
    ABNAWUER       03B8
    ABNCALLE       03D0
    ABNCMSG        0094
    ABNCODE        00F8
    ABNCSLPL       0210
    ABNDATSP       032A 80
    ABNDBUFF       019F
    ABNDCON        01B5
    ABNDDEFN       0160 03
    ABNDIAGA       0324
    ABNDIAGL       0328
    ABNDICT        0320
    ABNDNCON       01B3
    ABNDNUM        0160
    ABNDPCMD       0184
    ABNDPLN        0190 00000017
    ABNDPLNA       019B 0000001B
    ABNDPLST       015C
    ABNDUMPA       0158 20
    ABNDUMPC       0158 10
    ABNDUMPE       0158 02
    ABNERDP        032C
    ABNERLST       004C
    ABNEXAID       015A
    ABNFILTV       03B5
    ABNFLAG        032A
    ABNFLAG1       0158
    ABNFLSDW       0284
    ABNFNCPM       0210
    ABNFREGS       0110
    ABNFRWRK       0178
    ABNFSA         02F0
    ABNFSPRL       0285 80
    ABNFUNCT       0230
    ABNF2SDW       0285
    ABNINT         0282
    ABNITPMS       032A 20
    ABNITPSV       032A 10
    ABNJFXAW       03CC
    ABNJFXFV       03C8
    ABNJFXP        03BC
    ABNJFXRC       03BC
    ABNJFXRS       03C0
    ABNJFXST       03C4
    ABNKEY         0281
    ABNLDRND       0180
    ABNLDRST       017C
    ABNLENPL       00FC
    ABNMCIC        02FC
    ABNMCKAB       0284 80
    ABNNDANC       0208
    ABNNDFPL       0208
    ABNNDTYP       020C
    ABNNODMP       0158 08
    ABNNOFLU       0158 04
    ABNNUCND       0170
    ABNNUCST       016C
    ABNOPSWG       0610
    ABNOPSWS       0130
    ABNPARM1       021C
    ABNPARM2       0220
    ABNPAS13       004C
    ABNPAT         0174
    ABNPCKAB       0284 40
    ABNPILC        015B
    ABNPLBEG       03DC
    ABNPLCMD       03D8
    ABNPLEND       03E0
    ABNPSW         0040
    ABNPSWG        0600
    ABNREAPM       0218
    ABNREASN       022C
    ABNREGS        0000
    ABNREGSH       0660
    ABNRELAL       02F8
    ABNRETCD       0228
    ABNRETPM       0214
    ABNRR          0048
    ABNSAVPL       03E4
    ABNSAV13       036C
    ABNSCBN        0100
    ABNSDERR       0288
    ABNSDWA        02F4
    ABNSELTY       03B4
    ABNSPSCA       0208
    ABNSPSPL       0208
    ABNSTRT        0158 01
    ABNSVCAB       0284 10
    ABNSYST        0159 20
    ABNTM          0280
    ABNTRAP        032A 40
    ABNTXCP        027C
    ABNUSER        0159 10
    ABNUWRD        00F4
    ABNVSAVE       0158 80
    ABNVSERR       0158 40
    ABNVSTAT       0108
    ABNWKUTA       020C
    ABNXCLEN       027C 00000044
    OLDEXIS        0204
    STRPLIST       01C0
    THISEXIS       0200

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:36:08 EDT.
Copyright IBM Corporation, 1990, 2020