$VMDBK | Back to Index page

| Prolog Control Block Contents $VMDBK DSECT Storage Layout Cross Reference (Contains links to field and bit definitions) |
Programming Interface Information: This information is NOT intended to be used as Programming Interfaces of z/VM.

$VMDBK Prolog | Top of page

     NAME       : LGRVMDBK
     DESCRIPTION: Relocation mapping for HCPVMDBK
     DSECT      : $VMDBK
     FUNCTION   : LGRVMDBK describes those fields of the VMDBK that
                  will be migrated to the destination system during
                  guest relocation.
     LOCATED BY : This is a mapping of the RDODATA area within the
                  RDOBK during guest relocation.
     RELOCATION CONSIDERATIONS : This control block is used during live guest
                  relocation.  It is used to relocate a control block
                  defined in a corresponding HCP COPY file.  Any
                  fields or bits defined in HCPVMDBK which are
                  required on the destination system must be defined
                  here, and code must be added to migrate the field
                  or bit during a relocation.

$VMDBK Control Block Content | Top of page

     $VMDBK DSECT
    Top of page

    Hex   Dec Type/Val   Lng Label (dup)    Comments
    ---- ---- --------- ---- -------------- --------
    0000    0 Structure      $VMDBK         Relocation mapping for HCPVMDBK
              00000007       $VMD_VER       7 Mapping version number
    0000    0 Signed       2 $VMD_HDRL      Header length (in bytes)
    0002    2 Signed       2 $VMD_BITL      Length of mapped bits (in bytes)
    0004    4 Signed       2 *              Reserved for future use
    0006    6 Bitstring    1 $VMD_FLGS      General flag byte
              1... ....      $VMD_BASE      X'80' $VMD_BASE Mapping is for a
                                            base VMDBK
              .1.. ....      $VMD_SUP       X'40' $VMD_SUP Copy of
                                            VMDPUST(VMDAFSUP)
              ..1. ....      $VMD_HHCR      X'20' $VMD_HHCR Indicates the
                                            guest is in ESA/390 compatibility
                                            mode and the high halves of the
                                            control registers must be saved
                                            in a buffer in case the guest
                                            does SIGP 18 code 2
    0007    7 Bitstring    1 *              Reserved for future use
              00000008       $VMD_HDLN      *-$VMDBK Length of header (bytes)
          Bit map: Contains the VMDBK flags that are subject to
                   relocation. These bits are defined sequentially,
                   regardless of how they are defined in HCPVMDBK.
                   This yields a consistent mapping that ensures
                   compatibility when a guest is relocated between
                   systems at differing service levels.
                   Names in the comments column indicate the control
                   block byte which contains the flag. This name is
                   subject to change if the flag definition changes.
             ====> NEVER change bits which already exist here.
             ====> NEVER change the order of bits in this section.
             ====> ALWAYS add new bits at the end of this section,
                   together with new flag bytes as required.
    0008    8 Signed       2 $VMD_BITS (0)  Bit map area
    0008    8 Bitstring    1 $VMD0
              1... ....      $VMDDIA4C      X'80' $VMDDIA4C VMDDIAST
              .1.. ....      $VMDUDST       X'40' $VMDUDST VMDDIAST
              ..1. ....      $VMDNETA       X'20' $VMDNETA VMDACFL
              ...1 ....      $VMDNETR       X'10' $VMDNETR VMDACFL
              .... 1...      $VMDSTOPD      X'08' $VMDSTOPD VMDCFCTL
              .... .1..      $VMDUTERM      X'04' $VMDUTERM VMDCFLAG
              .... ..1.      $VMDAUTOL      X'02' $VMDAUTOL VMDOSTAT
              .... ...1      $VMDXAUTO      X'01' $VMDXAUTO VMDOSTAT
    0009    9 Bitstring    1 $VMD1
              1... ....      $VMDSTOP       X'80' $VMDSTOP VMDCWAIT
              .1.. ....      $VMDSLEEP      X'40' $VMDSLEEP VMDCWAIT
              ..1. ....      $VMDCKST       X'20' $VMDCKST VMDCWAIT
              ...1 ....      $VMDDSCWT      X'10' $VMDDSCWT VMDCWAIT
              .... 1...      $VMDSKSLP      X'08' $VMDSKSLP VMDCWAIT
              .... .1..      $VMDBOMBA      X'04' $VMDBOMBA VMDCFOPT
              .... ..1.      $VMDBOMBE      X'02' $VMDBOMBE VMDCFOPT
              .... ...1      $VMDBOMBS      X'01' $VMDBOMBS VMDCFOPT
    000A   10 Bitstring    1 $VMD2
              1... ....      $VMDCFRUN      X'80' $VMDCFRUN VMDCFOPT
              .1.. ....      $VMDCFMCP      X'40' $VMDCFMCP VMDCFOPT
              ..1. ....      $VMDCFMCE      X'20' $VMDCFMCE VMDCFOPT
              ...1 ....      $VMDCFPCL      X'10' $VMDCFPCL VMDCFOPT
              .... 1...      $VMDNOAUT      X'08' $VMDNOAUT VMDJURNL
              .... .1..      $VMDMSGON      X'04' $VMDMSGON VMDMLVL
              .... ..1.      $VMDWNGON      X'02' $VMDWNGON VMDMLVL
              .... ...1      $VMDMCODE      X'01' $VMDMCODE VMDMLVL
    000B   11 Bitstring    1 $VMD3
              1... ....      $VMDMTEXT      X'80' $VMDMTEXT VMDMLVL
              .1.. ....      $VMDSPMSG      X'40' $VMDSPMSG VMDMLVL
              ..1. ....      $VMDMIMSG      X'20' $VMDMIMSG VMDMLVL
              ...1 ....      $VMDMCNFG      X'10' $VMDMCNFG VMDMLVL
              .... 1...      $VMDMSGIU      X'08' $VMDMSGIU VMDMIUCV
              .... .1..      $VMDWNGIU      X'04' $VMDWNGIU VMDMIUCV
              .... ..1.      $VMDEMSGI      X'02' $VMDEMSGI VMDMIUCV
              .... ...1      $VMDSMSGI      X'01' $VMDSMSGI VMDMIUCV
    000C   12 Bitstring    1 $VMD4
              1... ....      $VMDIMSGI      X'80' $VMDIMSGI VMDMIUCV
              .1.. ....      $VMDCPCOI      X'40' $VMDCPCOI VMDMIUCV
              ..1. ....      $VMDVMCOI      X'20' $VMDVMCOI VMDMIUCV
              ...1 ....      $VMDMSSVP      X'10' $VMDMSSVP VMDMSSFL
              .... 1...      $VMDMSSCS      X'08' $VMDMSSCS VMDMSSFL
              .... .1..      $VMDMSAVP      X'04' $VMDMSAVP VMDMSSFL
              .... ..1.      $VMDMSACS      X'02' $VMDMSACS VMDMSSFL
              .... ...1      $VMDPDPPF      X'01' $VMDPDPPF VMDWPEND
    000D   13 Bitstring    1 $VMD5
              1... ....      $VMDCKPSW      X'80' $VMDCKPSW VMDWPEND
              .1.. ....      $VMDPDTMR      X'40' $VMDPDTMR VMDWPEND
              ..1. ....      $VMDPDIRP      X'20' $VMDPDIRP VMDWPEND
              ...1 ....      $VMDPDCFM      X'10' $VMDPDCFM VMDWPEND
              .... 1...      $VMDPDSIE      X'08' $VMDPDSIE VMDWPEND
              .... .1..      $VMDPDTRD      X'04' $VMDPDTRD VMDWPEND
              .... ..1.      $VMDPD9CW      X'02' $VMDPD9CW VMDWPEND
              .... ...1      $VMDXTKEY      X'01' $VMDXTKEY VMDIPEND
    000E   14 Bitstring    1 $VMD6
              1... ....      $VMDEXMCK      X'80' $VMDEXMCK VMDIPEND
              .1.. ....      $VMDPTRQ       X'40' $VMDPTRQ VMDTIMER
              ..1. ....      $VMDITMRL      X'20' $VMDITMRL VMDTIMER
              ...1 ....      $VMDVPTRK      X'10' $VMDVPTRK VMDTIMER
              .... 1...      $VMDINTTR      X'08' $VMDINTTR VMDTIMER
              .... .1..      $VMDITMRI      X'04' $VMDITMRI VMDTIMER
              .... ..1.      $VMDITMOF      X'02' $VMDITMOF VMDTIMER
              .... ...1      $VMDCPUAF      X'01' $VMDCPUAF VMDCFGEM
    000F   15 Bitstring    1 $VMD7
              1... ....      $VMD8LOCK      X'80' $VMD8LOCK VMDIAGF1
              .1.. ....      $VMD8LOG       X'40' $VMD8LOG VMDIAGF1
              ..1. ....      $VMD8FAIL      X'20' $VMD8FAIL VMDIAGF1
              ...1 ....      $VMDNOFSL      X'10' $VMDNOFSL VMDIAGF2
              .... 1...      $VMDCSRMI      X'08' $VMDCSRMI VMDIAGF2
              .... .1..      $VMDNOINS      X'04' $VMDNOINS VMDIAGF2
              .... ..1.      $VMDLNKS       X'02' $VMDLNKS VMDIAGF2
              .... ...1      $VMDLNKE       X'01' $VMDLNKE VMDIAGF2
    0010   16 Bitstring    1 $VMD8
              1... ....      $VMDEXCLD      X'80' $VMDEXCLD VMDIAGF2
              .1.. ....      $VMDSHARE      X'40' $VMDSHARE VMDIAGF2
              ..1. ....      $VMDIAG98      X'20' $VMDIAG98 VMDIAGFL
              ...1 ....      $VMDLNKNP      X'10' $VMDLNKNP VMDIAGFL
              .... 1...      $VMDD84NP      X'08' $VMDD84NP VMDIAGFL
              .... .1..      $VMDSETOR      X'04' $VMDSETOR VMDIAGFL
              .... ..1.      $VMDDEVI       X'02' $VMDDEVI VMDIAGFL
              .... ...1      $VMDDEVM       X'01' $VMDDEVM VMDIAGFL
    0011   17 Bitstring    1 $VMD9
              1... ....      $VMDMCCW       X'80' $VMDMCCW VMDIAGFL
              .1.. ....      $VMDIAG88      X'40' $VMDIAG88 VMDIAGFL
              ..1. ....      $VMDSVMST      X'20' $VMDSVMST VMDRFEAT
              ...1 ....      $VMDVERP       X'10' $VMDVERP VMDRFEAT
              .... 1...      $VMDCFLF       X'08' $VMDCFLF VMDRFEAT
              .... .1..      $VMDCMSRV      X'04' $VMDCMSRV VMDRFEAT
              .... ..1.      $VMDACTRC      X'02' $VMDACTRC VMDRFEAT
              .... ...1      $VMDVTOD       X'01' $VMDVTOD VMDRFEAT
    0012   18 Bitstring    1 $VMD10
              1... ....      $VMDPAGEX      X'80' $VMDPAGEX VMDSTORE
              .1.. ....      $VMDPFTOK      X'40' $VMDPFTOK VMDSTORE
              ..1. ....      $VMDPFTK2      X'20' $VMDPFTK2 VMDSTORE
              ...1 ....      $VMDMASST      X'10' $VMDMASST VMDSTORE
              .... 1...      $VMDMAOFF      X'08' $VMDMAOFF VMDSTORE
              .... .1..      $VMDPTRQQ      X'04' $VMDPTRQQ VMDEMCTL
              .... ..1.      $VMDPTRQL      X'02' $VMDPTRQL VMDEMCTL
              .... ...1      $VMDMRG32      X'01' $VMDMRG32 VMDMMODE
    0013   19 Bitstring    1 $VMD11
              1... ....      $VMDMRG64      X'80' $VMDMRG64 VMDMMODE
              .1.. ....      $VMDMXC        X'40' $VMDMXC VMDMMODE
              ..1. ....      $VMDMESA       X'20' $VMDMESA VMDMMODE
              ...1 ....      $VMDM370       X'10' $VMDM370 VMDMMODE
              .... 1...      $VMDSETXA      X'08' $VMDSETXA VMDMFEAT
              .... .1..      $VMD370AC      X'04' $VMD370AC VMDMFEAT
              .... ..1.      $VMDVEXFP      X'02' $VMDVEXFP VMDMFEAT
              .... ...1      $VMDLIBC       X'01' $VMDLIBC VMDSTDV1
    0014   20 Bitstring    1 $VMD12
              1... ....      $VMDTZA        X'80' $VMDTZA VMDSTDV1
              .1.. ....      $VMDCRYPT      X'40' $VMDCRYPT VMDCFDIR
              ..1. ....      $VMDVAPXA      X'20' $VMDVAPXA VMDCFDIR
              ...1 ....      $VMDVAPIN      X'10' $VMDVAPIN VMDCFDIR
              .... 1...      $VMDVVECT      X'08' $VMDVVECT VMDMFEAT
              .... .1..      $VMDAPCR       X'04' $VMDAPCR VMDCFDIR
              .... ..1.      $VMDAPDED      X'02' $VMDAPDED VMDCFDIR
              .... ...1      $VMDAPMS       X'01' $VMDAPMS VMDCRYMF
    0015   21 Bitstring    1 $VMD13
              1... ....      $SHORTDAT      X'80' $SHORTDAT VMDDATFL
              .1.. ....      $FULLDATE      X'40' $FULLDATE VMDDATFL
              ..1. ....      $ISODATE       X'20' $ISODATE VMDDATFL
              ...1 ....      $SDEFAULT      X'10' $SDEFAULT VMDDATFL
              .... 1...      $VMDCLEXT      X'08' $VMDCLEXT VMDTOPTN
              .... .1..      $VMDEDIT       X'04' $VMDEDIT VMDTOPTN
              .... ..1.      $VMDATTCP      X'02' $VMDATTCP VMDTOPTN
              .... ...1      $VMDTSTAM      X'01' $VMDTSTAM VMDTOPTN
    0016   22 Bitstring    1 $VMD14
              1... ....      $VMDNOBKY      X'80' $VMDNOBKY VMDTOPTN
              .1.. ....      $VMDPFIKY      X'40' $VMDPFIKY VMDTOPTN
              ..1. ....      $VMDGSTCL      X'20' $VMDGSTCL VMDTOPTN
              ...1 ....      $VMDHLITE      X'10' $VMDHLITE VMDTOPTN
              .... 1...      $VMDCRMOR      X'08' $VMDCRMOR VMDSCREN
              .... .1..      $VMDCRHLD      X'04' $VMDCRHLD VMDSCREN
              .... ..1.      $VMDNHOLD      X'02' $VMDNHOLD VMDSCREN
              .... ...1      $VMDNULLD      X'01' $VMDNULLD VMDSCREN
    0017   23 Bitstring    1 $VMD15
              1... ....      $VMDTLEOV      X'80' $VMDTLEOV VMDTOPT2
              .1.. ....      $VMDNOCTL      X'40' $VMDNOCTL VMDTOPT2
              ..1. ....      $VMDSTAMP      X'20' $VMDSTAMP VMDTOPT2
              ...1 ....      $VMDBRMIN      X'10' $VMDBRMIN VMDTOPT2
              .... 1...      $VMDAUTCR      X'08' $VMDAUTCR VMDTOPT2
              .... .1..      $VMDCFINP      X'04' $VMDCFINP VMDTOPT2
              .... ..1.      $VMDIPSSL      X'02' $VMDIPSSL VMDIPLST
              .... ...1      $VMDIPDEV      X'01' $VMDIPDEV VMDIPLST
    0018   24 Bitstring    1 $VMD16
              1... ....      $VMDIPLOG      X'80' $VMDIPLOG VMDIPLST
              .1.. ....      $VMDIPVMI      X'40' $VMDIPVMI VMDIPLST
              ..1. ....      $VMDUNDSC      X'20' $VMDUNDSC VMDCMDOP
              ...1 ....      $VMDPSWTS      X'10' $VMDPSWTS VMDCMDOP
              .... 1...      $VMDPSWTD      X'08' $VMDPSWTD VMDCMDOP
              .... .1..      $VMDPROAP      X'04' $VMDPROAP VMDPROFL
              .... ..1.      $VMDPROTB      X'02' $VMDPROTB VMDPROFL
              .... ...1      $VMDUSECO      X'01' $VMDUSECO VMDSECF
    0019   25 Bitstring    1 $VMD17
              1... ....      $VMDDGNAU      X'80' $VMDDGNAU VMDSECU1
              .1.. ....      $VMDDGNPR      X'40' $VMDDGNPR VMDSECU1
              ..1. ....      $VMDANYAU      X'20' $VMDANYAU VMDSECU1
              ...1 ....      $VMDANYPR      X'10' $VMDANYPR VMDSECU1
              .... 1...      $VMDANYMC      X'08' $VMDANYMC VMDSECU1
              .... .1..      $VMDDGNMC      X'04' $VMDDGNMC VMDSECU1
              .... ..1.      $VMDCMESA      X'02' $VMDCMESA VMDCMODE
              .... ...1      $VMDCMLIN      X'01' $VMDCMLIN VMDCMODE
    001A   26 Bitstring    1 $VMD18
              1... ....      $VMDCMVM       X'80' $VMDCMVM VMDCMODE
              .1.. ....      $VMDCMCF       X'40' $VMDCMCF VMDCMODE
              ..1. ....      $VMDFAUTO      X'20' $VMDFAUTO VMDCCWOP
              ...1 ....      $VMDNOP        X'10' $VMDNOP VMDCCWOP
              .... 1...      $VMDQDSPU      X'08' $VMDQDSPU VMDSCDF1
              .... ..1.      $VMDMXSHA      X'02' $VMDMXSHA VMDSCDF3
              .... ...1      $VMDNMSHA      X'01' $VMDNMSHA VMDSCDF3
    001B   27 Bitstring    1 $VMD19
              1... ....      $VMDIUANY      X'80' $VMDIUANY VMDAPPCF
              .1.. ....      $VMDIUALL      X'40' $VMDIUALL VMDAPPCF
              ..1. ....      $VMDWKRUN      X'20' $VMDWKRUN VMDWRKLL
              ...1 ....      $VMDCHVSP      X'10' $VMDCHVSP VMDCCWOP
              .... 1...      $VMDAMDIR      X'08' $VMDAMDIR VMDMONFA
              .... .1..      $VMDAPBUF      X'04' $VMDAPBUF VMDMONFA
              .... ..1.      $VMDMONEU      X'02' $VMDMONEU VMDMONST
              .... ...1      $VMDMONSD      X'01' $VMDMONSD VMDMONST
    001C   28 Bitstring    1 $VMD20
              1... ....      $VMDMONEC      X'80' $VMDMONEC VMDMONST
              .1.. ....      $VMDMONTV      X'40' $VMDMONTV VMDMONST
              ..1. ....      $VMDMONSV      X'20' $VMDMONSV VMDMONST
              ...1 ....      $VMDSIGAC      X'10' $VMDSIGAC VMDMSTAT
              .... 1...      $VMDPQDBA      X'08' $VMDPQDBA VMDPXFL1
              .... .1..      $VMDPESIA      X'04' $VMDPESIA VMDPXFL1
              .... ..1.      $VMDPSIDA      X'02' $VMDPSIDA VMDPXFL1
              .... ...1      $VMDPQDBB      X'01' $VMDPQDBB VMDPXFL1
    001D   29 Bitstring    1 $VMD21
              1... ....      $VMDPESIB      X'80' $VMDPESIB VMDPXFL1
              .1.. ....      $VMDPSIDB      X'40' $VMDPSIDB VMDPXFL1
              ..1. ....      $VMDMAACT      X'20' $VMDMAACT VMDSTORE
              ...1 ....      $VMDESMON      X'10' $VMDESMON VMDSTAT2
              .... 1...      $VMDREOFL      X'08' $VMDREOFL This bit,
                                            formerly in VMDSTMFS, is no
                                            longer used because SET REORDER
                                            can only be specified as OFF.
                                            However, this flag must not be
                                            reused due to compatibility
                                            issues when relocating to
                                            previous releases as described in
                                            the prolog.
              .... .1..      $VMDRLONA      X'04' $VMDRLONA VMDSTRLO
              .... ..1.      $VMDUSECM      X'02' $VMDUSECM VMDSECF
              .... ...1      $VMDUSECP      X'01' $VMDUSECP VMDSECF
    001E   30 Bitstring    1 $VMD22
              1... ....      $VMDUSECA      X'80' $VMDUSECA VMDSECF
              .1.. ....      $VMDPCIUC      X'40' $VMDPCIUC VMDVIOF
              ..1. ....      $VMDMZ         X'20' $VMDMZ VMDMMODE
              ...1 ....      $VMDROPNO      X'10' $VMDROPNO VMDVIOF
              .... 1...      $VMDSHLOV      X'08' $VMDSHLOV VMDSHELD
              .... .1..      $VMDSHLON      X'04' $VMDSHLON VMDSHELD
              1... ....      $VMDQCIR       X'80' $VMDQCIR VMDCFDIR
    001F   31 Bitstring    1 $VMD23
              1... ....      $VMDSTHYU      X'80' $VMDSTHYU VMDSTHYU
              .1.. ....      $VMDSTHYG      X'40' $VMDSTHYG VMDSTHYG
              ..1. ....      $VMDSTHYR      X'20' $VMDSTHYR VMDSTHYR
              ...1 ....      $VMDPRCSM      X'10' $VMDPRCSM VMDTOPT2
              00000018       $VMD_BLEN23    *-$VMD_BITS Length of bit map
                                            area with $VMD23 included.
              00000018       $VMD_BLEN      *-$VMD_BITS Length of bit map
                                            area
          Data:    Contains all HCPVMDBK data that is subject to
                   relocation, except for flag bits, which are
                   handled separately.
                   All fields are defined as XLnn to avoid alignment
                   warnings and to pack the data efficiently.
             ====> NEVER change fields which already exist here.
             ====> NEVER change the order of fields in this section.
             ====> ALWAYS add new fields at the end of this section.
          For the initial release, the fields here appear in the
          same relative order as in the VMDBK.
          Most of the fields listed here are copied as-is to the
          destination system, but some require special processing.
          Such fields are marked with '**' (e.g. see $VMDTODON).
    0020   32 Bitstring    1 $VMD_DATA (0)  Start of data map
    0020   32 Bitstring    8 $VMD_TOD       Effective guest TOD at quiesce
                                            time
    0028   40 Bitstring    4 $VMD_SIE       -> RDO offset to $SIEBK
    002C   44 Bitstring    4 $VMD_PTY       -> RDO offset to proprietary
                                            data
    0030   48 Bitstring    4 $VMD_MDG       -> RDO offset to $MDGBK
    0034   52 Bitstring    4 $VMDBOMBT      -> RDO offset to $TBOMB
    0038   56 Bitstring    4 $VMDCFBUF      -> RDO offset to $GSDBK
    003C   60 Bitstring    4 $VMDOSTAK      -> RDO offset to $GSDBK
    0040   64 Bitstring    4 $VMDTRQDL      -> RDO offset to $ZZZZZ
    0044   68 Bitstring    4 $VMDXTSFI      -> RDO offset to $SFXBK
    0048   72 Bitstring    4 $VMDFIN        -> RDO offset to $FINBK
    004C   76 Bitstring    4 $VMDPPFPT      -> RDO offset to $PPFBK
    0050   80 Bitstring    4 $VMDMCV        -> RDO offset to $MCVBK
    0054   84 Bitstring    4 $VMDSVPBK      -> RDO offset to $SVPBK
    0058   88 Bitstring    4 $VMDPFUNC      -> RDO offset to $PFUNC
    005C   92 Bitstring    4 $VMDPCBUF      -> RDO offset to $PCBUF
    0060   96 Bitstring    4 $VMDPROBK      -> RDO offset to $PROBK
    0064  100 Bitstring    4 $VMDIPLCM      -> RDO offset to $IPLCM
    0068  104 Bitstring    4 $VMDFIDTE      -> RDO offset to $FILENTRY
    006C  108 Bitstring    4 $VMDSSHBK      -> RDO offset to $SHVBK
    0070  112 Bitstring    4 $VMDIPQPT      -> RDO offset to $IPQBK
    0074  116 Bitstring    4 $VMDIUCVB      -> RDO offset to $IUCVB
    0078  120 Bitstring    4 $VMDPXIBK      -> RDO offset to $PXIBK
    007C  124 Bitstring    4 *              No longer used (was $VMDPPFAR)
    0080  128 Bitstring    4 $VMDLLOAD      -> RDO offset to $FCLBK
    0084  132 Bitstring    4 $VMDLDUMP      -> RDO offset to $FCLBK
    0088  136 Bitstring    4 $VMDPDIPL      -> RDO offset to $LDIBK
    008C  140 Bitstring    8 $VMDCPUID      Guest machine CPU ID (for STIDP)
    0094  148 Bitstring    8 $VMDACTID      Accounting user identification
    009C  156 Bitstring    8 $VMDALGID      Userid causing this user's logon
    00A4  164 Bitstring    8 $VMDACTNO      User accounting number
    00AC  172 Bitstring    8 $VMDDIST       User distribution code
    00B4  180 Bitstring    8 $VMDGRPN       RACF ACI group name (This field
                                            is deprecated but left here and
                                            filled in during relocation in
                                            case the destination is a
                                            backlevel CP and requires it
    00BC  188 Bitstring    4 $VMDTODON      ** Session logon TOD, bits 0-31
    00C0  192 Bitstring    8 $VMDATTMP      MT1 value of VMDTTMP at last ACNT
    00C8  200 Bitstring    8 $VMDAVTMP      MT1 value of VMDVTMP at last ACNT
    00D0  208 Bitstring    8 $VMDADIST      Dist field when VMDDIA4C is on
    00D8  216 Bitstring    4 $VMDSIGCT      Count of SIGA instructions
    00DC  220 Bitstring    4 $VMDCCSIO      Count of completed virt i/o
                                            starts
    00E0  224 Bitstring    8 $VMDATTMS      MT1 value of VMDTTMS at last ACNT
    00E8  232 Bitstring    8 $VMDAVTMS      MT1 value of VMDVTMS at last ACNT
    00F0  240 Bitstring    4 $VMDACRDR      Cards read from virtual reader
    00F4  244 Bitstring    4 $VMDACPCH      Cards written to virtual punch
    00F8  248 Bitstring    4 $VMDACPRT      Lines printed on virtual printer
    00FC  252 Bitstring    4 $VMDARSIO      Virtual I/O starts incomplete
    0100  256 Bitstring    4 $VMDACSIO      Virtual I/O starts completed
    0104  260 Bitstring    8 $VMDCOMND      Last CP command executed
    010C  268 Bitstring    1 $VMDCFPND      Console function is pending.
    010D  269 Bitstring    1 $VMDCFPDR      Console function read pending.
    010E  270 Bitstring    4 $VMDCFCPU      ** (CPUAD of) VMDBK to receive
                                            #CP cmds
    0112  274 Bitstring    1 $VMDCMDMC      ACI 'mac' authorized privilege
                                            classes
    0113  275 Bitstring    1 *              Reserved for future use
    0114  276 Bitstring    4 $VMDPCL        Authorised privilege classes
    0118  280 Bitstring    1 $VMDCTPWD      Diagnose LINK password count
    0119  281 Bitstring    2 $VMDCTRAU      #AUTOLOGs w/invalid password
    011B  283 Bitstring    8 $VMDHXID       User who told us to HX
    0123  291 Bitstring   64 $VMDARS        Guest Access Registers
    0163  355 Bitstring  128 $VMDGGRS       Guest General Purpose Registers
    01E3  483 Bitstring  128 $VMDFPRS       Guest Floating Point Registers
    0263  611 Bitstring    1 $VMDPUTYP      CPU type
    0264  612 Bitstring    2 $VMDCPUAD      CPU address of virtual CPU
    0266  614 Bitstring    1 $VMDCPULT      Max MP guest CPU count - 1
    0267  615 Bitstring    1 $VMDRCAPG      Recording-capable-guest flag
    0268  616 Bitstring    8 $VMDGTEID      Translation exception
                                            identification
    0270  624 Bitstring    1 $VMDFEAID      Exception access identification
    0271  625 Bitstring    4 $VMDCPCAA      Guest abs addr of CP comms area
    0275  629 Bitstring    4 $VMDCPCAS      Size of CP communications area in
                                            DW
    0279  633 Bitstring    4 $VMDFPCR       Floating-point control register
    027D  637 Bitstring    8 $VMDXTMFA      Bit mask of vCPUs which have made
                                            malfunction alerts pending on
                                            this virtual CPU
    0285  645 Bitstring    8 $VMDXTEMS      Bit mask of vCPUs which have made
                                            external emergency signals
                                            pending on this virtual CPU.
    028D  653 Bitstring    4 $VMDSFIPM      Software-generated-intrpt enable
                                            mask
    0291  657 Bitstring    2 $VMDMORTM      TERM MORE time intervals
    0293  659 Bitstring    1 $VMDTLEND      The line-end character
    0294  660 Bitstring    1 $VMDTLDEL      The line-delete character
    0295  661 Bitstring    1 $VMDTCDEL      The character-delete character
    0296  662 Bitstring    1 $VMDTESCP      The escape caracter
    0297  663 Bitstring    1 $VMDEXVMO      SCREEN VMOUT
    0298  664 Bitstring    1 $VMDEXINR      SCREEN INREDISP
    0299  665 Bitstring    1 $VMDEXINA      SCREEN INAREA
    029A  666 Bitstring    1 $VMDEXSTA      SCREEN STATAREA
    029B  667 Bitstring    1 $VMDEXCPO      SCREEN CPOUT
    029C  668 Bitstring    1 $VMDTTAB       TERM TAB character
    029D  669 Bitstring    1 $VMDBRKKY      TERM BRKKEY character
    029E  670 Bitstring    8 $VMDIPLNM      IPL'd device number or NSS name
    02A6  678 Bitstring    8 $VMDLDPRM      IPL load parameter (LOADPARM)
    02AE  686 Bitstring    8 $VMDSLAB       Security label for user's VMDBK
                                            (This field is deprecated but
                                            left here and filled in during a
                                            relocation in case the
                                            destination is a backlevel CP and
                                            requires it
    02B6  694 Bitstring    5 $VMDLANG       ** Address of active LANGBK
    02BB  699 Bitstring    8 $VMDSECU       Userid of the secondary user
    02C3  707 Bitstring    1 $VMDCMDAU      ACI audit auth priv classes, byte
                                            0
    02C4  708 Bitstring    1 $VMDCMDPR      ACI protect auth priv classes,
                                            byte 0
    02C5  709 Bitstring   12 $VMDCSQOP      CP command name, SET or QUERY
                                            operand.
    02D1  721 Bitstring    8 $VMDBYVAL      The byuser ID who logged us on
    02D9  729 Bitstring    8 $VMDTTIME      ** MT1 session total CPU time
                                            used
    02E1  737 Bitstring    8 $VMDVTIME      ** MT1 session virtual CPU time
                                            used
    02E9  745 Bitstring    8 $VMDVTZPT      Delta from VMDVTIME for exp-timer
    02F1  753 Bitstring    4 $VMDCTSIO      #virtual I/O starts not in
                                            VMDCCSIO
    02F5  757 Bitstring    4 $VMDCTRDR      #virtual cards read
    02F9  761 Bitstring    4 $VMDCTPCH      #virtual cards punched
    02FD  765 Bitstring    4 $VMDCTPRT      #virtual lines printed
    0301  769 Bitstring    4 $VMDVDISK      #I/Os to a v-disk
    0305  773 Bitstring   16 $VMDSVZPSW     Saved z/architecture PSW
    0315  789 Bitstring    8 $VMDPFXMK      Guest prefix mask
    031D  797 Bitstring    4 $VMDTODAG      Guest address for TOD accounting
    0321  801 Bitstring    4 $VMDCTSPR      Count of spooling page reads
    0325  805 Bitstring    4 $VMDCTSPW      Count of spooling page writes
    0329  809 Bitstring    2 $VMDASMMX      Max non-base addr spaces user may
                                            have
    032B  811 Bitstring    4 $VMDASTMX      Max MB non-base addr spaces usr
                                            may own
    032F  815 Bitstring    2 $VMDACLMX      Max allowed size of user's access
                                            list
    0331  817 Bitstring    8 $VMDVTIMD      Copy of VMDVTIME for 370ACCOM
                                            guest
    0339  825 Bitstring    4 $VMDMXSHR      Guest's max-share, abs or rel
    033D  829 Bitstring    4 $VMDMAXVF      Max sink value for VMCF
    0341  833 Bitstring    4 $VMDPXCAI      POSIX communication area
    0345  837 Bitstring    8 $VMDGPFAUL     Guest real addr of PFAULT token
    034D  845 Bitstring    8 $VMDSELMK      PSW selection mask
    0355  853 Bitstring    8 $VMDCMPMK      PSW comparison mask
    035D  861 Bitstring    8 $VMDTTMP       ** MT1 tot virt&sim time on prim
                                            CPU
    0365  869 Bitstring    8 $VMDVTMP       ** MT1 tot virt time on primary
                                            CPU
    036D  877 Bitstring    8 $VMDTTMS       ** MT1 tot virt&sim time on sec
                                            CPU
    0375  885 Bitstring    8 $VMDVTMS       ** MT1 tot virt time on sec CPU
    037D  893 Bitstring    8 $VMDITRES      Interval timer residue
    0385  901 Bitstring    4 $VMDLKTOT      Count of LINK commands
    0389  905 Bitstring    4 $VMDLKPLX      Count of SSI consults due to LINK
    038D  909 Bitstring    8 $VMDLKTOD      Time spent consulting SSI for
                                            LINK
    0395  917 Bitstring    4 $VMDDTTOT      Count of DETACH commands
    0399  921 Bitstring    4 $VMDDTPLX      Count of SSI consults due to
                                            DETACH
    039D  925 Bitstring    8 $VMDDTTOD      Time spent consulting SSI for
                                            DETACH
    03A5  933 Bitstring    4 $VMDWKTOT      Count of SET WRKALLEG ON commands
    03A9  937 Bitstring    4 $VMDWKPLX      Count of SSI consults due to
                                            WRKALLEG ON
    03AD  941 Bitstring    8 $VMDWKTOD      Time spend consulting SSI for
                                            WRKALLEG ON
    03B5  949 Bitstring    8 $VMDRLOLG      SSI member where guest first
                                            logged on
    03BD  957 Bitstring    8 $VMDEPOCH      TOD difference from original
                                            source sys
    03C5  965 Character    8 $VMDRLODM      Relocation domain name
    03CD  973 Bitstring    4 $VMDARDBK      -> RDO offset to $ARDBK
    03D1  977 Bitstring    2 $VMDALGSL      Slot num of userid that caused
                                            this user to be logged on
    03D3  979 Bitstring    4 $VMDIBM3       CRCBK
    03D7  983 Bitstring    4 $VMDUSER1      Installation use field
    03DB  987 Bitstring    4 $VMDUSER2      Installation use field
    03DF  991 Bitstring    4 $VMDUSER3      Installation use field
    03E3  995 Bitstring    4 $VMDUSER4      Installation use field
    03E7  999 Bitstring    4 $VMDUSER5      Installation use field
    03EB 1003 Bitstring    4 $VMDUSER6      Installation use field
    03EF 1007 Bitstring    4 $VMDUSER7      Installation use field
    03F3 1011 Bitstring    4 $VMDUSER8      Installation use field
    03F7 1015 Bitstring    1 $VMDUSKCK      VMDUSER1-8 elig check skip flags
    03F8 1016 Bitstring    1 $VMDUSRMV      VMDUSER1-8 relocation move flags
          With the MT-2 line item, there are now two sets of books
          which are sent from the source system to the destination
          system.  These two sets of books are in the VMDBK as:
           - VMDxxxxx     = the RAW CPU timer value reported by
                            the hardware.
           - VMDxxxxx_MT1 = the MT-1 equivalent CPU timer value
                            maintained by systems with PFXCBF<>0 &
                            calculated by systems with PFXCBF=0 at
                            relocation time.
          When relocating from a system with 2 sets of books to a
          system with 1 set of books, the MT1 times are to be used
          on the pre-MT system so the fields are sent as follows:
           - The $VMDxxxxx fields listed above will now be set to
             hold the VMDxxxxx_MT1 values instead of the VMDxxxxx
             RAW VALUES that they held previously.
           - The $VMDxxxxx_RAW fields listed below will be used to
             hold the VMDxxxxx RAW values.
           - The original $VMDAxxxx accounting fields will be set to
             their $VMDxxxx values so a pre-MT destination system
             does not double bill in accounting records.  Systems
             with this code will not use any $VMDAxxxx values.
    03F9 1017 Bitstring    8 $VMDTTIME_RAW  Raw session total CPU time used
    0401 1025 Bitstring    8 $VMDVTIME_RAW  Raw session virtual CPU time used
    0409 1033 Bitstring    8 $VMDTTMP_RAW   Raw tot virt&sim time on prim CPU
    0411 1041 Bitstring    8 $VMDVTMP_RAW   Raw tot virt time on primary CPU
    0419 1049 Bitstring    8 $VMDTTMS_RAW   Raw tot virt&sim time on sec CPU
    0421 1057 Bitstring    8 $VMDVTMS_RAW   Raw tot virt time on sec CPU
    0429 1065 Bitstring    4 $VMD_FPV       -> RDO offset to $FPVRB
    042D 1069 Bitstring    2 $VMDVRLEN      Vector register length
    042F 1071 Bitstring    7 $VMDVMACPVC    Guest CPVC
    0436 1078 Bitstring    4 $VMD_OCO2      (v6) -> RDO offset to
                                            secondary OCO data
          Host AP Crypto constants that remain attached to the VMDBK
          for simulation purposes.
    043A 1082 Bitstring    1 $VMDQCINA      Host QCI Na value
    043B 1083 Bitstring    1 $VMDQCIND      Host QCI Nd value
              0000043C       $VMD_LEN       *-$VMDBK Length of mapping block
              00000088       $VMD_SZ        ($VMD_LEN+7)/8 Size of mapping
                                            block

$VMDBK Storage Layout | Top of page

    *** $VMDBK - Relocation mapping for HCPVMDBK
    *
    *     +-------------+-------------+-------------+------+------+
    *   0 | $VMD_HDRL   | $VMD_BITL   |/////////////|(006) |//////|
    *     +------+------+------+------+------+------+------+------+
    *   8 |$VMD0 |$VMD1 |$VMD2 |$VMD3 |$VMD4 |$VMD5 |$VMD6 |$VMD7 |
    *     +------+------+------+------+------+------+------+------+
    *  10 |$VMD8 |$VMD9 |$VMD10|$VMD11|$VMD12|$VMD13|$VMD14|$VMD15|
    *     +------+------+------+------+------+------+------+------+
    *  18 |$VMD16|$VMD17|$VMD18|$VMD19|$VMD20|$VMD21|$VMD22|$VMD23|
    *     +------+------+------+------+------+------+------+------+
    *  20 |                       $VMD_TOD                        |
    *     +---------------------------+---------------------------+
    *  28 |         $VMD_SIE          |         $VMD_PTY          |
    *     +---------------------------+---------------------------+
    *  30 |         $VMD_MDG          |        $VMDBOMBT          |
    *     +---------------------------+---------------------------+
    *  38 |        $VMDCFBUF          |        $VMDOSTAK          |
    *     +---------------------------+---------------------------+
    *  40 |        $VMDTRQDL          |        $VMDXTSFI          |
    *     +---------------------------+---------------------------+
    *  48 |         $VMDFIN           |        $VMDPPFPT          |
    *     +---------------------------+---------------------------+
    *  50 |         $VMDMCV           |        $VMDSVPBK          |
    *     +---------------------------+---------------------------+
    *  58 |        $VMDPFUNC          |        $VMDPCBUF          |
    *     +---------------------------+---------------------------+
    *  60 |        $VMDPROBK          |        $VMDIPLCM          |
    *     +---------------------------+---------------------------+
    *  68 |        $VMDFIDTE          |        $VMDSSHBK          |
    *     +---------------------------+---------------------------+
    *  70 |        $VMDIPQPT          |        $VMDIUCVB          |
    *     +---------------------------+---------------------------+
    *  78 |        $VMDPXIBK          |///////////////////////////|
    *     +---------------------------+---------------------------+
    *  80 |        $VMDLLOAD          |        $VMDLDUMP          |
    *     +---------------------------+---------------------------+
    *  88 |        $VMDPDIPL          |        $VMDCPUID-         |
    *     +---------------------------+---------------------------+
    *  90 |          -(08C)           |        $VMDACTID-         |
    *     +---------------------------+---------------------------+
    *  98 |          -(094)           |        $VMDALGID-         |
    *     +---------------------------+---------------------------+
    *  A0 |          -(09C)           |        $VMDACTNO-         |
    *     +---------------------------+---------------------------+
    *  A8 |          -(0A4)           |        $VMDDIST-          |
    *     +---------------------------+---------------------------+
    *  B0 |          -(0AC)           |        $VMDGRPN-          |
    *     +---------------------------+---------------------------+
    *  B8 |          -(0B4)           |        $VMDTODON          |
    *     +---------------------------+---------------------------+
    *  C0 |                      $VMDATTMP                        |
    *     +-------------------------------------------------------+
    *  C8 |                      $VMDAVTMP                        |
    *     +-------------------------------------------------------+
    *  D0 |                      $VMDADIST                        |
    *     +---------------------------+---------------------------+
    *  D8 |        $VMDSIGCT          |        $VMDCCSIO          |
    *     +---------------------------+---------------------------+
    *  E0 |                      $VMDATTMS                        |
    *     +-------------------------------------------------------+
    *  E8 |                      $VMDAVTMS                        |
    *     +---------------------------+---------------------------+
    *  F0 |        $VMDACRDR          |        $VMDACPCH          |
    *     +---------------------------+---------------------------+
    *  F8 |        $VMDACPRT          |        $VMDARSIO          |
    *     +---------------------------+---------------------------+
    * 100 |        $VMDACSIO          |        $VMDCOMND-         |
    *     +---------------------------+------+------+-------------+
    * 108 |          -(104)           |(10C) |(10D) | $VMDCFCPU-  |
    *     +-------------+------+------+------+------+-------------+
    * 110 |   -(10E)    |(112) |//////|         $VMDPCL           |
    *     +------+------+------+------+---------------------------+
    * 118 |(118) | $VMDCTRAU   |            $VMDHXID-             |
    *     +------+-------------+----------------------------------+
    * 120 |      -(11B)        |                                  |
    *     +--------------------+                                  |
    * 128 |                                                       |
    *     =                       $VMDARS                         =
    *     |                    +----------------------------------+
    *     |                    |                                  |
    *     +--------------------+                                  |
    * 168 |                                                       |
    *     =                       $VMDGGRS                        =
    *     |                    +----------------------------------+
    *     |                    |                                  |
    *     +--------------------+                                  |
    * 1E8 |                                                       |
    *     =                       $VMDFPRS                        =
    *     |                    +------+-------------+------+------+
    * 260 |                    |(263) | $VMDCPUAD   |(266) |(267) |
    *     +--------------------+------+-------------+------+------+
    * 268 |                      $VMDGTEID                        |
    *     +------+---------------------------+--------------------+
    * 270 |(270) |        $VMDCPCAA          |    $VMDCPCAS-      |
    *     +------+---------------------------+--------------------+
    * 278 |-(275)|         $VMDFPCR          |      (27D)-        |
    *     +------+---------------------------+--------------------+
    * 280 |           -$VMDXTMFA             |      (285)-        |
    *     +----------------------------------+--------------------+
    * 288 |           -$VMDXTEMS             |    $VMDSFIPM-      |
    *     +------+-------------+------+------+------+------+------+
    * 290 |-(28D)| $VMDMORTM   |(293) |(294) |(295) |(296) |(297) |
    *     +------+------+------+------+------+------+------+------+
    * 298 |(298) |(299) |(29A) |(29B) |:DTTAB|(29D) |   (29E)-    |
    *     +------+------+------+------+------+------+-------------+
    * 2A0 |               -$VMDIPLNM                |   (2A6)-    |
    *     +-----------------------------------------+-------------+
    * 2A8 |               -$VMDLDPRM                |   (2AE)-    |
    *     +-----------------------------------------+-------------+
    * 2B0 |               -$VMDSLAB                 |   (2B6)-    |
    *     +--------------------+--------------------+-------------+
    * 2B8 |     -$VMDLANG      |            $VMDSECU-             |
    *     +--------------------+------+------+--------------------+
    * 2C0 |      -(2BB)        |(2C3) |(2C4) |                    |
    *     +--------------------+------+------+                    |
    *     |                      $VMDCSQOP                        |
    *     |      +------------------------------------------------+
    *     |      |                  $VMDBYVAL-                    |
    *     +------+------------------------------------------------+
    * 2D8 |-(2D1)|                  $VMDTTIME-                    |
    *     +------+------------------------------------------------+
    * 2E0 |-(2D9)|                  $VMDVTIME-                    |
    *     +------+------------------------------------------------+
    * 2E8 |-(2E1)|                  $VMDVTZPT-                    |
    *     +------+---------------------------+--------------------+
    * 2F0 |-(2E9)|        $VMDCTSIO          |    $VMDCTRDR-      |
    *     +------+---------------------------+--------------------+
    * 2F8 |-(2F5)|        $VMDCTPCH          |    $VMDCTPRT-      |
    *     +------+---------------------------+--------------------+
    * 300 |-(2FD)|        $VMDVDISK          |                    |
    *     +------+---------------------------+                    |
    *     |                      $VMDSVZPSW                       |
    *     |                                  +--------------------+
    *     |                                  |      (315)-        |
    *     +----------------------------------+--------------------+
    * 318 |           -$VMDPFXMK             |    $VMDTODAG-      |
    *     +------+---------------------------+--------------------+
    * 320 |-(31D)|        $VMDCTSPR          |    $VMDCTSPW-      |
    *     +------+-------------+-------------+-------------+------+
    * 328 |-(325)| $VMDASMMX   |        $VMDASTMX          |(32F)-|
    *     +------+-------------+---------------------------+------+
    * 330 |-(32F)|                  $VMDVTIMD-                    |
    *     +------+---------------------------+--------------------+
    * 338 |-(331)|        $VMDMXSHR          |    $VMDMAXVF-      |
    *     +------+---------------------------+--------------------+
    * 340 |-(33D)|        $VMDPXCAI          |      (345)-        |
    *     +------+---------------------------+--------------------+
    * 348 |           -$VMDGPFAUL            |      (34D)-        |
    *     +----------------------------------+--------------------+
    * 350 |           -$VMDSELMK             |      (355)-        |
    *     +----------------------------------+--------------------+
    * 358 |           -$VMDCMPMK             |      (35D)-        |
    *     +----------------------------------+--------------------+
    * 360 |            -$VMDTTMP             |      (365)-        |
    *     +----------------------------------+--------------------+
    * 368 |            -$VMDVTMP             |      (36D)-        |
    *     +----------------------------------+--------------------+
    * 370 |            -$VMDTTMS             |      (375)-        |
    *     +----------------------------------+--------------------+
    * 378 |            -$VMDVTMS             |      (37D)-        |
    *     +----------------------------------+--------------------+
    * 380 |           -$VMDITRES             |    $VMDLKTOT-      |
    *     +------+---------------------------+--------------------+
    * 388 |-(385)|        $VMDLKPLX          |      (38D)-        |
    *     +------+---------------------------+--------------------+
    * 390 |           -$VMDLKTOD             |    $VMDDTTOT-      |
    *     +------+---------------------------+--------------------+
    * 398 |-(395)|        $VMDDTPLX          |      (39D)-        |
    *     +------+---------------------------+--------------------+
    * 3A0 |           -$VMDDTTOD             |    $VMDWKTOT-      |
    *     +------+---------------------------+--------------------+
    * 3A8 |-(3A5)|        $VMDWKPLX          |      (3AD)-        |
    *     +------+---------------------------+--------------------+
    * 3B0 |           -$VMDWKTOD             |      (3B5)-        |
    *     +----------------------------------+--------------------+
    * 3B8 |           -$VMDRLOLG             |      (3BD)-        |
    *     +----------------------------------+--------------------+
    * 3C0 |           -$VMDEPOCH             |      (3C5)-        |
    *     +----------------------------------+--------------------+
    * 3C8 |           -$VMDRLODM             |    $VMDARDBK-      |
    *     +------+-------------+-------------+-------------+------+
    * 3D0 |-(3CD)| $VMDALGSL   |         $VMDIBM3          |(3D7)-|
    *     +------+-------------+---------------------------+------+
    * 3D8 |    -$VMDUSER1      |        $VMDUSER2          |(3DF)-|
    *     +--------------------+---------------------------+------+
    * 3E0 |    -$VMDUSER3      |        $VMDUSER4          |(3E7)-|
    *     +--------------------+---------------------------+------+
    * 3E8 |    -$VMDUSER5      |        $VMDUSER6          |(3EF)-|
    *     +--------------------+---------------------------+------+
    * 3F0 |    -$VMDUSER7      |        $VMDUSER8          |(3F7) |
    *     +------+-------------+---------------------------+------+
    * 3F8 |(3F8) |                $VMDTTIME_RAW-                  |
    *     +------+------------------------------------------------+
    * 400 |-(3F9)|                $VMDVTIME_RAW-                  |
    *     +------+------------------------------------------------+
    * 408 |-(401)|                 $VMDTTMP_RAW-                  |
    *     +------+------------------------------------------------+
    * 410 |-(409)|                 $VMDVTMP_RAW-                  |
    *     +------+------------------------------------------------+
    * 418 |-(411)|                 $VMDTTMS_RAW-                  |
    *     +------+------------------------------------------------+
    * 420 |-(419)|                 $VMDVTMS_RAW-                  |
    *     +------+---------------------------+-------------+------+
    * 428 |-(421)|         $VMD_FPV          | $VMDVRLEN   |(42F)-|
    *     +------+---------------------------+------+------+------+
    * 430 |              -$VMDVMACPVC               | $VMD_OCO2-  |
    *     +-------------+------+------+-------------+-------------+
    * 438 |   -(436)    |(43A) |(43B) | 43C
    *     +-------------+------+------+
    *
    *** $VMDBK - Relocation mapping for HCPVMDBK

$VMDBK Cross Reference | Top of page

    Symbol         Dspl Value
    -------------- ---- -----
    $FULLDATE      0015 40
    $ISODATE       0015 20
    $SDEFAULT      0015 10
    $SHORTDAT      0015 80
    $VMD_BASE      0006 80
    $VMD_BITL      0002
    $VMD_BITS      0008
    $VMD_BLEN      001F 00000018
    $VMD_BLEN23    001F 00000018
    $VMD_DATA      0020
    $VMD_FLGS      0006
    $VMD_FPV       0429
    $VMD_HDLN      0007 00000008
    $VMD_HDRL      0000
    $VMD_HHCR      0006 20
    $VMD_LEN       043B 0000043C
    $VMD_MDG       0030
    $VMD_OCO2      0436
    $VMD_PTY       002C
    $VMD_SIE       0028
    $VMD_SUP       0006 40
    $VMD_SZ        043B 00000088
    $VMD_TOD       0020
    $VMD_VER       0000 00000007
    $VMDACLMX      032F
    $VMDACPCH      00F4
    $VMDACPRT      00F8
    $VMDACRDR      00F0
    $VMDACSIO      0100
    $VMDACTID      0094
    $VMDACTNO      00A4
    $VMDACTRC      0011 02
    $VMDADIST      00D0
    $VMDALGID      009C
    $VMDALGSL      03D1
    $VMDAMDIR      001B 08
    $VMDANYAU      0019 20
    $VMDANYMC      0019 08
    $VMDANYPR      0019 10
    $VMDAPBUF      001B 04
    $VMDAPCR       0014 04
    $VMDAPDED      0014 02
    $VMDAPMS       0014 01
    $VMDARDBK      03CD
    $VMDARS        0123
    $VMDARSIO      00FC
    $VMDASMMX      0329
    $VMDASTMX      032B
    $VMDATTCP      0015 02
    $VMDATTMP      00C0
    $VMDATTMS      00E0
    $VMDAUTCR      0017 08
    $VMDAUTOL      0008 02
    $VMDAVTMP      00C8
    $VMDAVTMS      00E8
    $VMDBOMBA      0009 04
    $VMDBOMBE      0009 02
    $VMDBOMBS      0009 01
    $VMDBOMBT      0034
    $VMDBRKKY      029D
    $VMDBRMIN      0017 10
    $VMDBYVAL      02D1
    $VMDCCSIO      00DC
    $VMDCFBUF      0038
    $VMDCFCPU      010E
    $VMDCFINP      0017 04
    $VMDCFLF       0011 08
    $VMDCFMCE      000A 20
    $VMDCFMCP      000A 40
    $VMDCFPCL      000A 10
    $VMDCFPDR      010D
    $VMDCFPND      010C
    $VMDCFRUN      000A 80
    $VMDCHVSP      001B 10
    $VMDCKPSW      000D 80
    $VMDCKST       0009 20
    $VMDCLEXT      0015 08
    $VMDCMCF       001A 40
    $VMDCMDAU      02C3
    $VMDCMDMC      0112
    $VMDCMDPR      02C4
    $VMDCMESA      0019 02
    $VMDCMLIN      0019 01
    $VMDCMPMK      0355
    $VMDCMSRV      0011 04
    $VMDCMVM       001A 80
    $VMDCOMND      0104
    $VMDCPCAA      0271
    $VMDCPCAS      0275
    $VMDCPCOI      000C 40
    $VMDCPUAD      0264
    $VMDCPUAF      000E 01
    $VMDCPUID      008C
    $VMDCPULT      0266
    $VMDCRHLD      0016 04
    $VMDCRMOR      0016 08
    $VMDCRYPT      0014 40
    $VMDCSQOP      02C5
    $VMDCSRMI      000F 08
    $VMDCTPCH      02F9
    $VMDCTPRT      02FD
    $VMDCTPWD      0118
    $VMDCTRAU      0119
    $VMDCTRDR      02F5
    $VMDCTSIO      02F1
    $VMDCTSPR      0321
    $VMDCTSPW      0325
    $VMDDEVI       0010 02
    $VMDDEVM       0010 01
    $VMDDGNAU      0019 80
    $VMDDGNMC      0019 04
    $VMDDGNPR      0019 40
    $VMDDIA4C      0008 80
    $VMDDIST       00AC
    $VMDDSCWT      0009 10
    $VMDDTPLX      0399
    $VMDDTTOD      039D
    $VMDDTTOT      0395
    $VMDD84NP      0010 08
    $VMDEDIT       0015 04
    $VMDEMSGI      000B 02
    $VMDEPOCH      03BD
    $VMDESMON      001D 10
    $VMDEXCLD      0010 80
    $VMDEXCPO      029B
    $VMDEXINA      0299
    $VMDEXINR      0298
    $VMDEXMCK      000E 80
    $VMDEXSTA      029A
    $VMDEXVMO      0297
    $VMDFAUTO      001A 20
    $VMDFEAID      0270
    $VMDFIDTE      0068
    $VMDFIN        0048
    $VMDFPCR       0279
    $VMDFPRS       01E3
    $VMDGGRS       0163
    $VMDGPFAUL     0345
    $VMDGRPN       00B4
    $VMDGSTCL      0016 20
    $VMDGTEID      0268
    $VMDHLITE      0016 10
    $VMDHXID       011B
    $VMDIAG88      0011 40
    $VMDIAG98      0010 20
    $VMDIBM3       03D3
    $VMDIMSGI      000C 80
    $VMDINTTR      000E 08
    $VMDIPDEV      0017 01
    $VMDIPLCM      0064
    $VMDIPLNM      029E
    $VMDIPLOG      0018 80
    $VMDIPQPT      0070
    $VMDIPSSL      0017 02
    $VMDIPVMI      0018 40
    $VMDITMOF      000E 02
    $VMDITMRI      000E 04
    $VMDITMRL      000E 20
    $VMDITRES      037D
    $VMDIUALL      001B 40
    $VMDIUANY      001B 80
    $VMDIUCVB      0074
    $VMDLANG       02B6
    $VMDLDPRM      02A6
    $VMDLDUMP      0084
    $VMDLIBC       0013 01
    $VMDLKPLX      0389
    $VMDLKTOD      038D
    $VMDLKTOT      0385
    $VMDLLOAD      0080
    $VMDLNKE       000F 01
    $VMDLNKNP      0010 10
    $VMDLNKS       000F 02
    $VMDMAACT      001D 20
    $VMDMAOFF      0012 08
    $VMDMASST      0012 10
    $VMDMAXVF      033D
    $VMDMCCW       0011 80
    $VMDMCNFG      000B 10
    $VMDMCODE      000A 01
    $VMDMCV        0050
    $VMDMESA       0013 20
    $VMDMIMSG      000B 20
    $VMDMONEC      001C 80
    $VMDMONEU      001B 02
    $VMDMONSD      001B 01
    $VMDMONSV      001C 20
    $VMDMONTV      001C 40
    $VMDMORTM      0291
    $VMDMRG32      0012 01
    $VMDMRG64      0013 80
    $VMDMSACS      000C 02
    $VMDMSAVP      000C 04
    $VMDMSGIU      000B 08
    $VMDMSGON      000A 04
    $VMDMSSCS      000C 08
    $VMDMSSVP      000C 10
    $VMDMTEXT      000B 80
    $VMDMXC        0013 40
    $VMDMXSHA      001A 02
    $VMDMXSHR      0339
    $VMDMZ         001E 20
    $VMDM370       0013 10
    $VMDNETA       0008 20
    $VMDNETR       0008 10
    $VMDNHOLD      0016 02
    $VMDNMSHA      001A 01
    $VMDNOAUT      000A 08
    $VMDNOBKY      0016 80
    $VMDNOCTL      0017 40
    $VMDNOFSL      000F 10
    $VMDNOINS      000F 04
    $VMDNOP        001A 10
    $VMDNULLD      0016 01
    $VMDOSTAK      003C
    $VMDPAGEX      0012 80
    $VMDPCBUF      005C
    $VMDPCIUC      001E 40
    $VMDPCL        0114
    $VMDPDCFM      000D 10
    $VMDPDIPL      0088
    $VMDPDIRP      000D 20
    $VMDPDPPF      000C 01
    $VMDPDSIE      000D 08
    $VMDPDTMR      000D 40
    $VMDPDTRD      000D 04
    $VMDPD9CW      000D 02
    $VMDPESIA      001C 04
    $VMDPESIB      001D 80
    $VMDPFIKY      0016 40
    $VMDPFTK2      0012 20
    $VMDPFTOK      0012 40
    $VMDPFUNC      0058
    $VMDPFXMK      0315
    $VMDPPFPT      004C
    $VMDPQDBA      001C 08
    $VMDPQDBB      001C 01
    $VMDPRCSM      001F 10
    $VMDPROAP      0018 04
    $VMDPROBK      0060
    $VMDPROTB      0018 02
    $VMDPSIDA      001C 02
    $VMDPSIDB      001D 40
    $VMDPSWTD      0018 08
    $VMDPSWTS      0018 10
    $VMDPTRQ       000E 40
    $VMDPTRQL      0012 02
    $VMDPTRQQ      0012 04
    $VMDPUTYP      0263
    $VMDPXCAI      0341
    $VMDPXIBK      0078
    $VMDQCINA      043A
    $VMDQCIND      043B
    $VMDQCIR       001E 80
    $VMDQDSPU      001A 08
    $VMDRCAPG      0267
    $VMDREOFL      001D 08
    $VMDRLODM      03C5
    $VMDRLOLG      03B5
    $VMDRLONA      001D 04
    $VMDROPNO      001E 10
    $VMDSECU       02BB
    $VMDSELMK      034D
    $VMDSETOR      0010 04
    $VMDSETXA      0013 08
    $VMDSFIPM      028D
    $VMDSHARE      0010 40
    $VMDSHLON      001E 04
    $VMDSHLOV      001E 08
    $VMDSIGAC      001C 10
    $VMDSIGCT      00D8
    $VMDSKSLP      0009 08
    $VMDSLAB       02AE
    $VMDSLEEP      0009 40
    $VMDSMSGI      000B 01
    $VMDSPMSG      000B 40
    $VMDSSHBK      006C
    $VMDSTAMP      0017 20
    $VMDSTHYG      001F 40
    $VMDSTHYR      001F 20
    $VMDSTHYU      001F 80
    $VMDSTOP       0009 80
    $VMDSTOPD      0008 08
    $VMDSVMST      0011 20
    $VMDSVPBK      0054
    $VMDSVZPSW     0305
    $VMDTCDEL      0295
    $VMDTESCP      0296
    $VMDTLDEL      0294
    $VMDTLEND      0293
    $VMDTLEOV      0017 80
    $VMDTODAG      031D
    $VMDTODON      00BC
    $VMDTRQDL      0040
    $VMDTSTAM      0015 01
    $VMDTTAB       029C
    $VMDTTIME      02D9
    $VMDTTIME_RAW  03F9
    $VMDTTMP       035D
    $VMDTTMP_RAW   0409
    $VMDTTMS       036D
    $VMDTTMS_RAW   0419
    $VMDTZA        0014 80
    $VMDUDST       0008 40
    $VMDUNDSC      0018 20
    $VMDUSECA      001E 80
    $VMDUSECM      001D 02
    $VMDUSECO      0018 01
    $VMDUSECP      001D 01
    $VMDUSER1      03D7
    $VMDUSER2      03DB
    $VMDUSER3      03DF
    $VMDUSER4      03E3
    $VMDUSER5      03E7
    $VMDUSER6      03EB
    $VMDUSER7      03EF
    $VMDUSER8      03F3
    $VMDUSKCK      03F7
    $VMDUSRMV      03F8
    $VMDUTERM      0008 04
    $VMDVAPIN      0014 10
    $VMDVAPXA      0014 20
    $VMDVDISK      0301
    $VMDVERP       0011 10
    $VMDVEXFP      0013 02
    $VMDVMACPVC    042F
    $VMDVMCOI      000C 20
    $VMDVPTRK      000E 10
    $VMDVRLEN      042D
    $VMDVTIMD      0331
    $VMDVTIME      02E1
    $VMDVTIME_RAW  0401
    $VMDVTMP       0365
    $VMDVTMP_RAW   0411
    $VMDVTMS       0375
    $VMDVTMS_RAW   0421
    $VMDVTOD       0011 01
    $VMDVTZPT      02E9
    $VMDVVECT      0014 08
    $VMDWKPLX      03A9
    $VMDWKRUN      001B 20
    $VMDWKTOD      03AD
    $VMDWKTOT      03A5
    $VMDWNGIU      000B 04
    $VMDWNGON      000A 02
    $VMDXAUTO      0008 01
    $VMDXTEMS      0285
    $VMDXTKEY      000D 01
    $VMDXTMFA      027D
    $VMDXTSFI      0044
    $VMD0          0008
    $VMD1          0009
    $VMD10         0012
    $VMD11         0013
    $VMD12         0014
    $VMD13         0015
    $VMD14         0016
    $VMD15         0017
    $VMD16         0018
    $VMD17         0019
    $VMD18         001A
    $VMD19         001B
    $VMD2          000A
    $VMD20         001C
    $VMD21         001D
    $VMD22         001E
    $VMD23         001F
    $VMD3          000B
    $VMD370AC      0013 04
    $VMD4          000C
    $VMD5          000D
    $VMD6          000E
    $VMD7          000F
    $VMD8          0010
    $VMD8FAIL      000F 20
    $VMD8LOCK      000F 80
    $VMD8LOG       000F 40
    $VMD9          0011

This information is based on z/VM 7.2.0 Last updated on 24 Jun 2020 at 09:32:17 EDT.
Copyright IBM Corporation, 1990, 2020