Programming Interface Information: The Monitor Records are intended Programming Interfaces that allow the customer to write programs to obtain services of z/VM.

#### MRSCLADL

Prolog
Control Block Contents
Cross Reference

#### MRSCLADL Prolog

     DSECT NAME - SCLADL
     FUNCTION - Map a Monitor record.
     LOCATED BY -
            Through the Monitor Control Area
     REFERENCED CONTROL BLOCKS -
            MRRECHDR    Monitor Record Header
     NAME - MRSCLADL
     DESCRIPTIVE NAME - Monitor Event Record
                        Domain 2 - Scheduler Domain
                        Record 4 - Add User To Dispatch List
     DESCRIPTION - Indicates conditions after user has been added to
                   dispatch list.  A separate record is generated for
                   each VMDBK in the virtual machine MP complex.
     NOTES:
          - To give a fuller picture of time consumed, three
            sets of used processor time are reported in this
            monitor record.  When multithreading is enabled on
            the system, all three are also reported in the Type
            1 and F accounting records. Timer field names
            ending with _MT1 are MT-1 Equivalent times. Timer
            field names ending with _PRO are Prorated Core
            Times.  Timer field names without an _MT1 or _PRO
            suffix contain Raw Time values.
          - Raw Time is tracked for ALL users for their entire
            session.  Raw Time is the CPU time each virtual CPU
            spent dispatched on a thread and is the CPU Timer
            information provided directly by the hardware.
          - MT-1 Equivalent Time is tracked for ALL users for
            their entire session. This calculated CPU time
            approximates the time that would have been spent
            if the workload had been run with multithreading
            disabled, that is, with all core resources available
            to one thread.  When a user is running on a system
            where multithreading is not installed or not
            enabled, MT-1 Equivalent Time consumed will be
            identical to Raw Time.  However, if a guest has
            relocated from an MT-enabled system to an
            MT-disabled system, the cumulative raw and MT-1
            Equivalent times reported in monitor records may
            differ due to the prior execution in the MT
            environment.
          - Prorated Core Time charges for core utilization in
            a way suitable to core-based software licensing.
            Time is charged by dividing the time the core was
            dispatched evenly among the threads dispatched in
            that interval. Since Prorated Core Time is not
            always calculated, additional information
            is reported regarding the Prorated Core Time values:
            * The _VMAPRCAL bit indicates whether the Prorated
              Core Time values in this record are valid.
            When the user is relocated to any other system
            (even a Multithreading aware/enabled system),
            Prorated Core Time is reset. This means:
            * the _VMAPRCAL bit is set based on whether the
              source system will be calculating prorated core
              time or not.
            * all _VMAxxxxx_PRO fields are reset to PFXTMMAX.

#### MRSCLADL Control Block Contents

    Offsets
    Dec  Hex  Type        Len  Name (Dim)             Description

       0   0  Structure   336  SCLADL                 Start of monitor record
       0   0  Character     0  SCLADL_MRHDR           Record header. See MRRECHDR
                                                      for details.
       0   0  Character    20  MRHDR
       0   0  Unsigned      2  MRHDRLEN
       2   2  Unsigned      2  MRHDRZER
       4   4  Unsigned      1  MRHDRDM
       5   5  Unsigned      1  *
       6   6  Unsigned      2  MRHDRRC
       8   8  Character     8  MRHDRTOD
      16  10  Character     4  *
      20  14  Character     0  MRHDR_END
      20  14  Character     8  SCLADL_VMDUSER         Userid
      28  1C  Unsigned      4  SCLADL_SRMTOTST        Memory available to the
                                                      scheduler to assign to users
                                                      as they enter the dispatch
                                                      list
      32  20  Unsigned      4  SCLADL_SRMWSSDL        Accumulated count of all
                                                      dispatch list users' working
                                                      set sizes. This is an
                                                      instantaneous (not a
                                                      smoothed) value.
      36  24  Unsigned      2  SCLADL_SRMCDISP        Cardinal count of users in
                                                      the dispatch list.
      38  26  Unsigned      2  SCLADL_SRMC1DSP        Cardinal count of short,
                                                      medium, and long running
                                                      users in the dispatch list.
      40  28  Unsigned      2  SCLADL_SRMC2DSP        Cardinal count of medium
                                                      and long running users in the
                                                      dispatch list. This includes
                                                      all Q2 and Q3 users. It
                                                      includes no Q1 or Q0 users.
      42  2A  Unsigned      2  SCLADL_SRMC3DSP        Cardinal count of long
                                                      running users in the dispatch
                                                      list. It includes all Q3
                                                      users. It includes no Q1, Q2,
                                                      or Q0 users.
      44  2C  Character     8  SCLADL_VMDSVMID        VMDBK name for the last
                                                      successful IUCV, VMCF or
                                                      APPC/VM Send for this virtual
                                                      machine. Valid in base VMDBK
                                                      only.
      52  34  Bitstring     1  SCLADL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLADL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF or
                                                      APPC.
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      53  35  Character     0  SCLADL_VMDSVMW2        back-up byte to the
                                                      VMDSVMWT byte. Its contents
                                                      will persist longer than they
                                                      would in VMDSVMWT. Valid in
                                                      base VMDBK only.
      53  35  Bitstring     1  SCLADL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLADL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF or
                                                      APPC.
      54  36  Character     0  SCLADL_VMDRDYCM        Flag byte set by IUCV,
                                                      VMCF, or APPC whenever
                                                      IUCV/VMCF/APPC makes an
                                                      external interrupt pending in
                                                      a virtual machine. It is sort
                                                      of a "reference bit" that
                                                      tells the scheduler that
                                                      IUCV/VMCF/APPC has been
                                                      active recently. Valid in
                                                      base VMDBK only.
      54  36  Bitstring     1  SCLADL_VMDSVMWT        Service-virtual-machine
                                                      (SVM) wait flag - valid in
                                                      base VMDBK only.
              1... ....        SCLADL_VMDSVMWF         VMDBK is waiting for a
                                                      response from IUCV, VMCF or
                                                      APPC.
      55  37  Bitstring     1  SCLADL_CALFLAG1        Flag byte
              1... ....        SCLADL_CALBASE          If on, this is base VMDBK.
                                                      VMDBASE
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
      56  38  Unsigned      4  SCLADL_VMDWSSPR        This user's projected
                                                      working set size. This is the
                                                      scheduler's estimate of the
                                                      amount of storage this user
                                                      will require to be resident
                                                      as it runs during its next
                                                      stay in the dispatch list. It
                                                      is based upon the user's past
                                                      behavior, and in some cases,
                                                      on the behavior of similar
                                                      types of users.
      60  3C  Unsigned      4  SCLADL_VMDPGRTE        Number of pages per second
                                                      which this user read in
                                                      during its last stay in the
                                                      dispatch list
      64  40  Bitstring     1  SCLADL_CALQSTAT        Scheduling status of user
              1... ....        SCLADL_VMDHOTRQ         Hot Shot scheduling
                                                      requested
              .1.. ....        SCLADL_VMDHOTST         Hot Shot user scheduling
                                                      granted
              ..1. ....        SCLADL_VMDLOADU         Loading user designation
              ...1 ....        SCLADL_VMDIABIA         Interactive bias is in
                                                      effect
              .... 1...        *
              .... .1..        SCLADL_VMDLKSHT         "Lockshot" scheduling in
                                                      effect for this user. Set
                                                      only in the base VMDBK.
              .... ..1.        *
              .... ...1        SCLADL_VMDNULL          User is logging off
      65  41  Unsigned      1  SCLADL_VMDELIST        This user's dispatch list
                                                      class. It can be 0, 1, 2, or
                                                      3. Class 1-3 relate to the
                                                      time this (scheduler
                                                      determined) transaction has
                                                      been running. Class 1 are
                                                      short-running, class 2,
                                                      medium-running and class 3,
                                                      long-running.
      66  42  Unsigned      2  SCLADL_VMDCPUAD        Virtual processor address
      68  44  Unsigned      4  SCLADL_VMDRPLIM        Resident page growth limit
      72  48  Unsigned      4  SCLADL_VMDCTPVR        Cardinal count of resident
                                                      pages in private address
                                                      spaces belonging to this
                                                      user. This monitor field is
                                                      actually the sum of VMDCTPVR
                                                      + VMDCTPVG which is the
                                                      resident pages above and
                                                      below the 2GB line. To get
                                                      the count of resident pages
                                                      below the 2GB line, subtract
                                                      SCLADL_VMDCTPVG from
                                                      SCLADL_VMDCTPVR.
      76  4C  Character     8  SCLADL_VMDVTIME        Total Raw Time that this
                                                      user was running, doing
                                                      productive work. It does not
                                                      include any time that CP
                                                      spends on behalf of that user
                                                      doing such things as
                                                      instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format. The
                                                      complement of SCLADL_VMDVTIME
                                                      is the accumulated time in
                                                      TOD clock units.
      84  54  Character     8  SCLADL_VMDTTIME        Total Raw Time which has
                                                      been expended on this VMDBK.
                                                      This includes time which the
                                                      VMDBK spent doing its own
                                                      work and also time which CP
                                                      spent doing work on behalf of
                                                      the VMDBK. It is in CPU timer
                                                      format. The complement of
                                                      SCLADL_VMDTTIME is the
                                                      elapsed time in TOD clock
                                                      units.
      92  5C  Character     8  SCLADL_VMDEPRTY        The eligible list priority,
                                                      in TOD clock units. This is
                                                      the the scheduler's estimate
                                                      of the latest time this VMDBK
                                                      should be selected to go into
                                                      the dispatch list from the
                                                      eligible list. It is used to
                                                      order users in the eligible
                                                      list.
     100  64  Character     8  SCLADL_VMDDPRTY        The user's dispatch list
                                                      priority. This is based upon
                                                      the user's SHARE, its time
                                                      spent in the eligible list
                                                      and SHARES of all other
                                                      dispatch list users. It is
                                                      then adjusted by such factors
                                                      as interactive bias, paging
                                                      bias and limits on how large
                                                      or small this priority is
                                                      allowed to be. It represents
                                                      the relative order in which
                                                      this user will be selected to
                                                      be dispatched.
     108  6C  Character     8  SCLADL_VMDOPRTY        This user's dispatch
                                                      priority before adjustment
                                                      factors such as interactive
                                                      bias and paging bias
     116  74  Unsigned      4  SCLADL_VMDRTHRU        This user's 'required
                                                      throughput' or 'resource
                                                      access' in the dispatch list
     120  78  Unsigned      4  *                      Reserved for IBM use - was
                                                      SCLADL_VMDCTXBK
     124  7C  Unsigned      4  *                      Reserved for IBM used - was
                                                      SCLADL_VMDFLREO
     128  80  Unsigned      4  *                      Reserved for IBM use - was
                                                      SCLADL_VMDCTORF
     132  84  Unsigned      4  SCLADL_CALCPPST        Cumulative count of pages
                                                      reclaimed from this user's
                                                      addr spaces while they were
                                                      private.
     136  88  Bitstring     1  SCLADL_CALOSTAT        Virtual machine operating
                                                      status
              1... ....        SCLADL_VMDSYSOP         User is primary system
                                                      operator
              .1.. ....        SCLADL_VMDUSRCT         User is counted as being
                                                      logged on
              ..1. ....        *
              ...1 ....        SCLADL_VMDFORCE         User is to be logged off.
                                                      This may be requested by CP,
                                                      a forced logoff, or user's
                                                      logoff command.
              .... 1...        SCLADL_VMDUFORC         User is forced to logoff
                                                      the system
              .... .1..        SCLADL_VMDDISC          User is running
                                                      disconnected
              .... ..1.        SCLADL_VMDAUTOL         AUTOLOG/XAUTOLOG in
                                                      progress. User has been
                                                      automatically logged on. This
                                                      bit is set off when the
                                                      user's IPL statement is
                                                      processed, or (if there is no
                                                      IPL to process) when the user
                                                      enters a LOGON command from a
                                                      terminal to RECONNECT.
              .... ...1        SCLADL_VMDXAUTO         The original command was
                                                      XAUTOLOG. Valid for the base
                                                      VMDBK only.
     137  89  Bitstring     1  SCLADL_CALSHARF        Set Share flags
              1... ....        SCLADL_VMDMXSHA         Max share is Absolute if
                                                      ON. Max share is Relative if
                                                      OFF.
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        SCLADL_VMDLIMTH         Max Share is Limithard if
                                                      ON. Max Share is Limitsoft if
                                                      OFF.
              .... ...1        *
     138  8A  Signed        2  SCLADL_VMDSLCNT        Count of minor time slices
                                                      that have expired since the
                                                      start of current transaction.
     140  8C  Character     8  SCLADL_VMDESLIC        The elapsed time slice this
                                                      user will receive in the
                                                      dispatch list before having
                                                      to return to the eligible
                                                      list.
     148  94  Unsigned      4  SCLADL_VMDRELSH        This virtual CPU's RELATIVE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Set to zero when this VMDBK
                                                      has an ABSOLUTE share value,
                                                      or has a virtual processor
                                                      dedicated to it, or is in the
                                                      process of being logged off.
     152  98  Unsigned      4  SCLADL_VMDABSSH        This virtual CPU's ABSOLUTE
                                                      share of the system, as set
                                                      in the user's directory or
                                                      via the SET SHARE command.
                                                      Unit of value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Set to zero when this VMDBK
                                                      has a RELATIVE share value.
     156  9C  Unsigned      4  SCLADL_VMDVUSCT        Cumulative count of virtual
                                                      SSCH requests to
                                                      virtual unit record devices
     160  A0  Signed        4  SCLADL_SRMABSDL        Cardinal count of total
                                                      absolute shares of all VMDBKs
                                                      in the dispatch list. The
                                                      unit of value is the same as
                                                      SCLADL_VMDABSSH. Applies to
                                                      real primary processor on
                                                      which user is dispatched.
     164  A4  Signed        4  SCLADL_SRMRELDL        Cardinal count of total
                                                      relative shares of all VMDBKs
                                                      in the dispatch list. Applies
                                                      to real primary processor on
                                                      which user is dispatched.
     168  A8  Unsigned      4  SCLADL_VMDCTCRT        Count of CP
                                                      critical-processes this VMDBK
                                                      is responsible for. VMDBK
                                                      must not wait in eligible
                                                      list while this count is
                                                      greater than 0. Valid only in
                                                      base VMDBK.
     172  AC  Unsigned      4  SCLADL_VMDMXSHR        The virtual CPU's max share
                                                      of the system, as set in the
                                                      user's directory or via the
                                                      SET SHARE command. This value
                                                      is set to zero if no Max
                                                      share exists. If the Max
                                                      share is Absolute, then the
                                                      unit of the value is a
                                                      hexadecimal factor scaled 16
                                                      bits. For example,
                                                      X'00010000' = 1.00(100%),
                                                      X'0000C000' = 0.75(75%),
                                                      X'00008000' = 0.50(50%), etc.
                                                      Check SCLADL_VMDMXSHA to
                                                      determine if Max share is
                                                      absolute or relative.
     176  B0  Character     8  SCLADL_SRMATOD         Artificial TOD. This TOD
                                                      only advances at the rate the
                                                      system is running user work.
                                                      Applies to real primary
                                                      processor on which user is
                                                      dispatched.
     184  B8  Character     8  SCLADL_SRMATOD2        Artificial TOD2. This TOD
                                                      only advances with each CPU's
                                                      user time and each CPU's wait
                                                      time. Applies to real primary
                                                      processor on which user is
                                                      dispatched.
     192  C0  Unsigned      4  SCLADL_VMDCTPVG        Count of private address
                                                      space resident pages in DPA
                                                      owned by this virtual machine
                                                      which are above the 2GB line.
                                                      Valid only in base VMDBK. To
                                                      get total resident pages
                                                      under the 2GB line, subtract
                                                      this field from
                                                      SCLADL_VMDCTPVR.
     196  C4  Bitstring     1  SCLADL_VMDCFGEM        Virtual configuration
                                                      indicators. Valid in base
                                                      VMDBK only
              1... ....        *
              .1.. ....        SCLADL_VMDCPUAF         User requested CPU
                                                      Affinity
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     197  C5  Bitstring     1  SCLADL_VMDPUST         CPU Status flag
              1... ....        SCLADL_VMDAFSUP         CPU Affinity suppressed
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     198  C6  Character     2  *                      Reserved for IBM use
     200  C8  Character     8  SCLADL_VMDVTMP         Total raw virtual time for
                                                      the user on primary
                                                      processor.
     208  D0  Character     8  SCLADL_VMDTTMP         Total raw virtual and
                                                      simulation time for the user
                                                      on primary processor.
     216  D8  Character     8  SCLADL_VMDVTMS         Total raw virtual time for
                                                      the user on secondary
                                                      processor.
     224  E0  Character     8  SCLADL_VMDTTMS         Total raw virtual and
                                                      simulation time for the user
                                                      on secondary processor.
     232  E8  Character     8  SCLADL_VMDTTIME_MT1    Total MT-1 Equivalent time
                                                      which has been expended on
                                                      this VMDBK. This includes
                                                      time which the VMDBK spent
                                                      doing its own work and also
                                                      time which CP spent doing
                                                      work on behalf of the VMDBK.
                                                      It is in CPU timer format.
     240  F0  Character     8  SCLADL_VMDVTIME_MT1    Total MT-1 Equivalent time
                                                      that this user was running
                                                      and doing productive work. It
                                                      does NOT include any time
                                                      that CP spends on behalf of
                                                      that user doing such things
                                                      as instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format.
     248  F8  Character     8  SCLADL_VMDVTMP_MT1     MT-1 Equivalent virtual
                                                      time for the user on primary
                                                      processor
     256 100  Character     8  SCLADL_VMDTTMP_MT1     MT-1 Equivalent total
                                                      virtual and simulation time
                                                      for the user on primary
                                                      processor.
     264 108  Character     8  SCLADL_VMDVTMS_MT1     MT-1 Equivalent total
                                                      virtual time for the user on
                                                      secondary processor.
     272 110  Character     8  SCLADL_VMDTTMS_MT1     MT-1 Equivalent total
                                                      virtual and simulation time
                                                      for the user on secondary
                                                      processor.
     280 118  Character     8  SCLADL_VMATTIME_PRO    Total Prorated Core Time
                                                      which has been expended on
                                                      this VMDBK. This includes
                                                      time which the VMDBK spent
                                                      doing its own work and also
                                                      time which CP spent doing
                                                      work on behalf of the VMDBK.
                                                      It is in CPU timer format.
                                                      See the notes above.
     288 120  Character     8  SCLADL_VMAVTIME_PRO    Total Prorated Core Time
                                                      that this user was running
                                                      and doing productive work. It
                                                      does NOT include any time
                                                      that CP spends on behalf of
                                                      that user doing such things
                                                      as instruction simulation or
                                                      page translation. This is in
                                                      CPU timer format. See the
                                                      notes above.
     296 128  Character     8  SCLADL_VMAVTMP_PRO     Total Prorated Core virtual
                                                      time for user on primary
                                                      processor. See the notes
                                                      above.
     304 130  Character     8  SCLADL_VMATTMP_PRO     Total Prorated Core virtual
                                                      and simulation time for the
                                                      user on primary processor.
                                                      See the notes above.
     312 138  Character     8  SCLADL_VMAVTMS_PRO     Total Prorated Core virtual
                                                      time for user on secondary
                                                      processor. See the notes
                                                      above.
     320 140  Character     8  SCLADL_VMATTMS_PRO     Total Prorated Core virtual
                                                      and simulation time for the
                                                      user on secondary processor.
                                                      See the notes above.
     328 148  Unsigned      4  *                      Reserved for IBM use
     332 14C  Bitstring     1  SCLADL_PROBITS         Prorated Core Time bits
                                                      needed to understand those
                                                      fields.
              1... ....        SCLADL_VMAPRCAL         Indicates whether the
                                                      Prorated Core Time values in
                                                      this record are valid (only
                                                      use if valid): 0 = values not
                                                      valid 1 = values are valid
              .1.. ....        *
              ..1. ....        *
              ...1 ....        *
              .... 1...        *
              .... .1..        *
              .... ..1.        *
              .... ...1        *
     333 14D  Bitstring     1  *                      Reserved for IBM use
     334 14E  Unsigned      2  *                      Reserved for IBM use
     336 150  Character     0  SCLADL_END

#### MRSCLADL Cross Reference

                          Hex           Hex
    Name                  Offset Length Value

    MRHDR                      0     20
    MRHDR_END                 14      0
    MRHDRDM                    4      1
    MRHDRLEN                   0      2
    MRHDRRC                    6      2
    MRHDRTOD                   8      8
    MRHDRZER                   2      2
    SCLADL                     0    336
    SCLADL_CALBASE            37           80
    SCLADL_CALCPPST           84      4
    SCLADL_CALFLAG1           37      1
    SCLADL_CALOSTAT           88      1
    SCLADL_CALQSTAT           40      1
    SCLADL_CALSHARF           89      1
    SCLADL_END               150      0
    SCLADL_MRHDR               0      0
    SCLADL_PROBITS           14C      1
    SCLADL_SRMABSDL           A0      4
    SCLADL_SRMATOD            B0      8
    SCLADL_SRMATOD2           B8      8
    SCLADL_SRMCDISP           24      2
    SCLADL_SRMC1DSP           26      2
    SCLADL_SRMC2DSP           28      2
    SCLADL_SRMC3DSP           2A      2
    SCLADL_SRMRELDL           A4      4
    SCLADL_SRMTOTST           1C      4
    SCLADL_SRMWSSDL           20      4
    SCLADL_VMAPRCAL          14C           80
    SCLADL_VMATTIME_PRO      118      8
    SCLADL_VMATTMP_PRO       130      8
    SCLADL_VMATTMS_PRO       140      8
    SCLADL_VMAVTIME_PRO      120      8
    SCLADL_VMAVTMP_PRO       128      8
    SCLADL_VMAVTMS_PRO       138      8
    SCLADL_VMDABSSH           98      4
    SCLADL_VMDAFSUP           C5           80
    SCLADL_VMDAUTOL           88           02
    SCLADL_VMDCFGEM           C4      1
    SCLADL_VMDCPUAD           42      2
    SCLADL_VMDCPUAF           C4           40
    SCLADL_VMDCTCRT           A8      4
    SCLADL_VMDCTPVG           C0      4
    SCLADL_VMDCTPVR           48      4
    SCLADL_VMDDISC            88           04
    SCLADL_VMDDPRTY           64      8
    SCLADL_VMDELIST           41      1
    SCLADL_VMDEPRTY           5C      8
    SCLADL_VMDESLIC           8C      8
    SCLADL_VMDFORCE           88           10
    SCLADL_VMDHOTRQ           40           80
    SCLADL_VMDHOTST           40           40
    SCLADL_VMDIABIA           40           10
    SCLADL_VMDLIMTH           89           02
    SCLADL_VMDLKSHT           40           04
    SCLADL_VMDLOADU           40           20
    SCLADL_VMDMXSHA           89           80
    SCLADL_VMDMXSHR           AC      4
    SCLADL_VMDNULL            40           01
    SCLADL_VMDOPRTY           6C      8
    SCLADL_VMDPGRTE           3C      4
    SCLADL_VMDPUST            C5      1
    SCLADL_VMDRDYCM           36      0
    SCLADL_VMDRELSH           94      4
    SCLADL_VMDRPLIM           44      4
    SCLADL_VMDRTHRU           74      4
    SCLADL_VMDSLCNT           8A      2
    SCLADL_VMDSVMID           2C      8
    SCLADL_VMDSVMWF           34           80
    SCLADL_VMDSVMWF           35           80
    SCLADL_VMDSVMWF           36           80
    SCLADL_VMDSVMWT           34      1
    SCLADL_VMDSVMWT           35      1
    SCLADL_VMDSVMWT           36      1
    SCLADL_VMDSVMW2           35      0
    SCLADL_VMDSYSOP           88           80
    SCLADL_VMDTTIME           54      8
    SCLADL_VMDTTIME_MT1       E8      8
    SCLADL_VMDTTMP            D0      8
    SCLADL_VMDTTMP_MT1       100      8
    SCLADL_VMDTTMS            E0      8
    SCLADL_VMDTTMS_MT1       110      8
    SCLADL_VMDUFORC           88           08
    SCLADL_VMDUSER            14      8
    SCLADL_VMDUSRCT           88           40
    SCLADL_VMDVTIME           4C      8
    SCLADL_VMDVTIME_MT1       F0      8
    SCLADL_VMDVTMP            C8      8
    SCLADL_VMDVTMP_MT1        F8      8
    SCLADL_VMDVTMS            D8      8
    SCLADL_VMDVTMS_MT1       108      8
    SCLADL_VMDVUSCT           9C      4
    SCLADL_VMDWSSPR           38      4
    SCLADL_VMDXAUTO           88           01

    This information is
    based on z/VM V7R2.0.

    Last updated on 08 August 2020 at 16:07:13.

    Copyright IBM Corporation, 1990, 2020